|  | 4.2 |
| Signals and Noise
|  | 4.2.7 |
| Time-based parameters
Propagation delay is a simple measurement of how long it takes for a signal to travel along the cable being tested. The delay in a wire pair depends on its length, twist rate, and electrical properties. Delays are measured in hundredths of nanoseconds. One nanosecond is one-billionth of a second, or 0.000000001 second. The TIA/EIA-568-B standard sets a limit for propagation delay for the various categories of UTP. Propagation delay measurements are the basis of the cable length measurement. TIA/EIA-568-B-1 specifies that the physical length of the link shall be calculated using the wire pair with the shortest electrical delay. Testers measure the length of the wire based on the electrical delay as measured by a Time Domain Reflectometry (TDR) test, not by the physical length of the cable jacket. Since the wires inside the cable are twisted, signals actually travel farther than the physical length of the cable. When a cable tester makes a TDR measurement, it sends a pulse signal down a wire pair and measures the amount of time required for the pulse to return on the same wire pair. The TDR test is used not only to determine length, but also to identify the distance to wiring faults such as shorts and opens. When the pulse encounters an open, short, or poor connection, all or part of the pulse energy is reflected back to the tester. This can calculate the approximate distance to the wiring fault. The approximate distance can be helpful in locating a faulty connection point along a cable run, such as a wall jack. The propagation delays of different wire pairs in a single cable can differ slightly because of differences in the number of twists and electrical properties of each wire pair. The delay difference between pairs is called delay skew. Delay skew is a critical parameter for high-speed networks in which data is simultaneously transmitted over multiple wire pairs, such as 1000BASE-T Ethernet. If the delay skew between the pairs is too great, the bits arrive at different times and the data cannot be properly reassembled. Even though a cable link may not be intended for this type of data transmission, testing for delay skew helps ensure that the link will support future upgrades to high-speed networks. All cable links in a LAN must pass all of the tests previously mentioned as specified in the TIA/EIA-568-B standard. These tests ensure that the cable links will function reliably at high speeds and frequencies. Cable tests should be performed when the cable is installed and afterward on a regular basis to ensure that LAN cabling meets industry standards. High quality cable test instruments should be correctly used to ensure that the tests are accurate. Test results should also be carefully documented.
Web Links
Computer Basics http://www.cabletesting.com/CableTesting/ default.htm