|  | 3.2 |
| Optical Media
|  | 3.2.7 |
| Single-mode fiber
Single-mode fiber consists of the same parts as multimode. The outer jacket of single-mode fiber is usually yellow. The major difference between multimode and single-mode fiber is that single-mode allows only one mode of light to propagate through the smaller, fiber-optic core. The single-mode core is eight to ten microns in diameter. Nine-micron cores are the most common. A 9/125 marking on the jacket of the single-mode fiber indicates that the core fiber has a diameter of 9 microns and the surrounding cladding is 125 microns in diameter. An infrared laser is used as the light source in single-mode fiber. The ray of light it generates enters the core at a 90-degree angle. As a result, the data carrying light ray pulses in single-mode fiber are essentially transmitted in a straight line right down the middle of the core. This greatly increases both the speed and the distance that data can be transmitted. Because of its design, single-mode fiber is capable of higher rates of data transmission (bandwidth) and greater cable run distances than multimode fiber. Single-mode fiber can carry LAN data up to 3000 meters. Multimode is only capable of carrying up to 2000 meters. Lasers and single-mode fibers are more expensive than LEDs and multimode fiber. Because of these characteristics, single-mode fiber is often used for inter-building connectivity.
WARNING: The laser light used with single-mode has a longer wavelength than can be seen. The laser is so strong that it can seriously damage eyes. Never look at the near end of a fiber that is connected to a device at the far end. Never look into the transmit port on a NIC, switch, or router. Remember to keep protective covers over the ends of fiber and inserted into the fiber-optic ports of switches and routers. Be very careful.
Figure compares the relative sizes of the core and cladding for both types of fiber optic in different sectional views. The much smaller and more refined fiber core in single-mode fiber is the reason single-mode has a higher bandwidth and cable run distance than multimode fiber. However, it entails more manufacturing costs.
Web Links
Single Mode Fiber http://searchnetworking.techtarget.com/ sDefinition/0,,sid7_ gci212992,00.htm