|  | 6.2 |
| Ethernet Operation
|  | 6.2.5 |
| Error handling
The most common error condition on an Ethernet is the collision. Collisions are the mechanism for resolving contention for network access. A few collisions provide a smooth, simple, low overhead way for network nodes to arbitrate contention for the network resource. When network contention becomes too great, collisions can become a significant impediment to useful network operation. Collisions result in network bandwidth loss that is equal to the initial transmission and the collision jam signal. This is consumption delay and affects all network nodes possibly causing significant reduction in network throughput. The considerable majority of collisions occur very early in the frame, often before the SFD. Collisions occurring before the SFD are usually not reported to the higher layers, as if the collision did not occur. As soon as a collision is detected, the sending stations transmit a 32-bit “jam” signal that will enforce the collision. This is done so that any data being transmitted is thoroughly corrupted and all stations have a chance to detect the collision. In Figure two stations listen to ensure that the cable is idle, then transmit. Station 1 was able to transmit a significant percentage of the frame before the signal even reached the last cable segment. Station 2 had not received the first bit of the transmission prior to beginning its own transmission and was only able to send several bits before the NIC sensed the collision. Station 2 immediately truncated the current transmission, substituted the 32-bit jam signal and ceased all transmissions. During the collision and jam event that Station 2 was experiencing, the collision fragments were working their way back through the repeated collision domain toward Station 1. Station 2 completed transmission of the 32-bit jam signal and became silent before the collision propagated back to Station 1 which was still unaware of the collision and continued to transmit. When the collision fragments finally reached Station 1, it also truncated the current transmission and substituted a 32-bit jam signal in place of the remainder of the frame it was transmitting. Upon sending the 32-bit jam signal Station 1 ceased all transmissions. A jam signal may be composed of any binary data so long as it does not form a proper checksum for the portion of the frame already transmitted. The most commonly observed data pattern for a jam signal is simply a repeating one, zero, one, zero pattern, the same as Preamble. When viewed by a protocol analyzer this pattern appears as either a repeating hexadecimal 5 or A sequence. The corrupted, partially transmitted messages are often referred to as collision fragments or runts. Normal collisions are less than 64 octets in length and therefore fail both the minimum length test and the FCS checksum test.
Web Links
Error Handling http://www.usyd.edu.au/is/comms/networkcourse/ USydNet_mod3_ ethernet.html#tocDuplex