|  | 3.3 |
| Wireless Media
|  | 3.3.5 |
| The radiowave and microwave spectrums
Computers send data signals electronically. Radio transmitters convert these electrical signals to radio waves. Changing electric currents in the antenna of a transmitter generates the radio waves. These radio waves radiate out in straight lines from the antenna. However, radio waves attenuate as they move out from the transmitting antenna. In a WLAN, a radio signal measured at a distance of just 10 meters (30 feet) from the transmitting antenna would be only 1/100th of its original strength. Like light, radio waves can be absorbed by some materials and reflected by others. When passing from one material, like air, into another material, like a plaster wall, radio waves are refracted. Radio waves are also scattered and absorbed by water droplets in the air. These qualities of radio waves are important to remember when a WLAN is being planned for a building or for a campus. The process of evaluating a location for the installation of a WLAN is called making a Site Survey. Because radio signals weaken as they travel away from the transmitter, the receiver must also be equipped with an antenna. When radio waves hit the antenna of a receiver, weak electric currents are generated in that antenna. These electric currents, caused by the received radio waves, are equal to the currents that originally generated the radio waves in the antenna of the transmitter. The receiver amplifies the strength of these weak electrical signals. In a transmitter, the electrical (data) signals from a computer or a LAN are not sent directly into the antenna of the transmitter. Rather, these data signals are used to alter a second, strong signal called the carrier signal. The process of altering the carrier signal that will enter the antenna of the transmitter is called modulation. There are three basic ways in which a radio carrier signal can be modulated. For example, Amplitude Modulated (AM) radio stations modulate the height (amplitude) of the carrier signal. Frequency Modulated (FM) radio stations modulate the frequency of the carrier signal as determined by the electrical signal from the microphone. In WLANs, a third type of modulation called phase modulation is used to superimpose the data signal onto the carrier signal that is broadcast by the transmitter. In this type of modulation, the data bits in the electrical signal change the phase of the carrier signal. A receiver demodulates the carrier signal that arrives from its antenna. The receiver interprets the phase changes of the carrier signal and reconstructs from it the original electrical data signal.
|  | Interactive Media Activity
Point and Click: Electromagnetic Fields and Polarization This activity includes a series of animated, graphical explanations of EM fields and polarization. Interactive Media Activity 3.3.5a is located in the CCNA 3.0 Bridge 1 Activities and Quizzes file. The Activities and Quizzes file can be downloaded in the Course Material section of your class homepage.
|  | Interactive Media Activity
Interactivity: Electromagnetic Spectrum This activity allows you to scroll through the EM spectrum by moving your mouse to the left or right over the graphic. Interactive Media Activity 3.3.5b is located in the CCNA 3.0 Bridge 1 Activities and Quizzes file. The Activities and Quizzes file can be downloaded in the Course Material section of your class homepage.
Web Links
The Electromagnetic (RF) Spectrum http://www.sss-mag.com/spectrum.html