|  | 3.3 |
| Wireless Media
|  | 3.3.1 |
| Wireless LAN organizations and standards
An understanding of the regulations and standards that apply to wireless technology will ensure that deployed networks will be interoperable and in compliance. Just as in cabled networks, IEEE is the prime issuer of standards for wireless networks. The standards have been created within the framework of the regulations created by the Federal Communications Commission (FCC). A key technology contained within the 802.11 standard is Direct Sequence Spread Spectrum (DSSS). DSSS applies to wireless devices operating within a 1 to 2 Mbps range. A DSSS system may operate at up to 11 Mbps but will not be considered compliant above 2 Mbps. The next standard approved was 802.11b, which increased transmission capabilities to 11 Mbps. Even though DSSS WLANs were able to interoperate with the Frequency Hopping Spread Spectrum (FHSS) WLANs, problems developed prompting design changes by the manufacturers. In this case, IEEE’s task was simply to create a standard that matched the manufacturer’s solution. 802.11b may also be called Wi-Fi™ or high-speed wireless and refers to DSSS systems that operate at 1, 2, 5.5 and 11 Mbps. All 802.11b systems are backward compliant in that they also support 802.11 for 1 and 2 Mbps data rates for DSSS only. This backward compatibility is extremely important as it allows upgrading of the wireless network without replacing the NICs or access points. 802.11b devices achieve the higher data throughput rate by using a different coding technique from 802.11, allowing for a greater amount of data to be transferred in the same time frame. The majority of 802.11b devices still fail to match the 11 Mbps throughput and generally function in the 2 to 4 Mbps range. 802.11a covers WLAN devices operating in the 5 GHZ transmission band. Using the 5 GHZ range disallows interoperability of 802.11b devices as they operate within 2.4 GHZ. 802.11a is capable of supplying data throughput of 54 Mbps and with proprietary technology known as "rate doubling" has achieved 108 Mbps. In production networks, a more standard rating is 20-26 Mbps. 802.11g provides the same throughout as 802.11a but with backwards compatibility for 802.11b devices using Othogonal Frequency Division Multiplexing (OFDM) modulation technology. Cisco has developed an access point that permits 802.11b and 802.11a devices to coexist on the same WLAN. The access point supplies ‘gateway’ services allowing these otherwise incompatible devices to communicate.
Web Links
Wireless Netowrking Standards and Organizations http://www.wlana.org/pdf/wlan_standards _orgs.pdf