
intLoopBackC.addSC("access-expression", "Build a bridge boolean access expression");
	intLoopBackC["access-expression"].addSC("input", "Filter input packets");
		intLoopBackC["access-expression"].input.addSC("LINE", "A boolean expression of bridge access lists");
	intLoopBackC["access-expression"].addSC("output", "Filter output packets");
		intLoopBackC["access-expression"].output.addSC("LINE", "A boolean expression of bridge access lists");
intLoopBackC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	intLoopBackC.arp.addSC("arpa", "Standard arp protocol");
	intLoopBackC.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
	intLoopBackC.arp.addSC("probe", "HP style arp protocol");
	intLoopBackC.arp.addSC("snap", "IEEE 802.3 style arp");
	intLoopBackC.arp.addSC("timeout", "Set ARP cache timeout");
		intLoopBackC.arp.timeout.addSC("<0-2147483>", "Seconds");
intLoopBackC.addSC("backup", "Modify backup parameters");
intLoopBackC.addSC("bandwidth", "Set bandwidth informational parameter");
	intLoopBackC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
intLoopBackC.addSC("bridge-group", "Transparent bridging interface parameters");
intLoopBackC.addSC("carrier-delay", "Specify delay for interface transitions");
	intLoopBackC["carrier-delay"].addSC("<0-60>", "Carrier Transitions delay seconds");
	intLoopBackC["carrier-delay"].addSC("msec", "delay specified in milliseconds");
		intLoopBackC["carrier-delay"].msec.addSC("<0-1000>", "Carrier Transitions delay milliseconds");
intLoopBackC.addSC("cdp", "CDP interface subcommands");
	intLoopBackC.cdp.addSC("enable", "Enable CDP on interface");
intLoopBackC.addSC("default", "Set a command to its defaults");
intLoopBackC.addSC("delay", "Specify interface throughput delay");
	intLoopBackC.delay.addSC("<1-16777215>", "Throughput delay (tens of microseconds)");
intLoopBackC.addSC("description", "Interface specific description");
	intLoopBackC.description.addSC("LINE", "Up to 240 characters describing this interface");
intLoopBackC.addSC("exit", "Exit from interface configuration mode");
intLoopBackC.addSC("help", "Description of the interactive help system");
intLoopBackC.addSC("hold-queue", "Set hold queue depth");
	intLoopBackC["hold-queue"].addSC("<0-4096>", "Queue length");
		intLoopBackC["hold-queue"]["<0-4096>"].addSC("in", "Input queue");
		intLoopBackC["hold-queue"]["<0-4096>"].addSC("out", "Output queue");
intLoopBackC.addSC("ip", "Interface Internet Protocol config commands");
	intLoopBackC.ip.addSC("access-group", "Specify access control for packets");
		intLoopBackC.ip["access-group"].addSC("<1-199>", "IP access list (standard or extended)");
			intLoopBackC.ip["access-group"]["<1-199>"].addSC("in", "inbound packets");
			intLoopBackC.ip["access-group"]["<1-199>"].addSC("out", "outbound packets");
		intLoopBackC.ip["access-group"].addSC("<1300-2699>", "IP expanded access list (standard or extended)");
			intLoopBackC.ip["access-group"]["<1300-2699>"].addSC("in", "inbound packets");
			intLoopBackC.ip["access-group"]["<1300-2699>"].addSC("out", "outbound packets");
		intLoopBackC.ip["access-group"].addSC("WORD", "Access-list name");
			intLoopBackC.ip["access-group"].WORD.addSC("in", "inbound packets");
			intLoopBackC.ip["access-group"].WORD.addSC("out", "outbound packets");
	intLoopBackC.ip.addSC("accounting", "Enable IP accounting on this interface");
	intLoopBackC.ip.addSC("address", "Set the IP address of an interface");
		intLoopBackC.ip.address.addSC("A.B.C.D", "IP address");
			intLoopBackC.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
				intLoopBackC.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
		intLoopBackC.ip.address.addSC("pool", "IP Address autoconfigured from a local DHCP pool");
			intLoopBackC.ip.address.pool.addSC("WORD", "Pool name");
	intLoopBackC.ip.addSC("authentication", "authentication subcommands");
		intLoopBackC.ip.authentication.addSC("key-chain", "key-chain");
			intLoopBackC.ip.authentication["key-chain"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intLoopBackC.ip.authentication["key-chain"].eigrp.addSC("<1-65535>", "Autonomous system number");
					intLoopBackC.ip.authentication["key-chain"].eigrp["<1-65535>"].addSC("LINE", "name of key-chain");
		intLoopBackC.ip.authentication.addSC("mode", "mode");
			intLoopBackC.ip.authentication.mode.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intLoopBackC.ip.authentication.mode.eigrp.addSC("<1-65535>", "Autonomous system number");
					intLoopBackC.ip.authentication.mode.eigrp["<1-65535>"].addSC("md5", "Keyed message digest");
	intLoopBackC.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
		intLoopBackC.ip["bandwidth-percent"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			intLoopBackC.ip["bandwidth-percent"].eigrp.addSC("<1-65535>", "Autonomous system number");
				intLoopBackC.ip["bandwidth-percent"].eigrp["<1-65535>"].addSC("<1-999999>", "Maximum bandwidth percentage that EIGRP may use");
	intLoopBackC.ip.addSC("bgp", "BGP interface commands");
	intLoopBackC.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
	intLoopBackC.ip.addSC("cef", "Cisco Express Fowarding interface commands");
	intLoopBackC.ip.addSC("cgmp", "Enable/disable CGMP");
	intLoopBackC.ip.addSC("dhcp", "Configure DHCP parameters for this interface");
	intLoopBackC.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
	intLoopBackC.ip.addSC("dvmrp", "DVMRP interface commands");
	intLoopBackC.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
		intLoopBackC.ip["hello-interval"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			intLoopBackC.ip["hello-interval"].eigrp.addSC("<1-65535>", "Autonomous system number");
				intLoopBackC.ip["hello-interval"].eigrp["<1-65535>"].addSC("<1-65535>", "Seconds between hello transmissions");
	intLoopBackC.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
	intLoopBackC.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
		intLoopBackC.ip["hold-time"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			intLoopBackC.ip["hold-time"].eigrp.addSC("<1-65535>", "Autonomous system number");
				intLoopBackC.ip["hold-time"].eigrp["<1-65535>"].addSC("<1-65535>", "Seconds before neighbor is considered down");
	intLoopBackC.ip.addSC("idle-group", "Specify interesting packets for idle-timer");
		intLoopBackC.ip["idle-group"].addSC("<1-199>", "IP access list (standard or extended)");
	intLoopBackC.ip.addSC("igmp", "IGMP interface commands");
			intLoopBackC.ip.igmp.version.addSC("<1-3>", "version number");
	intLoopBackC.ip.addSC("irdp", "ICMP Router Discovery Protocol");
	intLoopBackC.ip.addSC("load-sharing", "Style of load sharing");
		intLoopBackC.ip["load-sharing"].addSC("per-destination", "Deterministic distribution");
		intLoopBackC.ip["load-sharing"].addSC("per-packet", "Random distribution");
	intLoopBackC.ip.addSC("local-proxy-arp", "Enable local-proxy ARP");
	intLoopBackC.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
	intLoopBackC.ip.addSC("mrm", "Configure IP Multicast Routing Monitor tester");
	intLoopBackC.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		intLoopBackC.ip.mtu.addSC("<68-1000000>", "MTU (bytes)");
	intLoopBackC.ip.addSC("multicast", "IP multicast interface commands");
			intLoopBackC.ip.multicast["ttl-threshold"].addSC("<0-255>", "TTL threshold");
	intLoopBackC.ip.addSC("nat", "NAT interface commands");
		intLoopBackC.ip.nat.addSC("inside", "Inside interface for address translation");
		intLoopBackC.ip.nat.addSC("outside", "Outside interface for address translation");
	intLoopBackC.ip.addSC("nbar", "Network-Based Application Recognition");
	intLoopBackC.ip.addSC("ospf", "OSPF interface commands");
			intLoopBackC.ip.ospf.addSC("authentication", "Enable authentication");
			intLoopBackC.ip.ospf.addSC("authentication-key", "Authentication password (key)");
			intLoopBackC.ip.ospf.addSC("cost", "Interface cost");
				intLoopBackC.ip.ospf.cost.addSC("<1-65535>",  "Cost");
			intLoopBackC.ip.ospf.addSC("database-filter", "Filter OSPF LSA during synchronization and flooding");
			intLoopBackC.ip.ospf.addSC("dead-interval", "Interval after which a neighbor is declared dead");
				intLoopBackC.ip.ospf["dead-interval"].addSC("<1-65535>", "Seconds");
			intLoopBackC.ip.ospf.addSC("demand-circuit", "OSPF demand circuit");
			intLoopBackC.ip.ospf.addSC("flood-reduction", "OSPF Flood Reduction");
			intLoopBackC.ip.ospf.addSC("hello-interval", "Time between HELLO packets");
				intLoopBackC.ip.ospf["hello-interval"].addSC("<1-65535>", "Seconds");
			intLoopBackC.ip.ospf.addSC("message-digest-key", "Message digest authentication password (key)");
			intLoopBackC.ip.ospf.addSC("mtu-ignore", "Ignores the MTU in DBD packets");
			intLoopBackC.ip.ospf.addSC("network", "Network type");
			intLoopBackC.ip.ospf.addSC("priority", "Router priority");
			intLoopBackC.ip.ospf.addSC("retransmit-interval", "Time between retransmitting lost link state advertisements");
			intLoopBackC.ip.ospf.addSC("transmit-delay", "Link state transmit delay");

	intLoopBackC.ip.addSC("pgm", "PGM Reliable Transport Protocol");
	intLoopBackC.ip.addSC("pim", "PIM interface commands");
	intLoopBackC.ip.addSC("policy", "Enable policy routing");
		intLoopBackC.ip.policy.addSC("route-map", "Policy route map");
			intLoopBackC.ip.policy["route-map"].addSC("WORD", "Route map name");
	intLoopBackC.ip.addSC("probe", "Enable HP Probe support");
		intLoopBackC.ip.probe.addSC("proxy", "Proxy support");
	intLoopBackC.ip.addSC("proxy-arp", "Enable proxy ARP");
	intLoopBackC.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
		intLoopBackC.ip["rarp-server"].addSC("A.B.C.D", "IP server address");
	intLoopBackC.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
	intLoopBackC.ip.addSC("rgmp", "Enable/disable RGMP");
	intLoopBackC.ip.addSC("rip", "Router Information Protocol");
		intLoopBackC.ip.rip.addSC("authentication", "Authentication control");
		intLoopBackC.ip.rip.addSC("receive", "advertisement reception");
		intLoopBackC.ip.rip.addSC("send", "advertisement transmission");
			intLoopBackC.ip.rip.send.addSC("version", "version control");
				intLoopBackC.ip.rip.send.version.addSC("<1-1>", "RIP version 1");
				intLoopBackC.ip.rip.send.version.addSC("<2-2>", "RIP version 2");
		intLoopBackC.ip.rip.addSC("v2-broadcast", "send ip broadcast v2 update");
	intLoopBackC.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
intLoopBackC.addSC("ipv6", "IPv6 interface subcommands");
intLoopBackC.addSC("keepalive", "Enable keepalive");
	intLoopBackC.keepalive.addSC("<0-32767>", "Keepalive period (default 10 seconds)");
intLoopBackC.addSC("llc2", "LLC2 Interface Subcommands");
intLoopBackC.addSC("load-interval", "Specify interval for load calculation for an interface");
	intLoopBackC["load-interval"].addSC("<30-600>", "Load interval delay in seconds");
intLoopBackC.addSC("logging", "Configure logging for interface");
	intLoopBackC.logging.addSC("event", "Interface events");
		intLoopBackC.logging.event.addSC("link-status", "UPDOWN and CHANGE messages");
intLoopBackC.addSC("max-reserved-bandwidth", "Maximum Reservable Bandwidth on an Interface");
	intLoopBackC["max-reserved-bandwidth"].addSC("<1-100>", "Max. reservable bandwidth as % of interface bandwidth");
intLoopBackC.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
intLoopBackC.addSC("multilink-group", "Put interface in a multilink bundle");
intLoopBackC.addSC("netbios", "Use a defined NETBIOS access list or enable name-caching");
intLoopBackC.addSC("no", "Negate a command or set its defaults");
	intLoopBackC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
		intLoopBackC.no.arp.addSC("arpa", "Standard arp protocol");
		intLoopBackC.no.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
	intLoopBackC.no.addSC("bandwidth", "Set bandwidth informational parameter");
		intLoopBackC.no["bridge-group"].addSC("<1-255>", "Assign an interface to a Bridge Group.");
	intLoopBackC.no.addSC("cdp", "CDP interface subcommands");
		intLoopBackC.no.cdp.addSC("enable", "Enable CDP on interface");
	intLoopBackC.no.addSC("delay", "Specify interface throughput delay");
	intLoopBackC.no.addSC("description", "Interface specific description");
	intLoopBackC.no.addSC("hold-queue", "Set hold queue depth");
	intLoopBackC.no.addSC("ip", "Interface Internet Protocol config commands");
		intLoopBackC.no.ip.addSC("access-group", "Specify access control for packets");
		intLoopBackC.no.ip.addSC("address", "Set the IP address of an interface");
		intLoopBackC.no.ip.addSC("authentication", "authentication subcommands");
		intLoopBackC.no.ip.addSC("dhcp", "Configure DHCP parameters for this interface");
		intLoopBackC.no.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
	intLoopBackC.no.addSC("keepalive", "Enable keepalive");
		intLoopBackC.no.keepalive.addSC("<0-32767>", "Keepalive period (default 10 seconds)");
	intLoopBackC.no.addSC("load-interval", "Specify interval for load calculation for an interface");
intLoopBackC.addSC("ntp", "Configure NTP");
	intLoopBackC.ntp.addSC("broadcast", "Configure NTP broadcast service");
	intLoopBackC.ntp.addSC("disable", "Disable NTP");
	intLoopBackC.ntp.addSC("multicast", "Configure NTP multicast service");
intLoopBackC.addSC("rate-limit", "Rate Limit");
	intLoopBackC["rate-limit"].addSC("input", "Rate limit on input");
	intLoopBackC["rate-limit"].addSC("output", "Rate limit on output");
intLoopBackC.addSC("service-policy", "Configure QoS Service Policy");
intLoopBackC.addSC("shutdown", "Shutdown the selected interface");
intLoopBackC.addSC("snapshot", "Configure snapshot support on the interface");
intLoopBackC.addSC("snmp", "Modify SNMP interface parameters");
intLoopBackC.addSC("timeout", "Define timeout values for this interface");
	intLoopBackC.timeout.addSC("absolute", "Define session timeout value for this interface");
		intLoopBackC.timeout.absolute.addSC("<0-35790>", "Session lifetime (in minutes)");
intLoopBackC.addSC("transmit-interface", "Assign a transmit interface to a receive-only interface");
intLoopBackC.addSC("trunk-group", "Configure interface to be in a trunk group");
	intLoopBackC["trunk-group"].addSC("<1-1000>", "Trunk group number");
intLoopBackC.addSC("tx-ring-limit", "Configure PA level transmit ring limit");
	intLoopBackC["tx-ring-limit"].addSC("<1-32767>", "Number (ring limit)");
