
routerRIPC.addSC("address-family", "Enter Address Family command mode");
	routerRIPC["address-family"].addSC("ipv4", "Address family");
		routerRIPC["address-family"].ipv4.addSC("unicast", "Address Family Modifier");
		routerRIPC["address-family"].ipv4.addSC("vrf", "Specify parameters for a VPN Routing/Forwarding instance");
			routerRIPC["address-family"].ipv4.vrf.addSC("WORD", "VPN Routing/Forwarding instance name");
routerRIPC.addSC("auto-summary", "Enable automatic network number summarization");
routerRIPC.addSC("default", "Set a command to its defaults");
routerRIPC.addSC("default-information", "Control distribution of default information");
	routerRIPC["default-information"].addSC("originate", "Distribute a default route");
		routerRIPC["default-information"].originate.addSC("route-map", "Route-map reference");
			routerRIPC["default-information"].originate["route-map"].addSC("WORD", "Route map name");
routerRIPC.addSC("default-metric", "Set metric of redistributed routes");
routerRIPC.addSC("distance", "Define an administrative distance");
	routerRIPC.distance.addSC("<1-255>", "Administrative distance");
		routerRIPC.distance["<1-255>"].addSC("A.B.C.D", "IP Source address");
			routerRIPC.distance["<1-255>"]["A.B.C.D"].addSC("A.B.C.D", "IP address mask");
				routerRIPC.distance["<1-255>"]["A.B.C.D"]["A.B.C.D"].addSC("<1-99>", "IP Standard access list number");
				routerRIPC.distance["<1-255>"]["A.B.C.D"]["A.B.C.D"].addSC("<1300-1999>", "IP Standard expanded access list number");
				routerRIPC.distance["<1-255>"]["A.B.C.D"]["A.B.C.D"].addSC("WORD", "Standard access-list name");
routerRIPC.addSC("distribute-list", "Filter networks in routing updates");
	routerRIPC["distribute-list"].addSC("<1-199>", "IP access list number");
		routerRIPC["distribute-list"]["<1-199>"].addSC("in", "Filter incoming routing updates");
			routerRIPC["distribute-list"]["<1-199>"]["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerRIPC["distribute-list"]["<1-199>"]["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerRIPC["distribute-list"]["<1-199>"]["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerRIPC["distribute-list"]["<1-199>"]["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerRIPC["distribute-list"]["<1-199>"]["in"].addSC("Loopback", "Loopback interface");
				routerRIPC["distribute-list"]["<1-199>"]["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerRIPC["distribute-list"]["<1-199>"]["in"].addSC("Null", "Null interface");
				routerRIPC["distribute-list"]["<1-199>"]["in"].Null.addSC("<0-0>", "Null interface number");
			routerRIPC["distribute-list"]["<1-199>"]["in"].addSC("Vlan", "Catalyst Vlans");
				routerRIPC["distribute-list"]["<1-199>"]["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
		routerRIPC["distribute-list"]["<1-199>"].addSC("out", "Filter outgoing routing updates");
			routerRIPC["distribute-list"]["<1-199>"].out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerRIPC["distribute-list"]["<1-199>"].out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerRIPC["distribute-list"]["<1-199>"].out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerRIPC["distribute-list"]["<1-199>"].out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerRIPC["distribute-list"]["<1-199>"].out.addSC("Loopback", "Loopback interface");
				routerRIPC["distribute-list"]["<1-199>"].out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerRIPC["distribute-list"]["<1-199>"].out.addSC("Null", "Null interface");
				routerRIPC["distribute-list"]["<1-199>"].out.Null.addSC("<0-0>", "Null interface number");
			routerRIPC["distribute-list"]["<1-199>"].out.addSC("Vlan", "Catalyst Vlans");
				routerRIPC["distribute-list"]["<1-199>"].out.Vlan.addSC("<1-1001>", "Vlan interface number");
			routerRIPC["distribute-list"]["<1-199>"].out.addSC("bgp", "Border Gateway Protocol (BGP)");
				routerRIPC["distribute-list"]["<1-199>"].out.bgp.addSC("<1-65535>", "Autonomous system number");
			routerRIPC["distribute-list"]["<1-199>"].out.addSC("connected", "Connected");
			routerRIPC["distribute-list"]["<1-199>"].out.addSC("egp", "Exterior Gateway Protocol (EGP)");
				routerRIPC["distribute-list"]["<1-199>"].out.egp.addSC("<0-65535>", "Remote autonomous system number");
			routerRIPC["distribute-list"]["<1-199>"].out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				routerRIPC["distribute-list"]["<1-199>"].out.eigrp.addSC("<1-65535>", "Autonomous system number");
			routerRIPC["distribute-list"]["<1-199>"].out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				routerRIPC["distribute-list"]["<1-199>"].out.igrp.addSC("<1-65535>", "Autonomous system number");
			routerRIPC["distribute-list"]["<1-199>"].out.addSC("ospf", "Open Shortest Path First (OSPF)");
				routerRIPC["distribute-list"]["<1-199>"].out.ospf.addSC("<1-65535>", "Process ID");
					routerRIPC["distribute-list"]["<1-199>"].out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
						routerRIPC["distribute-list"]["<1-199>"].out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
			routerRIPC["distribute-list"]["<1-199>"].out.addSC("rip", "Routing Information Protocol (RIP)");
			routerRIPC["distribute-list"]["<1-199>"].out.addSC("static", "Static routes");
	routerRIPC["distribute-list"].addSC("<1300-2699>", "IP expanded access list number");
		routerRIPC["distribute-list"]["<1300-2699>"].addSC("in", "Filter incoming routing updates");
			routerRIPC["distribute-list"]["<1300-2699>"]["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerRIPC["distribute-list"]["<1300-2699>"]["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerRIPC["distribute-list"]["<1300-2699>"]["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerRIPC["distribute-list"]["<1300-2699>"]["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerRIPC["distribute-list"]["<1300-2699>"]["in"].addSC("Loopback", "Loopback interface");
				routerRIPC["distribute-list"]["<1300-2699>"]["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerRIPC["distribute-list"]["<1300-2699>"]["in"].addSC("Null", "Null interface");
				routerRIPC["distribute-list"]["<1300-2699>"]["in"].Null.addSC("<0-0>", "Null interface number");
			routerRIPC["distribute-list"]["<1300-2699>"]["in"].addSC("Vlan", "Catalyst Vlans");
				routerRIPC["distribute-list"]["<1300-2699>"]["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
		routerRIPC["distribute-list"]["<1300-2699>"].addSC("out", "Filter outgoing routing updates");
			routerRIPC["distribute-list"]["<1300-2699>"].out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerRIPC["distribute-list"]["<1300-2699>"].out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerRIPC["distribute-list"]["<1300-2699>"].out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerRIPC["distribute-list"]["<1300-2699>"].out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerRIPC["distribute-list"]["<1300-2699>"].out.addSC("Loopback", "Loopback interface");
				routerRIPC["distribute-list"]["<1300-2699>"].out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerRIPC["distribute-list"]["<1300-2699>"].out.addSC("Null", "Null interface");
				routerRIPC["distribute-list"]["<1300-2699>"].out.Null.addSC("<0-0>", "Null interface number");
			routerRIPC["distribute-list"]["<1300-2699>"].out.addSC("Vlan", "Catalyst Vlans");
				routerRIPC["distribute-list"]["<1300-2699>"].out.Vlan.addSC("<1-1001>", "Vlan interface number");
			routerRIPC["distribute-list"]["<1300-2699>"].out.addSC("bgp", "Border Gateway Protocol (BGP)");
				routerRIPC["distribute-list"]["<1300-2699>"].out.bgp.addSC("<1-65535>", "Autonomous system number");
			routerRIPC["distribute-list"]["<1300-2699>"].out.addSC("connected", "Connected");
			routerRIPC["distribute-list"]["<1300-2699>"].out.addSC("egp", "Exterior Gateway Protocol (EGP)");
				routerRIPC["distribute-list"]["<1300-2699>"].out.egp.addSC("<0-65535>", "Remote autonomous system number");
			routerRIPC["distribute-list"]["<1300-2699>"].out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				routerRIPC["distribute-list"]["<1300-2699>"].out.eigrp.addSC("<1-65535>", "Autonomous system number");
			routerRIPC["distribute-list"]["<1300-2699>"].out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				routerRIPC["distribute-list"]["<1300-2699>"].out.igrp.addSC("<1-65535>", "Autonomous system number");
			routerRIPC["distribute-list"]["<1300-2699>"].out.addSC("ospf", "Open Shortest Path First (OSPF)");
				routerRIPC["distribute-list"]["<1300-2699>"].out.ospf.addSC("<1-65535>", "Process ID");
					routerRIPC["distribute-list"]["<1300-2699>"].out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
						routerRIPC["distribute-list"]["<1300-2699>"].out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
			routerRIPC["distribute-list"]["<1300-2699>"].out.addSC("rip", "Routing Information Protocol (RIP)");
			routerRIPC["distribute-list"]["<1300-2699>"].out.addSC("static", "Static routes");
	routerRIPC["distribute-list"].addSC("WORD", "Access-list name");
		routerRIPC["distribute-list"].WORD.addSC("in", "Filter incoming routing updates");
			routerRIPC["distribute-list"].WORD["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerRIPC["distribute-list"].WORD["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerRIPC["distribute-list"].WORD["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerRIPC["distribute-list"].WORD["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerRIPC["distribute-list"].WORD["in"].addSC("Loopback", "Loopback interface");
				routerRIPC["distribute-list"].WORD["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerRIPC["distribute-list"].WORD["in"].addSC("Null", "Null interface");
				routerRIPC["distribute-list"].WORD["in"].Null.addSC("<0-0>", "Null interface number");
			routerRIPC["distribute-list"].WORD["in"].addSC("Vlan", "Catalyst Vlans");
				routerRIPC["distribute-list"].WORD["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
		routerRIPC["distribute-list"].WORD.addSC("out", "Filter outgoing routing updates");
			routerRIPC["distribute-list"].WORD.out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerRIPC["distribute-list"].WORD.out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerRIPC["distribute-list"].WORD.out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerRIPC["distribute-list"].WORD.out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerRIPC["distribute-list"].WORD.out.addSC("Loopback", "Loopback interface");
				routerRIPC["distribute-list"].WORD.out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerRIPC["distribute-list"].WORD.out.addSC("Null", "Null interface");
				routerRIPC["distribute-list"].WORD.out.Null.addSC("<0-0>", "Null interface number");
			routerRIPC["distribute-list"].WORD.out.addSC("Vlan", "Catalyst Vlans");
				routerRIPC["distribute-list"].WORD.out.Vlan.addSC("<1-1001>", "Vlan interface number");
			routerRIPC["distribute-list"].WORD.out.addSC("bgp", "Border Gateway Protocol (BGP)");
				routerRIPC["distribute-list"].WORD.out.bgp.addSC("<1-65535>", "Autonomous system number");
			routerRIPC["distribute-list"].WORD.out.addSC("connected", "Connected");
			routerRIPC["distribute-list"].WORD.out.addSC("egp", "Exterior Gateway Protocol (EGP)");
				routerRIPC["distribute-list"].WORD.out.egp.addSC("<0-65535>", "Remote autonomous system number");
			routerRIPC["distribute-list"].WORD.out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				routerRIPC["distribute-list"].WORD.out.eigrp.addSC("<1-65535>", "Autonomous system number");
			routerRIPC["distribute-list"].WORD.out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				routerRIPC["distribute-list"].WORD.out.igrp.addSC("<1-65535>", "Autonomous system number");
			routerRIPC["distribute-list"].WORD.out.addSC("ospf", "Open Shortest Path First (OSPF)");
				routerRIPC["distribute-list"].WORD.out.ospf.addSC("<1-65535>", "Process ID");
					routerRIPC["distribute-list"].WORD.out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
						routerRIPC["distribute-list"].WORD.out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
			routerRIPC["distribute-list"].WORD.out.addSC("rip", "Routing Information Protocol (RIP)");
			routerRIPC["distribute-list"].WORD.out.addSC("static", "Static routes");
	routerRIPC["distribute-list"].addSC("gateway", "Filtering incoming updates based on gateway");
		routerRIPC["distribute-list"].gateway.addSC("WORD", "Name of an IP prefix-list");
			routerRIPC["distribute-list"].gateway.WORD.addSC("in", "Filter incoming routing updates");
				routerRIPC["distribute-list"].gateway.WORD["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routerRIPC["distribute-list"].gateway.WORD["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routerRIPC["distribute-list"].gateway.WORD["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routerRIPC["distribute-list"].gateway.WORD["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routerRIPC["distribute-list"].gateway.WORD["in"].addSC("Loopback", "Loopback interface");
					routerRIPC["distribute-list"].gateway.WORD["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerRIPC["distribute-list"].gateway.WORD["in"].addSC("Null", "Null interface");
					routerRIPC["distribute-list"].gateway.WORD["in"].Null.addSC("<0-0>", "Null interface number");
				routerRIPC["distribute-list"].gateway.WORD["in"].addSC("Vlan", "Catalyst Vlans");
					routerRIPC["distribute-list"].gateway.WORD["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
			routerRIPC["distribute-list"].gateway.WORD.addSC("out", "Filter outgoing routing updates");
				routerRIPC["distribute-list"].gateway.WORD.out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routerRIPC["distribute-list"].gateway.WORD.out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routerRIPC["distribute-list"].gateway.WORD.out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routerRIPC["distribute-list"].gateway.WORD.out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routerRIPC["distribute-list"].gateway.WORD.out.addSC("Loopback", "Loopback interface");
					routerRIPC["distribute-list"].gateway.WORD.out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerRIPC["distribute-list"].gateway.WORD.out.addSC("Null", "Null interface");
					routerRIPC["distribute-list"].gateway.WORD.out.Null.addSC("<0-0>", "Null interface number");
				routerRIPC["distribute-list"].gateway.WORD.out.addSC("Vlan", "Catalyst Vlans");
					routerRIPC["distribute-list"].gateway.WORD.out.Vlan.addSC("<1-1001>", "Vlan interface number");
				routerRIPC["distribute-list"].gateway.WORD.out.addSC("bgp", "Border Gateway Protocol (BGP)");
					routerRIPC["distribute-list"].gateway.WORD.out.bgp.addSC("<1-65535>", "Autonomous system number");
				routerRIPC["distribute-list"].gateway.WORD.out.addSC("connected", "Connected");
				routerRIPC["distribute-list"].gateway.WORD.out.addSC("egp", "Exterior Gateway Protocol (EGP)");
					routerRIPC["distribute-list"].gateway.WORD.out.egp.addSC("<0-65535>", "Remote autonomous system number");
				routerRIPC["distribute-list"].gateway.WORD.out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
					routerRIPC["distribute-list"].gateway.WORD.out.eigrp.addSC("<1-65535>", "Autonomous system number");
				routerRIPC["distribute-list"].gateway.WORD.out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
					routerRIPC["distribute-list"].gateway.WORD.out.igrp.addSC("<1-65535>", "Autonomous system number");
				routerRIPC["distribute-list"].gateway.WORD.out.addSC("ospf", "Open Shortest Path First (OSPF)");
					routerRIPC["distribute-list"].gateway.WORD.out.ospf.addSC("<1-65535>", "Process ID");
						routerRIPC["distribute-list"].gateway.WORD.out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
							routerRIPC["distribute-list"].gateway.WORD.out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
				routerRIPC["distribute-list"].gateway.WORD.out.addSC("rip", "Routing Information Protocol (RIP)");
				routerRIPC["distribute-list"].gateway.WORD.out.addSC("static", "Static routes");
	routerRIPC["distribute-list"].addSC("prefix", "Filter prefixes in routing updates");
		routerRIPC["distribute-list"].prefix.addSC("WORD", "Name of an IP prefix-list");
			routerRIPC["distribute-list"].prefix.WORD.addSC("gateway", "Filtering incoming updates based on gateway");
			routerRIPC["distribute-list"].prefix.WORD.addSC("in", "Filter incoming routing updates");
				routerRIPC["distribute-list"].prefix.WORD["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routerRIPC["distribute-list"].prefix.WORD["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routerRIPC["distribute-list"].prefix.WORD["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routerRIPC["distribute-list"].prefix.WORD["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routerRIPC["distribute-list"].prefix.WORD["in"].addSC("Loopback", "Loopback interface");
					routerRIPC["distribute-list"].prefix.WORD["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerRIPC["distribute-list"].prefix.WORD["in"].addSC("Null", "Null interface");
					routerRIPC["distribute-list"].prefix.WORD["in"].Null.addSC("<0-0>", "Null interface number");
				routerRIPC["distribute-list"].prefix.WORD["in"].addSC("Vlan", "Catalyst Vlans");
					routerRIPC["distribute-list"].prefix.WORD["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
			routerRIPC["distribute-list"].prefix.WORD.addSC("out", "Filter outgoing routing updates");
				routerRIPC["distribute-list"].prefix.WORD.out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routerRIPC["distribute-list"].prefix.WORD.out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routerRIPC["distribute-list"].prefix.WORD.out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routerRIPC["distribute-list"].prefix.WORD.out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routerRIPC["distribute-list"].prefix.WORD.out.addSC("Loopback", "Loopback interface");
					routerRIPC["distribute-list"].prefix.WORD.out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerRIPC["distribute-list"].prefix.WORD.out.addSC("Null", "Null interface");
					routerRIPC["distribute-list"].prefix.WORD.out.Null.addSC("<0-0>", "Null interface number");
				routerRIPC["distribute-list"].prefix.WORD.out.addSC("Vlan", "Catalyst Vlans");
					routerRIPC["distribute-list"].prefix.WORD.out.Vlan.addSC("<1-1001>", "Vlan interface number");
				routerRIPC["distribute-list"].prefix.WORD.out.addSC("bgp", "Border Gateway Protocol (BGP)");
					routerRIPC["distribute-list"].prefix.WORD.out.bgp.addSC("<1-65535>", "Autonomous system number");
				routerRIPC["distribute-list"].prefix.WORD.out.addSC("connected", "Connected");
				routerRIPC["distribute-list"].prefix.WORD.out.addSC("egp", "Exterior Gateway Protocol (EGP)");
					routerRIPC["distribute-list"].prefix.WORD.out.egp.addSC("<0-65535>", "Remote autonomous system number");
				routerRIPC["distribute-list"].prefix.WORD.out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
					routerRIPC["distribute-list"].prefix.WORD.out.eigrp.addSC("<1-65535>", "Autonomous system number");
				routerRIPC["distribute-list"].prefix.WORD.out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
					routerRIPC["distribute-list"].prefix.WORD.out.igrp.addSC("<1-65535>", "Autonomous system number");
				routerRIPC["distribute-list"].prefix.WORD.out.addSC("ospf", "Open Shortest Path First (OSPF)");
					routerRIPC["distribute-list"].prefix.WORD.out.ospf.addSC("<1-65535>", "Process ID");
						routerRIPC["distribute-list"].prefix.WORD.out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
							routerRIPC["distribute-list"].prefix.WORD.out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
				routerRIPC["distribute-list"].prefix.WORD.out.addSC("rip", "Routing Information Protocol (RIP)");
				routerRIPC["distribute-list"].prefix.WORD.out.addSC("static", "Static routes");
routerRIPC.addSC("exit", "Exit from routing protocol configuration mode");
routerRIPC.addSC("flash-update-threshold", "Specify flash update threshold in second");
routerRIPC.addSC("help", "Description of the interactive help system");
routerRIPC.addSC("input-queue", "Specify input queue depth");
routerRIPC.addSC("maximum-paths", "Forward packets over multiple paths");
	routerRIPC["maximum-paths"].addSC("<1-8>", "Number of paths");
routerRIPC.addSC("neighbor", "Specify a neighbor router");
	routerRIPC.neighbor.addSC("A.B.C.D", "Neighbor address");
routerRIPC.addSC("network", "Enable routing on an IP network");
	routerRIPC.network.addSC("A.B.C.D", "Network number");
routerRIPC.addSC("no", "Negate a command or set its defaults");
routerRIPC.addSC("offset-list", "Add or subtract offset from IGRP or RIP metrics");
routerRIPC.addSC("output-delay", "Interpacket delay for RIP updates");
routerRIPC.addSC("passive-interface", "Suppress routing updates on an interface");
	routerRIPC["passive-interface"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
		routerRIPC["passive-interface"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
	routerRIPC["passive-interface"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
		routerRIPC["passive-interface"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
	routerRIPC["passive-interface"].addSC("Loopback", "Loopback interface");
		routerRIPC["passive-interface"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
	routerRIPC["passive-interface"].addSC("Null", "Null interface");
		routerRIPC["passive-interface"].Null.addSC("<0-0>", "Null interface number");
	routerRIPC["passive-interface"].addSC("Vlan", "Catalyst Vlans");
		routerRIPC["passive-interface"].Vlan.addSC("<1-1001>", "Vlan interface number");
	routerRIPC["passive-interface"].addSC("default", "Suppress routing updates on all interfaces");
routerRIPC.addSC("redistribute", "Redistribute information from another routing protocol");
	routerRIPC.redistribute.addSC("bgp", "Border Gateway Protocol (BGP)");
		routerRIPC.redistribute.bgp.addSC("<1-65535>", "Autonomous system number");
	routerRIPC.redistribute.addSC("connected", "Connected");
	routerRIPC.redistribute.addSC("egp", "Exterior Gateway Protocol (EGP)");
		routerRIPC.redistribute.egp.addSC("<0-65535>", "Remote autonomous system number");
	routerRIPC.redistribute.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
		routerRIPC.redistribute.eigrp.addSC("<1-65535>", "Autonomous system number");
	routerRIPC.redistribute.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
		routerRIPC.redistribute.igrp.addSC("<1-65535>", "Autonomous system number");
	routerRIPC.redistribute.addSC("isis", "ISO IS-IS");
		routerRIPC.redistribute.isis.addSC("level-1", "IS-IS level-1 routes only");
		routerRIPC.redistribute.isis.addSC("level-1-2", "IS-IS level-1 and level-2 routes");
		routerRIPC.redistribute.isis.addSC("level-2", "IS-IS level-2 routes only");
		routerRIPC.redistribute.isis.addSC("WORD", "ISO routing area tag");
			routerRIPC.redistribute.isis.WORD.addSC("level-1", "IS-IS level-1 routes only");
			routerRIPC.redistribute.isis.WORD.addSC("level-1-2", "IS-IS level-1 and level-2 routes");
			routerRIPC.redistribute.isis.WORD.addSC("level-2", "IS-IS level-2 routes only");
	routerRIPC.redistribute.addSC("iso-igrp", "IGRP for OSI networks");
		routerRIPC.redistribute["iso-igrp"].addSC("WORD", "ISO routing area tag");
	routerRIPC.redistribute.addSC("metric", "Metric for redistributed routes");
		routerRIPC.redistribute.metric.addSC("<0-16>", "Default metric");
		routerRIPC.redistribute.metric.addSC("transparent", "Transparently redistribute metric");
	routerRIPC.redistribute.addSC("mobile", "Mobile routes");
		routerRIPC.redistribute.mobile.addSC("metric", "Metric for redistributed routes");
			routerRIPC.redistribute.mobile.metric.addSC("<0-16>", "Default metric");
			routerRIPC.redistribute.mobile.metric.addSC("transparent", "Transparently redistribute metric");
	routerRIPC.redistribute.addSC("odr", "On Demand stub Routes");
		routerRIPC.redistribute.odr.addSC("metric", "Metric for redistributed routes");
			routerRIPC.redistribute.odr.metric.addSC("<0-16>", "Default metric");
			routerRIPC.redistribute.odr.metric.addSC("transparent", "Transparently redistribute metric");
	routerRIPC.redistribute.addSC("ospf", "Open Shortest Path First (OSPF)");
		routerRIPC.redistribute.ospf.addSC("<1-65535>", "Process ID");
			routerRIPC.redistribute.ospf["<1-65535>"].addSC("match", "Redistribution of OSPF routes");
				routerRIPC.redistribute.ospf["<1-65535>"].match.addSC("external", "Redistribute OSPF external routes");
					routerRIPC.redistribute.ospf["<1-65535>"].match.external.addSC("<1-1>", "Redistribute external type 1 routes");
					routerRIPC.redistribute.ospf["<1-65535>"].match.external.addSC("<2-2>", "Redistribute external type 2 routes");
				routerRIPC.redistribute.ospf["<1-65535>"].match.addSC("internal", "Redistribute OSPF internal routes");
					routerRIPC.redistribute.ospf["<1-65535>"].match.internal.addSC("external", "Redistribute OSPF external routes");
						routerRIPC.redistribute.ospf["<1-65535>"].match.internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
						routerRIPC.redistribute.ospf["<1-65535>"].match.internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
				routerRIPC.redistribute.ospf["<1-65535>"].match.addSC("nssa-external", "Redistribute OSPF NSSA external routes");
					routerRIPC.redistribute.ospf["<1-65535>"].match["nssa-external"].addSC("<1-1>", "Redistribute NSSA external type 1 routes");
					routerRIPC.redistribute.ospf["<1-65535>"].match["nssa-external"].addSC("<2-2>", "Redistribute NSSA external type 2 routes");
					routerRIPC.redistribute.ospf["<1-65535>"].match["nssa-external"].addSC("external", "Redistribute OSPF external routes");
						routerRIPC.redistribute.ospf["<1-65535>"].match["nssa-external"].external.addSC("<1-1>", "Redistribute external type 1 routes");
						routerRIPC.redistribute.ospf["<1-65535>"].match["nssa-external"].external.addSC("<2-2>", "Redistribute external type 2 routes");
					routerRIPC.redistribute.ospf["<1-65535>"].match["nssa-external"].addSC("internal", "Redistribute OSPF internal routes");
						routerRIPC.redistribute.ospf["<1-65535>"].match["nssa-external"].internal.addSC("external", "Redistribute OSPF external routes");
							routerRIPC.redistribute.ospf["<1-65535>"].match["nssa-external"].internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
							routerRIPC.redistribute.ospf["<1-65535>"].match["nssa-external"].internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
			routerRIPC.redistribute.ospf["<1-65535>"].addSC("metric", "Metric for redistributed routes");
				routerRIPC.redistribute.ospf["<1-65535>"].metric.addSC("<0-16>", "Default metric");
					routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].addSC("match", "Redistribution of OSPF routes");
						routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match.addSC("external", "Redistribute OSPF external routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match.external.addSC("<1-1>", "Redistribute external type 1 routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match.external.addSC("<2-2>", "Redistribute external type 2 routes");
						routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match.addSC("internal", "Redistribute OSPF internal routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match.internal.addSC("external", "Redistribute OSPF external routes");
								routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match.internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
								routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match.internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
						routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match.addSC("nssa-external", "Redistribute OSPF NSSA external routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match["nssa-external"].addSC("<1-1>", "Redistribute NSSA external type 1 routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match["nssa-external"].addSC("<2-2>", "Redistribute NSSA external type 2 routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match["nssa-external"].addSC("external", "Redistribute OSPF external routes");
								routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match["nssa-external"].external.addSC("<1-1>", "Redistribute external type 1 routes");
								routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match["nssa-external"].external.addSC("<2-2>", "Redistribute external type 2 routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match["nssa-external"].addSC("internal", "Redistribute OSPF internal routes");
								routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match["nssa-external"].internal.addSC("external", "Redistribute OSPF external routes");
									routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match["nssa-external"].internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
									routerRIPC.redistribute.ospf["<1-65535>"].metric["<0-16>"].match["nssa-external"].internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
				routerRIPC.redistribute.ospf["<1-65535>"].metric.addSC("transparent", "Transparently redistribute metric");
					routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.addSC("match", "Redistribution of OSPF routes");
						routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match.addSC("external", "Redistribute OSPF external routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match.external.addSC("<1-1>", "Redistribute external type 1 routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match.external.addSC("<2-2>", "Redistribute external type 2 routes");
						routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match.addSC("internal", "Redistribute OSPF internal routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match.internal.addSC("external", "Redistribute OSPF external routes");
								routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match.internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
								routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match.internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
						routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match.addSC("nssa-external", "Redistribute OSPF NSSA external routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match["nssa-external"].addSC("<1-1>", "Redistribute NSSA external type 1 routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match["nssa-external"].addSC("<2-2>", "Redistribute NSSA external type 2 routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match["nssa-external"].addSC("external", "Redistribute OSPF external routes");
								routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match["nssa-external"].external.addSC("<1-1>", "Redistribute external type 1 routes");
								routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match["nssa-external"].external.addSC("<2-2>", "Redistribute external type 2 routes");
							routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match["nssa-external"].addSC("internal", "Redistribute OSPF internal routes");
								routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match["nssa-external"].internal.addSC("external", "Redistribute OSPF external routes");
									routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match["nssa-external"].internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
									routerRIPC.redistribute.ospf["<1-65535>"].metric.transparent.match["nssa-external"].internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
			routerRIPC.redistribute.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
				routerRIPC.redistribute.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
					routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.addSC("match", "Redistribution of OSPF routes");
						routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.addSC("external", "Redistribute OSPF external routes");
							routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.external.addSC("<1-1>", "Redistribute external type 1 routes");
							routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.external.addSC("<2-2>", "Redistribute external type 2 routes");
						routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.addSC("internal", "Redistribute OSPF internal routes");
							routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.internal.addSC("external", "Redistribute OSPF external routes");
								routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
								routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
						routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.addSC("nssa-external", "Redistribute OSPF NSSA external routes");
							routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].addSC("<1-1>", "Redistribute NSSA external type 1 routes");
							routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].addSC("<2-2>", "Redistribute NSSA external type 2 routes");
							routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].addSC("external", "Redistribute OSPF external routes");
								routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].external.addSC("<1-1>", "Redistribute external type 1 routes");
								routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].external.addSC("<2-2>", "Redistribute external type 2 routes");
							routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].addSC("internal", "Redistribute OSPF internal routes");
								routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].internal.addSC("external", "Redistribute OSPF external routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
					routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.addSC("metric", "Metric for redistributed routes");
						routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.addSC("<0-16>", "Default metric");
							routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<0-16>"].addSC("match", "Redistribution of OSPF routes");
								routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<0-16>"].match.addSC("external", "Redistribute OSPF external routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<0-16>"].match.external.addSC("<1-1>", "Redistribute external type 1 routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<0-16>"].match.external.addSC("<2-2>", "Redistribute external type 2 routes");
								routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<0-16>"].match.addSC("internal", "Redistribute OSPF internal routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<0-16>"].match.internal.addSC("external", "Redistribute OSPF external routes");
								routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<0-16>"].match.addSC("nssa-external", "Redistribute OSPF NSSA external routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<0-16>"].match["nssa-external"].addSC("<1-1>", "Redistribute NSSA external type 1 routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<0-16>"].match["nssa-external"].addSC("<2-2>", "Redistribute NSSA external type 2 routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<0-16>"].match["nssa-external"].addSC("external", "Redistribute OSPF external routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<0-16>"].match["nssa-external"].addSC("internal", "Redistribute OSPF internal routes");
						routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.addSC("transparent", "Transparently redistribute metric");
							routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.transparent.addSC("match", "Redistribution of OSPF routes");
								routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.transparent.match.addSC("external", "Redistribute OSPF external routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.transparent.match.external.addSC("<1-1>", "Redistribute external type 1 routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.transparent.match.external.addSC("<2-2>", "Redistribute external type 2 routes");
								routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.transparent.match.addSC("internal", "Redistribute OSPF internal routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.transparent.match.internal.addSC("external", "Redistribute OSPF external routes");
								routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.transparent.match.addSC("nssa-external", "Redistribute OSPF NSSA external routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.transparent.match["nssa-external"].addSC("<1-1>", "Redistribute NSSA external type 1 routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.transparent.match["nssa-external"].addSC("<2-2>", "Redistribute NSSA external type 2 routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.transparent.match["nssa-external"].addSC("external", "Redistribute OSPF external routes");
									routerRIPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.transparent.match["nssa-external"].addSC("internal", "Redistribute OSPF internal routes");
	routerRIPC.redistribute.addSC("rip", "Routing Information Protocol (RIP)");
		routerRIPC.redistribute.rip.addSC("metric", "Metric for redistributed routes");
			routerRIPC.redistribute.rip.metric.addSC("<0-16>", "Default metric");
			routerRIPC.redistribute.rip.metric.addSC("transparent", "Transparently redistribute metric");
	routerRIPC.redistribute.addSC("route-map", "Route map reference");
		routerRIPC.redistribute["route-map"].addSC("WORD", "Pointer to route-map entries");
			routerRIPC.redistribute["route-map"].WORD.addSC("metric", "Metric for redistributed routes");
				routerRIPC.redistribute["route-map"].WORD.metric.addSC("<0-16>", "Default metric");
				routerRIPC.redistribute["route-map"].WORD.metric.addSC("transparent", "Transparently redistribute metric");
	routerRIPC.redistribute.addSC("static", "Static routes");
		routerRIPC.redistribute.static.addSC("metric", "Metric for redistributed routes");
			routerRIPC.redistribute.static.metric.addSC("<0-16>", "Default metric");
			routerRIPC.redistribute.static.metric.addSC("transparent", "Transparently redistribute metric");
		routerRIPC.redistribute.static.addSC("route-map", "Route map reference");
			routerRIPC.redistribute.static["route-map"].addSC("WORD", "Pointer to route-map entries");
				routerRIPC.redistribute.static["route-map"].WORD.addSC("metric", "Metric for redistributed routes");
					routerRIPC.redistribute.static["route-map"].WORD.metric.addSC("<0-16>", "Default metric");
					routerRIPC.redistribute.static["route-map"].WORD.metric.addSC("transparent", "Transparently redistribute metric");
routerRIPC.addSC("timers", "Adjust routing timers");
	routerRIPC.timers.addSC("basic", "Basic routing protocol update timers");
		routerRIPC.timers.basic.addSC("<0-4294967295>", "Interval between updates");
			routerRIPC.timers.basic["<0-4294967295>"].addSC("<1-4294967295>", "Invalid");
				routerRIPC.timers.basic["<0-4294967295>"]["<1-4294967295>"].addSC("<0-4294967295>", "Holddown");
					routerRIPC.timers.basic["<0-4294967295>"]["<1-4294967295>"]["<0-4294967295>"].addSC("<1-4294967295>", "Flush");
						routerRIPC.timers.basic["<0-4294967295>"]["<1-4294967295>"]["<0-4294967295>"]["<1-4294967295>"].addSC("<1-4294967295>", "Sleep time, in milliseconds");
routerRIPC.addSC("traffic-share", "How to compute traffic share over alternate paths");
	routerRIPC["traffic-share"].addSC("min", "All traffic shared among min metric paths");
		routerRIPC["traffic-share"].min.addSC("across-interfaces", "Use different interfaces for equal-cost paths");
routerRIPC.addSC("validate-update-source", "Perform sanity checks against source address of routing updates");
routerRIPC.addSC("version", "Set routing protocol version");
	routerRIPC.version.addSC("<1-2>", "version");
