
userC.addSC("access-enable", "Create a temporary Access-List entry");
userC.addSC("access-profile", "Apply user-profile to interface");
userC.addSC("clear", "Reset functions");
userC.addSC("connect", "Open a terminal connection");
userC.addSC("disable", "Turn off privileged commands");
userC.addSC("disconnect", "Disconnect an existing network connection");
userC.addSC("enable", "Turn on privileged commands");
	userC.enable.addSC("<0-15>", "Enable level");
userC.addSC("exit", "Exit from the EXEC");
userC.addSC("help", "Description of the interactive help system");
userC.addSC("lock", "Lock the terminal");
userC.addSC("login", "Log in as a particular user");
userC.addSC("logout", "Exit from the EXEC");
userC.addSC("mrinfo", "Request neighbor and version information from a multicast router");
userC.addSC("mstat", "Show statistics after multiple multicast traceroutes");
userC.addSC("mtrace", "Trace reverse multicast path from destination to source");
userC.addSC("name-connection", "Name an existing network connection");
userC.addSC("ping", "Send echo messages");
	userC.ping.addSC("WORD", "Ping destination address or hostname");
	userC.ping.addSC("ip", "IP echo");
		userC.ping.ip.addSC("WORD", "Ping destination address or hostname");
	userC.ping.addSC("ipx", "Novell/IPX echo");
		userC.ping.ipx.addSC("WORD", "Ping destination address or hostname");
	userC.ping.addSC("tag", "Tag encapsulated IP echo");
		userC.ping.tag.addSC("WORD", "Ping destination address or hostname");
userC.addSC("ppp", "Start IETF Point-to-Point Protocol (PPP)");
userC.addSC("resume", "Resume an active network connection");
userC.addSC("rlogin", "Open an rlogin connection");
userC.addSC("show", "Show running system information");
	userC.show.addSC("atm", "ATM information");
	userC.show.addSC("call", "Show call");
	userC.show.addSC("cca", "CCA information");
	userC.show.addSC("cef", "Cisco Express Forwarding");
	userC.show.addSC("class-map", "Show QoS Class Map");
	userC.show.addSC("clock", "Display the system clock");
	userC.show.addSC("cns", "CNS subsystem");
	userC.show.addSC("compress", "Show compression statistics");
	userC.show.addSC("dial-peer", "Dial Plan Mapping Table for, e.g. VoIP Peers");
	userC.show.addSC("dialer", "Dialer parameters and statistics");
	userC.show.addSC("dsl", "DSL Show Commands");
	userC.show.addSC("exception", "exception informations");
	userC.show.addSC("flash:", "display information about flash: file system");
	userC.show.addSC("gateway", "Show status of gateway");
	userC.show.addSC("history", "Display the session command history");
	userC.show.addSC("hosts", "IP domain-name, lookup style, nameservers, and host table");
	userC.show.addSC("location", "Display the system location");
	userC.show.addSC("mgcp", "Display Media Gateway Control Protocol information");
	userC.show.addSC("num-exp", "Number Expansion (Speed Dial) information");
	userC.show.addSC("policy-map", "Show QoS Policy Map");
		userC.show["policy-map"].addSC("interface", "Show Qos Policy Interface");
			userC.show["policy-map"].interface.addSC("ATM", "ATM interface");
				userC.show["policy-map"].interface.ATM.addSC("<0-0>", "ATM interface number");
					userC.show["policy-map"].interface.ATM["<0-0>"].addSC("input", "Input policy");
						userC.show["policy-map"].interface.ATM["<0-0>"].input.addSC("class", "Show statistics for a indvidual class");
					userC.show["policy-map"].interface.ATM["<0-0>"].addSC("output", "Output policy");
						userC.show["policy-map"].interface.ATM["<0-0>"].output.addSC("class", "Show statistics for a indvidual class");
					userC.show["policy-map"].interface.ATM["<0-0>"].addSC("vc", "VC Service-Policy");
						userC.show["policy-map"].interface.ATM["<0-0>"].vc.addSC("<0-255>", "Enter VPI/VCI value(slash required)");
						userC.show["policy-map"].interface.ATM["<0-0>"].vc.addSC("<1-65535>", "Enter VCI value");
			userC.show["policy-map"].interface.addSC("Async", "Async interface");
				userC.show["policy-map"].interface.Async.addSC("<1-0>", "Async interface number");
			userC.show["policy-map"].interface.addSC("BVI", "Bridge-Group Virtual Interface");
				userC.show["policy-map"].interface.BVI.addSC("<1-255>", "BVI interface number");
			userC.show["policy-map"].interface.addSC("CTunnel", "CTunnel interface");
				userC.show["policy-map"].interface.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
			userC.show["policy-map"].interface.addSC("Dialer", "Dialer interface");
				userC.show["policy-map"].interface.Dialer.addSC("<0-255>", "Dialer interface number");
					userC.show["policy-map"].interface.Dialer["<0-255>"].addSC("input", "Input policy");
						userC.show["policy-map"].interface.Dialer["<0-255>"].input.addSC("class", "Show statistics for a indvidual class");
					userC.show["policy-map"].interface.Dialer["<0-255>"].addSC("output", "Output policy");
						userC.show["policy-map"].interface.Dialer["<0-255>"].output.addSC("class", "Show statistics for a indvidual class");
					userC.show["policy-map"].interface.Dialer["<0-255>"].addSC("vc", "VC Service-Policy");
						userC.show["policy-map"].interface.Dialer["<0-255>"].vc.addSC("<0-255>", "Enter VPI/VCI value(slash required)");
						userC.show["policy-map"].interface.Dialer["<0-255>"].vc.addSC("<1-65535>", "Enter VCI value");
			userC.show["policy-map"].interface.addSC("Ethernet", "IEEE 802.3");
				userC.show["policy-map"].interface.Ethernet.addSC("<0-0>", "Ethernet interface number");
					userC.show["policy-map"].interface.Ethernet["<0-0>"].addSC("input", "Input policy");
						userC.show["policy-map"].interface.Ethernet["<0-0>"].input.addSC("class", "Show statistics for a indvidual class");
					userC.show["policy-map"].interface.Ethernet["<0-0>"].addSC("output", "Output policy");
						userC.show["policy-map"].interface.Ethernet["<0-0>"].output.addSC("class", "Show statistics for a indvidual class");
					userC.show["policy-map"].interface.Ethernet["<0-0>"].addSC("vc", "VC Service-Policy");
						userC.show["policy-map"].interface.Ethernet["<0-0>"].vc.addSC("<0-255>", "Enter VPI/VCI value(slash required)");
						userC.show["policy-map"].interface.Ethernet["<0-0>"].vc.addSC("<1-65535>", "Enter VCI value");
			userC.show["policy-map"].interface.addSC("Group-Async", "Async Group interface");
				userC.show["policy-map"].interface["Group-Async"].addSC("<0-0>", "Group-Async interface number");
			userC.show["policy-map"].interface.addSC("Lex", "Lex interface");
				userC.show["policy-map"].interface.Lex.addSC("<0-2147483647>", "Lex interface number");
			userC.show["policy-map"].interface.addSC("Loopback", "Loopback interface");
				userC.show["policy-map"].interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			userC.show["policy-map"].interface.addSC("Multilink", "Multilink-group interface");
				userC.show["policy-map"].interface.Multilink.addSC("<0-2147483647>", "Multilink interface number");
			userC.show["policy-map"].interface.addSC("Null", "Null interface");
				userC.show["policy-map"].interface.Null.addSC("<0-0>", "Null interface number");
					userC.show["policy-map"].interface.Null["<0-0>"].addSC("input", "Input policy");
						userC.show["policy-map"].interface.Null["<0-0>"].input.addSC("class", "Show statistics for a indvidual class");
					userC.show["policy-map"].interface.Null["<0-0>"].addSC("output", "Output policy");
						userC.show["policy-map"].interface.Null["<0-0>"].output.addSC("class", "Show statistics for a indvidual class");
					userC.show["policy-map"].interface.Null["<0-0>"].addSC("vc", "VC Service-Policy");
						userC.show["policy-map"].interface.Null["<0-0>"].vc.addSC("<0-255>", "Enter VPI/VCI value(slash required)");
						userC.show["policy-map"].interface.Null["<0-0>"].vc.addSC("<1-65535>", "Enter VCI value");
			userC.show["policy-map"].interface.addSC("Tunnel", "Tunnel interface");
				userC.show["policy-map"].interface.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
			userC.show["policy-map"].interface.addSC("Vif", "PGM Multicast Host interface");
			userC.show["policy-map"].interface.addSC("Virtual-Template", "Virtual Template interface");
			userC.show["policy-map"].interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
	userC.show.addSC("pots", "POTS information");
	userC.show.addSC("ppp", "PPP parameters and statistics");
	userC.show.addSC("queue", "Show queue contents");
	userC.show.addSC("queueing", "Show queueing configuration");
	userC.show.addSC("sessions", "Information about Telnet connections");
	userC.show.addSC("snmp", "snmp statistics");
	userC.show.addSC("srcp", "Display SRCP Protocol information");
	userC.show.addSC("tacacs", "Shows tacacs+ server statistics");
	userC.show.addSC("template", "Template information");
	userC.show.addSC("terminal", "Display terminal configuration parameters");
	userC.show.addSC("translation-rule", "Show translation rule table");
	userC.show.addSC("users", "Display information about terminal lines");
	userC.show.addSC("version", "System hardware and software status");
	userC.show.addSC("voice", "Voice port configuration & stats");
	userC.show.addSC("vpdn", "VPDN information");
userC.addSC("slip", "Start Serial-line IP (SLIP)");
userC.addSC("systat", "Display information about terminal lines");
userC.addSC("telnet", "Open a telnet connection");
userC.addSC("terminal", "Set terminal line parameters");
userC.addSC("traceroute", "Trace route to destination");
	userC.traceroute.addSC("WORD", "Trace route to destination address or hostname");
	userC.traceroute.addSC("appletalk", "AppleTalk Trace");
		userC.traceroute.appletalk.addSC("WORD", "Trace route to destination address or hostname");
	userC.traceroute.addSC("clns", "ISO CLNS Trace");
		userC.traceroute.clns.addSC("WORD", "Trace route to destination address or hostname");
	userC.traceroute.addSC("ip", "IP Trace");
		userC.traceroute.ip.addSC("WORD", "Trace route to destination address or hostname");
	userC.traceroute.addSC("ipv6", "IPv6 Trace");
		userC.traceroute.ipv6.addSC("WORD", "Trace route to destination address or hostname");
	userC.traceroute.addSC("ipx", "IPX Trace");
		userC.traceroute.ipx.addSC("WORD", "Trace route to destination address or hostname");
	userC.traceroute.addSC("oldvines", "Vines Trace (Cisco)");
		userC.traceroute.oldvines.addSC("WORD", "Trace route to destination address or hostname");
	userC.traceroute.addSC("vines", "Vines Trace (Banyan)");
		userC.traceroute.vines.addSC("WORD", "Trace route to destination address or hostname");
userC.addSC("tunnel", "Open a tunnel connection");
userC.addSC("where", "List active connections");
