
subintSC.addSC("appletalk", "Appletalk interface subcommands");
subintSC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
subintSC.addSC("backup", "Modify backup parameters");
subintSC.addSC("bandwidth", "Set bandwidth informational parameter");
	subintSC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
subintSC.addSC("bridge-group", "Transparent bridging interface parameters");
subintSC.addSC("carrier-delay", "Specify delay for interface transitions");
subintSC.addSC("cdp", "CDP interface subcommands");
subintSC.addSC("crypto", "Encryption/Decryption commands");
	subintSC.crypto.addSC("map", "Assign a Crypto Map");
		subintSC.crypto.map.addSC("WORD", "Crypto Map tag");
subintSC.addSC("decnet", "Interface DECnet config commands");
subintSC.addSC("default", "Set a command to its defaults");
subintSC.addSC("delay", "Specify interface throughput delay");
subintSC.addSC("description", "Interface specific description");
subintSC.addSC("dspu", "Down Stream PU");
subintSC.addSC("dxi", "ATM-DXI configuration commands");
subintSC.addSC("encapsulation", "Set encapsulation type for an interface");
	subintSC.encapsulation.addSC("sde", "IEEE 802.10 Virtual LAN - Secure Data Exchange");
subintSC.addSC("exit", "Exit from interface configuration mode");
subintSC.addSC("fras", "DLC Switch Interface Command");
subintSC.addSC("ip", "Interface Internet Protocol config commands");
	subintSC.ip.addSC("access-group", "Specify access control for packets");
	subintSC.ip.addSC("accounting", "Enable IP accounting on this interface");
	subintSC.ip.addSC("address", "Set the IP address of an interface");
		subintSC.ip.address.addSC("A.B.C.D", "IP address");
			subintSC.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
				subintSC.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
	subintSC.ip.addSC("audit", "Apply IDS audit name");
	subintSC.ip.addSC("auth-proxy", "Apply authenticaton proxy");
	subintSC.ip.addSC("authentication", "authentication subcommands");
	subintSC.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
			subintSC.ip["bandwidth-percent"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				subintSC.ip["bandwidth-percent"].eigrp.addSC("<1-65535>",  "Autonomous system number");
					subintSC.ip["bandwidth-percent"].eigrp["<1-65535>"].addSC("<1-999999>",  "Maximum bandwidth percentage that EIGRP may use");

	subintSC.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
	subintSC.ip.addSC("cgmp", "Enable/disable CGMP");
	subintSC.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
	subintSC.ip.addSC("dvmrp", "DVMRP interface commands");
	subintSC.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
	subintSC.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
	subintSC.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
	subintSC.ip.addSC("igmp", "IGMP interface commands");
	subintSC.ip.addSC("inspect", "Apply inspect name");
	subintSC.ip.addSC("irdp", "ICMP Router Discovery Protocol");
	subintSC.ip.addSC("load-sharing", "Style of load sharing");
	subintSC.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
	subintSC.ip.addSC("mobile", "Mobile IP support");
	subintSC.ip.addSC("mrm", "Configure IP Multicast Routing Monitor tester");
	subintSC.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
	subintSC.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
	subintSC.ip.addSC("multicast", "IP multicast interface commands");
	subintSC.ip.addSC("nat", "NAT interface commands");
		subintSC.ip.nat.addSC("inside", "Inside interface for address translation");
		subintSC.ip.nat.addSC("outside", "Outside interface for address translation");
	subintSC.ip.addSC("nhrp", "NHRP interface subcommands");
	subintSC.ip.addSC("ospf", "OSPF interface commands");
		subintSC.ip.ospf.addSC("authentication-key", "Authentication password (key)");
		subintSC.ip.ospf.addSC("cost", "Interface cost");
		subintSC.ip.ospf.addSC("database-filter", "Filter OSPF LSA during synchronization and flooding");
		subintSC.ip.ospf.addSC("dead-interval", "Interval after which a neighbor is declared dead");
			subintSC.ip.ospf["dead-interval"].addSC("<1-65535>", "Seconds");
		subintSC.ip.ospf.addSC("demand-circuit", "OSPF demand circuit");
		subintSC.ip.ospf.addSC("hello-interval", "Time between HELLO packets");
			subintSC.ip.ospf["hello-interval"].addSC("<1-65535>", "Seconds");
		subintSC.ip.ospf.addSC("message-digest-key", "Message digest authentication password (key)");
		subintSC.ip.ospf.addSC("network", "Network type");
		subintSC.ip.ospf.addSC("priority", "Router priority");
		subintSC.ip.ospf.addSC("retransmit-interval", "Time between retransmitting lost link state advertisements");
		subintSC.ip.ospf.addSC("transmit-delay", "Link state transmit delay");
	subintSC.ip.addSC("pgm", "PGM Reliable Transport Protocol");
	subintSC.ip.addSC("pim", "PIM interface commands");
	subintSC.ip.addSC("policy", "Enable policy routing");
	subintSC.ip.addSC("probe", "Enable HP Probe support");
	subintSC.ip.addSC("proxy-arp", "Enable proxy ARP");
	subintSC.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
	subintSC.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
	subintSC.ip.addSC("rip", "Router Information Protocol");
	subintSC.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
	subintSC.ip.addSC("router", "IP router interface commands");
		subintSC.ip.router.addSC("isis", "IS-IS Routing for IP");
			subintSC.ip.router.isis.addSC("WORD", "Routing process tag");
	subintSC.ip.addSC("rsvp", "RSVP interface commands");
	subintSC.ip.addSC("sap", "Session Advertisement Protocol interface commands");
	subintSC.ip.addSC("sdr", "Session Directory Protocol interface commands");
	subintSC.ip.addSC("security", "DDN IP Security Option");
	subintSC.ip.addSC("split-horizon", "Perform split horizon");
	subintSC.ip.addSC("summary-address", "Perform address summarization");
      subintSC.ip["summary-address"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
         subintSC.ip["summary-address"].eigrp.addSC("<1-65535>", "Autonomous system number");
            subintSC.ip["summary-address"].eigrp["<1-65535>"].addSC("A.B.C.D", "IP address");
               subintSC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"].addSC("A.B.C.D", "IP network mask");
                  subintSC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"]["A.B.C.D"].addSC("<1-255>", "Administrative distance");
      subintSC.ip["summary-address"].addSC("rip", "Routing Information Protocol (RIP)");
         subintSC.ip["summary-address"].rip.addSC("A.B.C.D", "IP address");
            subintSC.ip["summary-address"].rip["A.B.C.D"].addSC("A.B.C.D", "IP network mask");

	subintSC.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
	subintSC.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
	subintSC.ip.addSC("verify", "Enable per packet validation");
	subintSC.ip.addSC("vrf", "VPN Routing/Forwarding parameters on the interface");
	subintSC.ip.addSC("wccp", "WCCP interface commands");
subintSC.addSC("llc2", "LLC2 Interface Subcommands");
subintSC.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
subintSC.addSC("netbios", "Use a defined NETBIOS access list or enable name-caching");
subintSC.addSC("no", "Negate a command or set its defaults");
	subintSC.no.addSC("appletalk", "Appletalk interface subcommands");
	subintSC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	subintSC.no.addSC("backup", "Modify backup parameters");
	subintSC.no.addSC("bandwidth", "Set bandwidth informational parameter");
	subintSC.no.addSC("bridge-group", "Transparent bridging interface parameters");
	subintSC.no.addSC("carrier-delay", "Specify delay for interface transitions");
	subintSC.no.addSC("cdp", "CDP interface subcommands");
	subintSC.no.addSC("crypto", "Encryption/Decryption commands");
	subintSC.no.addSC("decnet", "Interface DECnet config commands");
	subintSC.no.addSC("delay", "Specify interface throughput delay");
	subintSC.no.addSC("description", "Interface specific description");
	subintSC.no.addSC("dspu", "Down Stream PU");
	subintSC.no.addSC("dxi", "ATM-DXI configuration commands");
	subintSC.no.addSC("encapsulation", "Set encapsulation type for an interface");
	subintSC.no.addSC("fras", "DLC Switch Interface Command");
	subintSC.no.addSC("ip", "Interface Internet Protocol config commands");
		subintSC.no.ip.addSC("access-group", "Specify access control for packets");
		subintSC.no.ip.addSC("accounting", "Enable IP accounting on this interface");
		subintSC.no.ip.addSC("address", "Set the IP address of an interface");
			subintSC.no.ip.address.addSC("A.B.C.D", "IP address");
				subintSC.no.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
					subintSC.no.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
		subintSC.no.ip.addSC("audit", "Apply IDS audit name");
		subintSC.no.ip.addSC("auth-proxy", "Apply authenticaton proxy");
		subintSC.no.ip.addSC("authentication", "authentication subcommands");
		subintSC.no.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
		subintSC.no.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		subintSC.no.ip.addSC("cgmp", "Enable/disable CGMP");
		subintSC.no.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
		subintSC.no.ip.addSC("dvmrp", "DVMRP interface commands");
		subintSC.no.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
		subintSC.no.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
		subintSC.no.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
		subintSC.no.ip.addSC("igmp", "IGMP interface commands");
		subintSC.no.ip.addSC("inspect", "Apply inspect name");
		subintSC.no.ip.addSC("irdp", "ICMP Router Discovery Protocol");
		subintSC.no.ip.addSC("load-sharing", "Style of load sharing");
		subintSC.no.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
		subintSC.no.ip.addSC("mobile", "Mobile IP support");
		subintSC.no.ip.addSC("mrm", "Configure IP Multicast Routing Monitor tester");
		subintSC.no.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
		subintSC.no.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		subintSC.no.ip.addSC("multicast", "IP multicast interface commands");
		subintSC.no.ip.addSC("nat", "NAT interface commands");
		subintSC.no.ip.addSC("nhrp", "NHRP interface subcommands");
		subintSC.no.ip.addSC("ospf", "OSPF interface commands");
		subintSC.no.ip.addSC("pgm", "PGM Reliable Transport Protocol");
		subintSC.no.ip.addSC("pim", "PIM interface commands");
		subintSC.no.ip.addSC("policy", "Enable policy routing");
		subintSC.no.ip.addSC("probe", "Enable HP Probe support");
		subintSC.no.ip.addSC("proxy-arp", "Enable proxy ARP");
		subintSC.no.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
		subintSC.no.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
		subintSC.no.ip.addSC("rip", "Router Information Protocol");
		subintSC.no.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
		subintSC.no.ip.addSC("router", "IP router interface commands");
		subintSC.no.ip.addSC("rsvp", "RSVP interface commands");
		subintSC.no.ip.addSC("sap", "Session Advertisement Protocol interface commands");
		subintSC.no.ip.addSC("sdr", "Session Directory Protocol interface commands");
		subintSC.no.ip.addSC("security", "DDN IP Security Option");
		subintSC.no.ip.addSC("split-horizon", "Perform split horizon");
		subintSC.no.ip.addSC("summary-address", "Perform address summarization");
		subintSC.no.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
		subintSC.no.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
		subintSC.no.ip.addSC("verify", "Enable per packet validation");
		subintSC.no.ip.addSC("vrf", "VPN Routing/Forwarding parameters on the interface");
		subintSC.no.ip.addSC("wccp", "WCCP interface commands");
	subintSC.no.addSC("llc2", "LLC2 Interface Subcommands");
	subintSC.no.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
	subintSC.no.addSC("netbios", "Use a defined NETBIOS access list or enable name-caching");
subintSC.addSC("ntp", "Configure NTP");
subintSC.addSC("rate-limit", "Rate Limit");
subintSC.addSC("service-policy", "Configure QoS Service Policy");
subintSC.addSC("shutdown", "Shutdown the selected interface");
subintSC.addSC("smds", "Modify SMDS parameters");
subintSC.addSC("smrp", "Simple Multicast Routing Protocol interface subcommands");
subintSC.addSC("sna", "SNA pu configuration");
subintSC.addSC("snapshot", "Configure snapshot support on the interface");
subintSC.addSC("timeout", "Define timeout values for this interface");
subintSC.addSC("traffic-shape", "Enable Traffic Shaping on an Interface or Sub-Interface");
subintSC.addSC("vines", "VINES interface subcommands");
subintSC.addSC("xns", "XNS interface subcommands");
