
lineauxC.addSC("absolute-timeout", "Set absolute timeout for line disconnection");
	lineauxC["absolute-timeout"].addSC("<0-10000>", "Absolute timeout interval in minutes");
lineauxC.addSC("access-class", "Filter connections based on an IP access list");
	lineauxC["access-class"].addSC("<1-199>", "IP access list");
	lineauxC["access-class"].addSC("<1300-2699>", "IP expanded access list");
lineauxC.addSC("activation-character", "Define the activation character");
	lineauxC["activation-character"].addSC("CHAR or <0-127>", "Activation character or its decimal equivalent");
lineauxC.addSC("arap", "Appletalk Remote Access Protocol");
	lineauxC.arap.addSC("dedicated", "Set line to only accept ARAP connections");
	lineauxC.arap.addSC("enable", "Enable ARAP connections");
	lineauxC.arap.addSC("net-access-list", "Net access list");
	lineauxC.arap.addSC("noguest", "Disallow guest logins");
	lineauxC.arap.addSC("require-manual-password", "Require manual entry of ARAP passwords");
	lineauxC.arap.addSC("timelimit", "Set maximum connection time");
	lineauxC.arap.addSC("use-tacacs", "Use TACACS to verify ARAP authentications");
	lineauxC.arap.addSC("warningtime", "Set connection disconnect warning time");
	lineauxC.arap.addSC("zonelist", "Zone access list");
lineauxC.addSC("autobaud", "Set line to normal autobaud");
lineauxC.addSC("autocommand", "Automatically execute an EXEC command");
	lineauxC.autocommand.addSC("LINE", "Appropriate EXEC command");
	lineauxC.autocommand.addSC("no-suppress-linenumber", "Display service linenumber message");
lineauxC.addSC("autocommand-options", "Autocommand options");
	lineauxC["autocommand-options"].addSC("abort-character", "Autocommand abort character");
	lineauxC["autocommand-options"].addSC("delay", "Delay autocommand execution");
	lineauxC["autocommand-options"].addSC("nohangup", "No hangup after autocommand completion");
lineauxC.addSC("autohangup", "Automatically hangup when last connection closes");
	lineauxC.autohangup.addSC("session-timeout", "Automatically hangup when current session Times-out");
lineauxC.addSC("autoselect", "Set line to autoselect");
	lineauxC.autoselect.addSC("arap", "Set line to allow ARAP autoselection");
	lineauxC.autoselect.addSC("during-login", "Do autoselect at the Username/Password prompt");
	lineauxC.autoselect.addSC("ppp", "Set line to allow PPP autoselection");
	lineauxC.autoselect.addSC("slip", "Set line to allow SLIP autoselection");
	lineauxC.autoselect.addSC("timeout", "Set wait timeout for initial autoselect byte");
lineauxC.addSC("buffer-length", "Set DMA buffer length");
	lineauxC["buffer-length"].addSC("<16-1536>", "buffer length in bytes");
lineauxC.addSC("callback", "Callback settings");
	lineauxC.callback.addSC("forced-wait", "Forced wait before callback script driven to modem");
	lineauxC.callback.addSC("nodsr-wait", "Extended wait time for DSR to go down");
lineauxC.addSC("data-character-bits", "Size of characters being handled");
	lineauxC["data-character-bits"].addSC("<7-8>", "Bits per character");
lineauxC.addSC("databits", "Set number of data bits per character");
	lineauxC.databits.addSC("5", "Number of data bits");
	lineauxC.databits.addSC("6", "");
	lineauxC.databits.addSC("<7-7>", "");
	lineauxC.databits.addSC("8", "");
lineauxC.addSC("default", "Set a command to its defaults");
	lineauxC["default"].addSC("absolute-timeout", "Set absolute timeout for line disconnection");
	lineauxC["default"].addSC("access-class", "Filter connections based on an IP access list");
	lineauxC["default"].addSC("activation-character", "Define the activation character");
	lineauxC["default"].addSC("arap", "Appletalk Remote Access Protocol");
	lineauxC["default"].addSC("autobaud", "Set line to normal autobaud");
	lineauxC["default"].addSC("autocommand", "Automatically execute an EXEC command");
	lineauxC["default"].addSC("autocommand-options", "Autocommand options");
	lineauxC["default"].addSC("autohangup", "Automatically hangup when last connection closes");
	lineauxC["default"].addSC("autoselect", "Set line to autoselect");
	lineauxC["default"].addSC("buffer-length", "Set DMA buffer length");
	lineauxC["default"].addSC("callback", "Callback settings");
	lineauxC["default"].addSC("data-character-bits", "Size of characters being handled");
	lineauxC["default"].addSC("databits", "Set number of data bits per character");
	lineauxC["default"].addSC("keymap-type", "Specify a keymap entry to");
lineauxC.addSC("disconnect-character", "Define the disconnect character");
	lineauxC["disconnect-character"].addSC("CHAR or <0-255>", "Disconnect character or its decimal equivalent");
lineauxC.addSC("dispatch-character", "Define the dispatch character");
	lineauxC["dispatch-character"].addSC("CHAR or <0-127>", "Dispatch character or its decimal equivalent");
lineauxC.addSC("dispatch-machine", "Reference a TCP dispatch state machine");
	lineauxC["dispatch-machine"].addSC("WORD", "Name of a defined state machine");
lineauxC.addSC("dispatch-timeout", "Set the dispatch timer");
	lineauxC["dispatch-timeout"].addSC("<0-4294967294>", "Dispatch timer in milliseconds");
lineauxC.addSC("domain-lookup", "Enable domain lookups in show commands");
lineauxC.addSC("editing", "Enable command line editing");
lineauxC.addSC("escape-character", "Change the current line's escape character");
	lineauxC["escape-character"].addSC("BREAK", "Cause escape on BREAK");
	lineauxC["escape-character"].addSC("CHAR or <0-255>", "Escape character or its ASCII decimal equivalent");
	lineauxC["escape-character"].addSC("DEFAULT", "Use default escape character");
	lineauxC["escape-character"].addSC("NONE", "Disable escape entirely");
	lineauxC["escape-character"].addSC("soft", "Set the soft escape character for this line");
lineauxC.addSC("exec", "Start an EXEC process");
lineauxC.addSC("exec-banner", "Enable the display of the EXEC banner");
lineauxC.addSC("exec-character-bits", "Size of characters to the command exec");
	lineauxC["exec-character-bits"].addSC("<7-8>", "Bits per character");
lineauxC.addSC("exec-timeout", "Set the EXEC timeout");
	lineauxC["exec-timeout"].addSC("<0-35791>", "Timeout in minutes");
		lineauxC["exec-timeout"]["<0-35791>"].addSC("<0-2147483>", "Timeout in seconds");
lineauxC.addSC("exit", "Exit from line configuration mode");
lineauxC.addSC("flowcontrol", "Set the flow control");
	lineauxC.flowcontrol.addSC("NONE", "Set no flow control");
	lineauxC.flowcontrol.addSC("hardware", "Set hardware flow control");
		lineauxC.flowcontrol.hardware.addSC("in", "Listen to flow control from the attached device");
		lineauxC.flowcontrol.hardware.addSC("out", "Send flow control information to the attached device");
	lineauxC.flowcontrol.addSC("software", "Set software flow control");
lineauxC.addSC("flush-at-activation", "Clear input stream at activation");
lineauxC.addSC("full-help", "Provide help to unprivileged user");
lineauxC.addSC("help", "Description of the interactive help system");
lineauxC.addSC("history", "Enable and control the command history function");
	lineauxC.history.addSC("size", "Set history buffer size");
lineauxC.addSC("hold-character", "Define the hold character");
	lineauxC["hold-character"].addSC("CHAR or <0-255>", "Hold character or its decimal equivalent");
lineauxC.addSC("insecure", "Mark line as 'insecure' for LAT");
lineauxC.addSC("international", "Enable international 8-bit character support");
lineauxC.addSC("ip", "IP options");
	lineauxC.ip.addSC("netmask-format", "Change display of netmasks");
	lineauxC.ip.addSC("tcp", "TCP options");
lineauxC.addSC("keymap-type", "Specify a keymap entry to use");
	lineauxC["keymap-type"].addSC("LINE", "Name of a keymap entry");
lineauxC.addSC("lat", "DEC Local Area Transport (LAT) protocol-specific configuration");
	lineauxC.lat.addSC("out-group", "Define group list for outgoing user-initiated connections");
	lineauxC.lat.addSC("remote-modification", "Set line to be remote modifiable");
//lineauxC.addSC("length", "Set number of lines on a screen");
	//lineauxC.length.addSC("<0-512>", "Number of lines on screen (0 for no pausing)");
lineauxC.addSC("location", "Enter terminal location description");
	lineauxC.location.addSC("LINE", "One text line describing the terminal's location");
lineauxC.addSC("lockable", "Allow users to lock a line");
lineauxC.addSC("logging", "Modify message logging facilities");
	lineauxC.logging.addSC("synchronous", "Synchronized message output");
lineauxC.addSC("login", "Enable password checking");
	lineauxC.login.addSC("local", "Local password checking");
	lineauxC.login.addSC("tacacs", "Use tacacs server for password checking");
lineauxC.addSC("logout-warning", "Set Warning countdown for absolute timeout of line");
	lineauxC["logout-warning"].addSC("<0-4294967295>", "Warning time in seconds");
lineauxC.addSC("modem", "Configure the Modem Control Lines");
	lineauxC.modem.addSC("CTS-Alarm", "Alarm device which only uses CTS for call control");
	lineauxC.modem.addSC("DTR-active", "Leave DTR low unless line has an active incoming connection or EXEC");
	lineauxC.modem.addSC("Dialin", "Configure line for a modern dial-in modem");
	lineauxC.modem.addSC("Host", "Devices that expect an incoming modem call");
	lineauxC.modem.addSC("InOut", "Configure line for incoming AND outgoing use of modem");
	lineauxC.modem.addSC("Printer", "Devices that require DSR/CD active");
	lineauxC.modem.addSC("answer-timeout", "Set interval between raising DTR and CTS response");
	lineauxC.modem.addSC("autoconfigure", "Automatically configure modem on line");
	lineauxC.modem.addSC("busyout", "Block calls to and from the modem");
	lineauxC.modem.addSC("dtr-delay", "Set interval during which DTR is held low");
lineauxC.addSC("monitor", "Copy debug output to the current terminal line");
lineauxC.addSC("motd-banner", "Enable the display of the MOTD banner");
lineauxC.addSC("no", "Negate a command or set its defaults");
	lineauxC.no.addSC("absolute-timeout", "Set absolute timeout for line disconnection");
	lineauxC.no.addSC("access-class", "Filter connections based on an IP access list");
	lineauxC.no.addSC("activation-character", "Define the activation character");
	lineauxC.no.addSC("arap", "Appletalk Remote Access Protocol");
	lineauxC.no.addSC("autobaud", "Set line to normal autobaud");
	lineauxC.no.addSC("autocommand", "Automatically execute an EXEC command");
	lineauxC.no.addSC("autocommand-options", "Autocommand options");
	lineauxC.no.addSC("autohangup", "Automatically hangup when last connection closes");
	lineauxC.no.addSC("autoselect", "Set line to autoselect");
	lineauxC.no.addSC("buffer-length", "Set DMA buffer length");
	lineauxC.no.addSC("callback", "Callback settings");
	lineauxC.no.addSC("data-character-bits", "Size of characters being handled");
	lineauxC.no.addSC("databits", "Set number of data bits per character");
	lineauxC.no.addSC("disconnect-character", "Define the disconnect character");
	lineauxC.no.addSC("dispatch-character", "Define the dispatch character");
	lineauxC.no.addSC("dispatch-machine", "Reference a TCP dispatch state machine");
	lineauxC.no.addSC("dispatch-timeout", "Set the dispatch timer");
	lineauxC.no.addSC("domain-lookup", "Enable domain lookups in show commands");
	lineauxC.no.addSC("editing", "Enable command line editing");
	lineauxC.no.addSC("escape-character", "Change the current line's escape character");
	lineauxC.no.addSC("exec", "Start an EXEC process");
	lineauxC.no.addSC("exec-banner", "Enable the display of the EXEC banner");
	lineauxC.no.addSC("exec-character-bits", "Size of characters to the command exec");
	lineauxC.no.addSC("exec-timeout", "Set the EXEC timeout");
	lineauxC.no.addSC("flowcontrol", "Set the flow control");
	lineauxC.no.addSC("flush-at-activation", "Clear input stream at activation");
	lineauxC.no.addSC("full-help", "Provide help to unprivileged user");
	lineauxC.no.addSC("history", "Enable and control the command history function");
	lineauxC.no.addSC("hold-character", "Define the hold character");
	lineauxC.no.addSC("insecure", "Mark line as 'insecure' for LAT");
	lineauxC.no.addSC("international", "Enable international 8-bit character support");
	lineauxC.no.addSC("ip", "IP options");
	lineauxC.no.addSC("keymap-type", "Specify a keymap entry to use");
	lineauxC.no.addSC("lat", "DEC Local Area Transport (LAT) protocol-specific configuration");
//	lineauxC.no.addSC("length", "Set number of lines on a screen");
	lineauxC.no.addSC("location", "Enter terminal location description");
	lineauxC.no.addSC("lockable", "Allow users to lock a line");
	lineauxC.no.addSC("logging", "Modify message logging facilities");
	lineauxC.no.addSC("login", "Enable password checking");
	lineauxC.no.addSC("logout-warning", "Set Warning countdown for absolute timeout of line");
	lineauxC.no.addSC("modem", "Configure the Modem Control Lines");
	lineauxC.no.addSC("monitor", "Copy debug output to the current terminal line");
	lineauxC.no.addSC("motd-banner", "Enable the display of the MOTD banner");
lineauxC.addSC("notify", "Inform users of output from concurrent sessions");
lineauxC.addSC("ntp", "Configure NTP");
	lineauxC.ntp.addSC("pps-discipline", "Use PPS pulse to discipline system clock");
	lineauxC.ntp.addSC("refclock", "NTP Reference Clock");
lineauxC.addSC("padding", "Set padding for a specified output character");
	lineauxC.padding.addSC("CHAR or <0-127>", "Character to be padded");
lineauxC.addSC("parity", "Set terminal parity");
	lineauxC.parity.addSC("even", "Even parity");
	lineauxC.parity.addSC("mark", "Mark parity");
	lineauxC.parity.addSC("none", "No parity");
	lineauxC.parity.addSC("odd", "Odd parity");
	lineauxC.parity.addSC("space", "Space parity");
lineauxC.addSC("password", "Set a password");
	lineauxC.password.addSC("<0-0>", "Specifies an UNENCRYPTED password will follow");
	lineauxC.password.addSC("<7-7>", "Specifies a HIDDEN password will follow");
		lineauxC.password["<7-7>"].addSC("WORD", "The HIDDEN line password string");
	lineauxC.password.addSC("LINE", "The UNENCRYPTED (cleartext) line password");
lineauxC.addSC("private", "Configuration options that user can set will remain in effect between terminal sessions");
lineauxC.addSC("privilege", "Change privilege level for line");
	lineauxC.privilege.addSC("level", "Assign default privilege level for line");
lineauxC.addSC("refuse-message", "Define a refuse banner");
	lineauxC["refuse-message"].addSC("LINE", "c refuse-text c, where 'c' is a delimiting character");
lineauxC.addSC("rotary", "Add line to a rotary group");
	lineauxC.rotary.addSC("<1-99>", "Rotary group to add line to");
lineauxC.addSC("rxspeed", "Set the receive speed");
	lineauxC.rxspeed.addSC("<0-4294967295>", "Receive speed");
lineauxC.addSC("script", "specify event related chat scripts to run on the line");
	lineauxC.script.addSC("activation", "chat script to run whenever line is activated");
	lineauxC.script.addSC("arap-callback", "chat script to run on line whenever ARAP callback is initiated");
	lineauxC.script.addSC("callback", "chat script to run on line whenever callback is initiated");
	lineauxC.script.addSC("connection", "chat script to run whenever connection is made to the line");
	lineauxC.script.addSC("dialer", "chat script to run whenever dialer makes an outgoing call");
	lineauxC.script.addSC("reset", "chat script to run whenever line is reset");
	lineauxC.script.addSC("startup", "chat script to run at system startup");
lineauxC.addSC("session-disconnect-warning", "Set warning countdown for session-timeout");
	lineauxC["session-disconnect-warning"].addSC("<0-4294967295>", "Session timeout warning in seconds");
lineauxC.addSC("session-limit", "Set maximum number of sessions");
	lineauxC["session-limit"].addSC("<0-4294967295>", "Maximum number of sessions");
lineauxC.addSC("session-timeout", "Set interval for closing connection when there is no input traffic");
	lineauxC["session-timeout"].addSC("<0-35791>", "Session timeout interval in minutes");
lineauxC.addSC("special-character-bits", "Size of the escape (and other special) characters");
	lineauxC["special-character-bits"].addSC("<7-8>", "Bits per character");
lineauxC.addSC("speed", "Set the transmit and receive speeds");
	lineauxC.speed.addSC("<0-4294967295>", "Transmit and receive speeds");
lineauxC.addSC("start-character", "Define the start character");
	lineauxC["start-character"].addSC("CHAR or <0-255>", "Start character or its decimal equivalent");
lineauxC.addSC("stop-character", "Define the stop character");
	lineauxC["stop-character"].addSC("CHAR or <0-255>", "Stop character or its decimal equivalent");
lineauxC.addSC("stopbits", "Set async line stop bits");
	lineauxC.stopbits.addSC("<1-1>", "One stop bit");
	lineauxC.stopbits.addSC("1.5", "One and one-half stop bits");
	lineauxC.stopbits.addSC("<2-2>", "Two stop bits");
lineauxC.addSC("telnet", "Telnet protocol-specific configuration");
	lineauxC.telnet.addSC("break-on-ip", "Send break signal when interrupt is received");
	lineauxC.telnet.addSC("ip-on-break", "Send interrupt signal when break is received");
	lineauxC.telnet.addSC("refuse-negotiations", "Suppress negotiations of Telnet Remote Echo and Suppress Go Ahead options");
	lineauxC.telnet.addSC("speed", "Specify line speeds");
	lineauxC.telnet.addSC("sync-on-break", "Send a Telnet Synchronize signal after receiving a Telnet Break signal");
	lineauxC.telnet.addSC("transparent", "Send a CR as a CR followed by a NULL instead of a CR followed by a LF");
lineauxC.addSC("terminal-type", "Set the terminal type");
	lineauxC["terminal-type"].addSC("WORD", "Terminal type");
lineauxC.addSC("timeout", "Timeouts for the line");
	lineauxC.timeout.addSC("login", "Timeouts related to the login sequence");
lineauxC.addSC("transport", "Define transport protocols for line");
	lineauxC.transport.addSC("input", "Define which protocols to use when connecting to the terminal server");
		lineauxC.transport.input.addSC("all", "All protocols");
		lineauxC.transport.input.addSC("lapb-ta", "LAPB Terminal Adapter");
		lineauxC.transport.input.addSC("lat", "DEC LAT protocol");
		lineauxC.transport.input.addSC("mop", "DEC MOP Remote Console Protocol");
		lineauxC.transport.input.addSC("nasi", "NASI protocol");
		lineauxC.transport.input.addSC("none", "No protocols");
		lineauxC.transport.input.addSC("pad", "X.3 PAD");
		lineauxC.transport.input.addSC("rlogin", "Unix rlogin protocol");
		lineauxC.transport.input.addSC("ssh", "TCP/IP SSH protocol");
		lineauxC.transport.input.addSC("telnet", "TCP/IP Telnet protocol");
		lineauxC.transport.input.addSC("udptn", "UDPTN async via UDP protocol");
		lineauxC.transport.input.addSC("v120", "Async over ISDN");
	lineauxC.transport.addSC("output", "Define which protocols to use for outgoing connections");
	lineauxC.transport.addSC("preferred", "Specify the preferred protocol to use");
lineauxC.addSC("txspeed", "Set the transmit speeds");
	lineauxC.txspeed.addSC("<0-4294967295>", "Transmit speed");
lineauxC.addSC("vacant-message", "Define a vacant banner");
	lineauxC["vacant-message"].addSC("LINE", "c vacant-text c, where 'c' is a delimiting character");
lineauxC.addSC("width", "Set width of the display terminal");
	lineauxC.width.addSC("<0-512>", "Number of characters on a screen line");
lineauxC.addSC("x25", "X25 protocol-specific configuration");
	lineauxC.x25.addSC("subaddress", "Include subaddress in outgoing PAD calls");
