
routerEIGRPC.addSC("auto-summary", "Enable automatic network number summarization");
routerEIGRPC.addSC("default", "Set a command to its defaults");
	routerEIGRPC["default"].addSC("auto-summary", "Enable automatic network number summarization");
routerEIGRPC.addSC("default-information", "Control distribution of default information");
	routerEIGRPC["default-information"].addSC("allowed", "Allow default information");
	routerEIGRPC["default-information"].addSC("in", "Accept default routing information");
	routerEIGRPC["default-information"].addSC("out", "Output default routing information");
routerEIGRPC.addSC("default-metric", "Set metric of redistributed routes");
	routerEIGRPC["default-metric"].addSC("<1-4294967295>", "Bandwidth in Kbits per second");
routerEIGRPC.addSC("distance", "Define an administrative distance");
	routerEIGRPC.distance.addSC("<1-255>", "Administrative distance");
	routerEIGRPC.distance.addSC("eigrp", "IP-EIGRP distance");
routerEIGRPC.addSC("distribute-list", "Filter networks in routing updates");
	routerEIGRPC["distribute-list"].addSC("<1-199>", "IP access list number");
	routerEIGRPC["distribute-list"].addSC("<1300-2699>", "IP expanded access list number");
	routerEIGRPC["distribute-list"].addSC("WORD", "Access-list name");
	routerEIGRPC["distribute-list"].addSC("gateway", "Filtering incoming updates based on gateway");
	routerEIGRPC["distribute-list"].addSC("prefix", "Filter prefixes in routing updates");
routerEIGRPC.addSC("eigrp", "EIGRP specific commands");
	routerEIGRPC.eigrp.addSC("log-neighbor-changes", "Enable/Disable IP-EIGRP neighbor logging");
	routerEIGRPC.eigrp.addSC("log-neighbor-warnings", "Enable/Disable IP-EIGRP neighbor warnings");
	routerEIGRPC.eigrp.addSC("router-id", "router-id for this EIGRP process");
	routerEIGRPC.eigrp.addSC("stub", "Set IP-EIGRP as stubbed router");
routerEIGRPC.addSC("exit", "Exit from routing protocol configuration mode");
routerEIGRPC.addSC("help", "Description of the interactive help system");
routerEIGRPC.addSC("maximum-paths", "Forward packets over multiple paths");
	routerEIGRPC["maximum-paths"].addSC("<1-6>", "Number of paths");
routerEIGRPC.addSC("metric", "Modify IGRP routing metrics and parameters");
	routerEIGRPC.metric.addSC("holddown", "Enable IGRP holddown");
	routerEIGRPC.metric.addSC("maximum-hops", "Advertise IGRP routes greater than <hops> as unreachable");
	routerEIGRPC.metric.addSC("weights", "Modify IGRP metric coefficients");
routerEIGRPC.addSC("mpls", "Configure MPLS routing protocol parameters");
routerEIGRPC.addSC("neighbor", "Specify a neighbor router");
	routerEIGRPC.neighbor.addSC("A.B.C.D", "Neighbor address");
routerEIGRPC.addSC("network", "Enable routing on an IP network");
	routerEIGRPC.network.addSC("A.B.C.D", "Network number");
		routerEIGRPC.network["A.B.C.D"].addSC("A.B.C.D", "EIGRP wild card bits");
routerEIGRPC.addSC("no", "Negate a command or set its defaults");
	routerEIGRPC.no.addSC("auto-summary", "Enable automatic network number summarization");
	routerEIGRPC.no.addSC("default-information", "Control distribution of default information");
	routerEIGRPC.no.addSC("default-metric", "Set metric of redistributed routes");
	routerEIGRPC.no.addSC("distance", "Define an administrative distance");
	routerEIGRPC.no.addSC("distribute-list", "Filter networks in routing updates");
	routerEIGRPC.no.addSC("eigrp", "EIGRP specific commands");
	routerEIGRPC.no.addSC("maximum-paths", "Forward packets over multiple paths");
	routerEIGRPC.no.addSC("metric", "Modify IGRP routing metrics and parameters");
	routerEIGRPC.no.addSC("mpls", "Configure MPLS routing protocol parameters");
	routerEIGRPC.no.addSC("neighbor", "Specify a neighbor router");
	routerEIGRPC.no.addSC("network", "Enable routing on an IP network");
routerEIGRPC.addSC("offset-list", "Add or subtract offset from IGRP or RIP metrics");
	routerEIGRPC["offset-list"].addSC("<0-99>", "Access list of networks to apply offset (0 selects all networks)");
	routerEIGRPC["offset-list"].addSC("<1300-1999>", "Access list of networks to apply offset (expanded range)");
	routerEIGRPC["offset-list"].addSC("WORD", "Access-list name");
routerEIGRPC.addSC("passive-interface", "Suppress routing updates on an interface");
	routerEIGRPC["passive-interface"].addSC("Async", "Async interface");
	routerEIGRPC["passive-interface"].addSC("BRI", "ISDN Basic Rate Interface");
	routerEIGRPC["passive-interface"].addSC("BVI", "Bridge-Group Virtual Interface");
	routerEIGRPC["passive-interface"].addSC("CTunnel", "CTunnel interface");
	routerEIGRPC["passive-interface"].addSC("Dialer", "Dialer interface");
	routerEIGRPC["passive-interface"].addSC("Ethernet", "IEEE 802.3");
	routerEIGRPC["passive-interface"].addSC("Group-Async", "Async Group interface");
	routerEIGRPC["passive-interface"].addSC("Lex", "Lex interface");
	routerEIGRPC["passive-interface"].addSC("Loopback", "Loopback interface");
	routerEIGRPC["passive-interface"].addSC("Multilink", "Multilink-group interface");
	routerEIGRPC["passive-interface"].addSC("Null", "Null interface");
	routerEIGRPC["passive-interface"].addSC("Serial", "Serial");
	routerEIGRPC["passive-interface"].addSC("Tunnel", "Tunnel interface");
	routerEIGRPC["passive-interface"].addSC("Vif", "PGM Multicast Host interface");
	routerEIGRPC["passive-interface"].addSC("Virtual-Template", "Virtual Template interface");
	routerEIGRPC["passive-interface"].addSC("Virtual-TokenRing", "Virtual TokenRing");
	routerEIGRPC["passive-interface"].addSC("default", "Suppress routing updates on all interfaces");
routerEIGRPC.addSC("redistribute", "Redistribute information from another routing protocol");
	routerEIGRPC.redistribute.addSC("bgp", "Border Gateway Protocol (BGP)");
	routerEIGRPC.redistribute.addSC("connected", "Connected");
	routerEIGRPC.redistribute.addSC("egp", "Exterior Gateway Protocol (EGP)");
	routerEIGRPC.redistribute.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
	routerEIGRPC.redistribute.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
	routerEIGRPC.redistribute.addSC("isis", "ISO IS-IS");
	routerEIGRPC.redistribute.addSC("iso-igrp", "IGRP for OSI networks");
	routerEIGRPC.redistribute.addSC("metric", "Metric for redistributed routes");
	routerEIGRPC.redistribute.addSC("mobile", "Mobile routes");
	routerEIGRPC.redistribute.addSC("odr", "On Demand stub Routes");
	routerEIGRPC.redistribute.addSC("ospf", "Open Shortest Path First (OSPF)");
	routerEIGRPC.redistribute.addSC("rip", "Routing Information Protocol (RIP)");
	routerEIGRPC.redistribute.addSC("route-map", "Route map reference");
	routerEIGRPC.redistribute.addSC("static", "Static routes");
routerEIGRPC.addSC("timers", "Adjust routing timers");
	routerEIGRPC.timers.addSC("active-time", "EIGRP time limit for active state");
routerEIGRPC.addSC("traffic-share", "How to compute traffic share over alternate paths");
	routerEIGRPC["traffic-share"].addSC("balanced", "Share inversely proportional to metric");
	routerEIGRPC["traffic-share"].addSC("min", "All traffic shared among min metric paths");
routerEIGRPC.addSC("variance", "Control load balancing variance");
	routerEIGRPC.variance.addSC("<1-128>", "Metric variance multiplier");
