
subintSC.addSC("appletalk", "Appletalk interface subcommands");
	subintSC.appletalk.addSC("access-group", "Apply an access list to inbound or outbound packets");
	subintSC.appletalk.addSC("address", "Set appletalk Phase 1 address");
	subintSC.appletalk.addSC("arp-timeout", "arp-timeout");
	subintSC.appletalk.addSC("cable-range", "Set appletalk Phase 2 address");
	subintSC.appletalk.addSC("discovery", "Reset discovery mode for new cable range discovery");
	subintSC.appletalk.addSC("distribute-list", "Filter networks from routing updates");
	subintSC.appletalk.addSC("free-trade-zone", "Enhanced security for one-way shared networks");
	subintSC.appletalk.addSC("getzonelist-filter", "Filter zone-list replies");
	subintSC.appletalk.addSC("glean-packets", "Glean AARP information from packets");
	subintSC.appletalk.addSC("protocol", "Select AppleTalk routing protocol");
	subintSC.appletalk.addSC("route-cache", "Enable appletalk route cache");
	subintSC.appletalk.addSC("rtmp-splithorizon", "Enable Split Horizon processing generating AT/RTMP updates");
	subintSC.appletalk.addSC("rtmp-stub", "Send only RTMP stubs, no routes in updates");
	subintSC.appletalk.addSC("send-rtmps", "Send Appletalk routing updates");
	subintSC.appletalk.addSC("zip-reply-filter", "Filter ZIP replies");
	subintSC.appletalk.addSC("zone", "Assign an appletalk zone name");
subintSC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	subintSC.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
	subintSC.arp.addSC("timeout", "Set ARP cache timeout");
subintSC.addSC("backup", "Modify backup parameters");
	subintSC.backup.addSC("delay", "Delays before backup line up or down transitions");
	subintSC.backup.addSC("interface", "Configure an interface as a backup");
subintSC.addSC("bandwidth", "Set bandwidth informational parameter");
	subintSC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
subintSC.addSC("bridge-group", "Transparent bridging interface parameters");
	subintSC["bridge-group"].addSC("<1-255>", "Assign an interface to a Bridge Group.");
subintSC.addSC("cdp", "CDP interface subcommands");
	subintSC.cdp.addSC("enable", "Enable CDP on interface");
subintSC.addSC("clns", "CLNS interface subcommands");
	subintSC.clns.addSC("access-group", "Filter inbound or outbound CLNS traffic");
	subintSC.clns.addSC("adjacency-filter", "Filter adjacencies");
	subintSC.clns.addSC("checksum", "Enable checksum generation");
	subintSC.clns.addSC("cluster-alias", "Enable DECnet Phase V cluster aliasing");
	subintSC.clns.addSC("dec-compatible", "Received NSAPs do not contain N-selector octet");
	subintSC.clns.addSC("enable", "Enable CLNS and ES-IS routing on interface");
	subintSC.clns.addSC("erpdu-interval", "Minimum interval between ERPDUs");
	subintSC.clns.addSC("es-neighbor", "End system SNPA static mapping configuration");
	subintSC.clns.addSC("esct-time", "Suggested ES configuration time");
	subintSC.clns.addSC("is-neighbor", "Intermediate system SNPA static mapping configuration");
	subintSC.clns.addSC("mtu", "Set MTU packet size for interface");
	subintSC.clns.addSC("net", "Set the CLNS address for this interface");
	subintSC.clns.addSC("rdpdu-interval", "Define the minimum interval between Redirect PDUs");
	subintSC.clns.addSC("router", "Enable CLNS routing protocol on interface");
	subintSC.clns.addSC("send-erpdu", "Send error PDUs when an error is detected in a data PDU");
	subintSC.clns.addSC("send-rdpdu", "Send redirect PDUs to optimize routing");
	subintSC.clns.addSC("split-horizon", "Enable ISO-IGRP split horizon");
subintSC.addSC("crypto", "Encryption/Decryption commands");
	subintSC.crypto.addSC("map", "Assign a Crypto Map");
		subintSC.crypto.map.addSC("WORD", "Crypto Map tag");
subintSC.addSC("decnet", "Interface DECnet config commands");
	subintSC.decnet.addSC("<0-3>", "ATG network number");
	subintSC.decnet.addSC("access-group", "Set access control for outgoing packets");
	subintSC.decnet.addSC("cluster-holdtime", "Interval to hold PhaseIV VAX cluster adjacencies");
	subintSC.decnet.addSC("cost", "Set cost value for interface");
	subintSC.decnet.addSC("hello-timer", "Set interval between transmitted HELLO messages");
	subintSC.decnet.addSC("in-routing-filter", "Set up access control for incoming routing information");
	subintSC.decnet.addSC("out-routing-filter", "Set up access control for outgoing routing information");
	subintSC.decnet.addSC("router-priority", "Set priority for determining default router");
	subintSC.decnet.addSC("routing-timer", "Set interval between transmitted routing messages");
	subintSC.decnet.addSC("split-horizon", "Enable split horizon on interface");
subintSC.addSC("default", "Set a command to its defaults");
	subintSC["default"].addSC("appletalk", "Appletalk interface subcommands");
	subintSC["default"].addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	subintSC["default"].addSC("backup", "Modify backup parameters");
	subintSC["default"].addSC("bandwidth", "Set bandwidth informational parameter");
	subintSC["default"].addSC("bridge-group", "Transparent bridging interface parameters");
	subintSC["default"].addSC("cdp", "CDP interface subcommands");
	subintSC["default"].addSC("clns", "CLNS interface subcommands");
	subintSC["default"].addSC("crypto", "Encryption/Decryption commands");
	subintSC["default"].addSC("decnet", "Interface DECnet config commands");
subintSC.addSC("delay", "Specify interface throughput delay");
	subintSC.delay.addSC("<1-16777215>", "Throughput delay (tens of microseconds)");
subintSC.addSC("description", "Interface specific description");
	subintSC.description.addSC("LINE", "Up to 240 characters describing this interface");
subintSC.addSC("dspu", "Down Stream PU");
	subintSC.dspu.addSC("enable-host", "DSPU Enable Host command");
	subintSC.dspu.addSC("enable-pu", "DSPU Enable Pu command");
	subintSC.dspu.addSC("start", "DSPU Start command");
subintSC.addSC("dxi", "ATM-DXI configuration commands");
	subintSC.dxi.addSC("interface-dfa", "Define a DFA as part of a subinterface");
	subintSC.dxi.addSC("map", "Map a given VPI and VCI to a ATM-DXI DFA");
	subintSC.dxi.addSC("pvc", "define PVC attributes");
subintSC.addSC("encapsulation", "Set encapsulation type for an interface");
	subintSC.encapsulation.addSC("sde", "IEEE 802.10 Virtual LAN - Secure Data Exchange");
subintSC.addSC("exit", "Exit from interface configuration mode");
subintSC.addSC("fras", "DLC Switch Interface Command");
	subintSC.fras.addSC("backup", "Setup backup route");
	subintSC.fras.addSC("ban", "RFC 1490 bridged 802.5");
	subintSC.fras.addSC("ddr-backup", "Setup backup route");
	subintSC.fras.addSC("map", "Set forwarding of frames");
subintSC.addSC("ip", "Interface Internet Protocol config commands");
	subintSC.ip.addSC("access-group", "Specify access control for packets");
	subintSC.ip.addSC("accounting", "Enable IP accounting on this interface");
	subintSC.ip.addSC("address", "Set the IP address of an interface");
		subintSC.ip.address.addSC("A.B.C.D", "IP address");
			subintSC.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
				subintSC.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
	subintSC.ip.addSC("authentication", "authentication subcommands");
	subintSC.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
			subintSC.ip["bandwidth-percent"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				subintSC.ip["bandwidth-percent"].eigrp.addSC("<1-65535>",  "Autonomous system number");
					subintSC.ip["bandwidth-percent"].eigrp["<1-65535>"].addSC("<1-999999>",  "Maximum bandwidth percentage that EIGRP may use");

	subintSC.ip.addSC("bgp", "BGP interface commands");
	subintSC.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
	subintSC.ip.addSC("cef", "Cisco Express Fowarding interface commands");
	subintSC.ip.addSC("cgmp", "Enable/disable CGMP");
	subintSC.ip.addSC("dhcp", "Configure DHCP parameters for this interface");
	subintSC.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
	subintSC.ip.addSC("dvmrp", "DVMRP interface commands");
	subintSC.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
	subintSC.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
	subintSC.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
	subintSC.ip.addSC("igmp", "IGMP interface commands");
	subintSC.ip.addSC("irdp", "ICMP Router Discovery Protocol");
	subintSC.ip.addSC("load-sharing", "Style of load sharing");
	subintSC.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
	subintSC.ip.addSC("mobile", "Mobile IP support");
	subintSC.ip.addSC("mrm", "Configure IP Multicast Routing Monitor tester");
	subintSC.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
	subintSC.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
	subintSC.ip.addSC("multicast", "IP multicast interface commands");
	subintSC.ip.addSC("nat", "NAT interface commands");
		subintSC.ip.nat.addSC("inside", "Inside interface for address translation");
		subintSC.ip.nat.addSC("outside", "Outside interface for address translation");
	subintSC.ip.addSC("nbar", "Network-Based Application Recognition");
	subintSC.ip.addSC("nhrp", "NHRP interface subcommands");
	subintSC.ip.addSC("ospf", "OSPF interface commands");
		subintSC.ip.ospf.addSC("authentication", "Enable authentication");
		subintSC.ip.ospf.addSC("authentication-key", "Authentication password (key)");
		subintSC.ip.ospf.addSC("cost", "Interface cost");
			subintSC.ip.ospf.cost.addSC("<1-65535>",  "Cost");
		subintSC.ip.ospf.addSC("database-filter", "Filter OSPF LSA during synchronization and flooding");
		subintSC.ip.ospf.addSC("dead-interval", "Interval after which a neighbor is declared dead");
			subintSC.ip.ospf["dead-interval"].addSC("<1-65535>", "Seconds");
		subintSC.ip.ospf.addSC("demand-circuit", "OSPF demand circuit");
		subintSC.ip.ospf.addSC("flood-reduction", "OSPF Flood Reduction");
		subintSC.ip.ospf.addSC("hello-interval", "Time between HELLO packets");
			subintSC.ip.ospf["hello-interval"].addSC("<1-65535>", "Seconds");
		subintSC.ip.ospf.addSC("message-digest-key", "Message digest authentication password (key)");
		subintSC.ip.ospf.addSC("mtu-ignore", "Ignores the MTU in DBD packets");
		subintSC.ip.ospf.addSC("network", "Network type");
		subintSC.ip.ospf.addSC("priority", "Router priority");
		subintSC.ip.ospf.addSC("retransmit-interval", "Time between retransmitting lost link state advertisements");
		subintSC.ip.ospf.addSC("transmit-delay", "Link state transmit delay");
	subintSC.ip.addSC("pgm", "PGM Reliable Transport Protocol");
	subintSC.ip.addSC("pim", "PIM interface commands");
	subintSC.ip.addSC("policy", "Enable policy routing");
	subintSC.ip.addSC("probe", "Enable HP Probe support");
	subintSC.ip.addSC("proxy-arp", "Enable proxy ARP");
	subintSC.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
	subintSC.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
	subintSC.ip.addSC("rgmp", "Enable/disable RGMP");
	subintSC.ip.addSC("rip", "Router Information Protocol");
	subintSC.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
	subintSC.ip.addSC("router", "IP router interface commands");
	subintSC.ip.addSC("rsvp", "RSVP interface commands");
	subintSC.ip.addSC("sap", "Session Announcement Protocol interface commands");
	subintSC.ip.addSC("security", "DDN IP Security Option");
	subintSC.ip.addSC("split-horizon", "Perform split horizon");
	subintSC.ip.addSC("summary-address", "Perform address summarization");
      subintSC.ip["summary-address"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
         subintSC.ip["summary-address"].eigrp.addSC("<1-65535>", "Autonomous system number");
            subintSC.ip["summary-address"].eigrp["<1-65535>"].addSC("A.B.C.D", "IP address");
               subintSC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"].addSC("A.B.C.D", "IP network mask");
                  subintSC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"]["A.B.C.D"].addSC("<1-255>", "Administrative distance");
      subintSC.ip["summary-address"].addSC("rip", "Routing Information Protocol (RIP)");
         subintSC.ip["summary-address"].rip.addSC("A.B.C.D", "IP address");
            subintSC.ip["summary-address"].rip["A.B.C.D"].addSC("A.B.C.D", "IP network mask");

	subintSC.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
	subintSC.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
	subintSC.ip.addSC("urd", "Configure URL Rendezvousing");
	subintSC.ip.addSC("verify", "Enable per packet validation");
	subintSC.ip.addSC("vrf", "VPN Routing/Forwarding parameters on the interface");
	subintSC.ip.addSC("wccp", "WCCP interface commands");
subintSC.addSC("isis", "IS-IS commands");
	subintSC.isis.addSC("adjacency-filter", "Filter IS-IS adjacencies");
	subintSC.isis.addSC("circuit-type", "Configure circuit type for interface");
	subintSC.isis.addSC("csnp-interval", "Set CSNP interval in seconds");
	subintSC.isis.addSC("hello", "Add padding to IS-IS hello packets");
	subintSC.isis.addSC("hello-interval", "Set Hello interval in seconds");
	subintSC.isis.addSC("hello-multiplier", "Set multiplier for Hello holding time");
	subintSC.isis.addSC("lsp-interval", "Set LSP transmission interval");
	subintSC.isis.addSC("mesh-group", "Set ISIS mesh group");
	subintSC.isis.addSC("metric", "Configure the metric for interface");
	subintSC.isis.addSC("password", "Configure the authentication password for interface");
	subintSC.isis.addSC("priority", "Set priority for Designated Router election");
	subintSC.isis.addSC("retransmit-interval", "Set per-LSP retransmission interval");
	subintSC.isis.addSC("retransmit-throttle-interval", "Set interface LSP retransmission interval");
	subintSC.isis.addSC("three-way-handshake", "Select Cisco or IETF three-way handshake");
subintSC.addSC("iso-igrp", "ISO-IGRP interface subcommands");
	subintSC["iso-igrp"].addSC("adjacency-filter", "Filter ISO-IGRP adjacencies");
subintSC.addSC("lat", "LAT commands");
	subintSC.lat.addSC("enabled", "Enable LAT protocol translation");
	subintSC.lat.addSC("host", "Statically define LAT services");
subintSC.addSC("llc2", "LLC2 Interface Subcommands");
	subintSC.llc2.addSC("N2", "Number of times router should retry various operations");
	subintSC.llc2.addSC("ack-delay-time", "Max time the router allows incoming I-frames to stay unacknowledged");
	subintSC.llc2.addSC("ack-max", "Max number of I-frames received before an acknowledgment must be sent");
	subintSC.llc2.addSC("adm-timer-value", "How long router waits in ADM before giving up.");
	subintSC.llc2.addSC("dynwind", "Congestion control with dynamic window");
	subintSC.llc2.addSC("idle-time", "Frequency of polls during periods of idle traffic");
	subintSC.llc2.addSC("local-window", "Max number of I-frames to send before waiting for an acknowledgment");
	subintSC.llc2.addSC("t1-time", "How long router waits for an acknowledgment to transmitted I-frames");
	subintSC.llc2.addSC("tbusy-time", "Amount of time router waits while the other LLC2 station is in a busy state before attempting to poll the remote station");
	subintSC.llc2.addSC("tpf-time", "Amount of time router waits for a final response to a poll frame before re-sending the original poll frame");
	subintSC.llc2.addSC("trej-time", "Amount of time router waits for a resend of a rejected frame before sending the reject command");
	subintSC.llc2.addSC("txq-max", "Queue for holding llc2 information frames");
	subintSC.llc2.addSC("xid-neg-val-time", "Frequency of exchange of identification (XID)");
	subintSC.llc2.addSC("xid-retry-time", "How long router waits for reply to XID");
subintSC.addSC("mls", "mls sub/interface commands");
	subintSC.mls.addSC("rp", "rp");
subintSC.addSC("mpls", "Configure MPLS interface parameters");
	subintSC.mpls.addSC("ip", "Configure dynamic MPLS forwarding for IP");
	subintSC.mpls.addSC("mtu", "Set tag switching Maximum Transmission Unit");
	subintSC.mpls.addSC("netflow", "Configure Egress Netflow Accounting");
	subintSC.mpls.addSC("traffic-eng", "Configure Traffic Engineering parameters");
subintSC.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
	subintSC.mtu.addSC("<64-18000>", "MTU size in bytes");
subintSC.addSC("netbios", "Use a defined NETBIOS access list or enable name-caching");
	subintSC.netbios.addSC("input-access-filter", "Access list filter on incoming messages");
	subintSC.netbios.addSC("output-access-filter", "Access list filter on outgoing messages");
subintSC.addSC("no", "Negate a command or set its defaults");
	subintSC.no.addSC("appletalk", "Appletalk interface subcommands");
	subintSC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	subintSC.no.addSC("backup", "Modify backup parameters");
	subintSC.no.addSC("bandwidth", "Set bandwidth informational parameter");
	subintSC.no.addSC("bridge-group", "Transparent bridging interface parameters");
	subintSC.no.addSC("cdp", "CDP interface subcommands");
	subintSC.no.addSC("clns", "CLNS interface subcommands");
	subintSC.no.addSC("crypto", "Encryption/Decryption commands");
	subintSC.no.addSC("decnet", "Interface DECnet config commands");
	subintSC.no.addSC("delay", "Specify interface throughput delay");
	subintSC.no.addSC("description", "Interface specific description");
	subintSC.no.addSC("dspu", "Down Stream PU");
	subintSC.no.addSC("dxi", "ATM-DXI configuration commands");
	subintSC.no.addSC("encapsulation", "Set encapsulation type for an interface");
	subintSC.no.addSC("fras", "DLC Switch Interface Command");
	subintSC.no.addSC("ip", "Interface Internet Protocol config commands");
		subintSC.no.ip.addSC("access-group", "Specify access control for packets");
		subintSC.no.ip.addSC("accounting", "Enable IP accounting on this interface");
		subintSC.no.ip.addSC("address", "Set the IP address of an interface");
			subintSC.no.ip.address.addSC("A.B.C.D", "IP address");
				subintSC.no.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
					subintSC.no.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
		subintSC.no.ip.addSC("authentication", "authentication subcommands");
		subintSC.no.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
		subintSC.no.ip.addSC("bgp", "BGP interface commands");
		subintSC.no.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		subintSC.no.ip.addSC("cef", "Cisco Express Fowarding interface commands");
		subintSC.no.ip.addSC("cgmp", "Enable/disable CGMP");
		subintSC.no.ip.addSC("dhcp", "Configure DHCP parameters for this interface");
		subintSC.no.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
		subintSC.no.ip.addSC("dvmrp", "DVMRP interface commands");
		subintSC.no.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
		subintSC.no.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
		subintSC.no.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
		subintSC.no.ip.addSC("igmp", "IGMP interface commands");
		subintSC.no.ip.addSC("irdp", "ICMP Router Discovery Protocol");
		subintSC.no.ip.addSC("load-sharing", "Style of load sharing");
		subintSC.no.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
		subintSC.no.ip.addSC("mobile", "Mobile IP support");
		subintSC.no.ip.addSC("mrm", "Configure IP Multicast Routing Monitor tester");
		subintSC.no.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
		subintSC.no.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		subintSC.no.ip.addSC("multicast", "IP multicast interface commands");
		subintSC.no.ip.addSC("nat", "NAT interface commands");
		subintSC.no.ip.addSC("nbar", "Network-Based Application Recognition");
		subintSC.no.ip.addSC("nhrp", "NHRP interface subcommands");
		subintSC.no.ip.addSC("ospf", "OSPF interface commands");
		subintSC.no.ip.addSC("pgm", "PGM Reliable Transport Protocol");
		subintSC.no.ip.addSC("pim", "PIM interface commands");
		subintSC.no.ip.addSC("policy", "Enable policy routing");
		subintSC.no.ip.addSC("probe", "Enable HP Probe support");
		subintSC.no.ip.addSC("proxy-arp", "Enable proxy ARP");
		subintSC.no.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
		subintSC.no.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
		subintSC.no.ip.addSC("rgmp", "Enable/disable RGMP");
		subintSC.no.ip.addSC("rip", "Router Information Protocol");
		subintSC.no.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
		subintSC.no.ip.addSC("router", "IP router interface commands");
		subintSC.no.ip.addSC("rsvp", "RSVP interface commands");
		subintSC.no.ip.addSC("sap", "Session Announcement Protocol interface commands");
		subintSC.no.ip.addSC("security", "DDN IP Security Option");
		subintSC.no.ip.addSC("split-horizon", "Perform split horizon");
		subintSC.no.ip.addSC("summary-address", "Perform address summarization");
		subintSC.no.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
		subintSC.no.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
		subintSC.no.ip.addSC("urd", "Configure URL Rendezvousing");
		subintSC.no.ip.addSC("verify", "Enable per packet validation");
		subintSC.no.ip.addSC("vrf", "VPN Routing/Forwarding parameters on the interface");
		subintSC.no.ip.addSC("wccp", "WCCP interface commands");
	subintSC.no.addSC("isis", "IS-IS commands");
	subintSC.no.addSC("iso-igrp", "ISO-IGRP interface subcommands");
	subintSC.no.addSC("lat", "LAT commands");
	subintSC.no.addSC("llc2", "LLC2 Interface Subcommands");
	subintSC.no.addSC("mls", "mls sub/interface commands");
	subintSC.no.addSC("mpls", "Configure MPLS interface parameters");
	subintSC.no.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
	subintSC.no.addSC("netbios", "Use a defined NETBIOS access list or enable name-caching");
subintSC.addSC("ntp", "Configure NTP");
	subintSC.ntp.addSC("broadcast", "Configure NTP broadcast service");
	subintSC.ntp.addSC("disable", "Disable NTP");
	subintSC.ntp.addSC("multicast", "Configure NTP multicast service");
subintSC.addSC("pulse-time", "Force DTR low during resets");
	subintSC["pulse-time"].addSC("<0-60>", "DTR low time in seconds");
subintSC.addSC("rate-limit", "Rate Limit");
	subintSC["rate-limit"].addSC("input", "Rate limit on input");
	subintSC["rate-limit"].addSC("output", "Rate limit on output");
subintSC.addSC("service-policy", "Configure QoS Service Policy");
	subintSC["service-policy"].addSC("history", "Keep history of QoS metrics");
	subintSC["service-policy"].addSC("input", "Assign policy-map to the input of an interface");
	subintSC["service-policy"].addSC("output", "Assign policy-map to the output of an interface");
subintSC.addSC("shutdown", "Shutdown the selected interface");
subintSC.addSC("smds", "Modify SMDS parameters");
	subintSC.smds.addSC("address", "Set an interface SMDS address");
	subintSC.smds.addSC("enable-arp", "Enable ARP processing.");
	subintSC.smds.addSC("glean-mode", "SMDS GLEAN mode");
	subintSC.smds.addSC("multicast", "Set an SMDS multicast (or broadcast) address");
	subintSC.smds.addSC("static-map", "Map high level protocol address to SMDS address");
subintSC.addSC("smrp", "Simple Multicast Routing Protocol interface subcommands");
	subintSC.smrp.addSC("mroute-cache", "Enable SMRP route cache");
	subintSC.smrp.addSC("protocol", "Specify network layer service protocol");
subintSC.addSC("sna", "SNA pu configuration");
	subintSC.sna.addSC("enable-host", "SNA Enable Host command");
	subintSC.sna.addSC("start", "SNA Start command");
subintSC.addSC("snapshot", "Configure snapshot support on the interface");
	subintSC.snapshot.addSC("client", "Enable client control of Snapshot routing");
	subintSC.snapshot.addSC("server", "Send routing updates out this link when updates are received");
subintSC.addSC("tag-switching", "Tag Switching interface configuration commands");
	subintSC["tag-switching"].addSC("ip", "Configure IP dynamic Tag Switching");
	subintSC["tag-switching"].addSC("mtu", "Set tag switching Maximum Transmission Unit");
subintSC.addSC("tarp", "TARP interface subcommands");
	subintSC.tarp.addSC("enable", "Enable TARP on interface");
	subintSC.tarp.addSC("propagate", "Enable propagation of TARP PDU's out on this interface");
	subintSC.tarp.addSC("split-horizon", "Enable split horizon for TARP propagation on this interface");
subintSC.addSC("timeout", "Define timeout values for this interface");
	subintSC.timeout.addSC("absolute", "Define session timeout value for this interface");
subintSC.addSC("traffic-shape", "Enable Traffic Shaping on an Interface or Sub-Interface");
	subintSC["traffic-shape"].addSC("group", "configure token bucket: group <access-list> CIR (bps) [Bc (bits) [Be (bits)]]");
	subintSC["traffic-shape"].addSC("rate", "configure token bucket: CIR (bps) [Bc (bits) [Be (bits)]]");
subintSC.addSC("vines", "VINES interface subcommands");
	subintSC.vines.addSC("access-group", "Apply a VINES access list");
	subintSC.vines.addSC("arp-enable", "Supply VINES addresses to booting clients");
	subintSC.vines.addSC("encapsulation", "VINES encapsulation");
	subintSC.vines.addSC("input-network-filter", "Filter networks in received routing updates");
	subintSC.vines.addSC("input-router-filter", "Filter source of received routing updates");
	subintSC.vines.addSC("metric", "VINES processing on the selected interface");
	subintSC.vines.addSC("neighbor", "Create a static neighbor entry");
	subintSC.vines.addSC("output-network-filter", "Filter networks sent in routing updates");
	subintSC.vines.addSC("propagate", "Ignore 'class' field during broadcast forwarding");
	subintSC.vines.addSC("redirect", "Set redirect interval");
	subintSC.vines.addSC("route-cache", "Fast switch VINES packets out this interface");
	subintSC.vines.addSC("serverless", "The attached network has no Banyan server");
	subintSC.vines.addSC("split-horizon", "Split-horizon routing updates");
	subintSC.vines.addSC("update", "Set RTP update characteristics for this interface");
subintSC.addSC("xns", "XNS interface subcommands");
	subintSC.xns.addSC("access-group", "Apply an access list to output packets");
	subintSC.xns.addSC("encapsulation", "Set encapsulation method for XNS packets");
	subintSC.xns.addSC("flood", "Flood XNS packets");
	subintSC.xns.addSC("hear-rip", "Listen to RIP updates");
	subintSC.xns.addSC("helper-address", "Forward broadcasts to a specific address");
	subintSC.xns.addSC("input-network-filter", "Filter incoming routing updates");
	subintSC.xns.addSC("network", "Assign an XNS network & enable XNS routing");
	subintSC.xns.addSC("output-network-filter", "Filter outgoing routing updates");
	subintSC.xns.addSC("route-cache", "Enable fast switching");
	subintSC.xns.addSC("router-filter", "Filter sources of routing updates");
	subintSC.xns.addSC("update-time", "Set XNS routing update timer");
