
enableC.addSC("access-enable", "Create a temporary Access-List entry");
enableC.addSC("access-profile", "Apply user-profile to interface");
enableC.addSC("access-template", "Create a temporary Access-List entry");
enableC.addSC("archive", "manage archive files");
enableC.addSC("cd", "Change current directory");
enableC.addSC("clear", "Reset functions");
	enableC.clear.addSC("access-list", "Clear access list statistical information");
	enableC.clear.addSC("access-template", "Access-template");
	enableC.clear.addSC("arp-cache", "Clear the entire ARP cache");
	enableC.clear.addSC("bgp", "Clear BGP connections");
	enableC.clear.addSC("bridge", "Reset bridge forwarding cache");
	enableC.clear.addSC("cdp", "Reset cdp information");
	enableC.clear.addSC("counters", "Clear counters on one or all interfaces");
	enableC.clear.addSC("dialer", "Clear dialer statistics");
	enableC.clear.addSC("interface", "Clear the hardware logic on an interface");
	enableC.clear.addSC("ip", "IP");
		enableC.clear.ip.addSC("ospf", "OSPF clear commands");
		enableC.clear.ip.addSC("route", "Delete route table entries");
enableC.addSC("clock", "Manage the system clock");
	enableC.clock.addSC("set", "Set the time and date");
		enableC.clock.set.addSC("hh:mm:ss", "Current Time");
enableC.addSC("configure", "Enter configuration mode");
	enableC.configure.addSC("terminal", "Configure from the terminal");
enableC.addSC("connect", "Open a terminal connection");
	enableC.copy.addSC("nvram:", "Copy from nvram: file system");
	enableC.copy.addSC("running-config", "Copy from current system configuration");
		enableC.copy["running-config"].addSC("startup-config", "Copy to startup configuration");
	enableC.copy.addSC("startup-config", "Copy from startup configuration");
		enableC.copy["startup-config"].addSC("running-config", "Update (merge with) current system configuration");
		leC.copy.addSC("system:", "Copy from system: file system");
	enableC.copy.addSC("tftp:", "Copy from tftp: file system");
	enableC.copy.addSC("xmodem:", "Copy from xmodem: file system");
	enableC.copy.addSC("ymodem:", "Copy from ymodem: file system");
enableC.addSC("debug", "Debugging functions (see also 'undebug')");
    enableC.debug.addSC("aaa", "AAA Authentication, Authorization and Accounting");
  	enableC.debug.addSC("access-expression", "Boolean access expression");
  	enableC.debug.addSC("adjacency", "adjacency");
  	enableC.debug.addSC("all", "Enable all debugging");
  	enableC.debug.addSC("alps", "ALPS debug information");
  	enableC.debug.addSC("apollo", "Apollo information");
  	enableC.debug.addSC("apple", "Appletalk information");
  	enableC.debug.addSC("arap", "Appletalk Remote Access");
  	enableC.debug.addSC("arp", "IP ARP and HP Probe transactions");
  	enableC.debug.addSC("aspp", "ASPP information");
  	enableC.debug.addSC("async", "Async interface information");
  	enableC.debug.addSC("backup", "Backup events");
  	enableC.debug.addSC("bri-interface", "bri network interface events");
  	enableC.debug.addSC("bsc", "BSC information");
  	enableC.debug.addSC("bstun", "BSTUN information");
  	enableC.debug.addSC("call", "Call Information");
  	enableC.debug.addSC("call-mgmt", "Call Management");
  	enableC.debug.addSC("callback", "Callback activity");
  	enableC.debug.addSC("cca", "CCA activity");
  	enableC.debug.addSC("ccfrf11", "CCFRF11 information");
  	enableC.debug.addSC("cch323", "CCH323 information");
  	enableC.debug.addSC("ccsip", "CCSIP information");
  	enableC.debug.addSC("ccswvoice", "ccswvoice information");
  	enableC.debug.addSC("cdapi", "CDAPI information");
  	enableC.debug.addSC("cdp", "CDP information");
  	enableC.debug.addSC("ces-conn", "Connection Manager CES Client Info");
  	enableC.debug.addSC("chat", "Chat scripts activity");
  	enableC.debug.addSC("clns", "CLNS information");
  	enableC.debug.addSC("cls", "CLS Information");
  	enableC.debug.addSC("cns", "CNS Debugging");
  	enableC.debug.addSC("compress", "COMPRESS traffic");
  	enableC.debug.addSC("condition", "Condition");
  	enableC.debug.addSC("confmodem", "Modem configuration database");
  	enableC.debug.addSC("conn", "Connection Manager information");
  	enableC.debug.addSC("cops", "COPS");
  	enableC.debug.addSC("cpp", "Cpp information");
  	enableC.debug.addSC("crypto", "Cryptographic subsystem");
  		enableC.debug.crypto.addSC("ber", "decode ASN.1 BER data");
  		enableC.debug.crypto.addSC("engine", "Crypto Engine Debug");
  		enableC.debug.crypto.addSC("ipsec", "IPSEC processing");
  		enableC.debug.crypto.addSC("isakmp", "ISAKMP Key Management");
  		enableC.debug.crypto.addSC("pki", "PKI Client");
  		enableC.debug.crypto.addSC("verbose", "verbose decode");
  	enableC.debug.addSC("ctunnel", "Generic CTunnel Interface");
  	enableC.debug.addSC("custom-queue", "Custom output queueing");
  	enableC.debug.addSC("decnet", "DECnet information");
  	enableC.debug.addSC("dhcp", "DHCP client activity");
  	enableC.debug.addSC("dialer", "Dial on Demand");
  		enableC.debug.dhcp.addSC("detail", "DHCP packet content");
  	enableC.debug.addSC("dlsw", "Data Link Switching (DLSw) events");
  	enableC.debug.addSC("dnsix", "Dnsix information");
  	enableC.debug.addSC("domain", "Domain Name System");
		enableC.debug.domain.addSC("replies", "DNS replies only");

  	enableC.debug.addSC("drip", "DRiP debug information");
  	enableC.debug.addSC("dspu", "DSPU Information");
  	enableC.debug.addSC("dss", "Debug DSS");
  	enableC.debug.addSC("dxi", "atm-dxi information");
		enableC.debug.dxi.addSC("events", "Important atm-dxi events");
		enableC.debug.dxi.addSC("packet", "ATM DXI packets");

	enableC.addSC("eigrp",               "EIGRP Protocol information");
 	   enableC.debug.eigrp.addSC("fsm",        "EIGRP Dual Finite State Machine events/actions");
 	   enableC.debug.eigrp.addSC("neighbors",  "EIGRP neighbors");
 	   enableC.debug.eigrp.addSC("packets",    "EIGRP packets");
	   enableC.debug.eigrp.addSC("transmit",   "EIGRP transmission events");
  	enableC.debug.addSC("entry", "Incoming queue entries");
  	enableC.debug.addSC("ethernet-interface", "Ethernet network interface events");
  	enableC.debug.addSC("fastethernet", "Fast Ethernet interface information");
  	enableC.debug.addSC("fax", "Fax");
  	enableC.debug.addSC("frame-relay", "Frame Relay");
  	enableC.debug.addSC("fras", "FRAS Debug");
  	enableC.debug.addSC("fras-host", "FRAS Host Debug");
  	enableC.debug.addSC("funi", "FUNI interface packets");
  	enableC.debug.addSC("gssapi", "GSSAPI debugs");
  	enableC.debug.addSC("h225", "H.225 Library Debugging");
  	enableC.debug.addSC("h245", "H.245 Library Debugging");
  	enableC.debug.addSC("interface", "interface");
  	enableC.debug.addSC("ip", "IP information");
  		enableC.debug.ip.addSC("bgp", "BGP information");
  		enableC.debug.ip.addSC("cache", "IP cache operations");
  		enableC.debug.ip.addSC("casa", "Casa debugging");
  		enableC.debug.ip.addSC("cef", "IP CEF operations");
  		enableC.debug.ip.addSC("cgmp", "CGMP protocol activity");
  		enableC.debug.ip.addSC("dhcp", "Dynamic Host Configuration Protocol");
  		enableC.debug.ip.addSC("drp", "Director response protocol");
  		enableC.debug.ip.addSC("dvmrp", "DVMRP protocol activity");
  		enableC.debug.ip.addSC("egp", "EGP information");
  		enableC.debug.ip.addSC("eigrp", "IP-EIGRP information");
  		enableC.debug.ip.addSC("error", "IP error debugging");
  		enableC.debug.ip.addSC("flow", "IP Flow switching operations");
  		enableC.debug.ip.addSC("ftp", "FTP dialogue");
  		enableC.debug.ip.addSC("html", "HTML connections");
  		enableC.debug.ip.addSC("http", "HTTP connections");
  		enableC.debug.ip.addSC("icmp", "ICMP transactions");
  		enableC.debug.ip.addSC("igmp", "IGMP protocol activity");
  		enableC.debug.ip.addSC("igrp", "IGRP information");
  		enableC.debug.ip.addSC("interface", "IP interface configuration changes");
  		enableC.debug.ip.addSC("mbgp", "MBGP information");
  		enableC.debug.ip.addSC("mcache", "IP multicast cache operations");
  		enableC.debug.ip.addSC("mhbeat", "IP multicast heartbeat monitoring");
  		enableC.debug.ip.addSC("mobile", "IP Mobility");
  		enableC.debug.ip.addSC("mpacket", "IP multicast packet debugging");
  		enableC.debug.ip.addSC("mrm", "IP Multicast Routing Monitor");
  		enableC.debug.ip.addSC("mrouting", "IP multicast routing table activity");
  		enableC.debug.ip.addSC("msdp", "Multicast Source Discovery Protocol (MSDP)");
  		enableC.debug.ip.addSC("mtag", "IP multicast tagswitching activity");
  		enableC.debug.ip.addSC("nat", "NAT events");
  		enableC.debug.ip.addSC("nbar", "StILE - traffic classification Engine");
  		enableC.debug.ip.addSC("ospf", "OSPF information");
  			enableC.debug.ip.ospf.addSC("adj", "OSPF adjacency events");
  			enableC.debug.ip.ospf.addSC("database-timer", "OSPF database timer");
  			enableC.debug.ip.ospf.addSC("events", "OSPF events");
  			enableC.debug.ip.ospf.addSC("flood", "OSPF flooding");
  			enableC.debug.ip.ospf.addSC("hello", "OSPF hello events");
  			enableC.debug.ip.ospf.addSC("lsa-generation", "OSPF lsa generation");
  			enableC.debug.ip.ospf.addSC("mpls", "OSPF MPLS");
  			enableC.debug.ip.ospf.addSC("packet", "OSPF packets");
  			enableC.debug.ip.ospf.addSC("retransmission", "OSPF retransmission events");
  			enableC.debug.ip.ospf.addSC("spf", "OSPF spf");
  			enableC.debug.ip.ospf.addSC("tree", "OSPF database tree");
  		enableC.debug.ip.addSC("packet", "General IP debugging and IPSO security transactions");
  		enableC.debug.ip.addSC("peer", "IP peer address activity");
  		enableC.debug.ip.addSC("pgm", "PGM Reliable Transport Protocol");
  		enableC.debug.ip.addSC("pim", "PIM protocol activity");
  		enableC.debug.ip.addSC("policy", "Policy routing");
  		enableC.debug.ip.addSC("rgmp", "RGMP protocol activity");
  		enableC.debug.ip.addSC("rip", "RIP protocol transactions");
  			enableC.debug.ip.rip.addSC("database", "RIP database events");
  			enableC.debug.ip.rip.addSC("events", "RIP protocol events");
  			enableC.debug.ip.rip.addSC("trigger", "RIP trigger extension");
  		enableC.debug.ip.addSC("routing", "Routing table events");
  			enableC.debug.ip.routing.addSC("<1-199>", "Access list");
  			enableC.debug.ip.routing.addSC("<1300-2699>", "Access list (expanded range)");
  			enableC.debug.ip.routing.addSC("static", "IP Static routing");
  				enableC.debug.ip.routing.static.addSC("detail", "IP Static routing detail");
  				enableC.debug.ip.routing.static.addSC("route", "IP Static routing route");
  					enableC.debug.ip.routing.static.route.addSC("A.B.C.D", "Destination prefix");
  						enableC.debug.ip.routing.static.route["A.B.C.D"].addSC("A.B.C.D", "Destination prefix mask");
  				enableC.debug.ip.routing.static.addSC("summary", "IP Static routing control summary");
  				enableC.debug.ip.routing.static.addSC("time", "IP Static routing time spent");
  		enableC.debug.ip.addSC("rsvp", "RSVP protocol activity");
  		enableC.debug.ip.addSC("rtp", "RTP information");
  		enableC.debug.ip.addSC("sd", "Session Directory (SD)");
  		enableC.debug.ip.addSC("security", "IP security options");
  		enableC.debug.ip.addSC("slb", "SLB debug information");
  		enableC.debug.ip.addSC("socket", "Socket event");
  		enableC.debug.ip.addSC("ssh", "Incoming ssh connections");
  		enableC.debug.ip.addSC("tcp", "TCP information");
  		enableC.debug.ip.addSC("tempacl", "IP temporary ACL");
  		enableC.debug.ip.addSC("trigger-authentication", "Trigger authentication");
  		enableC.debug.ip.addSC("udp", "UDP based transactions");
  		enableC.debug.ip.addSC("urd", "URL RenDezvous (URD)");
  		enableC.debug.ip.addSC("wccp", "WCCP information");
  	enableC.debug.addSC("ipx", "Novell/IPX information");
  	enableC.debug.addSC("isdn", "ISDN information");
  	enableC.debug.addSC("isis", "IS-IS Information");
  	enableC.debug.addSC("kerberos", "KERBEROS authentication and authorization");
  	enableC.debug.addSC("lane", "LAN Emulation");
  	enableC.debug.addSC("lapb", "LAPB protocol transactions");
  	enableC.debug.addSC("lapb-ta", "LAPB Terminal Adapter information");
  	enableC.debug.addSC("lat", "LAT Information");
  	enableC.debug.addSC("ldap", "LDAP debug commands");
  	enableC.debug.addSC("lex", "LAN Extender protocol");
  	enableC.debug.addSC("list", "Set interface or/and access list for the next debug command");
  	enableC.debug.addSC("llc2", "LLC2 type II Information");
  	enableC.debug.addSC("lnm", "Lan Network Manager information");
  	enableC.debug.addSC("lnx", "generic qllc/llc2 conversion activity");
  	enableC.debug.addSC("local-ack", "Local ACKnowledgement information");
  	enableC.debug.addSC("management", "Management applications debugging");
  	enableC.debug.addSC("mdss", "MDSS information");
  	enableC.debug.addSC("mgcp", "Media Gateway Control Protocol");
  	enableC.debug.addSC("mls", "mls debugger information");
  	enableC.debug.addSC("modem", "Modem control/process activation");
  	enableC.debug.addSC("mop", "DECnet MOP server events");
  	enableC.debug.addSC("mpls", "MPLS debug");
  	enableC.debug.addSC("mpoa", "MPOA debug options");
  	enableC.debug.addSC("nbf", "NetBIOS information");
  	enableC.debug.addSC("ncia", "Native Client Interface Architecture (NCIA) events");
  	enableC.debug.addSC("netbios-name-cache", "NetBIOS name cache tracing");
  	enableC.debug.addSC("nhrp", "NHRP protocol");
  	enableC.debug.addSC("ntp", "NTP information");
  	enableC.debug.addSC("nvram", "Debug NVRAM behavior");
  	enableC.debug.addSC("packet", "Log unknown packets");
  	enableC.debug.addSC("pad", "X25 PAD protocol");
  	enableC.debug.addSC("ppp", "PPP (Point to Point Protocol) information");
  		enableC.debug.ppp.addSC("authentication", "CHAP and PAP authentication");
  		enableC.debug.ppp.addSC("bap", "BAP protocol transactions");
  		enableC.debug.ppp.addSC("cbcp", "Callback Control Protocol negotiation");
  		enableC.debug.ppp.addSC("compression", "PPP compression");
  		enableC.debug.ppp.addSC("error", "Protocol errors and error statistics");
  		enableC.debug.ppp.addSC("mppe", "MPPE Events");
  		enableC.debug.ppp.addSC("multilink", "Multilink activity");
  		enableC.debug.ppp.addSC("negotiation", "Protocol parameter negotiation");
  		enableC.debug.ppp.addSC("packet", "Low-level PPP packet dump");
  		enableC.debug.ppp.addSC("tasks", "PPP background tasks");
  	enableC.debug.addSC("printer", "LPD printer protocol");
  	enableC.debug.addSC("priority", "Priority output queueing");
  	enableC.debug.addSC("probe", "HP Probe Proxy Requests");
  	enableC.debug.addSC("qdm", "QoS Device Manager");
  	enableC.debug.addSC("qllc", "qllc debug information");
  	enableC.debug.addSC("radius", "RADIUS protocol");
  	enableC.debug.addSC("ras", "H.323 RAS Library");
  	enableC.debug.addSC("rif", "RIF cache transactions");
  	enableC.debug.addSC("rscmon", "Resource Monitor");
  	enableC.debug.addSC("rtpspi", "RTP Service Provider Interface.");
  	enableC.debug.addSC("rtr", "RTR Monitor Information");
  	enableC.debug.addSC("sdlc", "SDLC information");
  	enableC.debug.addSC("sdllc", "SDLLC media translation");
  	enableC.debug.addSC("serial", "Serial interface information");
  	enableC.debug.addSC("sgbp", "SGBP debugging");
  	enableC.debug.addSC("sgcp", "Simple Gateway Control Protocol");
  	enableC.debug.addSC("smf", "Software MAC filter");
  	enableC.debug.addSC("smrp", "SMRP information");
  	enableC.debug.addSC("sna", "SNA Information");
  	enableC.debug.addSC("snapshot", "Snapshot activity");
  	enableC.debug.addSC("snmp", "SNMP information");
  	enableC.debug.addSC("source", "Source bridging information");
  	enableC.debug.addSC("spanning-tree", "Spanning tree debugging");
  	enableC.debug.addSC("srcp", "Simple Resource Coordination Protocol");
  	enableC.debug.addSC("ssl", "SSL Debug command");
  	enableC.debug.addSC("standby", "Hot standby protocol");
  	enableC.debug.addSC("stun", "STUN information");
  	enableC.debug.addSC("tacacs", "TACACS authentication and authorization");
  	enableC.debug.addSC("tag-switching", "Tag Switching (obsolete use \"debug mpls ...\")");
  	enableC.debug.addSC("tarp", "TARP information");
  	enableC.debug.addSC("tbridge", "Transparent Bridging");
  	enableC.debug.addSC("tccs", "Transparent CCS information");
  	enableC.debug.addSC("tdm", "TDM connection information");
  	enableC.debug.addSC("telnet", "Incoming telnet connections");
  	enableC.debug.addSC("template", "Template activity");
  	enableC.debug.addSC("tftp", "TFTP debugging");
  	enableC.debug.addSC("tgrm", "Trunk Group Resource Manager info");
  	enableC.debug.addSC("token", "Token Ring information");
  	enableC.debug.addSC("translate", "Protocol translation events");
  	enableC.debug.addSC("translation", "translation rule information");
  	enableC.debug.addSC("tsp", "Telephony Service information");
  	enableC.debug.addSC("tunnel", "Generic Tunnel Interface");
  	enableC.debug.addSC("udptn", "UDPtn async data transport");
  	enableC.debug.addSC("v120", "V120 information");
  	enableC.debug.addSC("vines", "VINES information");
  	enableC.debug.addSC("vlan", "vLAN information");
  	enableC.debug.addSC("voice", "VOICE information");
  	enableC.debug.addSC("voip", "VOIP information");
  	enableC.debug.addSC("vpdn", "VPDN information");
  	enableC.debug.addSC("vpm", "Voice Port Module SPI information");
  	enableC.debug.addSC("vprofile", "Virtual Profile information");
  	enableC.debug.addSC("vtemplate", "Virtual Template information");
  	enableC.debug.addSC("vtsp", "Voice Telephony Call Control information");
  	enableC.debug.addSC("x25", "X.25, CMNS and XOT information");
  	enableC.debug.addSC("x28", "X28 mode");
  	enableC.debug.addSC("xcctsp", "External Call Control TSP information");
  	enableC.debug.addSC("xns", "XNS information");
	enableC.debug.addSC("xremote", "XREMOTE");

enableC.addSC("delete", "Delete a file");
	enableC["delete"].addSC("nvram:", "File to be deleted");
enableC.addSC("dir", "List files on a filesystem");
enableC.addSC("disable", "Turn off privileged commands");
enableC.addSC("disconnect", "Disconnect an existing network connection");
enableC.addSC("enable", "Turn on privileged commands");
enableC.addSC("erase", "Erase a filesystem");
enableC.addSC("exit", "Exit from the EXEC");
enableC.addSC("help", "Description of the interactive help system");
enableC.addSC("isdn", "Run an ISDN EXEC command on a BRI interface");
enableC.addSC("lock", "Lock the terminal");
enableC.addSC("login", "Log in as a particular user");
enableC.addSC("logout", "Exit from the EXEC");
enableC.addSC("modemui", "Start a modem-like user interface");
enableC.addSC("monitor", "Monitoring different system events");
enableC.addSC("more", "Display the contents of a file");
enableC.addSC("mrinfo", "Request neighbor and version information from a multicast router");
enableC.addSC("mrm", "IP Multicast Routing Monitor Test");
enableC.addSC("mstat", "Show statistics after multiple multicast traceroutes");
enableC.addSC("no", "Disable debugging functions");
	enableC.no.addSC("debug", "Disable debugging functions (see also 'undebug')");
		enableC.no.debug.addSC("aaa", "AAA Authentication, Authorization and Accounting");
		enableC.no.debug.addSC("all", "Enable all debugging");
		enableC.no.debug.addSC("arp", "IP ARP and HP Probe transactions");
		enableC.no.debug.addSC("async", "Async interface information");
		enableC.no.debug.addSC("bgp", "BGP information");
		enableC.no.debug.addSC("cdp", "CDP information");
		enableC.no.debug.addSC("confmodem", "Modem configuration database");
		enableC.no.debug.addSC("custom-queue", "Custom output queueing");
		enableC.no.debug.addSC("dhcp", "DHCP client activity");
		enableC.no.debug.addSC("dialer", "Dial on Demand");
		enableC.no.debug.addSC("dnsix", "Dnsix information");
		enableC.no.debug.addSC("eigrp", "EIGRP Protocol information");
		enableC.no.debug.addSC("fastethernet", "Fast Ethernet interface information");
		enableC.no.debug.addSC("frame-relay", "Frame Relay");
		enableC.no.debug.addSC("interface", "interface");
		enableC.no.debug.addSC("ip", "IP information");
		enableC.no.debug.addSC("nvram", "Debug NVRAM behavior");
		enableC.no.debug.addSC("ppp", "PPP (Point to Point Protocol) information");
		enableC.no.debug.addSC("priority", "Priority output queueing");
		enableC.no.debug.addSC("qdm", "QoS Device Manager");
		enableC.no.debug.addSC("radius", "RADIUS protocol");
		enableC.no.debug.addSC("tacacs", "TACACS authentication and authorization");
		enableC.no.debug.addSC("telnet", "Incoming telnet connections");
		enableC.no.debug.addSC("vpdn", "VPDN information");
		enableC.no.debug.addSC("vpn", "VPN information");
		enableC.no.debug.addSC("vprofile", "Virtual Profile information");
		enableC.no.debug.addSC("vtemplate", "Virtual Template information");
enableC.addSC("pad", "Open a X.29 PAD connection");
enableC.addSC("ping", "Send echo messages");
	enableC.ping.addSC("WORD", "Ping destination address or hostname");
	enableC.ping.addSC("ip", "IP echo");
		enableC.ping.ip.addSC("WORD", "Ping destination address or hostname");
enableC.addSC("ppp", "Start IETF Point-to-Point Protocol (PPP)");
	enableC.ppp.addSC("negotiate", "Use PPP negotiated IP address");
enableC.addSC("pwd", "Display current working directory");
enableC.addSC("reload", "Halt and perform a cold restart");
enableC.addSC("rename", "Rename a file");
enableC.addSC("restart", "Restart Connection");
enableC.addSC("resume", "Resume an active network connection");
enableC.addSC("rlogin", "Open an rlogin connection");
enableC.addSC("setup", "Run the SETUP command facility");
enableC.addSC("show", "Show running system information");
	enableC.show.addSC("aaa", "Show AAA values");
		enableC.show.aaa.addSC("attributes", "Show attributes supported by AAA subsystem");
		enableC.show.aaa.addSC("method-lists", "Show method lists defined in the AAA subsystem");
	enableC.show.addSC("access-expression", "List access expression");
	enableC.show.addSC("access-lists", "List access lists");
		enableC.show["access-lists"].addSC("<1-2699>", "ACL number");
		enableC.show["access-lists"].addSC("WORD", "ACL name");
		enableC.show["access-lists"].addSC("rate-limit", "Show rate-limit access lists");
			enableC.show["access-lists"]["rate-limit"].addSC("<1-299>", "Rate-limit ACL number");
	enableC.show.addSC("accounting", "Accounting data for active sessions");
	enableC.show.addSC("adjacency", "Adjacent nodes");
	enableC.show.addSC("aliases", "Display alias commands");
	enableC.show.addSC("arp", "ARP table");
	enableC.show.addSC("async", "Information on terminal lines used as router interfaces");
	enableC.show.addSC("backup", "Backup status");
	enableC.show.addSC("bgp", "BGP information");
		enableC.show.bgp.addSC("community", "Display routes matching the communities");
		enableC.show.bgp.addSC("neighbors", "Detailed information on TCP and BGP neighbor connections");
	enableC.show.addSC("buffers", "Buffer pool statistics");
	enableC.show.addSC("c1700", "Show c1700 information");
	enableC.show.addSC("cdapi", "CDAPI information");
	enableC.show.addSC("cdp", "CDP information");
		enableC.show.cdp.addSC("entry", "Information for specific neighbor entry");
			enableC.show.cdp.entry.addSC("*", "all CDP neighbor entries");
				enableC.show.cdp.entry["*"].addSC("protocol", "Protocol information");
				enableC.show.cdp.entry["*"].addSC("version", "Version information");
					enableC.show.cdp.entry["*"].version.addSC("protocol", "Protocol information");
			enableC.show.cdp.entry.addSC("WORD", "Name of CDP neighbor entry");
				enableC.show.cdp.entry.WORD.addSC("protocol", "Protocol information");
				enableC.show.cdp.entry.WORD.addSC("version", "Version information");
					enableC.show.cdp.entry.WORD.version.addSC("protocol", "Protocol information");
		enableC.show.cdp.addSC("interface", "CDP interface status and configuration");
		enableC.show.cdp.addSC("neighbors", "CDP neighbor entries");
			enableC.show.cdp.neighbors.addSC("detail", "Show detailed information");
	enableC.show.addSC("compress", "Show compression statistics");
		enableC.show.compress.addSC("detail-ccp", "additional ccp state info");
	enableC.show.addSC("configuration", "Contents of Non-Volatile memory");
	enableC.show.addSC("connection", "Show Connection");
	enableC.show.addSC("dhcp", "Dynamic Host Configuration Protocol status");
		enableC.show.dhcp.addSC("lease", "Show DHCP Addresses leased from a server");
			enableC.show.dhcp.lease.addSC("interface", "Show DHCP information on one interface");
				enableC.show.dhcp.lease.interface.addSC("Async", "Async interface");
					enableC.show.dhcp.lease.interface.Async.addSC("<1-5>", "Async interface number");
				enableC.show.dhcp.lease.interface.addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.dhcp.lease.interface["Virtual-Template"].addSC("<1-200>", "Virtual-Template interface number");
		enableC.show.dhcp.addSC("server", "Show DHCP Servers we know about");
	enableC.show.addSC("diag", "Show diagnostic information for port adapters/modules");
		enableC.show.diag.addSC("<0-3>", "Slot number");
	enableC.show.addSC("dialer", "Dialer parameters and statistics");
	enableC.show.addSC("frame-relay", "Frame-Relay information");
		enableC.show["frame-relay"].addSC("map", "Frame-Relay map table");
		enableC.show["frame-relay"].addSC("pvc", "show frame relay pvc statistics");
	enableC.show.addSC("hosts", "IP domain-name, lookup style, nameservers, and host table");
	enableC.show.addSC("interfaces", "Interface status and configuration");
		enableC.show.interfaces.addSC("Async", "Async interface");
			enableC.show.interfaces.Async.addSC("<1-5>", "Async interface number");
			enableC.show.interfaces.Dialer.addSC("<0-255>", "Dialer interface number");
		enableC.show.interfaces.addSC("FastEthernet", "FastEthernet IEEE 802.3");
			enableC.show.interfaces.FastEthernet.addSC("<0-0>", "FastEthernet interface number");
		enableC.show.interfaces.addSC("Loopback", "Loopback interface");
			enableC.show.interfaces.Loopback.addSC("<0-2147483647>", "Loopback interface number");
		enableC.show.interfaces.addSC("Null", "Null interface");
			enableC.show.interfaces.Null.addSC("<0-0>", "Null interface number");
		enableC.show.interfaces.addSC("Serial", "Serial");
			enableC.show.interfaces.Serial.addSC("<0-1>", "Serial interface number");
		enableC.show.interfaces.addSC("Tunnel", "Tunnel interface");
		enableC.show.addSC("ip", "IP information");
		enableC.show.ip.addSC("access-lists", "List IP access lists");
			enableC.show.ip["access-lists"].addSC("<1-199>", "Access list number");
			enableC.show.ip["access-lists"].addSC("<1300-2699>", "Access list number (expanded range)");
			enableC.show.ip["access-lists"].addSC("WORD", "Access list name");
		enableC.show.ip.addSC("arp", "IP ARP table");
		enableC.show.ip.addSC("bgp", "BGP information");
		enableC.show.ip.addSC("dhcp", "Show items in the DHCP database");
		enableC.show.ip.addSC("dvmrp", "DVMRP information");
		enableC.show.ip.addSC("interface", "IP interface status and configuration");
		enableC.show.ip.addSC("mroute", "IP multicast routing table");
			enableC.show.ip.mroute.addSC("Loopback", "Loopback interface");
			enableC.show.ip.mroute.addSC("MFR", "Multilink Frame Relay bundle interface");
			enableC.show.ip.mroute.addSC("active", "Active multicast sources");
			enableC.show.ip.mroute.addSC("count", "Route and packet count data");
			enableC.show.ip.mroute.addSC("pruned", "Pruned routes");
			enableC.show.ip.mroute.addSC("static", "Static multicast routes");
			enableC.show.ip.mroute.addSC("summary", "Provide abbreviated display");
			enableC.show.ip.msdp.addSC("summary", "MSDP Peer Summary");
		enableC.show.ip.addSC("mtag", "IP Multicast Tagswitching TIB");
		enableC.show.ip.addSC("nat", "IP NAT information");
			enableC.show.ip.nat.addSC("statistics", "Translation statistics");
			enableC.show.ip.nat.addSC("translations", "Translation entries");
				enableC.show.ip.nat.translations.addSC("verbose", "Show extra information");
		enableC.show.ip.addSC("nbar", "Network-Based Application Recognition");
		enableC.show.ip.addSC("nhrp", "NHRP information");
		enableC.show.ip.addSC("ospf", "OSPF information");
				enableC.show.ip.ospf.interface.addSC("Async", "Async interface");
					enableC.show.ip.ospf.interface.Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf.interface.addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf.interface.BRI.addSC("<0-6>", "BRI interface number");
				enableC.show.ip.ospf.interface.addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf.interface.BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.ospf.interface.addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf.interface.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.ospf.interface.addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf.interface.Dialer.addSC("<0-799>", "Dialer interface number");
				enableC.show.ip.ospf.interface.addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf.interface.Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf.interface.addSC("Lex", "Lex interface");
					enableC.show.ip.ospf.interface.Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.ospf.interface.addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf.interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				enableC.show.ip.ospf.interface.addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf.interface.Multilink.addSC("<1-2147483647>", "Multilink interface number");
				enableC.show.ip.ospf.interface.addSC("Null", "Null interface");
					enableC.show.ip.ospf.interface.Null.addSC("<0-0>", "Null interface number");
				enableC.show.ip.ospf.interface.addSC("Serial", "Serial");
					enableC.show.ip.ospf.interface.Serial.addSC("<0-6>", "Serial interface number");
				enableC.show.ip.ospf.interface.addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf.interface.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.ospf.interface.addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf.interface.Vif.addSC("<1-1>", "Vif interface number");
				enableC.show.ip.ospf.interface.addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.ospf.interface["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
				enableC.show.ip.ospf.interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
					enableC.show.ip.ospf.interface["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			enableC.show.ip.ospf.addSC("mpls", "MPLS related information");
				enableC.show.ip.ospf.mpls.addSC("traffic-eng", "Traffic Engineering information");
					enableC.show.ip.ospf.mpls["traffic-eng"].addSC("fragment", "MPLS fragment information");
					enableC.show.ip.ospf.mpls["traffic-eng"].addSC("link", "MPLS link information");
			enableC.show.ip.ospf.addSC("neighbor", "Neighbor list");
				enableC.show.ip.ospf.neighbor.addSC("Async", "Async interface");
					enableC.show.ip.ospf.neighbor.Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf.neighbor.addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf.neighbor.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.BRI.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.BRI.Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf.neighbor.addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf.neighbor.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.BVI.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.BVI.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.BVI.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.BVI.BRI.addSC("<0-6>", "BRI interface number");
				enableC.show.ip.ospf.neighbor.addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf.neighbor.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.CTunnel.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.CTunnel.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.CTunnel.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.CTunnel.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.CTunnel.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.CTunnel.BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.ospf.neighbor.addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Dialer.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Dialer.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Dialer.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Dialer.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.ospf.neighbor.addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Ethernet.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Ethernet.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Ethernet.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Ethernet.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Ethernet.Dialer.addSC("<0-799>", "Dialer interface number");
				enableC.show.ip.ospf.neighbor.addSC("Hostname or A.B.C.D", "Neighbor ID");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf.neighbor.addSC("Lex", "Lex interface");
					enableC.show.ip.ospf.neighbor.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Lex.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Lex.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Lex.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Lex.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Lex.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Lex.Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf.neighbor.addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("<0-2147483647>", "Loopback interface number");
						enableC.show.ip.ospf.neighbor.Loopback["<0-2147483647>"].addSC("Hostname or A.B.C.D", "Neighbor ID");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Loopback.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Loopback.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Loopback.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Loopback.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Loopback.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Loopback.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Loopback.Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.ospf.neighbor.addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Multilink.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Multilink.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Multilink.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Multilink.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Multilink.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Multilink.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Multilink.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Multilink.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				enableC.show.ip.ospf.neighbor.addSC("Null", "Null interface");
					enableC.show.ip.ospf.neighbor.Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.ospf.neighbor.Null["<0-0>"].addSC("Hostname or A.B.C.D", "Neighbor ID");
					enableC.show.ip.ospf.neighbor.Null.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Null.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Null.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Null.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Null.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Null.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Null.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Null.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Null.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.Null.Multilink.addSC("<1-2147483647>", "Multilink interface number");
				enableC.show.ip.ospf.neighbor.addSC("Serial", "Serial");
					enableC.show.ip.ospf.neighbor.Serial.addSC("<0-6>", "Serial interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Serial.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Serial.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Serial.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Serial.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Serial.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Serial.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Serial.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Serial.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.Serial.Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.Serial.Null.addSC("<0-0>", "Null interface number");
				enableC.show.ip.ospf.neighbor.addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Tunnel.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Tunnel.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Tunnel.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Tunnel.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.Tunnel.Serial.addSC("<0-6>", "Serial interface number");
				enableC.show.ip.ospf.neighbor.addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf.neighbor.Vif.addSC("<1-1>", "Vif interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Vif.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Vif.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Vif.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Vif.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Vif.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Vif.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Vif.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Vif.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.Vif.Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.Vif.Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.Vif.Serial.addSC("<0-6>", "Serial interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor.Vif.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.ospf.neighbor.addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Serial.addSC("<0-6>", "Serial interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Vif", "PGM Multicast Host interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Vif.addSC("<1-1>", "Vif interface number");
				enableC.show.ip.ospf.neighbor.addSC("Virtual-TokenRing", "Virtual TokenRing");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Serial.addSC("<0-6>", "Serial interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Vif", "PGM Multicast Host interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Vif.addSC("<1-1>", "Vif interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Virtual-Template", "Virtual Template interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"]["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
				enableC.show.ip.ospf.neighbor.addSC("detail", "detail of all neighbors");
					enableC.show.ip.ospf.neighbor.detail.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.detail.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.BRI.addSC("<0-6>", "BRI interface number");
						enableC.show.ip.ospf.neighbor.detail.BRI.addSC("Async", "Async interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.BVI.addSC("<1-255>", "BVI interface number");
						enableC.show.ip.ospf.neighbor.detail.BVI.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.BVI.addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
						enableC.show.ip.ospf.neighbor.detail.CTunnel.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.CTunnel.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.CTunnel.addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("<0-799>", "Dialer interface number");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("<0-6>", "Ethernet interface number");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Hostname or A.B.C.D", "Neighbor ID");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf.neighbor.detail.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("<0-2147483647>", "Lex interface number");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf.neighbor.detail.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("<0-2147483647>", "Loopback interface number");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("Lex", "Lex interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("<1-2147483647>", "Multilink interface number");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("<0-6>", "Serial interface number");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Null", "Null interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Serial", "Serial");
					enableC.show.ip.ospf.neighbor.detail.addSC("Vif", "PGM Multicast Host interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("<1-1>", "Vif interface number");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Virtual-Template", "Virtual Template interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Virtual-TokenRing", "Virtual TokenRing");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Vif", "PGM Multicast Host interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Virtual-Template", "Virtual Template interface");
			enableC.show.ip.ospf.addSC("request-list", "Link state request list");
				enableC.show.ip.ospf["request-list"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["request-list"].addSC("Async", "Async interface");
					enableC.show.ip.ospf["request-list"].Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf["request-list"].addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf["request-list"].BRI.addSC("<0-6>", "BRI interface number");
				enableC.show.ip.ospf["request-list"].addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf["request-list"].BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.ospf["request-list"].addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf["request-list"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.ospf["request-list"].addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf["request-list"].Dialer.addSC("<0-799>", "Dialer interface number");
						enableC.show.ip.ospf["request-list"].Dialer["<0-799>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["request-list"].addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf["request-list"].Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf["request-list"].addSC("Lex", "Lex interface");
					enableC.show.ip.ospf["request-list"].Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.ospf["request-list"].addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf["request-list"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
						enableC.show.ip.ospf["request-list"].Loopback["<0-2147483647>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["request-list"].addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf["request-list"].Multilink.addSC("<1-2147483647>", "Multilink interface number");
				enableC.show.ip.ospf["request-list"].addSC("Null", "Null interface");
					enableC.show.ip.ospf["request-list"].Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.ospf["request-list"].Null["<0-0>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["request-list"].addSC("Serial", "Serial");
					enableC.show.ip.ospf["request-list"].Serial.addSC("<0-6>", "Serial interface number");
				enableC.show.ip.ospf["request-list"].addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf["request-list"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.ospf["request-list"].addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf["request-list"].Vif.addSC("<1-1>", "Vif interface number");
				enableC.show.ip.ospf["request-list"].addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.ospf["request-list"]["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
				enableC.show.ip.ospf["request-list"].addSC("Virtual-TokenRing", "Virtual TokenRing");
					enableC.show.ip.ospf["request-list"]["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			enableC.show.ip.ospf.addSC("retransmission-list", "Link state retransmission list");
				enableC.show.ip.ospf["retransmission-list"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["retransmission-list"].addSC("Async", "Async interface");
					enableC.show.ip.ospf["retransmission-list"].Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf["retransmission-list"].BRI.addSC("<0-6>", "BRI interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf["retransmission-list"].BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf["retransmission-list"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf["retransmission-list"].Dialer.addSC("<0-799>", "Dialer interface number");
						enableC.show.ip.ospf["retransmission-list"].Dialer["<0-799>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["retransmission-list"].addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf["retransmission-list"].Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Lex", "Lex interface");
					enableC.show.ip.ospf["retransmission-list"].Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf["retransmission-list"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
						enableC.show.ip.ospf["retransmission-list"].Loopback["<0-2147483647>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["retransmission-list"].addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf["retransmission-list"].Multilink.addSC("<1-2147483647>", "Multilink interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Null", "Null interface");
					enableC.show.ip.ospf["retransmission-list"].Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.ospf["retransmission-list"].Null["<0-0>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["retransmission-list"].addSC("Serial", "Serial");
					enableC.show.ip.ospf["retransmission-list"].Serial.addSC("<0-6>", "Serial interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf["retransmission-list"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf["retransmission-list"].Vif.addSC("<1-1>", "Vif interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.ospf["retransmission-list"]["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Virtual-TokenRing", "Virtual TokenRing");
					enableC.show.ip.ospf["retransmission-list"]["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			enableC.show.ip.ospf.addSC("summary-address", "Summary-address redistribution Information");
			enableC.show.ip.ospf.addSC("virtual-links", "Virtual link information");
		enableC.show.ip.addSC("pgm", "PGM Reliable Transport Protocol");
		enableC.show.ip.addSC("protocols", "IP routing protocol process parameters and statistics");
		enableC.show.ip.addSC("rip", "IP RIP show commands");
		enableC.show.ip.addSC("route", "IP routing table");
			enableC.show.ip.route.addSC("bgp", "Border Gateway Protocol (BGP)");
			enableC.show.ip.route.addSC("connected", "Connected");
			enableC.show.ip.route.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			enableC.show.ip.route.addSC("ospf", "Open Shortest Path First (OSPF)");
			enableC.show.ip.route.addSC("profile", "IP routing table profile");
			enableC.show.ip.route.addSC("rip", "Routing Information Protocol (RIP)");
			enableC.show.ip.route.addSC("static", "Static routes");
			enableC.show.ip.route.addSC("summary", "Summary of all routes");
		enableC.show.ip.addSC("rpf", "Display RPF information for multicast source");
			enableC.show.ip.rpf.addSC("Hostname or A.B.C.D", "IP name or address of multicast source");
				enableC.show.ip.rpf["Hostname or A.B.C.D"].addSC("metric", "Metric");
		enableC.show.ip.addSC("rsvp", "RSVP information");
		enableC.show.ip.addSC("rtp", "RTP/UDP/IP header-compression statistics");
		enableC.show.ip.addSC("sap", "Session Announcement Protocol cache");
		enableC.show.ip.addSC("sockets", "Open IP sockets");
		enableC.show.ip.addSC("tcp", "TCP/IP header-compression statistics");
		enableC.show.ip.addSC("traffic", "IP protocol statistics");
		enableC.show.ip.addSC("vrf", "VPN Routing/Forwarding instance information");
			enableC.show.ip.vrf.addSC("WORD", "VPN Routing/Forwarding instance name");
			enableC.show.ip.vrf.addSC("brief", "Brief VPN Routing/Forwarding instance information");
				enableC.show.ip.vrf.brief.addSC("WORD", "VPN Routing/Forwarding instance name");
			enableC.show.ip.vrf.addSC("detail", "Detailed VPN Routing/Forwarding instance information");
				enableC.show.ip.vrf.detail.addSC("WORD", "VPN Routing/Forwarding instance name");
			enableC.show.ip.vrf.addSC("id", "Show VPN Routing/Forwarding VPN-ID information");
				enableC.show.ip.vrf.id.addSC("WORD", "VPN Routing/Forwarding instance name");
			enableC.show.ip.vrf.addSC("interfaces", "Show VPN Routing/Forwarding interface information");
				enableC.show.ip.vrf.interfaces.addSC("WORD", "VPN Routing/Forwarding instance name");
		enableC.show.ip.addSC("wccp", "WCCP information");
	enableC.show.addSC("ipv6", "IPv6 information");
	enableC.show.addSC("line", "TTY line information");
	enableC.show.addSC("modemcap", "Show Modem Capabilities database");
		enableC.show.modemcap.addSC("WORD", "Modem entry to use");
	enableC.show.addSC("parser", "Display parser information");
	enableC.show.addSC("policy-map", "Show QoS Policy Map");
	enableC.show.addSC("ppp", "PPP parameters and statistics");
		enableC.show.ppp.addSC("multilink", "Multilink PPP bundle information");
		enableC.show.ppp.addSC("queues", "PPP request queues");
	enableC.show.addSC("privilege", "Show current privilege level");
	enableC.show.addSC("processes", "Active process statistics");
		enableC.show.processes.addSC("cpu", "Show CPU use per process");
			enableC.show.processes.cpu.addSC("history", "Show CPU history in graph format");
		enableC.show.processes.addSC("memory", "Show memory use per process");
			enableC.show.processes.memory.addSC("<1-4294967295>", "[pid]");
	enableC.show.addSC("protocols", "Active network routing protocols");
	enableC.show.addSC("qdm", "Show information about QoS Device Manager");
		enableC.show.qdm.addSC("status", "Information and status about currently active QDM web-based clients");
	enableC.show.addSC("queue", "Show queue contents");
	enableC.show.addSC("queueing", "Show queueing configuration");
		enableC.show.queueing.addSC("interface", "");
		enableC.show.queueing.addSC("custom", "custom queueing list configuration");
		enableC.show.queueing.addSC("fair", "fair queueing configuration");
			enableC.show.queueing.fair.addSC("interface", "");
		enableC.show.queueing.addSC("priority", "priority queueing list configuration");
	enableC.show.addSC("reload", "Scheduled reload information");
	enableC.show.addSC("rhosts", "Remote-host+user equivalences");
	enableC.show.addSC("rif", "RIF cache entries");
	enableC.show.addSC("rmon", "rmon statistics");
	enableC.show.addSC("running-config", "Current operating configuration");
	enableC.show.addSC("snapshot", "Snapshot parameters and statistics");
	enableC.show.addSC("snmp", "snmp statistics");
	enableC.show.addSC("sntp", "Simple network time protocol");
	enableC.show.addSC("spanning-tree", "Spanning tree topology");
	enableC.show.addSC("standby", "Hot Standby Router Protocol (HSRP) information");
	enableC.show.addSC("startup-config", "Contents of startup configuration");
	enableC.show.addSC("subsys", "Show subsystem information");
	enableC.show.addSC("tacacs", "Shows tacacs+ server statistics");
	enableC.show.addSC("tcp", "Status of TCP connections");
	enableC.show.addSC("template", "Template information");
		enableC.show.template.addSC("WORD", "Specify template name");
	enableC.show.addSC("terminal", "Display terminal configuration parameters");
	enableC.show.addSC("tgrm", "Trunk Group Resource Mananger info");
	enableC.show.addSC("time-range", "Time range");
	enableC.show.addSC("track", "Tracking information");
	enableC.show.addSC("traffic-shape", "traffic rate shaping configuration");
	enableC.show.addSC("users", "Display information about terminal lines");
	enableC.show.addSC("version", "System hardware and software status");
	enableC.show.addSC("vpdn", "VPDN information");
		enableC.show.vpdn.addSC("domain", "VPDN domain info");
		enableC.show.vpdn.addSC("group", "VPDN group info");
			enableC.show.vpdn.group.addSC("WORD", "Name of VPDN group");
				enableC.show.vpdn.group.WORD.addSC("domain", "Domain session info");
				enableC.show.vpdn.group.WORD.addSC("endpoint", "Endpoint session info");
		enableC.show.vpdn.addSC("history", "History logging");
			enableC.show.vpdn.history.addSC("failure", "Show VPDN User Failure History Table");
				enableC.show.vpdn.history.failure.addSC("WORD", "Name of user");
		enableC.show.vpdn.addSC("multilink", "Multilink VPDN session info");
		enableC.show.vpdn.addSC("session", "Session (call) information");
			enableC.show.vpdn.session.addSC("all", "All session information");
				enableC.show.vpdn.session.state.addSC("username", "Username filter");
					enableC.show.vpdn.session.state.username.addSC("WORD", "Username");
		enableC.show.vpdn.addSC("tunnel", "Tunnel information");
			enableC.show.vpdn.tunnel.addSC("all", "All tunnel information");
	enableC.show.addSC("vtemplate", "Virtual Template interface information");
		enableC.show.vtemplate.addSC("<1-200>", "Virtual Template interface number");
	enableC.show.addSC("whoami", "Info on current tty line");
enableC.addSC("slip", "Start Serial-line IP (SLIP)");
enableC.addSC("squeeze", "Squeeze a filesystem");
enableC.addSC("start-chat", "Start a chat-script on a line");
enableC.addSC("systat", "Display information about terminal lines");
enableC.addSC("telnet", "Open a telnet connection");
	enableC.telnet.addSC("WORD", "IP address or hostname of a remote system");
enableC.addSC("terminal", "Set terminal line parameters");
	enableC.terminal.addSC("txspeed", "Set the transmit speeds");
		enableC.terminal.txspeed.addSC("<0-4294967295>", "Transmit speed");
	enableC.terminal.addSC("width", "Set width of the display terminal");
		enableC.terminal.width.addSC("<0-512>", "Number of characters on a screen line");
enableC.addSC("test", "Test subsystems, memory, and interfaces");
enableC.addSC("traceroute", "Trace route to destination");
	enableC.traceroute.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("ip", "IP Trace");
		enableC.traceroute.ip.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("ipv6", "IPv6 Trace");
		enableC.traceroute.ipv6.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("ipx", "IPX Trace");
		enableC.traceroute.ipx.addSC("WORD", "Trace route to destination address or hostname");
enableC.addSC("tunnel", "Open a tunnel connection");
	enableC.tunnel.addSC("WORD", "Address or hostname of a remote system");
		enableC.tunnel.WORD.addSC("debug", "Enable tunnel debugging output");
enableC.addSC("udptn", "Open an udptn connection");
enableC.addSC("undebug", "Disable debugging functions (see also 'debug')");
	enableC.undebug.addSC("aaa", "AAA Authentication, Authorization and Accounting");
		enableC.undebug.aaa.addSC("accounting", "Accounting");
		enableC.undebug.aaa.addSC("administrative", "Administrative");
		enableC.undebug.aaa.addSC("attr", "AAA Attr Manager");
		enableC.undebug.aaa.addSC("authentication", "Authentication");
		enableC.undebug.aaa.addSC("authorization", "Authorization");
		enableC.undebug.aaa.addSC("db", "AAA DB Manager");
		enableC.undebug.aaa.addSC("id", "AAA Unique Id");
		enableC.undebug.aaa.addSC("ipc", "AAA IPC");
		enableC.undebug.aaa.addSC("per-user", "Per-user attributes");
		enableC.undebug.aaa.addSC("pod", "AAA POD processing");
		enableC.undebug.aaa.addSC("protocol", "AAA protocol processing");
		enableC.undebug.aaa.addSC("subsys", "AAA Subsystem");
	enableC.undebug.addSC("all", "Enable all debugging");
	enableC.undebug.addSC("arp", "IP ARP and HP Probe transactions");
	enableC.undebug.addSC("async", "Async interface information");
		enableC.undebug.async.addSC("async-queue", "Rotary Line Queuing Activity");
		enableC.undebug.async.addSC("framing", "Packet framing");
		enableC.undebug.async.addSC("packet", "Packet I/O");
		enableC.undebug.async.addSC("state", "Interface state changes");
	enableC.undebug.addSC("bgp", "BGP information");
		enableC.undebug.bgp.addSC("dampening", "BGP dampening");
		enableC.undebug.bgp.addSC("events", "BGP events");
		enableC.undebug.bgp.addSC("ipv6", "Address family");
		enableC.undebug.bgp.addSC("keepalives", "BGP keepalives");
		enableC.undebug.bgp.addSC("nsap", "Address family");
		enableC.undebug.bgp.addSC("updates", "BGP updates");
	enableC.undebug.addSC("callback", "Callback activity");
	enableC.undebug.addSC("cdp", "CDP information");
		enableC.undebug.cdp.addSC("adjacency", "CDP neighbor info");
		enableC.undebug.cdp.addSC("events", "CDP events");
		enableC.undebug.cdp.addSC("ip", "CDP ip info");
		enableC.undebug.cdp.addSC("packets", "CDP packet-related information");
	enableC.undebug.addSC("chat", "Chat scripts activity");
		enableC.undebug.chat.addSC("line", "Single TTY line to debug scripts");
	enableC.undebug.addSC("compress", "COMPRESS traffic");
	enableC.undebug.addSC("condition", "Condition");
		enableC.undebug.condition.addSC("<1-1000>", "Condition identifier");
		enableC.undebug.condition.addSC("all", "All conditions");
		enableC.undebug.condition.addSC("called", "called number");
		enableC.undebug.condition.addSC("calling", "calling");
		enableC.undebug.condition.addSC("standby", "interface group");
		enableC.undebug.condition.addSC("username", "username");
	enableC.undebug.addSC("confmodem", "Modem configuration database");
	enableC.undebug.addSC("conn", "Connection Manager information");
	enableC.undebug.addSC("custom-queue", "Custom output queueing");
	enableC.undebug.addSC("dhcp", "DHCP client activity");
		enableC.undebug.dhcp.addSC("detail", "DHCP packet content");
	enableC.undebug.addSC("dialer", "Dial on Demand");
		enableC.undebug.dialer.addSC("events", "Dial on demand events");
		enableC.undebug.dialer.addSC("forwarding", "Dialer forwarding");
		enableC.undebug.dialer.addSC("map", "Dynamic dialer maps");
		enableC.undebug.dialer.addSC("packets", "Dial on demand traffic");
	enableC.undebug.addSC("dnsix", "Dnsix information");
		enableC.undebug.dnsix.addSC("dmdp", "Debug DNSIX/DMDP protocol");
		enableC.undebug.dnsix.addSC("dnssec", "Debug DNSSEC protocol");
		enableC.undebug.dnsix.addSC("nat", "Debug DNSIX/NAT protocol");
	enableC.undebug.addSC("domain", "Domain Name System");
		enableC.undebug.domain.addSC("replies", "DNS replies only");
	enableC.undebug.addSC("dxi", "atm-dxi information");
		enableC.undebug.dxi.addSC("events", "Important atm-dxi events");
		enableC.undebug.dxi.addSC("packet", "ATM DXI packets");
	enableC.undebug.addSC("eigrp", "EIGRP Protocol information");
		enableC.undebug.eigrp.addSC("fsm", "EIGRP Dual Finite State Machine events/actions");
		enableC.undebug.eigrp.addSC("neighbors", "EIGRP neighbors");
		enableC.undebug.eigrp.addSC("packets", "EIGRP packets");
		enableC.undebug.eigrp.addSC("transmit", "EIGRP transmission events");
	enableC.undebug.addSC("entry", "Incoming queue entries");
	enableC.undebug.addSC("ethernet-interface", "Ethernet network interface events");
	enableC.undebug.addSC("fastethernet", "Fast Ethernet interface information");
		enableC.undebug.fastethernet.addSC("events", "Fast Ethernet events");
		enableC.undebug.fastethernet.addSC("packets", "Fast Ethernet packets");
	enableC.undebug.addSC("frame-relay", "Frame Relay");
	enableC.undebug.addSC("interface", "interface");
		enableC.undebug.interface.addSC("Async", "Async interface");
		enableC.undebug.interface.addSC("BVI", "Bridge-Group Virtual Interface");
		enableC.undebug.interface.addSC("CTunnel", "CTunnel interface");
		enableC.undebug.interface.addSC("Dialer", "Dialer interface");
		enableC.undebug.interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
		enableC.undebug.interface.addSC("Group-Async", "Async Group interface");
		enableC.undebug.interface.addSC("Lex", "Lex interface");
		enableC.undebug.interface.addSC("Loopback", "Loopback interface");
		enableC.undebug.interface.addSC("MFR", "Multilink Frame Relay bundle interface");
		enableC.undebug.interface.addSC("Multilink", "Multilink-group interface");
		enableC.undebug.interface.addSC("Null", "Null interface");
		enableC.undebug.interface.addSC("Serial", "Serial");
		enableC.undebug.interface.addSC("Tunnel", "Tunnel interface");
		enableC.undebug.interface.addSC("Vif", "PGM Multicast Host interface");
		enableC.undebug.interface.addSC("Virtual-Template", "Virtual Template interface");
		enableC.undebug.interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
	enableC.undebug.addSC("ip", "IP information");
		enableC.undebug.ip.addSC("bgp", "BGP information");
		enableC.undebug.ip.addSC("cache", "IP cache operations");
		enableC.undebug.ip.addSC("cef", "IP CEF operations");
		enableC.undebug.ip.addSC("cgmp", "CGMP protocol activity");
		enableC.undebug.ip.addSC("dhcp", "Dynamic Host Configuration Protocol");
		enableC.undebug.ip.addSC("dvmrp", "DVMRP protocol activity");
		enableC.undebug.ip.addSC("eigrp", "IP-EIGRP information");
		enableC.undebug.ip.addSC("error", "IP error debugging");
		enableC.undebug.ip.addSC("flow", "IP Flow switching operations");
		enableC.undebug.ip.addSC("ftp", "FTP dialogue");
		enableC.undebug.ip.addSC("html", "HTML connections");
		enableC.undebug.ip.addSC("http", "HTTP connections");
		enableC.undebug.ip.addSC("icmp", "ICMP transactions");
		enableC.undebug.ip.addSC("igmp", "IGMP protocol activity");
		enableC.undebug.ip.addSC("igrp", "IGRP information");
		enableC.undebug.ip.addSC("interface", "IP interface configuration changes");
		enableC.undebug.ip.addSC("mbgp", "MBGP information");
		enableC.undebug.ip.addSC("mcache", "IP multicast cache operations");
		enableC.undebug.ip.addSC("mhbeat", "IP multicast heartbeat monitoring");
		enableC.undebug.ip.addSC("mpacket", "IP multicast packet debugging");
		enableC.undebug.ip.addSC("mrm", "IP Multicast Routing Monitor");
		enableC.undebug.ip.addSC("mrouting", "IP multicast routing table activity");
		enableC.undebug.ip.addSC("msdp", "Multicast Source Discovery Protocol (MSDP)");
		enableC.undebug.ip.addSC("mtag", "IP multicast tagswitching activity");
		enableC.undebug.ip.addSC("nat", "NAT events");
		enableC.undebug.ip.addSC("nbar", "StILE - traffic classification Engine");
		enableC.undebug.ip.addSC("ospf", "OSPF information");
		enableC.undebug.ip.addSC("packet", "General IP debugging and IPSO security transactions");
		enableC.undebug.ip.addSC("peer", "IP peer address activity");
		enableC.undebug.ip.addSC("pgm", "PGM Reliable Transport Protocol");
		enableC.undebug.ip.addSC("pim", "PIM protocol activity");
		enableC.undebug.ip.addSC("policy", "Policy routing");
		enableC.undebug.ip.addSC("rgmp", "RGMP protocol activity");
		enableC.undebug.ip.addSC("rip", "RIP protocol transactions");
		enableC.undebug.ip.addSC("routing", "Routing table events");
		enableC.undebug.ip.addSC("rsvp", "RSVP protocol activity");
		enableC.undebug.ip.addSC("rtp", "RTP information");
		enableC.undebug.ip.addSC("sd", "Session Directory (SD)");
		enableC.undebug.ip.addSC("security", "IP security options");
		enableC.undebug.ip.addSC("socket", "Socket event");
		enableC.undebug.ip.addSC("tcp", "TCP information");
		enableC.undebug.ip.addSC("tempacl", "IP temporary ACL");
		enableC.undebug.ip.addSC("udp", "UDP based transactions");
		enableC.undebug.ip.addSC("urd", "URL RenDezvous (URD)");
		enableC.undebug.ip.addSC("wccp", "WCCP information");
	enableC.undebug.addSC("ipv6", "IPv6 information");
	enableC.undebug.addSC("lapb", "LAPB protocol transactions");
	enableC.undebug.addSC("list", "Set interface or/and access list for the next debug command");
		enableC.undebug.list.addSC("<0-2699>", "access list");
		enableC.undebug.list.addSC("Async", "Async interface");
		enableC.undebug.list.addSC("BVI", "Bridge-Group Virtual Interface");
		enableC.undebug.list.addSC("CTunnel", "CTunnel interface");
		enableC.undebug.list.addSC("Dialer", "Dialer interface");
		enableC.undebug.list.addSC("FastEthernet", "FastEthernet IEEE 802.3");
		enableC.undebug.list.addSC("Group-Async", "Async Group interface");
		enableC.undebug.list.addSC("Lex", "Lex interface");
		enableC.undebug.list.addSC("Loopback", "Loopback interface");
		enableC.undebug.list.addSC("MFR", "Multilink Frame Relay bundle interface");
		enableC.undebug.list.addSC("Multilink", "Multilink-group interface");
		enableC.undebug.list.addSC("Null", "Null interface");
		enableC.undebug.list.addSC("Serial", "Serial");
		enableC.undebug.list.addSC("Tunnel", "Tunnel interface");
		enableC.undebug.list.addSC("Vif", "PGM Multicast Host interface");
		enableC.undebug.list.addSC("Virtual-Template", "Virtual Template interface");
		enableC.undebug.list.addSC("Virtual-TokenRing", "Virtual TokenRing");
	enableC.undebug.addSC("llc2", "LLC2 type II Information");
	enableC.undebug.addSC("modem", "Modem control/process activation");
	enableC.undebug.addSC("nvram", "Debug NVRAM behavior");
	enableC.undebug.addSC("ppp", "PPP (Point to Point Protocol) information");		enableC.undebug.ppp.addSC("authentication", "CHAP and PAP authentication");
		enableC.undebug.ppp.addSC("bap", "BAP protocol transactions");
		enableC.undebug.ppp.addSC("cbcp", "Callback Control Protocol negotiation");
		enableC.undebug.ppp.addSC("error", "Protocol errors and error statistics");
		enableC.undebug.ppp.addSC("events", "Detailed events");
		enableC.undebug.ppp.addSC("forwarding", "PPP layer 2 forwarding");
		enableC.undebug.ppp.addSC("mppe", "MPPE Events");
		enableC.undebug.ppp.addSC("multilink", "Multilink activity");
		enableC.undebug.ppp.addSC("negotiation", "Protocol parameter negotiation");
		enableC.undebug.ppp.addSC("packet", "Low-level PPP packet dump");
		enableC.undebug.ppp.addSC("tasks", "Event Manager");
	enableC.undebug.addSC("priority", "Priority output queueing");
	enableC.undebug.addSC("qdm", "QoS Device Manager");
	enableC.undebug.addSC("radius", "RADIUS protocol");
		enableC.undebug.radius.addSC("accounting", "RADIUS accounting packets only");
		enableC.undebug.radius.addSC("authentication", "RADIUS authentication packets only");
		enableC.undebug.radius.addSC("brief", "Only I/O transactions are recorded");
		enableC.undebug.radius.addSC("failover", "Packets sent upon fail-over");
		enableC.undebug.radius.addSC("retransmit", "Retransmission of packets");
	enableC.undebug.addSC("rif", "RIF cache transactions");
	enableC.undebug.addSC("rtr", "RTR Monitor Information");
		enableC.undebug.rtr.addSC("error", "Output RTR Error Messages");
		enableC.undebug.rtr.addSC("trace", "Trace RTR");
	enableC.undebug.addSC("serial", "Serial interface information");
		enableC.undebug.serial.addSC("event", "Serial network interface event");
		enableC.undebug.serial.addSC("interface", "Serial interface events");
		enableC.undebug.serial.addSC("m32_dma", "Serial M32 DMA");
		enableC.undebug.serial.addSC("mueslix", "Serial Mueslix");
		enableC.undebug.serial.addSC("packet", "Serial network interface packets");
		enableC.undebug.serial.addSC("revive", "Serial Revive");
	enableC.undebug.addSC("smf", "Software MAC filter");
		enableC.undebug.smf.addSC("updates", "address insertions and deletions");
	enableC.undebug.addSC("snapshot", "Snapshot activity");
	enableC.undebug.addSC("snmp", "SNMP information");
		enableC.undebug.snmp.addSC("headers", "SNMP packet headers");
		enableC.undebug.snmp.addSC("packets", "SNMP packets");
		enableC.undebug.snmp.addSC("timers", "SNMP timer activity");
	enableC.undebug.addSC("sntp", "SNTP information");
		enableC.undebug.sntp.addSC("adjust", "SNTP clock adjustments");
		enableC.undebug.sntp.addSC("packets", "SNTP packets");
		enableC.undebug.sntp.addSC("select", "SNTP clock selection");
	enableC.undebug.addSC("standby", "Hot Standby Router Protocol (HSRP)");
		enableC.undebug.standby.addSC("errors", "HSRP errors");
		enableC.undebug.standby.addSC("events", "HSRP events");
		enableC.undebug.standby.addSC("packets", "HSRP packets");
		enableC.undebug.standby.addSC("terse", "Display limited range of HSRP errors, events and packets");
	enableC.undebug.addSC("tacacs", "TACACS authentication and authorization");
		enableC.undebug.tacacs.addSC("accounting", "TACACS+ protocol accounting");
		enableC.undebug.tacacs.addSC("authentication", "TACACS+ protocol authentication");
		enableC.undebug.tacacs.addSC("authorization", "TACACS+ protocol authorization");
		enableC.undebug.tacacs.addSC("events", "TACACS+ protocol events");
		enableC.undebug.tacacs.addSC("packet", "TACACS+ packets");
	enableC.undebug.addSC("telnet", "Incoming telnet connections");
	enableC.undebug.addSC("template", "Template activity");
	enableC.undebug.addSC("tftp", "TFTP debugging");
		enableC.undebug.tftp.addSC("events", "TFTP events");
		enableC.undebug.tftp.addSC("packets", "TFTP packets");
	enableC.undebug.addSC("tunnel", "Generic Tunnel Interface");
	enableC.undebug.addSC("udptn", "UDPtn async data transport");
	enableC.undebug.addSC("vlan", "vLAN information");
		enableC.undebug.vlan.addSC("packets", "vLAN packet information");
	enableC.undebug.addSC("vpdn", "VPDN information");
		enableC.undebug.vpdn.addSC("call", "VPDN call");
		enableC.undebug.vpdn.addSC("error", "VPDN protocol errors");
		enableC.undebug.vpdn.addSC("event", "VPDN event");
		enableC.undebug.vpdn.addSC("l2tp-sequencing", "L2TP sequencing");
		enableC.undebug.vpdn.addSC("l2x-data", "L2F/L2TP data packets");
		enableC.undebug.vpdn.addSC("l2x-errors", "L2F/L2TP protocol errors");
		enableC.undebug.vpdn.addSC("l2x-events", "L2F/L2TP protocol events");
		enableC.undebug.vpdn.addSC("l2x-packets", "L2F/L2TP control packets");
		enableC.undebug.vpdn.addSC("message", "VPDN inter-process message");
		enableC.undebug.vpdn.addSC("packet", "VPDN packet");
		enableC.undebug.vpdn.addSC("pppoe-data", "PPPoE data packets");
		enableC.undebug.vpdn.addSC("pppoe-errors", "PPPoE protocol errors");
		enableC.undebug.vpdn.addSC("pppoe-events", "PPPoE protocol events");
		enableC.undebug.vpdn.addSC("pppoe-packets", "PPPoE control packets");
	enableC.undebug.addSC("vpn", "VPN information");
		enableC.undebug.vpn.addSC("authorization", "VPN authorization information");
	enableC.undebug.addSC("vprofile", "Virtual Profile information");
		enableC.undebug.vprofile.addSC("packet", "Virtual Profile packet");
		enableC.undebug.vprofile.addSC("subblock", "Virtual Profile subblock");
	enableC.undebug.addSC("vtemplate", "Virtual Template information");

enableC.addSC("verify", "Verify a file");
	enableC.verify.addSC("flash:", "File to be verified");
enableC.addSC("where", "List active connections");
enableC.addSC("write", "Write running configuration to memory, network, or terminal");
	enableC.write.addSC("erase", "Erase NV memory");
	enableC.write.addSC("memory", "Write to NV memory");
	enableC.write.addSC("terminal", "Write to terminal");
enableC.addSC("x28", "Become an X.28 PAD");
enableC.addSC("x3", "Set X.3 parameters on PAD");
