| 1.2 |  | Routers |
| 1.2.5 |  | Connecting console interfaces |

| The console port is a management port used to provide out-of-band access to the router. It is used for the initial configuration of the router, monitoring, and disaster recovery procedures. To connect to the console port, a rollover cable and a RJ-45 to DB-9 adapter are used to connect a PC. Cisco supplies the necessary adapter to connect to the console port. The PC or terminal must support VT100 terminal emulation. Terminal emulation software such as HyperTerminal is usually used. To connect the PC to a router: Configure terminal emulation software on the PC for: The appropriate com port 9600 baud 8 data bits No parity 1 stop bit No flow control Connect the RJ-45 connector of the rollover cable to the router console port. Connect the other end of the rollover cable to the RJ-45 to DB-9 adapter. Attach the female DB-9 adapter to a PC.
| Lab Activity Lab Exercise: Connecting Console Interfaces This lab is to connect a PC to a router using a console or rollover cable.
| Web Links Connecting the Console Terminal and Modem http://www.cisco.com/en/US/products/hw/ routers/ps259/products_installation_guide_ chapter09186a008007dff8.html#xtocid17