| 7.3 |  | IGRP |
| 7.3.7 |  | Verifying IGRP configuration |

| To verify that IGRP has been configured properly, enter the show ip route command and look for IGRP routes signified by an "I". Additional commands for checking IGRP configuration are as follows: show interface interface show running-config show running-config interface interface show running-config | begin interface interface show running-config | begin igrp show ip protocols To verify that the Ethernet interface is properly configured, enter the show interface fa0/0 command. Figure illustrates the output. To see if IGRP is enabled on the router, enter the show ip protocols command. Figure illustrates the output. The commands illustrated in Figures verify the network statements, IP addressing, and routing tables.
| Lab Activity e-Lab Activity: Verifying IGRP Configuration In this lab, the students will use IOS show commands to verify the operation of a router running IGRP.
| Lab Activity e-Lab Activity: IGRP In this lab, the students will set up dynamic routing between networks using IGRP.
| Web Links Configuring IGRP http://www.cisco.com/en/US/products/sw/ iosswrel/ps1831/ products_ onfiguration_guide_ chapter09186a00800d97f6.html