
routerEIGRPC.addSC("auto-summary", "Enable automatic network number summarization");
routerEIGRPC.addSC("default", "Set a command to its defaults");
routerEIGRPC.addSC("default-information", "Control distribution of default information");
	routerEIGRPC["default-information"].addSC("allowed", "Allow default information");
	routerEIGRPC["default-information"].addSC("in", "Accept default routing information");
		routerEIGRPC["default-information"]["in"].addSC("<1-99>", "A standard IP access list number");
		routerEIGRPC["default-information"]["in"].addSC("<1300-1999>", "A standard expanded IP access list number");
		routerEIGRPC["default-information"]["in"].addSC("WORD", "Standard Access-list name");
	routerEIGRPC["default-information"].addSC("out", "Output default routing information");
		routerEIGRPC["default-information"].out.addSC("<1-99>", "A standard IP access list number");
		routerEIGRPC["default-information"].out.addSC("<1300-1999>", "A standard expanded IP access list number");
		routerEIGRPC["default-information"].out.addSC("WORD", "Standard Access-list name");
routerEIGRPC.addSC("default-metric", "Set metric of redistributed routes");
routerEIGRPC.addSC("distance", "Define an administrative distance");
	routerEIGRPC.distance.addSC("<1-255>", "Administrative distance");
		routerEIGRPC.distance["<1-255>"].addSC("A.B.C.D", "IP Source address");
			routerEIGRPC.distance["<1-255>"]["A.B.C.D"].addSC("A.B.C.D", "IP address mask");
				routerEIGRPC.distance["<1-255>"]["A.B.C.D"]["A.B.C.D"].addSC("<1-99>", "IP Standard access list number");
				routerEIGRPC.distance["<1-255>"]["A.B.C.D"]["A.B.C.D"].addSC("<1300-1999>", "IP Standard expanded access list number");
	routerEIGRPC.distance.addSC("eigrp", "IP-EIGRP distance");
		routerEIGRPC.distance.eigrp.addSC("<1-255>", "Distance for internal routes");
			routerEIGRPC.distance.eigrp["<1-255>"].addSC("<1-255>", "Distance for external routes");
routerEIGRPC.addSC("distribute-list", "Filter networks in routing updates");
	routerEIGRPC["distribute-list"].addSC("<1-199>", "IP access list number");
		routerEIGRPC["distribute-list"]["<1-199>"].addSC("in", "Filter incoming routing updates");
			routerEIGRPC["distribute-list"]["<1-199>"]["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerEIGRPC["distribute-list"]["<1-199>"]["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerEIGRPC["distribute-list"]["<1-199>"]["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerEIGRPC["distribute-list"]["<1-199>"]["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerEIGRPC["distribute-list"]["<1-199>"]["in"].addSC("Loopback", "Loopback interface");
				routerEIGRPC["distribute-list"]["<1-199>"]["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerEIGRPC["distribute-list"]["<1-199>"]["in"].addSC("Null", "Null interface");
				routerEIGRPC["distribute-list"]["<1-199>"]["in"].Null.addSC("<0-0>", "Null interface number");
			routerEIGRPC["distribute-list"]["<1-199>"]["in"].addSC("Vlan", "Catalyst Vlans");
				routerEIGRPC["distribute-list"]["<1-199>"]["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
		routerEIGRPC["distribute-list"]["<1-199>"].addSC("out", "Filter outgoing routing updates");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerEIGRPC["distribute-list"]["<1-199>"].out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerEIGRPC["distribute-list"]["<1-199>"].out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Loopback", "Loopback interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Null", "Null interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out.Null.addSC("<0-0>", "Null interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Vlan", "Catalyst Vlans");
				routerEIGRPC["distribute-list"]["<1-199>"].out.Vlan.addSC("<1-1001>", "Vlan interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("bgp", "Border Gateway Protocol (BGP)");
				routerEIGRPC["distribute-list"]["<1-199>"].out.bgp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("connected", "Connected");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("egp", "Exterior Gateway Protocol (EGP)");
				routerEIGRPC["distribute-list"]["<1-199>"].out.egp.addSC("<0-65535>", "Remote autonomous system number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				routerEIGRPC["distribute-list"]["<1-199>"].out.eigrp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				routerEIGRPC["distribute-list"]["<1-199>"].out.igrp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("ospf", "Open Shortest Path First (OSPF)");
				routerEIGRPC["distribute-list"]["<1-199>"].out.ospf.addSC("<1-65535>", "Process ID");
					routerEIGRPC["distribute-list"]["<1-199>"].out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
						routerEIGRPC["distribute-list"]["<1-199>"].out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("rip", "Routing Information Protocol (RIP)");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("static", "Static routes");
	routerEIGRPC["distribute-list"].addSC("<1300-2699>", "IP expanded access list number");
		routerEIGRPC["distribute-list"]["<1300-2699>"].addSC("in", "Filter incoming routing updates");
			routerEIGRPC["distribute-list"]["<1300-2699>"]["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerEIGRPC["distribute-list"]["<1300-2699>"]["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"]["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerEIGRPC["distribute-list"]["<1300-2699>"]["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"]["in"].addSC("Loopback", "Loopback interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"]["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"]["in"].addSC("Null", "Null interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"]["in"].Null.addSC("<0-0>", "Null interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"]["in"].addSC("Vlan", "Catalyst Vlans");
				routerEIGRPC["distribute-list"]["<1300-2699>"]["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
		routerEIGRPC["distribute-list"]["<1300-2699>"].addSC("out", "Filter outgoing routing updates");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Loopback", "Loopback interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Null", "Null interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.Null.addSC("<0-0>", "Null interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Vlan", "Catalyst Vlans");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.Vlan.addSC("<1-1001>", "Vlan interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("bgp", "Border Gateway Protocol (BGP)");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.bgp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("connected", "Connected");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("egp", "Exterior Gateway Protocol (EGP)");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.egp.addSC("<0-65535>", "Remote autonomous system number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.eigrp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.igrp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("ospf", "Open Shortest Path First (OSPF)");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.ospf.addSC("<1-65535>", "Process ID");
					routerEIGRPC["distribute-list"]["<1300-2699>"].out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
						routerEIGRPC["distribute-list"]["<1300-2699>"].out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("rip", "Routing Information Protocol (RIP)");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("static", "Static routes");
	routerEIGRPC["distribute-list"].addSC("WORD", "Access-list name");
		routerEIGRPC["distribute-list"].WORD.addSC("in", "Filter incoming routing updates");
			routerEIGRPC["distribute-list"].WORD["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerEIGRPC["distribute-list"].WORD["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerEIGRPC["distribute-list"].WORD["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerEIGRPC["distribute-list"].WORD["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerEIGRPC["distribute-list"].WORD["in"].addSC("Loopback", "Loopback interface");
				routerEIGRPC["distribute-list"].WORD["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerEIGRPC["distribute-list"].WORD["in"].addSC("Null", "Null interface");
				routerEIGRPC["distribute-list"].WORD["in"].Null.addSC("<0-0>", "Null interface number");
			routerEIGRPC["distribute-list"].WORD["in"].addSC("Vlan", "Catalyst Vlans");
				routerEIGRPC["distribute-list"].WORD["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
		routerEIGRPC["distribute-list"].WORD.addSC("out", "Filter outgoing routing updates");
			routerEIGRPC["distribute-list"].WORD.out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerEIGRPC["distribute-list"].WORD.out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerEIGRPC["distribute-list"].WORD.out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Loopback", "Loopback interface");
				routerEIGRPC["distribute-list"].WORD.out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Null", "Null interface");
				routerEIGRPC["distribute-list"].WORD.out.Null.addSC("<0-0>", "Null interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Vlan", "Catalyst Vlans");
				routerEIGRPC["distribute-list"].WORD.out.Vlan.addSC("<1-1001>", "Vlan interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("bgp", "Border Gateway Protocol (BGP)");
				routerEIGRPC["distribute-list"].WORD.out.bgp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("connected", "Connected");
			routerEIGRPC["distribute-list"].WORD.out.addSC("egp", "Exterior Gateway Protocol (EGP)");
				routerEIGRPC["distribute-list"].WORD.out.egp.addSC("<0-65535>", "Remote autonomous system number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				routerEIGRPC["distribute-list"].WORD.out.eigrp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				routerEIGRPC["distribute-list"].WORD.out.igrp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("ospf", "Open Shortest Path First (OSPF)");
				routerEIGRPC["distribute-list"].WORD.out.ospf.addSC("<1-65535>", "Process ID");
					routerEIGRPC["distribute-list"].WORD.out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
						routerEIGRPC["distribute-list"].WORD.out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
			routerEIGRPC["distribute-list"].WORD.out.addSC("rip", "Routing Information Protocol (RIP)");
			routerEIGRPC["distribute-list"].WORD.out.addSC("static", "Static routes");
	routerEIGRPC["distribute-list"].addSC("gateway", "Filtering incoming updates based on gateway");
		routerEIGRPC["distribute-list"].gateway.addSC("WORD", "Name of an IP prefix-list");
			routerEIGRPC["distribute-list"].gateway.WORD.addSC("in", "Filter incoming routing updates");
				routerEIGRPC["distribute-list"].gateway.WORD["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routerEIGRPC["distribute-list"].gateway.WORD["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routerEIGRPC["distribute-list"].gateway.WORD["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routerEIGRPC["distribute-list"].gateway.WORD["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routerEIGRPC["distribute-list"].gateway.WORD["in"].addSC("Loopback", "Loopback interface");
					routerEIGRPC["distribute-list"].gateway.WORD["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerEIGRPC["distribute-list"].gateway.WORD["in"].addSC("Null", "Null interface");
					routerEIGRPC["distribute-list"].gateway.WORD["in"].Null.addSC("<0-0>", "Null interface number");
				routerEIGRPC["distribute-list"].gateway.WORD["in"].addSC("Vlan", "Catalyst Vlans");
					routerEIGRPC["distribute-list"].gateway.WORD["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
			routerEIGRPC["distribute-list"].gateway.WORD.addSC("out", "Filter outgoing routing updates");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routerEIGRPC["distribute-list"].gateway.WORD.out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routerEIGRPC["distribute-list"].gateway.WORD.out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Loopback", "Loopback interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Null", "Null interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out.Null.addSC("<0-0>", "Null interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Vlan", "Catalyst Vlans");
					routerEIGRPC["distribute-list"].gateway.WORD.out.Vlan.addSC("<1-1001>", "Vlan interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("bgp", "Border Gateway Protocol (BGP)");
					routerEIGRPC["distribute-list"].gateway.WORD.out.bgp.addSC("<1-65535>", "Autonomous system number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("connected", "Connected");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("egp", "Exterior Gateway Protocol (EGP)");
					routerEIGRPC["distribute-list"].gateway.WORD.out.egp.addSC("<0-65535>", "Remote autonomous system number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
					routerEIGRPC["distribute-list"].gateway.WORD.out.eigrp.addSC("<1-65535>", "Autonomous system number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
					routerEIGRPC["distribute-list"].gateway.WORD.out.igrp.addSC("<1-65535>", "Autonomous system number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("ospf", "Open Shortest Path First (OSPF)");
					routerEIGRPC["distribute-list"].gateway.WORD.out.ospf.addSC("<1-65535>", "Process ID");
						routerEIGRPC["distribute-list"].gateway.WORD.out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
							routerEIGRPC["distribute-list"].gateway.WORD.out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("rip", "Routing Information Protocol (RIP)");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("static", "Static routes");
	routerEIGRPC["distribute-list"].addSC("prefix", "Filter prefixes in routing updates");
		routerEIGRPC["distribute-list"].prefix.addSC("WORD", "Name of an IP prefix-list");
			routerEIGRPC["distribute-list"].prefix.WORD.addSC("gateway", "Filtering incoming updates based on gateway");
			routerEIGRPC["distribute-list"].prefix.WORD.addSC("in", "Filter incoming routing updates");
				routerEIGRPC["distribute-list"].prefix.WORD["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routerEIGRPC["distribute-list"].prefix.WORD["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routerEIGRPC["distribute-list"].prefix.WORD["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routerEIGRPC["distribute-list"].prefix.WORD["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routerEIGRPC["distribute-list"].prefix.WORD["in"].addSC("Loopback", "Loopback interface");
					routerEIGRPC["distribute-list"].prefix.WORD["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerEIGRPC["distribute-list"].prefix.WORD["in"].addSC("Null", "Null interface");
					routerEIGRPC["distribute-list"].prefix.WORD["in"].Null.addSC("<0-0>", "Null interface number");
				routerEIGRPC["distribute-list"].prefix.WORD["in"].addSC("Vlan", "Catalyst Vlans");
					routerEIGRPC["distribute-list"].prefix.WORD["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
			routerEIGRPC["distribute-list"].prefix.WORD.addSC("out", "Filter outgoing routing updates");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routerEIGRPC["distribute-list"].prefix.WORD.out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routerEIGRPC["distribute-list"].prefix.WORD.out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Loopback", "Loopback interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Null", "Null interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out.Null.addSC("<0-0>", "Null interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Vlan", "Catalyst Vlans");
					routerEIGRPC["distribute-list"].prefix.WORD.out.Vlan.addSC("<1-1001>", "Vlan interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("bgp", "Border Gateway Protocol (BGP)");
					routerEIGRPC["distribute-list"].prefix.WORD.out.bgp.addSC("<1-65535>", "Autonomous system number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("connected", "Connected");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("egp", "Exterior Gateway Protocol (EGP)");
					routerEIGRPC["distribute-list"].prefix.WORD.out.egp.addSC("<0-65535>", "Remote autonomous system number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
					routerEIGRPC["distribute-list"].prefix.WORD.out.eigrp.addSC("<1-65535>", "Autonomous system number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
					routerEIGRPC["distribute-list"].prefix.WORD.out.igrp.addSC("<1-65535>", "Autonomous system number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("ospf", "Open Shortest Path First (OSPF)");
					routerEIGRPC["distribute-list"].prefix.WORD.out.ospf.addSC("<1-65535>", "Process ID");
						routerEIGRPC["distribute-list"].prefix.WORD.out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
							routerEIGRPC["distribute-list"].prefix.WORD.out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("rip", "Routing Information Protocol (RIP)");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("static", "Static routes");
routerEIGRPC.addSC("eigrp", "EIGRP specific commands");
	routerEIGRPC.eigrp.addSC("log-neighbor-changes", "Enable/Disable IP-EIGRP neighbor logging");
	routerEIGRPC.eigrp.addSC("log-neighbor-warnings", "Enable/Disable IP-EIGRP neighbor warnings");
		routerEIGRPC.eigrp["log-neighbor-warnings"].addSC("<1-65535>", "Neighbor warning interval in seconds");
	routerEIGRPC.eigrp.addSC("router-id", "router-id for this EIGRP process");
		routerEIGRPC.eigrp["router-id"].addSC("A.B.C.D", "EIGRP Router-ID in IP address format");
	routerEIGRPC.eigrp.addSC("stub", "Set IP-EIGRP as stubbed router");
		routerEIGRPC.eigrp.stub.addSC("connected", "Do advertise connected routes");
		routerEIGRPC.eigrp.stub.addSC("receive-only", "Set IP-EIGRP as receive only neighbor");
		routerEIGRPC.eigrp.stub.addSC("static", "Do advertise static routes");
			routerEIGRPC.eigrp.stub.static.addSC("connected", "Do advertise connected routes");
		routerEIGRPC.eigrp.stub.addSC("summary", "Do advertise summary routes");
			routerEIGRPC.eigrp.stub.summary.addSC("connected", "Do advertise connected routes");
			routerEIGRPC.eigrp.stub.summary.addSC("static", "Do advertise static routes");
				routerEIGRPC.eigrp.stub.summary.static.addSC("connected", "Do advertise connected routes");
routerEIGRPC.addSC("exit", "Exit from routing protocol configuration mode");
routerEIGRPC.addSC("help", "Description of the interactive help system");
routerEIGRPC.addSC("maximum-paths", "Forward packets over multiple paths");
	routerEIGRPC["maximum-paths"].addSC("<1-8>", "Number of paths");
routerEIGRPC.addSC("metric", "Modify IGRP routing metrics and parameters");
	routerEIGRPC.metric.addSC("holddown", "Enable IGRP holddown");
	routerEIGRPC.metric.addSC("maximum-hops", "Advertise IGRP routes greater than <hops> as unreachable");
		routerEIGRPC.metric["maximum-hops"].addSC("<1-255>", "Hop count");
	routerEIGRPC.metric.addSC("weights", "Modify IGRP metric coefficients");
		routerEIGRPC.metric.weights.addSC("<0-8>", "Type Of Service (Only TOS 0 supported)");
			routerEIGRPC.metric.weights["<0-8>"].addSC("<0-4294967295>", "K1");
				routerEIGRPC.metric.weights["<0-8>"]["<0-4294967295>"].addSC("<0-4294967295>", "K2");
					routerEIGRPC.metric.weights["<0-8>"]["<0-4294967295>"]["<0-4294967295>"].addSC("<0-4294967295>", "K3");
						routerEIGRPC.metric.weights["<0-8>"]["<0-4294967295>"]["<0-4294967295>"]["<0-4294967295>"].addSC("<0-4294967295>", "K4");
							routerEIGRPC.metric.weights["<0-8>"]["<0-4294967295>"]["<0-4294967295>"]["<0-4294967295>"]["<0-4294967295>"].addSC("<0-4294967295>", "K5");
routerEIGRPC.addSC("neighbor", "Specify a neighbor router");
	routerEIGRPC.neighbor.addSC("A.B.C.D", "Neighbor address");
		routerEIGRPC.neighbor["A.B.C.D"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
			routerEIGRPC.neighbor["A.B.C.D"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
		routerEIGRPC.neighbor["A.B.C.D"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
			routerEIGRPC.neighbor["A.B.C.D"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
		routerEIGRPC.neighbor["A.B.C.D"].addSC("Loopback", "Loopback interface");
			routerEIGRPC.neighbor["A.B.C.D"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
		routerEIGRPC.neighbor["A.B.C.D"].addSC("Null", "Null interface");
			routerEIGRPC.neighbor["A.B.C.D"].Null.addSC("<0-0>", "Null interface number");
		routerEIGRPC.neighbor["A.B.C.D"].addSC("Vlan", "Catalyst Vlans");
			routerEIGRPC.neighbor["A.B.C.D"].Vlan.addSC("<1-1001>", "Vlan interface number");
routerEIGRPC.addSC("network", "Enable routing on an IP network");
	routerEIGRPC.network.addSC("A.B.C.D", "Network number");
		routerEIGRPC.network["A.B.C.D"].addSC("A.B.C.D", "EIGRP wild card bits");
routerEIGRPC.addSC("no", "Negate a command or set its defaults");
routerEIGRPC.addSC("offset-list", "Add or subtract offset from IGRP or RIP metrics");
routerEIGRPC.addSC("passive-interface", "Suppress routing updates on an interface");
	routerEIGRPC["passive-interface"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
		routerEIGRPC["passive-interface"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
	routerEIGRPC["passive-interface"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
		routerEIGRPC["passive-interface"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
	routerEIGRPC["passive-interface"].addSC("Loopback", "Loopback interface");
		routerEIGRPC["passive-interface"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
	routerEIGRPC["passive-interface"].addSC("Null", "Null interface");
		routerEIGRPC["passive-interface"].Null.addSC("<0-0>", "Null interface number");
	routerEIGRPC["passive-interface"].addSC("Vlan", "Catalyst Vlans");
		routerEIGRPC["passive-interface"].Vlan.addSC("<1-1001>", "Vlan interface number");
	routerEIGRPC["passive-interface"].addSC("default", "Suppress routing updates on all interfaces");
routerEIGRPC.addSC("redistribute", "Redistribute information from another routing protocol");
	routerEIGRPC.redistribute.addSC("bgp", "Border Gateway Protocol (BGP)");
		routerEIGRPC.redistribute.bgp.addSC("<1-65535>", "Autonomous system number");
	routerEIGRPC.redistribute.addSC("connected", "Connected");
	routerEIGRPC.redistribute.addSC("egp", "Exterior Gateway Protocol (EGP)");
		routerEIGRPC.redistribute.egp.addSC("<0-65535>", "Remote autonomous system number");
	routerEIGRPC.redistribute.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
		routerEIGRPC.redistribute.eigrp.addSC("<1-65535>", "Autonomous system number");
	routerEIGRPC.redistribute.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
		routerEIGRPC.redistribute.igrp.addSC("<1-65535>", "Autonomous system number");
	routerEIGRPC.redistribute.addSC("isis", "ISO IS-IS");
		routerEIGRPC.redistribute.isis.addSC("level-1", "IS-IS level-1 routes only");
		routerEIGRPC.redistribute.isis.addSC("level-1-2", "IS-IS level-1 and level-2 routes");
		routerEIGRPC.redistribute.isis.addSC("level-2", "IS-IS level-2 routes only");
		routerEIGRPC.redistribute.isis.addSC("WORD", "ISO routing area tag");
			routerEIGRPC.redistribute.isis.WORD.addSC("level-1", "IS-IS level-1 routes only");
			routerEIGRPC.redistribute.isis.WORD.addSC("level-1-2", "IS-IS level-1 and level-2 routes");
			routerEIGRPC.redistribute.isis.WORD.addSC("level-2", "IS-IS level-2 routes only");
	routerEIGRPC.redistribute.addSC("iso-igrp", "IGRP for OSI networks");
		routerEIGRPC.redistribute["iso-igrp"].addSC("WORD", "ISO routing area tag");
	routerEIGRPC.redistribute.addSC("metric", "Metric for redistributed routes");
		routerEIGRPC.redistribute.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
			routerEIGRPC.redistribute.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
				routerEIGRPC.redistribute.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
					routerEIGRPC.redistribute.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
						routerEIGRPC.redistribute.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
	routerEIGRPC.redistribute.addSC("mobile", "Mobile routes");
		routerEIGRPC.redistribute.mobile.addSC("metric", "Metric for redistributed routes");
			routerEIGRPC.redistribute.mobile.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
				routerEIGRPC.redistribute.mobile.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
					routerEIGRPC.redistribute.mobile.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
						routerEIGRPC.redistribute.mobile.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
							routerEIGRPC.redistribute.mobile.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
	routerEIGRPC.redistribute.addSC("odr", "On Demand stub Routes");
		routerEIGRPC.redistribute.odr.addSC("metric", "Metric for redistributed routes");
			routerEIGRPC.redistribute.odr.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
				routerEIGRPC.redistribute.odr.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
					routerEIGRPC.redistribute.odr.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
						routerEIGRPC.redistribute.odr.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
							routerEIGRPC.redistribute.odr.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
	routerEIGRPC.redistribute.addSC("ospf", "Open Shortest Path First (OSPF)");
		routerEIGRPC.redistribute.ospf.addSC("<1-65535>", "Process ID");
			routerEIGRPC.redistribute.ospf["<1-65535>"].addSC("match", "Redistribution of OSPF routes");
				routerEIGRPC.redistribute.ospf["<1-65535>"].match.addSC("external", "Redistribute OSPF external routes");
					routerEIGRPC.redistribute.ospf["<1-65535>"].match.external.addSC("<1-1>", "Redistribute external type 1 routes");
					routerEIGRPC.redistribute.ospf["<1-65535>"].match.external.addSC("<2-2>", "Redistribute external type 2 routes");
				routerEIGRPC.redistribute.ospf["<1-65535>"].match.addSC("internal", "Redistribute OSPF internal routes");
					routerEIGRPC.redistribute.ospf["<1-65535>"].match.internal.addSC("external", "Redistribute OSPF external routes");
						routerEIGRPC.redistribute.ospf["<1-65535>"].match.internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
						routerEIGRPC.redistribute.ospf["<1-65535>"].match.internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
				routerEIGRPC.redistribute.ospf["<1-65535>"].match.addSC("nssa-external", "Redistribute OSPF NSSA external routes");
					routerEIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].addSC("<1-1>", "Redistribute NSSA external type 1 routes");
					routerEIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].addSC("<2-2>", "Redistribute NSSA external type 2 routes");
					routerEIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].addSC("external", "Redistribute OSPF external routes");
						routerEIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].external.addSC("<1-1>", "Redistribute external type 1 routes");
						routerEIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].external.addSC("<2-2>", "Redistribute external type 2 routes");
					routerEIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].addSC("internal", "Redistribute OSPF internal routes");
						routerEIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].internal.addSC("external", "Redistribute OSPF external routes");
							routerEIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
							routerEIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
			routerEIGRPC.redistribute.ospf["<1-65535>"].addSC("metric", "Metric for redistributed routes");
				routerEIGRPC.redistribute.ospf["<1-65535>"].metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
					routerEIGRPC.redistribute.ospf["<1-65535>"].metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
						routerEIGRPC.redistribute.ospf["<1-65535>"].metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
							routerEIGRPC.redistribute.ospf["<1-65535>"].metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
								routerEIGRPC.redistribute.ospf["<1-65535>"].metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
									routerEIGRPC.redistribute.ospf["<1-65535>"].metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"]["<1-4294967295>"].addSC("match", "Redistribution of OSPF routes");
			routerEIGRPC.redistribute.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
				routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
					routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.addSC("match", "Redistribution of OSPF routes");
						routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.addSC("external", "Redistribute OSPF external routes");
							routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.external.addSC("<1-1>", "Redistribute external type 1 routes");
							routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.external.addSC("<2-2>", "Redistribute external type 2 routes");
						routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.addSC("internal", "Redistribute OSPF internal routes");
							routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.internal.addSC("external", "Redistribute OSPF external routes");
								routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
								routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
						routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.addSC("nssa-external", "Redistribute OSPF NSSA external routes");
							routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].addSC("<1-1>", "Redistribute NSSA external type 1 routes");
							routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].addSC("<2-2>", "Redistribute NSSA external type 2 routes");
							routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].addSC("external", "Redistribute OSPF external routes");
								routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].external.addSC("<1-1>", "Redistribute external type 1 routes");
								routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].external.addSC("<2-2>", "Redistribute external type 2 routes");
							routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].addSC("internal", "Redistribute OSPF internal routes");
								routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].internal.addSC("external", "Redistribute OSPF external routes");
									routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
									routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
					routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.addSC("metric", "Metric for redistributed routes");
						routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
							routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
								routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
									routerEIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
	routerEIGRPC.redistribute.addSC("rip", "Routing Information Protocol (RIP)");
		routerEIGRPC.redistribute.rip.addSC("metric", "Metric for redistributed routes");
			routerEIGRPC.redistribute.rip.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
				routerEIGRPC.redistribute.rip.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
					routerEIGRPC.redistribute.rip.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
						routerEIGRPC.redistribute.rip.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
							routerEIGRPC.redistribute.rip.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
	routerEIGRPC.redistribute.addSC("route-map", "Route map reference");
		routerEIGRPC.redistribute["route-map"].addSC("WORD", "Pointer to route-map entries");
			routerEIGRPC.redistribute["route-map"].WORD.addSC("metric", "Metric for redistributed routes");
				routerEIGRPC.redistribute["route-map"].WORD.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
					routerEIGRPC.redistribute["route-map"].WORD.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
						routerEIGRPC.redistribute["route-map"].WORD.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
							routerEIGRPC.redistribute["route-map"].WORD.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
								routerEIGRPC.redistribute["route-map"].WORD.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
	routerEIGRPC.redistribute.addSC("static", "Static routes");
		routerEIGRPC.redistribute.static.addSC("metric", "Metric for redistributed routes");
			routerEIGRPC.redistribute.static.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
				routerEIGRPC.redistribute.static.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
					routerEIGRPC.redistribute.static.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
						routerEIGRPC.redistribute.static.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
							routerEIGRPC.redistribute.static.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
		routerEIGRPC.redistribute.static.addSC("route-map", "Route map reference");
			routerEIGRPC.redistribute.static["route-map"].addSC("WORD", "Pointer to route-map entries");
				routerEIGRPC.redistribute.static["route-map"].WORD.addSC("metric", "Metric for redistributed routes");
					routerEIGRPC.redistribute.static["route-map"].WORD.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
						routerEIGRPC.redistribute.static["route-map"].WORD.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
							routerEIGRPC.redistribute.static["route-map"].WORD.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
								routerEIGRPC.redistribute.static["route-map"].WORD.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
									routerEIGRPC.redistribute.static["route-map"].WORD.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
routerEIGRPC.addSC("timers", "Adjust routing timers");
	routerEIGRPC.timers.addSC("active-time", "EIGRP time limit for active state");
		routerEIGRPC.timers["active-time"].addSC("<1-4294967295>", "EIGRP active-state time limit in minutes");
		routerEIGRPC.timers["active-time"].addSC("disabled", "disable EIGRP time limit for active state");
routerEIGRPC.addSC("traffic-share", "How to compute traffic share over alternate paths");
	routerEIGRPC["traffic-share"].addSC("balanced", "Share inversely proportional to metric");
	routerEIGRPC["traffic-share"].addSC("min", "All traffic shared among min metric paths");
		routerEIGRPC["traffic-share"].min.addSC("across-interfaces", "Use different interfaces for equal-cost paths");
routerEIGRPC.addSC("variance", "Control load balancing variance");
	routerEIGRPC.variance.addSC("<1-128>", "Metric variance multiplier");
