
		enableC.show.ip.addSC("pgm", "PGM Reliable Transport Protocol");
		enableC.show.ip.addSC("protocols", "IP routing protocol process parameters and statistics");
		enableC.show.ip.addSC("rip", "IP RIP show commands");
		enableC.show.ip.addSC("route", "IP routing table");
			enableC.show.ip.route.addSC("bgp", "Border Gateway Protocol (BGP)");
			enableC.show.ip.route.addSC("connected", "Connected");
			enableC.show.ip.route.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			enableC.show.ip.route.addSC("ospf", "Open Shortest Path First (OSPF)");
			enableC.show.ip.route.addSC("profile", "IP routing table profile");
			enableC.show.ip.route.addSC("rip", "Routing Information Protocol (RIP)");
			enableC.show.ip.route.addSC("static", "Static routes");
			enableC.show.ip.route.addSC("summary", "Summary of all routes");
		enableC.show.ip.addSC("rpf", "Display RPF information for multicast source");
			enableC.show.ip.rpf.addSC("Hostname or A.B.C.D", "IP name or address of multicast source");
				enableC.show.ip.rpf["Hostname or A.B.C.D"].addSC("metric", "Metric");
		enableC.show.ip.addSC("rsvp", "RSVP information");
		enableC.show.ip.addSC("rtp", "RTP/UDP/IP header-compression statistics");
		enableC.show.ip.addSC("sap", "Session Announcement Protocol cache");
		enableC.show.ip.addSC("sockets", "Open IP sockets");
		enableC.show.ip.addSC("tcp", "TCP/IP header-compression statistics");
		enableC.show.ip.addSC("traffic", "IP protocol statistics");
		enableC.show.ip.addSC("vrf", "VPN Routing/Forwarding instance information");
			enableC.show.ip.vrf.addSC("WORD", "VPN Routing/Forwarding instance name");
			enableC.show.ip.vrf.addSC("brief", "Brief VPN Routing/Forwarding instance information");
				enableC.show.ip.vrf.brief.addSC("WORD", "VPN Routing/Forwarding instance name");
			enableC.show.ip.vrf.addSC("detail", "Detailed VPN Routing/Forwarding instance information");
				enableC.show.ip.vrf.detail.addSC("WORD", "VPN Routing/Forwarding instance name");
			enableC.show.ip.vrf.addSC("id", "Show VPN Routing/Forwarding VPN-ID information");
				enableC.show.ip.vrf.id.addSC("WORD", "VPN Routing/Forwarding instance name");
			enableC.show.ip.vrf.addSC("interfaces", "Show VPN Routing/Forwarding interface information");
				enableC.show.ip.vrf.interfaces.addSC("WORD", "VPN Routing/Forwarding instance name");
		enableC.show.ip.addSC("wccp", "WCCP information");
	enableC.show.addSC("ipv6", "IPv6 information");
	enableC.show.addSC("line", "TTY line information");
	enableC.show.addSC("modemcap", "Show Modem Capabilities database");
		enableC.show.modemcap.addSC("WORD", "Modem entry to use");
	enableC.show.addSC("parser", "Display parser information");
	enableC.show.addSC("policy-map", "Show QoS Policy Map");
	enableC.show.addSC("ppp", "PPP parameters and statistics");
		enableC.show.ppp.addSC("multilink", "Multilink PPP bundle information");
		enableC.show.ppp.addSC("queues", "PPP request queues");
	enableC.show.addSC("privilege", "Show current privilege level");
	enableC.show.addSC("processes", "Active process statistics");
		enableC.show.processes.addSC("cpu", "Show CPU use per process");
			enableC.show.processes.cpu.addSC("history", "Show CPU history in graph format");
		enableC.show.processes.addSC("memory", "Show memory use per process");
			enableC.show.processes.memory.addSC("<1-4294967295>", "[pid]");
	enableC.show.addSC("protocols", "Active network routing protocols");
	enableC.show.addSC("qdm", "Show information about QoS Device Manager");
		enableC.show.qdm.addSC("status", "Information and status about currently active QDM web-based clients");
	enableC.show.addSC("queue", "Show queue contents");
	enableC.show.addSC("queueing", "Show queueing configuration");
		enableC.show.queueing.addSC("interface", "");
		enableC.show.queueing.addSC("custom", "custom queueing list configuration");
		enableC.show.queueing.addSC("fair", "fair queueing configuration");
			enableC.show.queueing.fair.addSC("interface", "");
		enableC.show.queueing.addSC("priority", "priority queueing list configuration");
	enableC.show.addSC("reload", "Scheduled reload information");
	enableC.show.addSC("rhosts", "Remote-host+user equivalences");
	enableC.show.addSC("rif", "RIF cache entries");
	enableC.show.addSC("rmon", "rmon statistics");
	enableC.show.addSC("running-config", "Current operating configuration");
	enableC.show.addSC("snapshot", "Snapshot parameters and statistics");
	enableC.show.addSC("snmp", "snmp statistics");
	enableC.show.addSC("sntp", "Simple network time protocol");
	enableC.show.addSC("spanning-tree", "Spanning tree topology");
	enableC.show.addSC("standby", "Hot Standby Router Protocol (HSRP) information");
	enableC.show.addSC("startup-config", "Contents of startup configuration");
	enableC.show.addSC("subsys", "Show subsystem information");
	enableC.show.addSC("tacacs", "Shows tacacs+ server statistics");
	enableC.show.addSC("tcp", "Status of TCP connections");
	enableC.show.addSC("template", "Template information");
		enableC.show.template.addSC("WORD", "Specify template name");
	enableC.show.addSC("terminal", "Display terminal configuration parameters");
	enableC.show.addSC("tgrm", "Trunk Group Resource Mananger info");
	enableC.show.addSC("time-range", "Time range");
	enableC.show.addSC("track", "Tracking information");
	enableC.show.addSC("traffic-shape", "traffic rate shaping configuration");
	enableC.show.addSC("users", "Display information about terminal lines");
	enableC.show.addSC("version", "System hardware and software status");
	enableC.show.addSC("vpdn", "VPDN information");
		enableC.show.vpdn.addSC("domain", "VPDN domain info");
		enableC.show.vpdn.addSC("group", "VPDN group info");
			enableC.show.vpdn.group.addSC("WORD", "Name of VPDN group");
				enableC.show.vpdn.group.WORD.addSC("domain", "Domain session info");
				enableC.show.vpdn.group.WORD.addSC("endpoint", "Endpoint session info");
		enableC.show.vpdn.addSC("history", "History logging");
			enableC.show.vpdn.history.addSC("failure", "Show VPDN User Failure History Table");
				enableC.show.vpdn.history.failure.addSC("WORD", "Name of user");
		enableC.show.vpdn.addSC("multilink", "Multilink VPDN session info");
		enableC.show.vpdn.addSC("session", "Session (call) information");
			enableC.show.vpdn.session.addSC("all", "All session information");
				enableC.show.vpdn.session.state.addSC("username", "Username filter");
					enableC.show.vpdn.session.state.username.addSC("WORD", "Username");
		enableC.show.vpdn.addSC("tunnel", "Tunnel information");
			enableC.show.vpdn.tunnel.addSC("all", "All tunnel information");
	enableC.show.addSC("vtemplate", "Virtual Template interface information");
		enableC.show.vtemplate.addSC("<1-200>", "Virtual Template interface number");
	enableC.show.addSC("whoami", "Info on current tty line");
enableC.addSC("slip", "Start Serial-line IP (SLIP)");
enableC.addSC("squeeze", "Squeeze a filesystem");
enableC.addSC("start-chat", "Start a chat-script on a line");
enableC.addSC("systat", "Display information about terminal lines");
enableC.addSC("telnet", "Open a telnet connection");
	enableC.telnet.addSC("WORD", "IP address or hostname of a remote system");
enableC.addSC("terminal", "Set terminal line parameters");
	enableC.terminal.addSC("txspeed", "Set the transmit speeds");
		enableC.terminal.txspeed.addSC("<0-4294967295>", "Transmit speed");
	enableC.terminal.addSC("width", "Set width of the display terminal");
		enableC.terminal.width.addSC("<0-512>", "Number of characters on a screen line");
enableC.addSC("test", "Test subsystems, memory, and interfaces");
enableC.addSC("traceroute", "Trace route to destination");
	enableC.traceroute.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("ip", "IP Trace");
		enableC.traceroute.ip.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("ipv6", "IPv6 Trace");
		enableC.traceroute.ipv6.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("ipx", "IPX Trace");
		enableC.traceroute.ipx.addSC("WORD", "Trace route to destination address or hostname");
enableC.addSC("tunnel", "Open a tunnel connection");
	enableC.tunnel.addSC("WORD", "Address or hostname of a remote system");
		enableC.tunnel.WORD.addSC("debug", "Enable tunnel debugging output");
enableC.addSC("udptn", "Open an udptn connection");
enableC.addSC("undebug", "Disable debugging functions (see also 'debug')");
	enableC.undebug.addSC("aaa", "AAA Authentication, Authorization and Accounting");
		enableC.undebug.aaa.addSC("accounting", "Accounting");
		enableC.undebug.aaa.addSC("administrative", "Administrative");
		enableC.undebug.aaa.addSC("attr", "AAA Attr Manager");
		enableC.undebug.aaa.addSC("authentication", "Authentication");
		enableC.undebug.aaa.addSC("authorization", "Authorization");
		enableC.undebug.aaa.addSC("db", "AAA DB Manager");
		enableC.undebug.aaa.addSC("id", "AAA Unique Id");
		enableC.undebug.aaa.addSC("ipc", "AAA IPC");
		enableC.undebug.aaa.addSC("per-user", "Per-user attributes");
		enableC.undebug.aaa.addSC("pod", "AAA POD processing");
		enableC.undebug.aaa.addSC("protocol", "AAA protocol processing");
		enableC.undebug.aaa.addSC("subsys", "AAA Subsystem");
	enableC.undebug.addSC("all", "Enable all debugging");
	enableC.undebug.addSC("arp", "IP ARP and HP Probe transactions");
	enableC.undebug.addSC("async", "Async interface information");
		enableC.undebug.async.addSC("async-queue", "Rotary Line Queuing Activity");
		enableC.undebug.async.addSC("framing", "Packet framing");
		enableC.undebug.async.addSC("packet", "Packet I/O");
		enableC.undebug.async.addSC("state", "Interface state changes");
	enableC.undebug.addSC("bgp", "BGP information");
		enableC.undebug.bgp.addSC("dampening", "BGP dampening");
		enableC.undebug.bgp.addSC("events", "BGP events");
		enableC.undebug.bgp.addSC("ipv6", "Address family");
		enableC.undebug.bgp.addSC("keepalives", "BGP keepalives");
		enableC.undebug.bgp.addSC("nsap", "Address family");
		enableC.undebug.bgp.addSC("updates", "BGP updates");
	enableC.undebug.addSC("callback", "Callback activity");
	enableC.undebug.addSC("cdp", "CDP information");
		enableC.undebug.cdp.addSC("adjacency", "CDP neighbor info");
		enableC.undebug.cdp.addSC("events", "CDP events");
		enableC.undebug.cdp.addSC("ip", "CDP ip info");
		enableC.undebug.cdp.addSC("packets", "CDP packet-related information");
	enableC.undebug.addSC("chat", "Chat scripts activity");
		enableC.undebug.chat.addSC("line", "Single TTY line to debug scripts");
	enableC.undebug.addSC("compress", "COMPRESS traffic");
	enableC.undebug.addSC("condition", "Condition");
		enableC.undebug.condition.addSC("<1-1000>", "Condition identifier");
		enableC.undebug.condition.addSC("all", "All conditions");
		enableC.undebug.condition.addSC("called", "called number");
		enableC.undebug.condition.addSC("calling", "calling");
		enableC.undebug.condition.addSC("standby", "interface group");
		enableC.undebug.condition.addSC("username", "username");
	enableC.undebug.addSC("confmodem", "Modem configuration database");
	enableC.undebug.addSC("conn", "Connection Manager information");
	enableC.undebug.addSC("custom-queue", "Custom output queueing");
	enableC.undebug.addSC("dhcp", "DHCP client activity");
		enableC.undebug.dhcp.addSC("detail", "DHCP packet content");
	enableC.undebug.addSC("dialer", "Dial on Demand");
		enableC.undebug.dialer.addSC("events", "Dial on demand events");
		enableC.undebug.dialer.addSC("forwarding", "Dialer forwarding");
		enableC.undebug.dialer.addSC("map", "Dynamic dialer maps");
		enableC.undebug.dialer.addSC("packets", "Dial on demand traffic");
	enableC.undebug.addSC("dnsix", "Dnsix information");
		enableC.undebug.dnsix.addSC("dmdp", "Debug DNSIX/DMDP protocol");
		enableC.undebug.dnsix.addSC("dnssec", "Debug DNSSEC protocol");
		enableC.undebug.dnsix.addSC("nat", "Debug DNSIX/NAT protocol");
	enableC.undebug.addSC("domain", "Domain Name System");
		enableC.undebug.domain.addSC("replies", "DNS replies only");
	enableC.undebug.addSC("dxi", "atm-dxi information");
		enableC.undebug.dxi.addSC("events", "Important atm-dxi events");
		enableC.undebug.dxi.addSC("packet", "ATM DXI packets");
	enableC.undebug.addSC("eigrp", "EIGRP Protocol information");
		enableC.undebug.eigrp.addSC("fsm", "EIGRP Dual Finite State Machine events/actions");
		enableC.undebug.eigrp.addSC("neighbors", "EIGRP neighbors");
		enableC.undebug.eigrp.addSC("packets", "EIGRP packets");
		enableC.undebug.eigrp.addSC("transmit", "EIGRP transmission events");
	enableC.undebug.addSC("entry", "Incoming queue entries");
	enableC.undebug.addSC("ethernet-interface", "Ethernet network interface events");
	enableC.undebug.addSC("fastethernet", "Fast Ethernet interface information");
		enableC.undebug.fastethernet.addSC("events", "Fast Ethernet events");
		enableC.undebug.fastethernet.addSC("packets", "Fast Ethernet packets");
	enableC.undebug.addSC("frame-relay", "Frame Relay");
	enableC.undebug.addSC("interface", "interface");
		enableC.undebug.interface.addSC("Async", "Async interface");
		enableC.undebug.interface.addSC("BVI", "Bridge-Group Virtual Interface");
		enableC.undebug.interface.addSC("CTunnel", "CTunnel interface");
		enableC.undebug.interface.addSC("Dialer", "Dialer interface");
		enableC.undebug.interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
		enableC.undebug.interface.addSC("Group-Async", "Async Group interface");
		enableC.undebug.interface.addSC("Lex", "Lex interface");
		enableC.undebug.interface.addSC("Loopback", "Loopback interface");
		enableC.undebug.interface.addSC("MFR", "Multilink Frame Relay bundle interface");
		enableC.undebug.interface.addSC("Multilink", "Multilink-group interface");
		enableC.undebug.interface.addSC("Null", "Null interface");
		enableC.undebug.interface.addSC("Serial", "Serial");
		enableC.undebug.interface.addSC("Tunnel", "Tunnel interface");
		enableC.undebug.interface.addSC("Vif", "PGM Multicast Host interface");
		enableC.undebug.interface.addSC("Virtual-Template", "Virtual Template interface");
		enableC.undebug.interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
	enableC.undebug.addSC("ip", "IP information");
		enableC.undebug.ip.addSC("bgp", "BGP information");
		enableC.undebug.ip.addSC("cache", "IP cache operations");
		enableC.undebug.ip.addSC("cef", "IP CEF operations");
		enableC.undebug.ip.addSC("cgmp", "CGMP protocol activity");
		enableC.undebug.ip.addSC("dhcp", "Dynamic Host Configuration Protocol");
		enableC.undebug.ip.addSC("dvmrp", "DVMRP protocol activity");
		enableC.undebug.ip.addSC("eigrp", "IP-EIGRP information");
		enableC.undebug.ip.addSC("error", "IP error debugging");
		enableC.undebug.ip.addSC("flow", "IP Flow switching operations");
		enableC.undebug.ip.addSC("ftp", "FTP dialogue");
		enableC.undebug.ip.addSC("html", "HTML connections");
		enableC.undebug.ip.addSC("http", "HTTP connections");
		enableC.undebug.ip.addSC("icmp", "ICMP transactions");
		enableC.undebug.ip.addSC("igmp", "IGMP protocol activity");
		enableC.undebug.ip.addSC("igrp", "IGRP information");
		enableC.undebug.ip.addSC("interface", "IP interface configuration changes");
		enableC.undebug.ip.addSC("mbgp", "MBGP information");
		enableC.undebug.ip.addSC("mcache", "IP multicast cache operations");
		enableC.undebug.ip.addSC("mhbeat", "IP multicast heartbeat monitoring");
		enableC.undebug.ip.addSC("mpacket", "IP multicast packet debugging");
		enableC.undebug.ip.addSC("mrm", "IP Multicast Routing Monitor");
		enableC.undebug.ip.addSC("mrouting", "IP multicast routing table activity");
		enableC.undebug.ip.addSC("msdp", "Multicast Source Discovery Protocol (MSDP)");
		enableC.undebug.ip.addSC("mtag", "IP multicast tagswitching activity");
		enableC.undebug.ip.addSC("nat", "NAT events");
		enableC.undebug.ip.addSC("nbar", "StILE - traffic classification Engine");
		enableC.undebug.ip.addSC("ospf", "OSPF information");
		enableC.undebug.ip.addSC("packet", "General IP debugging and IPSO security transactions");
		enableC.undebug.ip.addSC("peer", "IP peer address activity");
		enableC.undebug.ip.addSC("pgm", "PGM Reliable Transport Protocol");
		enableC.undebug.ip.addSC("pim", "PIM protocol activity");
		enableC.undebug.ip.addSC("policy", "Policy routing");
		enableC.undebug.ip.addSC("rgmp", "RGMP protocol activity");
		enableC.undebug.ip.addSC("rip", "RIP protocol transactions");
		enableC.undebug.ip.addSC("routing", "Routing table events");
		enableC.undebug.ip.addSC("rsvp", "RSVP protocol activity");
		enableC.undebug.ip.addSC("rtp", "RTP information");
		enableC.undebug.ip.addSC("sd", "Session Directory (SD)");
		enableC.undebug.ip.addSC("security", "IP security options");
		enableC.undebug.ip.addSC("socket", "Socket event");
		enableC.undebug.ip.addSC("tcp", "TCP information");
		enableC.undebug.ip.addSC("tempacl", "IP temporary ACL");
		enableC.undebug.ip.addSC("udp", "UDP based transactions");
		enableC.undebug.ip.addSC("urd", "URL RenDezvous (URD)");
		enableC.undebug.ip.addSC("wccp", "WCCP information");
	enableC.undebug.addSC("ipv6", "IPv6 information");
	enableC.undebug.addSC("lapb", "LAPB protocol transactions");
	enableC.undebug.addSC("list", "Set interface or/and access list for the next debug command");
		enableC.undebug.list.addSC("<0-2699>", "access list");
		enableC.undebug.list.addSC("Async", "Async interface");
		enableC.undebug.list.addSC("BVI", "Bridge-Group Virtual Interface");
		enableC.undebug.list.addSC("CTunnel", "CTunnel interface");
		enableC.undebug.list.addSC("Dialer", "Dialer interface");
		enableC.undebug.list.addSC("FastEthernet", "FastEthernet IEEE 802.3");
		enableC.undebug.list.addSC("Group-Async", "Async Group interface");
		enableC.undebug.list.addSC("Lex", "Lex interface");
		enableC.undebug.list.addSC("Loopback", "Loopback interface");
		enableC.undebug.list.addSC("MFR", "Multilink Frame Relay bundle interface");
		enableC.undebug.list.addSC("Multilink", "Multilink-group interface");
		enableC.undebug.list.addSC("Null", "Null interface");
		enableC.undebug.list.addSC("Serial", "Serial");
		enableC.undebug.list.addSC("Tunnel", "Tunnel interface");
		enableC.undebug.list.addSC("Vif", "PGM Multicast Host interface");
		enableC.undebug.list.addSC("Virtual-Template", "Virtual Template interface");
		enableC.undebug.list.addSC("Virtual-TokenRing", "Virtual TokenRing");
	enableC.undebug.addSC("llc2", "LLC2 type II Information");
	enableC.undebug.addSC("modem", "Modem control/process activation");
	enableC.undebug.addSC("nvram", "Debug NVRAM behavior");
	enableC.undebug.addSC("ppp", "PPP (Point to Point Protocol) information");		enableC.undebug.ppp.addSC("authentication", "CHAP and PAP authentication");
		enableC.undebug.ppp.addSC("bap", "BAP protocol transactions");
		enableC.undebug.ppp.addSC("cbcp", "Callback Control Protocol negotiation");
		enableC.undebug.ppp.addSC("error", "Protocol errors and error statistics");
		enableC.undebug.ppp.addSC("events", "Detailed events");
		enableC.undebug.ppp.addSC("forwarding", "PPP layer 2 forwarding");
		enableC.undebug.ppp.addSC("mppe", "MPPE Events");
		enableC.undebug.ppp.addSC("multilink", "Multilink activity");
		enableC.undebug.ppp.addSC("negotiation", "Protocol parameter negotiation");
		enableC.undebug.ppp.addSC("packet", "Low-level PPP packet dump");
		enableC.undebug.ppp.addSC("tasks", "Event Manager");
	enableC.undebug.addSC("priority", "Priority output queueing");
	enableC.undebug.addSC("qdm", "QoS Device Manager");
	enableC.undebug.addSC("radius", "RADIUS protocol");
		enableC.undebug.radius.addSC("accounting", "RADIUS accounting packets only");
		enableC.undebug.radius.addSC("authentication", "RADIUS authentication packets only");
		enableC.undebug.radius.addSC("brief", "Only I/O transactions are recorded");
		enableC.undebug.radius.addSC("failover", "Packets sent upon fail-over");
		enableC.undebug.radius.addSC("retransmit", "Retransmission of packets");
	enableC.undebug.addSC("rif", "RIF cache transactions");
	enableC.undebug.addSC("rtr", "RTR Monitor Information");
		enableC.undebug.rtr.addSC("error", "Output RTR Error Messages");
		enableC.undebug.rtr.addSC("trace", "Trace RTR");
	enableC.undebug.addSC("serial", "Serial interface information");
		enableC.undebug.serial.addSC("event", "Serial network interface event");
		enableC.undebug.serial.addSC("interface", "Serial interface events");
		enableC.undebug.serial.addSC("m32_dma", "Serial M32 DMA");
		enableC.undebug.serial.addSC("mueslix", "Serial Mueslix");
		enableC.undebug.serial.addSC("packet", "Serial network interface packets");
		enableC.undebug.serial.addSC("revive", "Serial Revive");
	enableC.undebug.addSC("smf", "Software MAC filter");
		enableC.undebug.smf.addSC("updates", "address insertions and deletions");
	enableC.undebug.addSC("snapshot", "Snapshot activity");
	enableC.undebug.addSC("snmp", "SNMP information");
		enableC.undebug.snmp.addSC("headers", "SNMP packet headers");
		enableC.undebug.snmp.addSC("packets", "SNMP packets");
		enableC.undebug.snmp.addSC("timers", "SNMP timer activity");
	enableC.undebug.addSC("sntp", "SNTP information");
		enableC.undebug.sntp.addSC("adjust", "SNTP clock adjustments");
		enableC.undebug.sntp.addSC("packets", "SNTP packets");
		enableC.undebug.sntp.addSC("select", "SNTP clock selection");
	enableC.undebug.addSC("standby", "Hot Standby Router Protocol (HSRP)");
		enableC.undebug.standby.addSC("errors", "HSRP errors");
		enableC.undebug.standby.addSC("events", "HSRP events");
		enableC.undebug.standby.addSC("packets", "HSRP packets");
		enableC.undebug.standby.addSC("terse", "Display limited range of HSRP errors, events and packets");
	enableC.undebug.addSC("tacacs", "TACACS authentication and authorization");
		enableC.undebug.tacacs.addSC("accounting", "TACACS+ protocol accounting");
		enableC.undebug.tacacs.addSC("authentication", "TACACS+ protocol authentication");
		enableC.undebug.tacacs.addSC("authorization", "TACACS+ protocol authorization");
		enableC.undebug.tacacs.addSC("events", "TACACS+ protocol events");
		enableC.undebug.tacacs.addSC("packet", "TACACS+ packets");
	enableC.undebug.addSC("telnet", "Incoming telnet connections");
	enableC.undebug.addSC("template", "Template activity");
	enableC.undebug.addSC("tftp", "TFTP debugging");
		enableC.undebug.tftp.addSC("events", "TFTP events");
		enableC.undebug.tftp.addSC("packets", "TFTP packets");
	enableC.undebug.addSC("tunnel", "Generic Tunnel Interface");
	enableC.undebug.addSC("udptn", "UDPtn async data transport");
	enableC.undebug.addSC("vlan", "vLAN information");
		enableC.undebug.vlan.addSC("packets", "vLAN packet information");
	enableC.undebug.addSC("vpdn", "VPDN information");
		enableC.undebug.vpdn.addSC("call", "VPDN call");
		enableC.undebug.vpdn.addSC("error", "VPDN protocol errors");
		enableC.undebug.vpdn.addSC("event", "VPDN event");
		enableC.undebug.vpdn.addSC("l2tp-sequencing", "L2TP sequencing");
		enableC.undebug.vpdn.addSC("l2x-data", "L2F/L2TP data packets");
		enableC.undebug.vpdn.addSC("l2x-errors", "L2F/L2TP protocol errors");
		enableC.undebug.vpdn.addSC("l2x-events", "L2F/L2TP protocol events");
		enableC.undebug.vpdn.addSC("l2x-packets", "L2F/L2TP control packets");
		enableC.undebug.vpdn.addSC("message", "VPDN inter-process message");
		enableC.undebug.vpdn.addSC("packet", "VPDN packet");
		enableC.undebug.vpdn.addSC("pppoe-data", "PPPoE data packets");
		enableC.undebug.vpdn.addSC("pppoe-errors", "PPPoE protocol errors");
		enableC.undebug.vpdn.addSC("pppoe-events", "PPPoE protocol events");
		enableC.undebug.vpdn.addSC("pppoe-packets", "PPPoE control packets");
	enableC.undebug.addSC("vpn", "VPN information");
		enableC.undebug.vpn.addSC("authorization", "VPN authorization information");
	enableC.undebug.addSC("vprofile", "Virtual Profile information");
		enableC.undebug.vprofile.addSC("packet", "Virtual Profile packet");
		enableC.undebug.vprofile.addSC("subblock", "Virtual Profile subblock");
	enableC.undebug.addSC("vtemplate", "Virtual Template information");

enableC.addSC("verify", "Verify a file");
	enableC.verify.addSC("flash:", "File to be verified");
enableC.addSC("where", "List active connections");
enableC.addSC("write", "Write running configuration to memory, network, or terminal");
	enableC.write.addSC("erase", "Erase NV memory");
	enableC.write.addSC("memory", "Write to NV memory");
	enableC.write.addSC("terminal", "Write to terminal");
enableC.addSC("x28", "Become an X.28 PAD");
enableC.addSC("x3", "Set X.3 parameters on PAD");