
subintFC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	subintFC.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
	subintFC.arp.addSC("timeout", "Set ARP cache timeout");
		subintFC.arp.timeout.addSC("<0-2147483>", "Seconds");
subintFC.addSC("backup", "Modify backup parameters");
	subintFC.backup.addSC("delay", "Delays before backup line up or down transitions");
		subintFC.backup.delay.addSC("<0-4294967294>", "Seconds");
	subintFC.backup.addSC("interface", "Configure an interface as a backup");
		subintFC.backup.interface.addSC("Async", "Async interface");
			subintFC.backup.interface.Async.addSC("<1-5>", "Async interface number");
		subintFC.backup.interface.addSC("BVI", "Bridge-Group Virtual Interface");
			subintFC.backup.interface.BVI.addSC("<1-255>", "BVI interface number");
		subintFC.backup.interface.addSC("CTunnel", "CTunnel interface");
			subintFC.backup.interface.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
		subintFC.backup.interface.addSC("Dialer", "Dialer interface");
			subintFC.backup.interface.Dialer.addSC("<0-255>", "Dialer interface number");
		subintFC.backup.interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
			subintFC.backup.interface.FastEthernet.addSC("<0-0>", "FastEthernet interface number");
		subintFC.backup.interface.addSC("Group-Async", "Async Group interface");
			subintFC.backup.interface["Group-Async"].addSC("<0-5>", "Group-Async interface number");
		subintFC.backup.interface.addSC("Lex", "Lex interface");
			subintFC.backup.interface.Lex.addSC("<0-2147483647>", "Lex interface number");
		subintFC.backup.interface.addSC("Loopback", "Loopback interface");
			subintFC.backup.interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
		subintFC.backup.interface.addSC("MFR", "Multilink Frame Relay bundle interface");
			subintFC.backup.interface.MFR.addSC("<0-2147483647>", "MFR interface number");
		subintFC.backup.interface.addSC("Multilink", "Multilink-group interface");
			subintFC.backup.interface.Multilink.addSC("<1-2147483647>", "Multilink interface number");
		subintFC.backup.interface.addSC("Null", "Null interface");
			subintFC.backup.interface.Null.addSC("<0-0>", "Null interface number");
		subintFC.backup.interface.addSC("Serial", "Serial");
			subintFC.backup.interface.Serial.addSC("<0-1>", "Serial interface number");
		subintFC.backup.interface.addSC("Tunnel", "Tunnel interface");
			subintFC.backup.interface.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
		subintFC.backup.interface.addSC("Vif", "PGM Multicast Host interface");
			subintFC.backup.interface.Vif.addSC("<1-1>", "Vif interface number");
		subintFC.backup.interface.addSC("Virtual-Template", "Virtual Template interface");
			subintFC.backup.interface["Virtual-Template"].addSC("<1-200>", "Virtual-Template interface number");
		subintFC.backup.interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
			subintFC.backup.interface["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
subintFC.addSC("bandwidth", "Set bandwidth informational parameter");
	subintFC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
subintFC.addSC("bridge-group", "Transparent bridging interface parameters");
	subintFC["bridge-group"].addSC("<1-255>", "Assign an interface to a Bridge Group.");
		subintFC["bridge-group"]["<1-255>"].addSC("input-address-list", "Filter packets by source address");
			subintFC["bridge-group"]["<1-255>"]["input-address-list"].addSC("<700-799>", "Ethernet address access list");
		subintFC["bridge-group"]["<1-255>"].addSC("input-lat-service-deny", "Deny input LAT service advertisements matching a group list");
			subintFC["bridge-group"]["<1-255>"]["input-lat-service-deny"].addSC("<grouplist>", "A list of LAT service advertisements");
			subintFC["bridge-group"]["<1-255>"]["input-lat-service-deny"].addSC("all", "All LAT groups");
				subintFC["bridge-group"]["<1-255>"]["input-lat-service-deny"].all.addSC("disabled", "Remove from existing group code list");
				subintFC["bridge-group"]["<1-255>"]["input-lat-service-deny"].all.addSC("enabled", "Add to existing group code list");
		subintFC["bridge-group"]["<1-255>"].addSC("input-lat-service-permit", "Permit input LAT service advertisements matching a group list");
			subintFC["bridge-group"]["<1-255>"]["input-lat-service-permit"].addSC("<grouplist>", "A list of LAT service advertisements");
			subintFC["bridge-group"]["<1-255>"]["input-lat-service-permit"].addSC("all", "All LAT groups");
				subintFC["bridge-group"]["<1-255>"]["input-lat-service-permit"].all.addSC("disabled", "Remove from existing group code list");
				subintFC["bridge-group"]["<1-255>"]["input-lat-service-permit"].all.addSC("enabled", "Add to existing group code list");
		subintFC["bridge-group"]["<1-255>"].addSC("input-lsap-list", "Filter incoming IEEE 802.3 encapsulated packets");
			subintFC["bridge-group"]["<1-255>"]["input-lsap-list"].addSC("<200-299>", "Ethernet type access list");
		subintFC["bridge-group"]["<1-255>"].addSC("input-pattern-list", "Filter input with a pattern list");
			subintFC["bridge-group"]["<1-255>"]["input-pattern-list"].addSC("<1100-1199>", "Pattern access list number");
		subintFC["bridge-group"]["<1-255>"].addSC("input-type-list", "Filter incoming Ethernet packets by type code");
			subintFC["bridge-group"]["<1-255>"]["input-type-list"].addSC("<200-299>", "Ethernet type access list");
		subintFC["bridge-group"]["<1-255>"].addSC("lat-compression", "Enable LAT compression over serial or ATM interfaces");
		subintFC["bridge-group"]["<1-255>"].addSC("output-address-list", "Filter packets by destination address");
			subintFC["bridge-group"]["<1-255>"]["output-address-list"].addSC("<700-799>", "Ethernet address access list");
		subintFC["bridge-group"]["<1-255>"].addSC("output-lat-service-deny", "Deny output LAT service advertisements matching a group list");
			subintFC["bridge-group"]["<1-255>"]["output-lat-service-deny"].addSC("<grouplist>", "A list of LAT service advertisements");
			subintFC["bridge-group"]["<1-255>"]["output-lat-service-deny"].addSC("all", "All LAT groups");
				subintFC["bridge-group"]["<1-255>"]["output-lat-service-deny"].all.addSC("disabled", "Remove from existing group code list");
				subintFC["bridge-group"]["<1-255>"]["output-lat-service-deny"].all.addSC("enabled", "Add to existing group code list");
		subintFC["bridge-group"]["<1-255>"].addSC("output-lat-service-permit", "Permit output LAT service advertisements matching a group list");
			subintFC["bridge-group"]["<1-255>"]["output-lat-service-permit"].addSC("<grouplist>", "A list of LAT service advertisements");
			subintFC["bridge-group"]["<1-255>"]["output-lat-service-permit"].addSC("all", "All LAT groups");
				subintFC["bridge-group"]["<1-255>"]["output-lat-service-permit"].all.addSC("disabled", "Remove from existing group code list");
				subintFC["bridge-group"]["<1-255>"]["output-lat-service-permit"].all.addSC("enabled", "Add to existing group code list");
		subintFC["bridge-group"]["<1-255>"].addSC("output-lsap-list", "Filter outgoing IEEE 802.3 encapsulated packets");
			subintFC["bridge-group"]["<1-255>"]["output-lsap-list"].addSC("<200-299>", "Ethernet type access list");
		subintFC["bridge-group"]["<1-255>"].addSC("output-pattern-list", "Filter output with a pattern list");
			subintFC["bridge-group"]["<1-255>"]["output-pattern-list"].addSC("<1100-1199>", "Pattern access list number");
		subintFC["bridge-group"]["<1-255>"].addSC("output-type-list", "Filter outgoing Ethernet packets by type code");
			subintFC["bridge-group"]["<1-255>"]["output-type-list"].addSC("<200-299>", "Ethernet type access list");
		subintFC["bridge-group"]["<1-255>"].addSC("path-cost", "Set interface path cost");
			subintFC["bridge-group"]["<1-255>"]["path-cost"].addSC("<0-65535>", "Path cost (higher values are higher costs)");
		subintFC["bridge-group"]["<1-255>"].addSC("priority", "Set interface priority");
			subintFC["bridge-group"]["<1-255>"].priority.addSC("<0-255>", "");
		subintFC["bridge-group"]["<1-255>"].addSC("spanning-disabled", "Disable spanning tree on a bridge group");
		subintFC["bridge-group"]["<1-255>"].addSC("subscriber-loop-control", "Configure subscriber loop control");
subintFC.addSC("cdp", "CDP interface subcommands");
	subintFC.cdp.addSC("enable", "Enable CDP on interface");
subintFC.addSC("default", "Set a command to its defaults");
	subintFC["default"].addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
		subintFC["default"].arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
		subintFC["default"].arp.addSC("timeout", "Set ARP cache timeout");
	subintFC["default"].addSC("backup", "Modify backup parameters");
		subintFC["default"].backup.addSC("delay", "Delays before backup line up or down transitions");
		subintFC["default"].backup.addSC("interface", "Configure an interface as a backup");
	subintFC["default"].addSC("bandwidth", "Set bandwidth informational parameter");
	subintFC["default"].addSC("bridge-group", "Transparent bridging interface parameters");
		subintFC["default"]["bridge-group"].addSC("<1-255>", "Assign an interface to a Bridge Group.");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("input-address-list", "Filter packets by source address");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("input-lat-service-deny", "Deny input LAT service advertisements matching a group list");
				subintFC["default"]["bridge-group"]["<1-255>"]["input-lat-service-deny"].addSC("<grouplist>", "A list of LAT service advertisements");
				subintFC["default"]["bridge-group"]["<1-255>"]["input-lat-service-deny"].addSC("all", "All LAT groups");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("input-lat-service-permit", "Permit input LAT service advertisements matching a group list");
				subintFC["default"]["bridge-group"]["<1-255>"]["input-lat-service-permit"].addSC("<grouplist>", "A list of LAT service advertisements");
				subintFC["default"]["bridge-group"]["<1-255>"]["input-lat-service-permit"].addSC("all", "All LAT groups");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("input-lsap-list", "Filter incoming IEEE 802.3 encapsulated packets");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("input-pattern-list", "Filter input with a pattern list");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("input-type-list", "Filter incoming Ethernet packets by type code");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("lat-compression", "Enable LAT compression over serial or ATM interfaces");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("output-address-list", "Filter packets by destination address");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("output-lat-service-deny", "Deny output LAT service advertisements matching a group list");
				subintFC["default"]["bridge-group"]["<1-255>"]["output-lat-service-deny"].addSC("<grouplist>", "A list of LAT service advertisements");
				subintFC["default"]["bridge-group"]["<1-255>"]["output-lat-service-deny"].addSC("all", "All LAT groups");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("output-lat-service-permit", "Permit output LAT service advertisements matching a group list");
				subintFC["default"]["bridge-group"]["<1-255>"]["output-lat-service-permit"].addSC("<grouplist>", "A list of LAT service advertisements");
				subintFC["default"]["bridge-group"]["<1-255>"]["output-lat-service-permit"].addSC("all", "All LAT groups");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("output-lsap-list", "Filter outgoing IEEE 802.3 encapsulated packets");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("output-pattern-list", "Filter output with a pattern list");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("output-type-list", "Filter outgoing Ethernet packets by type code");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("path-cost", "Set interface path cost");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("priority", "Set interface priority");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("spanning-disabled", "Disable spanning tree on a bridge group");
			subintFC["default"]["bridge-group"]["<1-255>"].addSC("subscriber-loop-control", "Configure subscriber loop control");
	subintFC["default"].addSC("cdp", "CDP interface subcommands");
		subintFC["default"].cdp.addSC("enable", "Enable CDP on interface");
subintFC.addSC("delay", "Specify interface throughput delay");
	subintFC.delay.addSC("<1-16777215>", "Throughput delay (tens of microseconds)");
subintFC.addSC("description", "Interface specific description");
	subintFC.description.addSC("LINE", "Up to 240 characters describing this interface");
subintFC.addSC("encapsulation", "Set encapsulation type for an interface");
	subintFC.encapsulation.addSC("dot1Q", "IEEE 802.1Q Virtual LAN");
		subintFC.encapsulation.dot1Q.addSC("<1-4095>", "IEEE 802.1Q VLAN ID required, range 1 - 0xFFF.");
			subintFC.encapsulation.dot1Q["<1-4095>"].addSC("native", "Make this as native vlan");
subintFC.addSC("exit", "Exit from interface configuration mode");
subintFC.addSC("ip", "Interface Internet Protocol config commands");
	subintFC.ip.addSC("access-group", "Specify access control for packets");
		subintFC.ip["access-group"].addSC("<1-199>", "IP access list (standard or extended)");
			subintFC.ip["access-group"]["<1-199>"].addSC("in", "inbound packets");
			subintFC.ip["access-group"]["<1-199>"].addSC("out", "outbound packets");
		subintFC.ip["access-group"].addSC("<1300-2699>", "IP expanded access list (standard or extended)");
			subintFC.ip["access-group"]["<1300-2699>"].addSC("in", "inbound packets");
			subintFC.ip["access-group"]["<1300-2699>"].addSC("out", "outbound packets");
		subintFC.ip["access-group"].addSC("WORD", "Access-list name");
			subintFC.ip["access-group"].WORD.addSC("in", "inbound packets");
			subintFC.ip["access-group"].WORD.addSC("out", "outbound packets");
	subintFC.ip.addSC("accounting", "Enable IP accounting on this interface");
		subintFC.ip.accounting.addSC("access-violations", "Account for IP packets violating access lists on this interface");
		subintFC.ip.accounting.addSC("mac-address", "Account for MAC addresses seen on this interface");
			subintFC.ip.accounting["mac-address"].addSC("input", "Source MAC address on received packets");
			subintFC.ip.accounting["mac-address"].addSC("output", "Destination MAC address on transmitted packets");
		subintFC.ip.accounting.addSC("output-packets", "Account for IP packets output on this interface");
		subintFC.ip.accounting.addSC("precedence", "Count packets by IP precedence on this interface");
			subintFC.ip.accounting.precedence.addSC("input", "received packets");
			subintFC.ip.accounting.precedence.addSC("output", "transmitted packets");
	subintFC.ip.addSC("address", "Set the IP address of an interface");
		subintFC.ip.address.addSC("A.B.C.D", "IP address");
			subintFC.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
				subintFC.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
		subintFC.ip.address.addSC("dhcp", "IP Address negotiated via DHCP");
			subintFC.ip.address.dhcp.addSC("client-id", "Specify client-id to use");
				subintFC.ip.address.dhcp["client-id"].addSC("FastEthernet", "FastEthernet IEEE 802.3");
					subintFC.ip.address.dhcp["client-id"].FastEthernet.addSC("<0-0>", "FastEthernet interface number");
	subintFC.ip.addSC("authentication", "authentication subcommands");
		subintFC.ip.authentication.addSC("key-chain", "key-chain");
			subintFC.ip.authentication["key-chain"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				subintFC.ip.authentication["key-chain"].eigrp.addSC("<1-65535>", "Autonomous system number");
					subintFC.ip.authentication["key-chain"].eigrp["<1-65535>"].addSC("LINE", "name of key-chain");
		subintFC.ip.authentication.addSC("mode", "mode");
			subintFC.ip.authentication.mode.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				subintFC.ip.authentication.mode.eigrp.addSC("<1-65535>", "Autonomous system number");
					subintFC.ip.authentication.mode.eigrp["<1-65535>"].addSC("md5", "Keyed message digest");
	subintFC.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
		subintFC.ip["bandwidth-percent"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			subintFC.ip["bandwidth-percent"].eigrp.addSC("<1-65535>", "Autonomous system number");
				subintFC.ip["bandwidth-percent"].eigrp["<1-65535>"].addSC("<1-999999>", "Maximum bandwidth percentage that EIGRP may use");
	subintFC.ip.addSC("bgp", "BGP interface commands");
	subintFC.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		subintFC.ip["broadcast-address"].addSC("A.B.C.D", "IP broadcast address");
	subintFC.ip.addSC("cef", "Cisco Express Fowarding interface commands");
		subintFC.ip.cef.addSC("accounting", "CEF accounting features for interface");
			subintFC.ip.cef.accounting.addSC("non-recursive", "CEF non-recursive accounting features");
				subintFC.ip.cef.accounting["non-recursive"].addSC("external", "Count input traffic in non-recursive external bin");
				subintFC.ip.cef.accounting["non-recursive"].addSC("internal", "Count input traffic in non-recursive internal bin");
	subintFC.ip.addSC("cgmp", "Enable/disable CGMP");
		subintFC.ip.cgmp.addSC("proxy", "CGMP for hosts and proxy for multicast routers");
		subintFC.ip.cgmp.addSC("router-only", "CGMP proxy for multicast routers only");
	subintFC.ip.addSC("dhcp", "Configure DHCP parameters for this interface");
		subintFC.ip.dhcp.addSC("relay", "DHCP relay configuration parameters");
			subintFC.ip.dhcp.relay.addSC("information", "DHCP relay information option");
				subintFC.ip.dhcp.relay.information.addSC("trusted", "Received DHCP packet may contain relay info option with zero giaddr");
	subintFC.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
		subintFC.ip["directed-broadcast"].addSC("<1-199>", "A standard IP access list number");
		subintFC.ip["directed-broadcast"].addSC("<1300-2699>", "A standard IP expanded access list number");
	subintFC.ip.addSC("dvmrp", "DVMRP interface commands");
	subintFC.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
		subintFC.ip["hello-interval"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			subintFC.ip["hello-interval"].eigrp.addSC("<1-65535>", "Autonomous system number");
				subintFC.ip["hello-interval"].eigrp["<1-65535>"].addSC("<1-65535>", "Seconds between hello transmissions");
	subintFC.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
		subintFC.ip["helper-address"].addSC("A.B.C.D", "IP destination address");
		subintFC.ip["helper-address"].addSC("global", "Helper-address is global");
			subintFC.ip["helper-address"].global.addSC("A.B.C.D", "IP destination address");
		subintFC.ip["helper-address"].addSC("vrf", "VRF name for helper-address (if different from interface VRF)");
			subintFC.ip["helper-address"].vrf.addSC("WORD", "VPN Routing/Forwarding instance name");
				subintFC.ip["helper-address"].vrf.WORD.addSC("A.B.C.D", "IP destination address");
	subintFC.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
	subintFC.ip.addSC("idle-group", "Specify interesting packets for idle-timer");
	subintFC.ip.addSC("igmp", "IGMP interface commands");
	subintFC.ip.addSC("irdp", "ICMP Router Discovery Protocol");
	subintFC.ip.addSC("load-sharing", "Style of load sharing");
		subintFC.ip["load-sharing"].addSC("per-destination", "Deterministic distribution");
		subintFC.ip["load-sharing"].addSC("per-packet", "Random distribution");
	subintFC.ip.addSC("local-proxy-arp", "Enable local-proxy ARP");
	subintFC.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
	subintFC.ip.addSC("mrm", "Configure IP Multicast Routing Monitor tester");
		subintFC.ip.mrm.addSC("test-receiver", "Enable IP MRM test receiver operation");
		subintFC.ip.mrm.addSC("test-sender", "Enable IP MRM test sender operation");
		subintFC.ip.mrm.addSC("test-sender-receiver", "Enable IP MRM test sender and receiver operation");
	subintFC.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
	subintFC.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		subintFC.ip.mtu.addSC("<68-1000000>", "MTU (bytes)");
	subintFC.ip.addSC("multicast", "IP multicast interface commands");
		subintFC.ip.multicast.addSC("tagswitch", "Enable IP Multicast Tagswitching");
		subintFC.ip.multicast.addSC("ttl-threshold", "TTL threshold for multicast packets");
			subintFC.ip.multicast["ttl-threshold"].addSC("<0-255>", "TTL threshold");
	subintFC.ip.addSC("nat", "NAT interface commands");
		subintFC.ip.nat.addSC("inside", "Inside interface for address translation");
		subintFC.ip.nat.addSC("outside", "Outside interface for address translation");
	subintFC.ip.addSC("nbar", "Network-Based Application Recognition");
		subintFC.ip.nbar.addSC("protocol-discovery", "Enable NBAR protocol discovery");
	subintFC.ip.addSC("nhrp", "NHRP interface subcommands");
	subintFC.ip.addSC("ospf", "OSPF interface commands");
	subintFC.ip.addSC("pgm", "PGM Reliable Transport Protocol");
		subintFC.ip.pgm.addSC("router", "router specific command");
	subintFC.ip.addSC("pim", "PIM interface commands");
	subintFC.ip.addSC("policy", "Enable policy routing");
		subintFC.ip.policy.addSC("route-map", "Policy route map");
			subintFC.ip.policy["route-map"].addSC("WORD", "Route map name");
	subintFC.ip.addSC("probe", "Enable HP Probe support");
		subintFC.ip.probe.addSC("proxy", "Proxy support");
	subintFC.ip.addSC("proxy-arp", "Enable proxy ARP");
	subintFC.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
		subintFC.ip["rarp-server"].addSC("A.B.C.D", "IP server address");
	subintFC.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
	subintFC.ip.addSC("rgmp", "Enable/disable RGMP");
	subintFC.ip.addSC("rip", "Router Information Protocol");
	subintFC.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
		subintFC.ip["route-cache"].addSC("same-interface", "Enable fast-switching on the same interface");
	subintFC.ip.addSC("rsvp", "RSVP interface commands");
	subintFC.ip.addSC("sap", "Session Announcement Protocol interface commands");
		subintFC.ip.sap.addSC("listen", "Listen for sap packets on interface");
	subintFC.ip.addSC("security", "DDN IP Security Option");
	subintFC.ip.addSC("split-horizon", "Perform split horizon");
	subintFC.ip.addSC("summary-address", "Perform address summarization");
      subintFC.ip["summary-address"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
         subintFC.ip["summary-address"].eigrp.addSC("<1-65535>", "Autonomous system number");
            subintFC.ip["summary-address"].eigrp["<1-65535>"].addSC("A.B.C.D", "IP address");
               subintFC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"].addSC("A.B.C.D", "IP network mask");
                  subintFC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"]["A.B.C.D"].addSC("<1-255>", "Administrative distance");
      subintFC.ip["summary-address"].addSC("rip", "Routing Information Protocol (RIP)");
         subintFC.ip["summary-address"].rip.addSC("A.B.C.D", "IP address");
            subintFC.ip["summary-address"].rip["A.B.C.D"].addSC("A.B.C.D", "IP network mask");

	subintFC.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
	subintFC.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
	subintFC.ip.addSC("urd", "Configure URL Rendezvousing");
		subintFC.ip.urd.addSC("proxy", "Enable IP URD proxy service");
	subintFC.ip.addSC("verify", "Enable per packet validation");
	subintFC.ip.addSC("vrf", "VPN Routing/Forwarding parameters on the interface");
	subintFC.ip.addSC("wccp", "WCCP interface commands");
subintFC.addSC("ipv6", "IPv6 interface subcommands");
subintFC.addSC("llc2", "LLC2 Interface Subcommands");
subintFC.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
	subintFC.mtu.addSC("<64-18000>", "MTU size in bytes");
subintFC.addSC("netbios", "Use a defined NETBIOS access list or enable name-caching");
subintFC.addSC("no", "Negate a command or set its defaults");
	subintFC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
		subintFC.no.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
		subintFC.no.arp.addSC("timeout", "Set ARP cache timeout");
	subintFC.no.addSC("backup", "Modify backup parameters");
		subintFC.no.backup.addSC("delay", "Delays before backup line up or down transitions");
		subintFC.no.backup.addSC("interface", "Configure an interface as a backup");
	subintFC.no.addSC("bandwidth", "Set bandwidth informational parameter");
	subintFC.no.addSC("bridge-group", "Transparent bridging interface parameters");
		subintFC.no["bridge-group"].addSC("<1-255>", "Assign an interface to a Bridge Group.");
	subintFC.no.addSC("cdp", "CDP interface subcommands");
		subintFC.no.cdp.addSC("enable", "Enable CDP on interface");
	subintFC.no.addSC("delay", "Specify interface throughput delay");
	subintFC.no.addSC("description", "Interface specific description");
	subintFC.no.addSC("encapsulation", "Set encapsulation type for an interface");
	subintFC.no.addSC("ip", "Interface Internet Protocol config commands");
	subintFC.no.addSC("ipv6", "IPv6 interface subcommands");
	subintFC.no.addSC("llc2", "LLC2 Interface Subcommands");
	subintFC.no.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
	subintFC.no.addSC("netbios", "Use a defined NETBIOS access list or enable name-caching");
subintFC.addSC("ntp", "Configure NTP");
subintFC.addSC("pppoe", "pppoe interface subcommands");
	subintFC.pppoe.addSC("enable", "Enable pppoe");
	subintFC.pppoe.addSC("max-sessions", "Maximum PPPOE sessions");
		subintFC.pppoe["max-sessions"].addSC("<1-292>", "Maximum PPPOE sessions");
subintFC.addSC("rate-limit", "Rate Limit");
subintFC.addSC("service-policy", "Configure QoS Service Policy");
subintFC.addSC("shutdown", "Shutdown the selected interface");
subintFC.addSC("snapshot", "Configure snapshot support on the interface");
subintFC.addSC("standby", "HSRP interface configuration commands");
subintFC.addSC("timeout", "Define timeout values for this interface");
subintFC.addSC("traffic-shape", "Enable Traffic Shaping on an Interface or Sub-Interface");
