
routerIGRPC.addSC("default", "Set a command to its defaults");
routerIGRPC.addSC("default-information", "Control distribution of default information");
routerIGRPC.addSC("default-metric", "Set metric of redistributed routes");
routerIGRPC.addSC("distance", "Define an administrative distance");
routerIGRPC.addSC("distribute-list", "Filter networks in routing updates");
routerIGRPC.addSC("exit", "Exit from routing protocol configuration mode");
routerIGRPC.addSC("help", "Description of the interactive help system");
routerIGRPC.addSC("maximum-paths", "");
routerIGRPC.addSC("metric", "Modify IGRP routing metrics and parameters");
routerIGRPC.addSC("neighbor", "Specify a neighbor router");
routerIGRPC.addSC("network", "Enable routing on an IP network");
	routerIGRPC.network.addSC("A.B.C.D", "Network number");
routerIGRPC.addSC("no", "Negate a command or set its defaults");
	routerIGRPC.no.addSC("default-information", "Control distribution of default information");
	routerIGRPC.no.addSC("default-metric", "Set metric of redistributed routes");
	routerIGRPC.no.addSC("distance", "Define an administrative distance");
	routerIGRPC.no.addSC("distribute-list", "Filter networks in routing updates");
	routerIGRPC.no.addSC("maximum-paths", "Forward packets over multiple paths");
	routerIGRPC.no.addSC("metric", "Modify IGRP routing metrics and parameters");
	routerIGRPC.no.addSC("neighbor", "Specify a neighbor router");
	routerIGRPC.no.addSC("network", "Enable routing on an IP network");
routerIGRPC.addSC("offset-list", "Add or subtract offset from IGRP or RIP metrics");
routerIGRPC.addSC("passive-interface", "Suppress routing updates on an interface");
	routerIGRPC["passive-interface"].addSC("Async", "Async interface");
	routerIGRPC["passive-interface"].addSC("Dialer", "Dialer interface");
	routerIGRPC["passive-interface"].addSC("FastEthernet", "FastEthernet IEEE 802.3");
	routerIGRPC["passive-interface"].addSC("Loopback", "Loopback interface");
	routerIGRPC["passive-interface"].addSC("Null", "Null interface");
	routerIGRPC["passive-interface"].addSC("Serial", "Serial");
	routerIGRPC["passive-interface"].addSC("default", "Suppress routing updates on all interfaces");
routerIGRPC.addSC("redistribute", "Redistribute information from another routing protocol");
routerIGRPC.addSC("timers", "Adjust routing timers");
routerIGRPC.addSC("validate-update-source", "Perform sanity checks against source address of routing updates");
routerIGRPC.addSC("variance", "Control load balancing variance");
