intLoopBackC.addSC("access-expression", "Build a bridge boolean access expression");
	intLoopBackC["access-expression"].addSC("input", "Filter input packets");
		intLoopBackC["access-expression"].input.addSC("LINE", "A boolean expression of bridge access lists");
	intLoopBackC["access-expression"].addSC("output", "Filter output packets");
		intLoopBackC["access-expression"].output.addSC("LINE", "A boolean expression of bridge access lists");
intLoopBackC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	intLoopBackC.arp.addSC("arpa", "Standard arp protocol");
	intLoopBackC.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
	intLoopBackC.arp.addSC("probe", "HP style arp protocol");
	intLoopBackC.arp.addSC("snap", "IEEE 802.3 style arp");
	intLoopBackC.arp.addSC("timeout", "Set ARP cache timeout");
		intLoopBackC.arp.timeout.addSC("<0-2147483>", "Seconds");
intLoopBackC.addSC("bandwidth", "Set bandwidth informational parameter");
	intLoopBackC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
intLoopBackC.addSC("bridge-group", "Transparent bridging interface parameters");
	intLoopBackC["bridge-group"].addSC("<1-255>", "Assign an interface to a Bridge Group.");

intLoopBackC.addSC("cdp", "CDP interface subcommands");
	intLoopBackC.cdp.addSC("enable", "Enable CDP on interface");
intLoopBackC.addSC("description", "Interface specific description");
	intLoopBackC.description.addSC("LINE", "Up to 240 characters describing this interface");

intLoopBackC.addSC("default", "Set a command to its defaults");
intLoopBackC.addSC("delay", "Specify interface throughput delay");
	intLoopBackC.delay.addSC("<1-16777215>", "Throughput delay (tens of microseconds)");
intLoopBackC.addSC("description", "Interface specific description");
	intLoopBackC.description.addSC("LINE", "Up to 240 characters describing this interface");

intLoopBackC.addSC("exit", "Exit from interface configuration mode");
intLoopBackC.addSC("help", "Description of the interactive help system");


intLoopBackC.addSC("hold-queue", "Set hold queue depth");
	intLoopBackC["hold-queue"].addSC("<0-4096>", "Queue length");
		intLoopBackC["hold-queue"]["<0-4096>"].addSC("in", "Input queue");
		intLoopBackC["hold-queue"]["<0-4096>"].addSC("out", "Output queue");
intLoopBackC.addSC("ip", "Interface Internet Protocol config commands");
	intLoopBackC.ip.addSC("access-group", "Specify access control for packets");
		intLoopBackC.ip["access-group"].addSC("<1-199>", "IP access list (standard or extended)");
			intLoopBackC.ip["access-group"]["<1-199>"].addSC("in", "inbound packets");
			intLoopBackC.ip["access-group"]["<1-199>"].addSC("out", "outbound packets");
		intLoopBackC.ip["access-group"].addSC("<1300-2699>", "IP expanded access list (standard or extended)");
			intLoopBackC.ip["access-group"]["<1300-2699>"].addSC("in", "inbound packets");
			intLoopBackC.ip["access-group"]["<1300-2699>"].addSC("out", "outbound packets");
		intLoopBackC.ip["access-group"].addSC("WORD", "Access-list name");
			intLoopBackC.ip["access-group"].WORD.addSC("in", "inbound packets");
			intLoopBackC.ip["access-group"].WORD.addSC("out", "outbound packets");
	intLoopBackC.ip.addSC("address", "Set the IP address of an interface");
		intLoopBackC.ip.address.addSC("A.B.C.D", "IP address");
			intLoopBackC.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
				intLoopBackC.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
	intLoopBackC.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		intLoopBackC.ip["broadcast-address"].addSC("A.B.C.D", "IP broadcast address");
	intLoopBackC.ip.addSC("cgmp", "Enable/disable CGMP");
		intLoopBackC.ip.cgmp.addSC("proxy", "CGMP for hosts and proxy for multicast routers");
		intLoopBackC.ip.cgmp.addSC("router-only", "CGMP proxy for multicast routers only");
	intLoopBackC.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
		intLoopBackC.ip["hello-interval"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			intLoopBackC.ip["hello-interval"].eigrp.addSC("<1-65535>", "Autonomous system number");
				intLoopBackC.ip["hello-interval"].eigrp["<1-65535>"].addSC("<1-65535>", "Seconds between hello transmissions");
	intLoopBackC.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		intLoopBackC.ip.mtu.addSC("<68-1000000>", "MTU (bytes)");

	intLoopBackC.ip.addSC("multicast", "IP multicast interface commands");
		intLoopBackC.ip.multicast.addSC("boundary", "Boundary for administratively scoped multicast addresses");
			intLoopBackC.ip.multicast.boundary.addSC("<1-99>", "Access-list number");
			intLoopBackC.ip.multicast.boundary.addSC("<1300-1999>", "<access-list> (expanded range)");
			intLoopBackC.ip.multicast.boundary.addSC("WORD", "IP Named Standard Access list");
		intLoopBackC.ip.multicast.addSC("helper-map", "Broadcast to Multicast map OR Multicast to Broadcast map");
			intLoopBackC.ip.multicast["helper-map"].addSC("A.B.C.D", "IP multicast address");
				intLoopBackC.ip.multicast["helper-map"]["A.B.C.D"].addSC("A.B.C.D", "IP multicast address or IP broadcast address");
			intLoopBackC.ip.multicast["helper-map"].addSC("broadcast", "Broadcast address");
				intLoopBackC.ip.multicast["helper-map"].broadcast.addSC("A.B.C.D", "IP multicast address or IP broadcast address");
		intLoopBackC.ip.multicast.addSC("rate-limit", "Rate limit multicast data packets");
			intLoopBackC.ip.multicast["rate-limit"].addSC("in", "Rate limit incoming packets");
			intLoopBackC.ip.multicast["rate-limit"].addSC("out", "Rate limit outgoing packets");
		intLoopBackC.ip.multicast.addSC("ttl-threshold", "TTL threshold for multicast packets");
			intLoopBackC.ip.multicast["ttl-threshold"].addSC("<0-255>", "TTL threshold");

	intLoopBackC.ip.addSC("ospf", "OSPF interface commands");
		intLoopBackC.ip.ospf.addSC("authentication", "Enable authentication");
			intLoopBackC.ip.ospf.authentication.addSC("message-digest", "Use message-digest authentication");
			intLoopBackC.ip.ospf.authentication.addSC("null", "Use no authentication");
		intLoopBackC.ip.ospf.addSC("authentication-key", "Authentication password (key)");
			intLoopBackC.ip.ospf["authentication-key"].addSC("<0-7>", "Encryption type (0 for not yet encrypted, 7 for proprietary)");
			intLoopBackC.ip.ospf["authentication-key"].addSC("LINE", "The OSPF password (key)");
		intLoopBackC.ip.ospf.addSC("cost", "Interface cost");
			intLoopBackC.ip.ospf.cost.addSC("<1-65535>", "Cost");
		intLoopBackC.ip.ospf.addSC("database-filter", "Filter OSPF LSA during synchronization and flooding");
			intLoopBackC.ip.ospf["database-filter"].addSC("all", "Filter all LSA");
				intLoopBackC.ip.ospf["database-filter"].all.addSC("out", "Outgoing LSA");
		intLoopBackC.ip.ospf.addSC("dead-interval", "Interval after which a neighbor is declared dead");
			intLoopBackC.ip.ospf["dead-interval"].addSC("<1-65535>", "Seconds");
		intLoopBackC.ip.ospf.addSC("demand-circuit", "OSPF demand circuit");
		intLoopBackC.ip.ospf.addSC("hello-interval", "Time between HELLO packets");
			intLoopBackC.ip.ospf["hello-interval"].addSC("<1-65535>", "Seconds");
		intLoopBackC.ip.ospf.addSC("message-digest-key", "Message digest authentication password (key)");
			intLoopBackC.ip.ospf["message-digest-key"].addSC("<1-255>", "Key ID");
				intLoopBackC.ip.ospf["message-digest-key"]["<1-255>"].addSC("md5", "Use MD5 algorithm");
		intLoopBackC.ip.ospf.addSC("mtu-ignore", "Ignores the MTU in DBD packets");
		intLoopBackC.ip.ospf.addSC("network", "Network type");
			intLoopBackC.ip.ospf.network.addSC("broadcast", "Specify OSPF broadcast multi-access network");
			intLoopBackC.ip.ospf.network.addSC("non-broadcast", "Specify OSPF NBMA network");
			intLoopBackC.ip.ospf.network.addSC("point-to-multipoint", "Specify OSPF point-to-multipoint network");
				intLoopBackC.ip.ospf.network["point-to-multipoint"].addSC("non-broadcast", "Specify non-broadcast point-to-mpoint network");
			intLoopBackC.ip.ospf.network.addSC("point-to-point", "Specify OSPF point-to-point network");
		intLoopBackC.ip.ospf.addSC("priority", "Router priority");
			intLoopBackC.ip.ospf.priority.addSC("<0-255>", "Priority");
		intLoopBackC.ip.ospf.addSC("retransmit-interval", "Time between retransmitting lost link state advertisements");
			intLoopBackC.ip.ospf["retransmit-interval"].addSC("<1-65535>", "Seconds");
		intLoopBackC.ip.ospf.addSC("transmit-delay", "Link state transmit delay");
			intLoopBackC.ip.ospf["transmit-delay"].addSC("<1-65535>", "Seconds");

	intLoopBackC.ip.addSC("rip", "Router Information Protocol");
		intLoopBackC.ip.rip.addSC("authentication", "Authentication control");
			intLoopBackC.ip.rip.authentication.addSC("key-chain", "Authentication key-chain");
				intLoopBackC.ip.rip.authentication["key-chain"].addSC("LINE", "name of key-chain");
			intLoopBackC.ip.rip.authentication.addSC("mode", "Authentication mode");
				intLoopBackC.ip.rip.authentication.mode.addSC("md5", "Keyed message digest");
				intLoopBackC.ip.rip.authentication.mode.addSC("text", "Clear text authentication");
		intLoopBackC.ip.rip.addSC("receive", "advertisement reception");
			intLoopBackC.ip.rip.receive.addSC("version", "version control");
				intLoopBackC.ip.rip.receive.version.addSC("<1-1>", "RIP version 1");
				intLoopBackC.ip.rip.receive.version.addSC("<2-2>", "RIP version 2");
		intLoopBackC.ip.rip.addSC("send", "advertisement transmission");
			intLoopBackC.ip.rip.send.addSC("version", "version control");
				intLoopBackC.ip.rip.send.version.addSC("<1-1>", "RIP version 1");
				intLoopBackC.ip.rip.send.version.addSC("<2-2>", "RIP version 2");
		intLoopBackC.ip.rip.addSC("v2-broadcast", "send ip broadcast v2 update");
intLoopBackC.addSC("keepalive", "Enable keepalive");
	intLoopBackC.keepalive.addSC("<0-32767>", "Keepalive period (default 10 seconds)");

intLoopBackC.addSC("load-interval", "Specify interval for load calculation for an interface");
	intLoopBackC["load-interval"].addSC("<30-600>", "Load interval delay in seconds");
intLoopBackC.addSC("logging", "Configure logging for interface");
	intLoopBackC.logging.addSC("event", "Interface events");
		intLoopBackC.logging.event.addSC("link-status", "UPDOWN and CHANGE messages");
intLoopBackC.addSC("max-reserved-bandwidth", "Maximum Reservable Bandwidth on an Interface");
	intLoopBackC["max-reserved-bandwidth"].addSC("<1-100>", "Max. reservable bandwidth as % of interface bandwidth");
intLoopBackC.addSC("mls", "Configure MultiLayer Switching characteristics");
intLoopBackC.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
	intLoopBackC.mtu.addSC("<64-2025>", "MTU size in bytes");
intLoopBackC.addSC("no", "Negate a command or set its defaults");
	intLoopBackC.no.addSC("access-expression", "Build a bridge boolean access expression");
		intLoopBackC.no["access-expression"].addSC("input", "Filter input packets");
		intLoopBackC.no["access-expression"].addSC("output", "Filter output packets");
	intLoopBackC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
		intLoopBackC.no.arp.addSC("arpa", "Standard arp protocol");
		intLoopBackC.no.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
		intLoopBackC.no.arp.addSC("probe", "HP style arp protocol");
		intLoopBackC.no.arp.addSC("snap", "IEEE 802.3 style arp");
		intLoopBackC.no.arp.addSC("timeout", "Set ARP cache timeout");
	intLoopBackC.no.addSC("bandwidth", "Set bandwidth informational parameter");
	intLoopBackC.no.addSC("bridge-group", "Transparent bridging interface parameters");
	intLoopBackC.no.addSC("carrier-delay", "Specify delay for interface transitions");
	intLoopBackC.no.addSC("cdp", "CDP interface subcommands");
		intLoopBackC.no.cdp.addSC("enable", "Enable CDP on interface");
	intLoopBackC.no.addSC("delay", "Specify interface throughput delay");
	intLoopBackC.no.addSC("description", "Interface specific description");
	intLoopBackC.no.addSC("hold-queue", "Set hold queue depth");
		intLoopBackC.no["hold-queue"].addSC("<0-4096>", "Queue length");
		intLoopBackC.no["hold-queue"].addSC("in", "Input queue");
		intLoopBackC.no["hold-queue"].addSC("out", "Output queue");
	intLoopBackC.no.addSC("ip", "Interface Internet Protocol config commands");
		intLoopBackC.no.ip.addSC("access-group", "Specify access control for packets");
			intLoopBackC.no.ip["access-group"].addSC("<1-199>", "IP access list (standard or extended)");
		intLoopBackC.no.ip.addSC("accounting", "Enable IP accounting on this interface");
			intLoopBackC.no.ip.accounting.addSC("access-violations", "Account for IP packets violating access lists on this interface");
		intLoopBackC.no.ip.addSC("address", "Set the IP address of an interface");
			intLoopBackC.no.ip.address.addSC("A.B.C.D", "IP address");
				intLoopBackC.no.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
		intLoopBackC.no.ip.addSC("authentication", "authentication subcommands");
			intLoopBackC.no.ip.authentication.addSC("key-chain", "key-chain");
				intLoopBackC.no.ip.authentication["key-chain"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			intLoopBackC.no.ip.authentication.addSC("mode", "mode");
				intLoopBackC.no.ip.authentication.mode.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
		intLoopBackC.no.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
			intLoopBackC.no.ip["bandwidth-percent"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intLoopBackC.no.ip["bandwidth-percent"].eigrp.addSC("<1-65535>", "Autonomous system number");
		intLoopBackC.no.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		intLoopBackC.no.ip.addSC("cef", "Cisco Express Fowarding interface commands");
			intLoopBackC.no.ip.cef.addSC("accounting", "CEF accounting features for interface");
				intLoopBackC.no.ip.cef.accounting.addSC("non-recursive", "CEF non-recursive accounting features");
		intLoopBackC.no.ip.addSC("cgmp", "Enable/disable CGMP");
		intLoopBackC.no.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
		intLoopBackC.no.ip.addSC("dvmrp", "DVMRP interface commands");
			intLoopBackC.no.ip.dvmrp.addSC("accept-filter", "DVMRP incoming Report filters");
		intLoopBackC.no.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
			intLoopBackC.no.ip["hello-interval"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intLoopBackC.no.ip["hello-interval"].eigrp.addSC("<1-65535>", "Autonomous system number");
		intLoopBackC.no.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
			intLoopBackC.no.ip["helper-address"].addSC("A.B.C.D", "IP destination address");
		intLoopBackC.no.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
			intLoopBackC.no.ip["hold-time"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intLoopBackC.no.ip["hold-time"].eigrp.addSC("<1-65535>", "Autonomous system number");
		intLoopBackC.no.ip.addSC("igmp", "IGMP interface commands");
			intLoopBackC.no.ip.igmp.addSC("access-group", "IGMP group access group");
			intLoopBackC.no.ip.igmp.addSC("helper-address", "IGMP helper address");
		intLoopBackC.no.ip.addSC("irdp", "ICMP Router Discovery Protocol");
			intLoopBackC.no.ip.irdp.addSC("address", "addresses to proxy-advertise");
				intLoopBackC.no.ip.irdp.address.addSC("A.B.C.D", "address to advertise");
			intLoopBackC.no.ip.irdp.addSC("holdtime", "how long a receiver should believe the information");
			intLoopBackC.no.ip.irdp.addSC("maxadvertinterval", "maximum time between advertisements");
			intLoopBackC.no.ip.irdp.addSC("minadvertinterval", "minimum time between advertisements");
			intLoopBackC.no.ip.irdp.addSC("multicast", "advertisements are sent with multicasts");
			intLoopBackC.no.ip.irdp.addSC("preference", "preference level for this interface");
				intLoopBackC.no.ip.irdp.preference.addSC("<-2147483648 - 2147483647>", "preference for this address (higher values preferred)");
		intLoopBackC.no.ip.addSC("load-sharing", "Style of load sharing");
			intLoopBackC.no.ip["load-sharing"].addSC("per-packet", "Random distribution");
		intLoopBackC.no.ip.addSC("local-proxy-arp", "Enable local-proxy ARP");
		intLoopBackC.no.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
		intLoopBackC.no.ip.addSC("mrm", "Configure IP Multicast Routing Monitor tester");
		intLoopBackC.no.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
		intLoopBackC.no.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		intLoopBackC.no.ip.addSC("multicast", "IP multicast interface commands");
			intLoopBackC.no.ip.multicast.addSC("boundary", "Boundary for administratively scoped multicast addresses");
			intLoopBackC.no.ip.multicast.addSC("helper-map", "Broadcast to Multicast map OR Multicast to Broadcast map");
		intLoopBackC.no.ip.addSC("ospf", "OSPF interface commands");
			intLoopBackC.no.ip.ospf.addSC("authentication", "Enable authentication");
			intLoopBackC.no.ip.ospf.addSC("authentication-key", "Authentication password (key)");
		intLoopBackC.no.ip.addSC("pim", "PIM interface commands");
			intLoopBackC.no.ip.pim.addSC("bsr-border", "Border of PIM domain");
			intLoopBackC.no.ip.pim.addSC("dense-mode", "Enable PIM dense-mode operation");
			intLoopBackC.no.ip.pim.addSC("nbma-mode", "Use Non-Broadcast Multi-Access (NBMA) mode on interface");
		intLoopBackC.no.ip.addSC("probe", "Enable HP Probe support");
			intLoopBackC.no.ip.probe.addSC("proxy", "Proxy support");
		intLoopBackC.no.ip.addSC("proxy-arp", "Enable proxy ARP");
		intLoopBackC.no.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
		intLoopBackC.no.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
		intLoopBackC.no.ip.addSC("rgmp", "Enable/disable RGMP");
		intLoopBackC.no.ip.addSC("rip", "Router Information Protocol");
			intLoopBackC.no.ip.rip.addSC("authentication", "Authentication control");
				intLoopBackC.no.ip.rip.authentication.addSC("key-chain", "Authentication key-chain");
				intLoopBackC.no.ip.rip.authentication.addSC("mode", "Authentication mode");
			intLoopBackC.no.ip.rip.addSC("receive", "advertisement reception");
		intLoopBackC.no.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
			intLoopBackC.no.ip["route-cache"].addSC("cef", "Enable Cisco Express Forwarding");
			intLoopBackC.no.ip["route-cache"].addSC("flow", "Enable Flow fast-switching cache");
			intLoopBackC.no.ip["route-cache"].addSC("policy", "Enable fast-switching policy cache for outgoing packets");
			intLoopBackC.no.ip["route-cache"].addSC("same-interface", "Enable fast-switching on the same interface");
		intLoopBackC.no.ip.addSC("sap", "Session Advertisement Protocol interface commands");
			intLoopBackC.no.ip.sap.addSC("listen", "Listen for sap packets on interface");
		intLoopBackC.no.ip.addSC("sdr", "Session Directory Protocol interface commands");
			intLoopBackC.no.ip.sdr.addSC("listen", "Listen for sap packets on interface");
		intLoopBackC.no.ip.addSC("security", "DDN IP Security Option");
			intLoopBackC.no.ip.security.addSC("add", "Ensure all outgoing packets have a basic security option");
			intLoopBackC.no.ip.security.addSC("aeso", "Specify AESO sources");
				intLoopBackC.no.ip.security.aeso.addSC("<0-255>", "ESO source");
			intLoopBackC.no.ip.security.addSC("eso-max", "Specify maximum sensitivity level");
		intLoopBackC.no.ip.addSC("split-horizon", "Perform split horizon");
			intLoopBackC.no.ip["split-horizon"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intLoopBackC.no.ip["split-horizon"].eigrp.addSC("<1-65535>", "Autonomous system number");
		intLoopBackC.no.ip.addSC("summary-address", "Perform address summarization");
			intLoopBackC.no.ip["summary-address"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intLoopBackC.no.ip["summary-address"].eigrp.addSC("<1-65535>", "Autonomous system number");
			intLoopBackC.no.ip["summary-address"].addSC("rip", "Routing Information Protocol (RIP)");
				intLoopBackC.no.ip["summary-address"].rip.addSC("A.B.C.D", "IP address");
		intLoopBackC.no.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
		intLoopBackC.no.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
		intLoopBackC.no.ip.addSC("verify", "Enable per packet validation");
			intLoopBackC.no.ip.verify.addSC("unicast", "Enable per packet validation for unicast");
				intLoopBackC.no.ip.verify.unicast.addSC("reverse-path", "Reverse path validation of source address");
		intLoopBackC.no.ip.addSC("vrf", "VPN Routing/Forwarding parameters on the interface");
			intLoopBackC.no.ip.vrf.addSC("forwarding", "Configure forwarding table");
				intLoopBackC.no.ip.vrf.forwarding.addSC("WORD", "Table name");
			intLoopBackC.no.ip.vrf.addSC("sitemap", "Configure route-map for routes received from this site");
	intLoopBackC.no.addSC("keepalive", "Enable keepalive");
		intLoopBackC.no.keepalive.addSC("<0-32767>", "Keepalive period (default 10 seconds)");
	intLoopBackC.no.addSC("load-interval", "Specify interval for load calculation for an interface");
	intLoopBackC.no.addSC("logging", "Configure logging for interface");
	intLoopBackC.no.addSC("max-reserved-bandwidth", "Maximum Reservable Bandwidth on an Interface");
		intLoopBackC.no["max-reserved-bandwidth"].addSC("<1-100>", "Max. reservable bandwidth as % of interface bandwidth");
	intLoopBackC.no.addSC("mls", "Configure MultiLayer Switching characteristics");
	intLoopBackC.no.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");

	intLoopBackC.no.addSC("shutdown", "Shutdown the selected interface");

intLoopBackC.addSC("ntp", "Configure NTP");
intLoopBackC.addSC("rmon", "Configure Remote Monitoring on an interface");
	intLoopBackC.rmon.addSC("collection", "Configure Remote Monitoring Collection on an interface");
		intLoopBackC.rmon.collection.addSC("history", "Configure history");
			intLoopBackC.rmon.collection.history.addSC("<1-65535>", "Set RMON collection control index");
				intLoopBackC.rmon.collection.history["<1-65535>"].addSC("buckets", "Requested buckets of intervals. Default is 50 buckets");
				intLoopBackC.rmon.collection.history["<1-65535>"].addSC("interval", "Interval to sample data for each bucket. Default is 1800 seconds");
				intLoopBackC.rmon.collection.history["<1-65535>"].addSC("owner", "Set the owner of this RMON collection");
		intLoopBackC.rmon.collection.addSC("stats", "Configure statistics");
			intLoopBackC.rmon.collection.stats.addSC("<1-65535>", "Set RMON collection control index");
				intLoopBackC.rmon.collection.stats["<1-65535>"].addSC("owner", "Configure the owner of this RMON collection");
	intLoopBackC.rmon.addSC("native", "Monitor the interface in native mode");
	intLoopBackC.rmon.addSC("promiscuous", "Monitor the interface in promiscuous mode");
intLoopBackC.addSC("service-policy", "Configure QoS Service Policy");

intLoopBackC.addSC("shutdown", "Shutdown the selected interface");
intLoopBackC.addSC("snmp", "Modify SNMP interface parameters");
	intLoopBackC.snmp.addSC("trap", "Allow a specific SNMP trap");
		intLoopBackC.snmp.trap.addSC("link-status", "Allow SNMP LINKUP and LINKDOWN traps");

intLoopBackC.addSC("spanning-tree", "Spanning Tree Subsystem");
	intLoopBackC["spanning-tree"].addSC("cost", "Change an interface's spanning tree port path cost");
		intLoopBackC["spanning-tree"].cost.addSC("<1-200000000>", "port path cost");
	intLoopBackC["spanning-tree"].addSC("guard", "Change an interface's spanning tree guard mode");
		intLoopBackC["spanning-tree"].guard.addSC("none", "Set guard mode to none");
		intLoopBackC["spanning-tree"].guard.addSC("root", "Set guard mode to root guard on interface");
	intLoopBackC["spanning-tree"].addSC("port-priority", "Change an interface's spanning tree port priority");
		intLoopBackC["spanning-tree"]["port-priority"].addSC("<0-255>", "port priority");
	intLoopBackC["spanning-tree"].addSC("portfast", "Enable an interface to move directly to forwarding on link up");
	intLoopBackC["spanning-tree"].addSC("stack-port", "Enable stack port");
intLoopBackC.addSC("timeout", "Define timeout values for this interface");
	intLoopBackC.timeout.addSC("absolute", "Define session timeout value for this interface");
		intLoopBackC.timeout.absolute.addSC("<0-35790>", "Session lifetime (in minutes)");
			intLoopBackC.timeout.absolute["<0-35790>"].addSC("<0-59>", "Session lifetime (in seconds)");

intLoopBackC.addSC("timeout", "Define timeout values for this interface");
	intLoopBackC.timeout.addSC("absolute", "Define session timeout value for this interface");
		intLoopBackC.timeout.absolute.addSC("<0-35790>", "Session lifetime (in minutes)");
			intLoopBackC.timeout.absolute["<0-35790>"].addSC("<0-59>", "Session lifetime (in seconds)");
intLoopBackC.addSC("transmit-interface", "Assign a transmit interface to a receive-only interface");
	intLoopBackC["transmit-interface"].addSC("Async", "Async interface");
		intLoopBackC["transmit-interface"].Async.addSC("<1-0>", "Async interface number");

intLoopBackC.addSC("tx-ring-limit", "Configure PA level transmit ring limit");
	intLoopBackC["tx-ring-limit"].addSC("<1-32767>", "Number (ring limit)");
