
globalC.addSC("aaa", "Authentication, Authorization and Accounting.");
	globalC.aaa.addSC("new-model", "Enable NEW access control commands and functions.(Disables OLD commands.)");
globalC.addSC("access-list", "Add an access list entry");
	globalC["access-list"].addSC("<1-99>", "IP standard access list");
		globalC["access-list"]["<1-99>"].addSC("deny", "Specify packets to reject");
		globalC["access-list"]["<1-99>"].addSC("permit", "Specify packets to forward");
	globalC["access-list"].addSC("<100-199>", "IP extended access list");
		globalC["access-list"]["<100-199>"].addSC("deny", "Specify packets to reject");
		globalC["access-list"]["<100-199>"].addSC("dynamic", "Specify a DYNAMIC list of PERMITs or DENYs");
		globalC["access-list"]["<100-199>"].addSC("permit", "Specify packets to forward");
	globalC["access-list"].addSC("<1100-1199>", "Extended 48-bit MAC address access list");
		globalC["access-list"]["<1100-1199>"].addSC("deny", "Specify packets to reject");
		globalC["access-list"]["<1100-1199>"].addSC("permit", "Specify packets to forward");
	globalC["access-list"].addSC("<1300-1999>", "IP standard access list (expanded range)");
		globalC["access-list"]["<1300-1999>"].addSC("deny", "Specify packets to reject");
		globalC["access-list"]["<1300-1999>"].addSC("permit", "Specify packets to forward");
	globalC["access-list"].addSC("<200-299>", "Protocol type-code access list");
		globalC["access-list"]["<200-299>"].addSC("deny", "Specify packets to reject");
		globalC["access-list"]["<200-299>"].addSC("permit", "Specify packets to forward");
	globalC["access-list"].addSC("<2000-2699>", "IP extended access list (expanded range)");
		globalC["access-list"]["<2000-2699>"].addSC("deny", "Specify packets to reject");
		globalC["access-list"]["<2000-2699>"].addSC("dynamic", "Specify a DYNAMIC list of PERMITs or DENYs");
		globalC["access-list"]["<2000-2699>"].addSC("permit", "Specify packets to forward");
globalC.addSC("alias", "Create command alias");
globalC.addSC("arp", "Set a static ARP entry");
globalC.addSC("async-bootp", "Modify system bootp parameters");
globalC.addSC("banner", "Define a login banner");
	globalC.banner.addSC("motd", "Set Message of the Day banner");
		globalC.banner.motd.addSC("LINE", "c banner-text c, where 'c' is a delimiting character");
globalC.addSC("boot", "Modify system boot parameters");
globalC.addSC("bridge", "Bridge Group.");
globalC.addSC("buffers", "Adjust system buffer pool parameters");
globalC.addSC("busy-message", "Display message when connection to host fails");
globalC.addSC("call-history-mib", "Define call history mib parameters");
globalC.addSC("cdp", "Global CDP configuration subcommands");
	globalC.cdp.addSC("run", "");
globalC.addSC("chat-script", "Define a modem chat script");
globalC.addSC("class-map", "Configure QoS Class Map");
	globalC["class-map"].addSC("WORD", "class-map name");
	globalC["class-map"].addSC("match-all", "Logical-AND all matching statements under this classmap");
		globalC["class-map"]["match-all"].addSC("WORD", "class-map name");
	globalC["class-map"].addSC("match-any", "Logical-OR all matching statements under this classmap");
		globalC["class-map"]["match-any"].addSC("WORD", "class-map name");
globalC.addSC("clock", "Configure time-of-day clock");
	globalC.clock.addSC("summer-time", "Configure summer (daylight savings) time");
		globalC.clock["summer-time"].addSC("WORD", "name of time zone in summer");
	globalC.clock.addSC("timezone", "Configure time zone");
		globalC.clock.timezone.addSC("WORD", "name of time zone");
globalC.addSC("cns", "CNS Subsystem");
globalC.addSC("config-register", "Define the configuration register");
	globalC["config-register"].addSC("<0x0-0xFFFF>", "Config register number");
globalC.addSC("connect", "cross-connect two interfaces");
globalC.addSC("controller", "Configure a specific controller");
globalC.addSC("default", "Set a command to its defaults");
globalC.addSC("default-value", "Default character-bits values");
globalC.addSC("define", "interface range macro definition");
globalC.addSC("dialer", "Dialer commands");
	globalC.dialer.addSC("clid", "Configure dialer CLID command");
		globalC.dialer.clid.addSC("group", "Configure dialer CLID group");
	globalC.dialer.addSC("dnis", "Configure dialer DNIS command");
		globalC.dialer.dnis.addSC("group", "Configure dialer DNIS group");
	globalC.dialer.addSC("watch-list", "Dialer watch list");
		globalC.dialer["watch-list"].addSC("<1-255>", "Dialer watch group number");
globalC.addSC("dialer-list", "Create a dialer list entry");
	globalC["dialer-list"].addSC("<1-128>", "Dialer group number");
		globalC["dialer-list"]["<1-128>"].addSC("protocol", "Permit or Deny based on protocols");
globalC.addSC("dnsix-dmdp", "Provide DMDP service for DNSIX");
globalC.addSC("dnsix-nat", "Provide DNSIX service for audit trails");
globalC.addSC("do", "To run exec commands in config mode");
	globalC["do"].addSC("LINE", "Exec Command");
globalC.addSC("downward-compatible-config", "Generate a configuration compatible with older software");
	globalC["downward-compatible-config"].addSC("<0-999999>.<0-999999>", "Version number");
globalC.addSC("enable", "Modify enable password parameters");
	globalC.enable.addSC("password", "Assign the privileged level password");
		globalC.enable.secret.addSC("LINE", "The UNENCRYPTED (cleartext) 'enable' secret");
		globalC.enable.secret.addSC("level", "Set exec level password");
	globalC.enable.addSC("use-tacacs", "Use TACACS to check enable passwords");
globalC.addSC("end", "Exit from configure mode");
globalC.addSC("exception", "Exception handling");
globalC.addSC("exit", "Exit from configure mode");
globalC.addSC("file", "Adjust file system parameters");
globalC.addSC("frame-relay", "global frame relay configuration commands");
globalC.addSC("help", "Description of the interactive help system");
globalC.addSC("hostname", "Set system's network name");
	globalC.hostname.addSC("WORD", "This system's network name");
globalC.addSC("interface", "Select an interface to configure");

	globalC.interface.addSC("Async", "Async interface");
		globalC.interface.Async.addSC("<1-5>", "Async interface number");
	globalC.interface.addSC("Dialer", "Dialer interface");
		globalC.interface.Dialer.addSIC("<0-255>", "Dialer interface number");
			globalC.interface.Dialer["<0-255>"].addSC("<0-4294967295>");

	globalC.interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
		globalC.interface.FastEthernet.addSIC("<0-0>", "FastEthernet interface number");
			globalC.interface.FastEthernet["<0-0>"].addSC("<0-4294967295>");

	globalC.interface.addSC("Loopback", "Loopback interface");
		globalC.interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
	globalC.interface.addSC("Multilink", "Multilink-group interface");
		globalC.interface.Multilink.addSC("<1-2147483647>", "Multilink interface number");
	globalC.interface.addSC("Null", "Null interface");
		globalC.interface.Null.addSC("<0-0>", "Null interface number");

	globalC.interface.addSC("Serial", "Serial");
		globalC.interface.Serial.addSIC("<0-1>", "Serial interface number");
			globalC.interface.Serial["<0-1>"].addSC("<0-4294967295>");

	globalC.interface.addSC("Virtual-Template", "Virtual Template interface");
		globalC.interface["Virtual-Template"].addSC("<1-200>", "Virtual-Template interface number");
globalC.addSC("ip", "Global IP configuration subcommands");
	globalC.ip.addSC("access-list", "Named access-list");
		globalC.ip["access-list"].addSC("extended", "Extended Access List");
		globalC.ip["access-list"].addSC("log-update", "Control access list log updates");
		globalC.ip["access-list"].addSC("logging", "Control access list logging");
		globalC.ip["access-list"].addSC("standard", "Standard Access List");
	globalC.ip.addSC("accounting-list", "Select hosts for which IP accounting information is kept");
	globalC.ip.addSC("accounting-threshold", "Sets the maximum number of accounting entries");
	globalC.ip.addSC("accounting-transits", "Sets the maximum number of transit entries");
	globalC.ip.addSC("address-pool", "Specify default IP address pooling mechanism");
	globalC.ip.addSC("alias", "Alias an IP address to a TCP port");
	globalC.ip.addSC("as-path", "BGP autonomous system path filter");
	globalC.ip.addSC("bgp-community", "format for BGP community");
	globalC.ip.addSC("bootp", "Config BOOTP services");
	globalC.ip.addSC("cef", "Cisco Express Forwarding");
	globalC.ip.addSC("classless", "Follow classless routing forwarding rules");
	globalC.ip.addSC("community-list", "Add a community list entry");
	globalC.ip.addSC("default-gateway", "Specify default gateway (if not routing IP)");
		globalC.ip["default-gateway"].addSC("A.B.C.D", "IP address of default gateway");
	globalC.ip.addSC("default-network", "Flags networks as candidates for default routes");
		globalC.ip["default-network"].addSC("A.B.C.D", "IP address of default network");
	globalC.ip.addSC("dhcp", "Configure DHCP server and relay parameters");
		globalC.ip.dhcp.addSC("pool", "Configure DHCP address pools");
	globalC.ip.addSC("dhcp-client", "Configure parameters for DHCP client operation");
	globalC.ip.addSC("dhcp-server", "Specify address of DHCP server to use");
	globalC.ip.addSC("domain", "IP DNS Resolver");
		globalC.ip.domain.addSC("lookup", "Enable IP Domain Name System hostname translation");
		globalC.ip.domain.addSC("name", "Define the default domain name");
	globalC.ip.addSC("domain-list", "Domain name to complete unqualified host names.");
	globalC.ip.addSC("domain-lookup", "Enable IP Domain Name System hostname translation");
	globalC.ip.addSC("domain-name", "Define the default domain name");
	globalC.ip.addSC("dvmrp", "DVMRP global commands");
	globalC.ip.addSC("extcommunity-list", "Add a extended community list entry");
	globalC.ip.addSC("finger", "finger server");
		globalC.ip.finger.addSC("rfc-compliant", "Comply with RFC 1288");
	globalC.ip.addSC("flow-aggregation", "Configure flow aggregation");
	globalC.ip.addSC("flow-cache", "Configure netflow cache parameters");
	globalC.ip.addSC("flow-export", "Specify host/port to send flow statistics");
	globalC.ip.addSC("forward-protocol", "Controls forwarding of physical and directed IP broadcasts");
	globalC.ip.addSC("ftp", "FTP configuration commands");
	globalC.ip.addSC("gratuitous-arps", "Generate gratuitous ARPs for PPP/SLIP peer addresses");
		globalC.ip["gratuitous-arps"].addSC("non-local", "Send only non-local PPP/SLIP gratuitous ARPs (default)");
	globalC.ip.addSC("host", "Add an entry to the ip hostname table");
		globalC.ip.host.addSC("WORD", "Name of host");
	globalC.ip.addSC("host-routing", "Enable host-based routing (proxy ARP and redirect)");
	globalC.ip.addSC("hp-host", "Enable the HP proxy probe service");
		globalC.ip["hp-host"].addSC("WORD", "HP host's name");
	globalC.ip.addSC("http", "HTTP server configuration");
	globalC.ip.addSC("icmp", "ICMP options");
		globalC.ip.icmp.addSC("rate-limit", "rate limit ICMP messages generated");
		globalC.ip.icmp.addSC("redirect", "Redirect type");
	globalC.ip.addSC("igmp", "IGMP global configuration");
		globalC.ip.igmp.addSC("immediate-leave", "Leave groups immediately without sending last member query, use for one host network only");
	globalC.ip.addSC("local", "Specify local options");
		globalC.ip.local.addSC("policy", "Enable policy routing");
		globalC.ip.local.addSC("pool", "IP Local address pool lists");
	globalC.ip.addSC("mrm", "Configure IP Multicast Routing Monitor test parameters");
		globalC.ip.mrm.addSC("accept-manager", "IP MRM manager filter for test sender and test receiver");
		globalC.ip.mrm.addSC("manager", "Configure IP MRM manager parameters");
	globalC.ip.addSC("mroute", "Configure static multicast routes");
		globalC.ip.mroute.addSC("A.B.C.D", "Source address");
	globalC.ip.addSC("msdp", "MSDP global commands");
	globalC.ip.addSC("multicast", "Global IP Multicast Commands");
	globalC.ip.addSC("multicast-routing", "Enable IP multicast forwarding");
	globalC.ip.addSC("name-server", "Specify address of name server to use");
	globalC.ip.addSC("nat", "NAT configuration commands");
		globalC.ip.nat.addSC("inside", "Inside address translation");
		globalC.ip.nat.addSC("outside", "Outside address translation");
		globalC.ip.nat.addSC("pool", "Define pool of addresses");
		globalC.ip.nat.addSC("service", "Special translation for application using non-standard port");
		globalC.ip.nat.addSC("translation", "NAT translation entry configuration");
	globalC.ip.addSC("nbar", "NBAR - Network Based Application Recognition");
	globalC.ip.addSC("ospf", "OSPF");
	globalC.ip.addSC("pgm", "PGM Reliable Transport Protocol");
	globalC.ip.addSC("pim", "PIM global commands");
	globalC.ip.addSC("prefix-list", "Build a prefix list");
	globalC.ip.addSC("radius", "RADIUS configuration commands");
		globalC.ip.radius.addSC("source-interface", "Specify interface for source address in RADIUS packets");
	globalC.ip.addSC("rcmd", "Rcmd commands");
		globalC.ip.rcmd.addSC("domain-lookup", "Enable IP DNS queries for Rcmd");
		globalC.ip.rcmd.addSC("source-interface", "Specify interface for source address in rcmd connections");
	globalC.ip.addSC("reflexive-list", "Reflexive access list");
		globalC.ip["reflexive-list"].addSC("timeout", "Timeout value for reflexive ACL entries");
	globalC.ip.addSC("route", "Establish static routes");
		globalC.ip.route.addSC("A.B.C.D", "Destination prefix");
		globalC.ip.route.addSC("profile", "Enable IP routing table profile");
	globalC.ip.addSC("routing", "Enable IP routing");
	globalC.ip.addSC("rsvp", "Configure static RSVP information");
	globalC.ip.addSC("rtcp", "RTCP parameters");
	globalC.ip.addSC("sap", "Global IP Multicast SAP Commands");
	globalC.ip.addSC("security", "Specify system wide security information");
	globalC.ip.addSC("subnet-zero", "Allow 'subnet zero' subnets");
	globalC.ip.addSC("tacacs", "TACACS configuration commands");
		globalC.ip.tacacs.addSC("source-interface", "Specify interface for source address in TACACS packets");
	globalC.ip.addSC("tcp", "Global TCP parameters");
	globalC.ip.addSC("telnet", "Specify telnet options");
		globalC.ip.telnet.addSC("comport", "Specify RFC 2217 options");
		globalC.ip.telnet.addSC("hidden", "Don't display telnet addresses or hostnames");
		globalC.ip.telnet.addSC("quiet", "Don't display non-error telnet messages");
		globalC.ip.telnet.addSC("source-interface", "Specify source interface");
		globalC.ip.telnet.addSC("tos", "Specify type of service");
	globalC.ip.addSC("tftp", "tftp configuration commands");
		globalC.ip.tftp.addSC("boot-interface", "Force interface to use for TFTP booting");
		globalC.ip.tftp.addSC("source-interface", "Specify interface for source address in TFTP connections");
	globalC.ip.addSC("udptn", "UDPTN configuration commands");
		globalC.ip.udptn.addSC("source-interface", "Specify source interface");
	globalC.ip.addSC("vrf", "Configure an IP VPN Routing/Forwarding instance");
		globalC.ip.vrf.addSC("WORD", "VPN Routing/Forwarding instance name");
	globalC.ip.addSC("wccp", "Web-Cache Coordination Protocol Commands");
		globalC.ip.wccp.addSC("<0-99>", "Dynamically defined service identifier number");
		globalC.ip.wccp.addSC("version", "protocol version");
		globalC.ip.wccp.addSC("web-cache", "Standard web caching service");
globalC.addSC("ipv6", "Global IPv6 configuration commands");
globalC.addSC("key", "Key management");
globalC.addSC("line", "Configure a terminal line");
	globalC.line.addSC("<0-10>", "First Line number");
		globalC.line["<0-10>"].addSC("<1-10>", "Last Line number");
	globalC.line.addSC("aux", "Auxiliary line");
		globalC.line.aux.addSC("<0-0>", "First Line number");
	globalC.line.addSC("console", "Primary terminal line");
		globalC.line.console.addSC("<0-0>", "First Line number");
	globalC.line.addSC("tty", "Terminal controller");
		globalC.line.tty.addSC("<1-4>", "First Line number");
	globalC.line.addSC("vty", "Virtual terminal");
		globalC.line.vty.addSC("<0-15>", "First Line number");
globalC.addSC("logging", "Modify message logging facilities");
	globalC.logging.addSC("Hostname or A.B.C.D", "IP address of the logging host");
	globalC.logging.addSC("buffered", "Set buffered logging parameters");
	globalC.logging.addSC("cns-events", "Set CNS Event logging level");
	globalC.logging.addSC("console", "Set console logging level");
	globalC.logging.addSC("count", "Count every log message and timestamp last occurance");
	globalC.logging.addSC("exception", "Limit size of exception flush output");
		globalC.logging.exception.addSC("<4096-2147483647>", "Set size of logging exception flush");
	globalC.logging.addSC("facility", "Facility parameter for syslog messages");
	globalC.logging.addSC("history", "Configure syslog history table");
	globalC.logging.addSC("monitor", "Set terminal line (monitor) logging level");
	globalC.logging.addSC("on", "Enable logging to all supported destinations");
	globalC.logging.addSC("rate-limit", "Set messages per second limit");
	globalC.logging.addSC("source-interface", "Specify interface for source address in logging transactions");
	globalC.logging.addSC("trap", "Set syslog server logging level");
globalC.addSC("login-string", "Define a host-specific login string");
globalC.addSC("map-class", "Configure static map class");
	globalC["map-class"].addSC("atm", "Asynchronous transfer mode");
		globalC["map-class"].atm.addSC("WORD", "Static map class name");
	globalC["map-class"].addSC("dialer", "Dial on Demand");
		globalC["map-class"].dialer.addSC("WORD", "Static map class name");
	globalC["map-class"].addSC("frame-relay", "Frame Relay");
		globalC["map-class"]["frame-relay"].addSC("WORD", "Static map class name");
globalC.addSC("map-list", "Configure static map list");
globalC.addSC("memory-size", "Adjust memory size by percentage");
globalC.addSC("menu", "Define a user-interface menu");
globalC.addSC("netbios", "NETBIOS access control filtering");
	globalC.netbios.addSC("access-list", "Define NETBIOS station access list");
globalC.addSC("modemcap", "Modem Capabilities database");
	globalC.modemcap.addSC("edit", "Edit a modemcap entry");
		globalC.modemcap.edit.addSC("WORD", "Modem type");
	globalC.modemcap.addSC("entry", "Give a full modemcap entry");
		globalC.modemcap.entry.addSC("LINE", "Modemcap entry for this modem");
globalC.addSC("multilink", "PPP multilink global configuration");
	globalC.multilink.addSC("bundle-name", "Select method for naming multilink bundles");
		globalC.multilink["bundle-name"].addSC("authenticated", "Use peer's authenticated name");
		globalC.multilink["bundle-name"].addSC("both", "Use peer's authenticated name and endpoint discriminator");
		globalC.multilink["bundle-name"].addSC("endpoint", "Use peer's endpoint discriminator");
	globalC.multilink.addSC("virtual-template", "virtual-template interface");
		globalC.multilink["virtual-template"].addSC("<1-200>", "virtual template number");
globalC.addSC("no", "Negate a command or set its defaults");
	globalC.no.addSC("aaa", "Authentication, Authorization and Accounting.");
	globalC.no.addSC("boot", "Modify system boot parameters");
	globalC.no.addSC("clock", "Configure time-of-day clock");
	globalC.no.addSC("config-register", "Define the configuration register");
	globalC.no.addSC("do", "To run exec commands in config mode");
	globalC.no.addSC("downward-compatible-config", "Generate a configuration compatible with older software");
	globalC.no.addSC("enable", "Modify enable password parameters");
		globalC.no.enable.addSC("password", "Assign the privileged level password");
		globalC.no.enable.addSC("secret", "Assign the privileged level secret");
		globalC.no.enable.addSC("use-tacacs", "Use TACACS to check enable passwords");
	globalC.no.addSC("hostname", "Set system's network name");
	globalC.no.addSC("ip", "Global IP configuration subcommands");
		globalC.no.ip.addSC("access-list", "Named access-list");
		globalC.no.ip.addSC("accounting-list", "Select hosts for which IP accounting information is kept");
		globalC.no.ip.addSC("accounting-threshold", "Sets the maximum number of accounting entries");
		globalC.no.ip.addSC("accounting-transits", "Sets the maximum number of transit entries");
		globalC.no.ip.addSC("address-pool", "Specify default IP address pooling mechanism");
		globalC.no.ip.addSC("as-path", "BGP autonomous system path filter");
		globalC.no.ip.addSC("bgp-community", "format for BGP community");
		globalC.no.ip.addSC("classless", "Follow classless routing forwarding rules");
		globalC.no.ip.addSC("community-list", "Add a community list entry");
		globalC.no.ip.addSC("default-gateway", "Specify default gateway (if not routing IP)");
		globalC.no.ip.addSC("default-network", "Flags networks as candidates for default routes");
		globalC.no.ip.addSC("dhcp", "Configure DHCP server and relay parameters");
		globalC.no.ip.addSC("dhcp-client", "Configure parameters for DHCP client operation");
		globalC.no.ip.addSC("dhcp-server", "Specify address of DHCP server to use");
		globalC.no.ip.addSC("domain", "IP DNS Resolver");
		globalC.no.ip.addSC("domain-list", "Domain name to complete unqualified host names.");
		globalC.no.ip.addSC("domain-lookup", "Enable IP Domain Name System hostname translation");
		globalC.no.ip.addSC("domain-name", "Define the default domain name");
		globalC.no.ip.addSC("dvmrp", "DVMRP global commands");
		globalC.no.ip.addSC("extcommunity-list", "Add a extended community list entry");
		globalC.no.ip.addSC("finger", "finger server");
		globalC.no.ip.addSC("flow-aggregation", "Configure flow aggregation");
		globalC.no.ip.addSC("flow-cache", "Configure netflow cache parameters");
		globalC.no.ip.addSC("flow-export", "Specify host/port to send flow statistics");
		globalC.no.ip.addSC("forward-protocol", "Controls forwarding of physical and directed IP broadcasts");
		globalC.no.ip.addSC("ftp", "FTP configuration commands");
		globalC.no.ip.addSC("gratuitous-arps", "Generate gratuitous ARPs for PPP/SLIP peer addresses");
		globalC.no.ip.addSC("host", "Add an entry to the ip hostname table");
		globalC.no.ip.addSC("host-routing", "Enable host-based routing (proxy ARP and redirect)");
		globalC.no.ip.addSC("http", "HTTP server configuration");
		globalC.no.ip.addSC("icmp", "ICMP options");
		globalC.no.ip.addSC("igmp", "IGMP global configuration");
		globalC.no.ip.addSC("local", "Specify local options");
		globalC.no.ip.addSC("nat", "NAT configuration commands");
		globalC.no.ip.addSC("ospf", "OSPF");
		globalC.no.ip.addSC("reflexive-list", "Reflexive access list");
		globalC.no.ip.addSC("route", "Establish static routes");
		globalC.no.ip.addSC("routing", "Enable IP routing");
		globalC.no.ip.addSC("sap", "Global IP Multicast SAP Commands");
		globalC.no.ip.addSC("subnet-zero", "Allow 'subnet zero' subnets");
		globalC.no.ip.addSC("tacacs", "TACACS configuration commands");
		globalC.no.ip.addSC("tcp", "Global TCP parameters");
		globalC.no.ip.addSC("telnet", "Specify telnet options");
globalC.addSC("ntp", "Configure NTP");
globalC.addSC("parser", "Configure parser");
globalC.addSC("partition", "Partition device");
globalC.addSC("policy-map", "Configure QoS Policy Map");
globalC.addSC("priority-list", "Build a priority list");
globalC.addSC("privilege", "Command privilege parameters");
globalC.addSC("process-max-time", "Maximum time for process to run before voluntarily relinquishing processor");
globalC.addSC("prompt", "Set system's prompt");
globalC.addSC("queue-list", "Build a custom queue list");
globalC.addSC("random-detect-group", "Configure random-detect class");
globalC.addSC("regexp", "regexp commands");
globalC.addSC("resume-string", "Define a host-specific resume string");
globalC.addSC("rif", "Source-route RIF cache");
globalC.addSC("rlogin", "Rlogin configuration commands");
globalC.addSC("rmon", "Remote Monitoring");
globalC.addSC("route-map", "Create route-map or enter route-map command mode");
	globalC["route-map"].addSC("WORD", "Route map tag");
		globalC["route-map"].WORD.addSC("<0-65535>", "Sequence to insert to/delete from existing route-map entry");
		globalC["route-map"].WORD.addSC("deny", "Route map denies set operations");
		globalC["route-map"].WORD.addSC("permit", "Route map permits set operations");
globalC.addSC("router", "Enable a routing process");
	globalC.router.addSC("bgp", "Border Gateway Protocol (BGP)");
		globalC.router.bgp.addSC("<1-65535>", "Autonomous system number");
	globalC.router.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
		globalC.router.eigrp.addSC("<1-65535>", "Autonomous system number");
	globalC.router.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
		globalC.router.igrp.addSC("<1-65535>", "Autonomous system number");
	globalC.router.addSC("ospf", "Open Shortest Path First (OSPF)");
		globalC.router.ospf.addSC("<1-65535>", "Process ID");
	globalC.router.addSC("rip", "Routing Information Protocol (RIP)");
	globalC.router.addSC("static", "Static routes");
globalC.addSC("rtr", "RTR Base Configuration");
globalC.addSC("scheduler", "Scheduler parameters");
globalC.addSC("service", "Modify use of network based services");
globalC.addSC("snmp", "Modify non engine SNMP parameters");
globalC.addSC("snmp-server", "Modify SNMP engine parameters");
globalC.addSC("sntp", "Configure SNTP");
globalC.addSC("stackmaker", "Specify stack name and add its member");
globalC.addSC("standby", "Global HSRP configuration commands");
globalC.addSC("state-machine", "Define a TCP dispatch state machine");
globalC.addSC("subscriber-policy", "Subscriber policy");
globalC.addSC("tacacs-server", "Modify TACACS query parameters");
globalC.addSC("template", "Select a template to configure");
globalC.addSC("terminal-queue", "Terminal queue commands");
globalC.addSC("tftp-server", "Provide TFTP service for netload requests");
globalC.addSC("time-range", "Define time range entries");
globalC.addSC("trunk", "Configure a trunk group");
globalC.addSC("username", "Establish User Name Authentication");
globalC.addSC("virtual-profile", "");
globalC.addSC("virtual-template", "Virtual Template configuration");
globalC.addSC("vpdn", "Virtual Private Dialup Network");
	globalC.vpdn.addSC("aaa", "VPDN AAA related options");
	globalC.vpdn.addSC("domain-delimiter", "Configure VPDN domain delimiter, prefix/suffix");
	globalC.vpdn.addSC("enable", "Enable VPDN");
	globalC.vpdn.addSC("history", "Enable history logging");
	globalC.vpdn.addSC("incoming", "Configure an incoming tunnel");
	globalC.vpdn.addSC("logging", "Configure logging for VPDN");
	globalC.vpdn.addSC("multihop", "Allow VPDN Multihop");
	globalC.vpdn.addSC("outgoing", "Configure an outgoing tunnel");
		globalC.vpdn.outgoing.addSC("WORD", "Name of GW domain");
	globalC.vpdn.addSC("source-ip", "Set Source IP address");
		globalC.vpdn["source-ip"].addSC("A.B.C.D", "IP source");
globalC.addSC("vpdn-group", "VPDN group configuration");
	globalC["vpdn-group"].addSC("WORD", "VPDN Group name");
globalC.addSC("vpdn-template", "VPDN template configuration");
globalC.addSC("x25", "X.25 Level 3");
globalC.addSC("x29", "X29 commands");
globalC.addSC("xot", "Global XOT commands");






