Modules: | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | CS | All |
Module 7: Distance Vector Routing Protocols
Module Overview |
7.1 | Distance Vector Routing
7.1.1 | Distance vector routing updates
7.1.2 | Distance vector routing loop issues
7.1.3 | Defining a maximum count
7.1.4 | Eliminating routing loops through split horizon
7.1.5 | Route poisoning
7.1.6 | Avoiding routing loops with triggered updates
7.1.7 | Preventing routing loops with holddown timers
7.2 | RIP
7.2.1 | RIP routing process
7.2.2 | Configuring RIP
7.2.3 | Using the ip classless command
7.2.4 | Common RIP configuration issues
7.2.5 | Verifying RIP configuration
7.2.6 | Troubleshooting RIP update issues
7.2.7 | Preventing routing updates through an interface
7.2.8 | Load balancing with RIP
7.2.9 | Load balancing across multiple paths
7.2.10 | Integrating static routes with RIP
7.3 | IGRP
7.3.1 | IGRP features
7.3.2 | IGRP metrics
7.3.3 | IGRP routes
7.3.4 | IGRP stability features
7.3.5 | Configuring IGRP
7.3.6 | Migrating RIP to IGRP
7.3.7 | Verifying IGRP configuration
7.3.8 | Troubleshooting IGRP
Module Summary |
Module Quiz |

| Close Window |

| All contents copyright © 2003 Cisco Systems, Inc. All rights reserved.