
routeMapC.addSC("default", "Set a command to its defaults");
routeMapC.addSC("description", "Route-map comment");
routeMapC.addSC("exit", "Exit from route-map configuration mode");
routeMapC.addSC("help", "Description of the interactive help system");
routeMapC.addSC("match", "Match values from routing table");
	routeMapC.match.addSC("interface", "Match first hop interface of route");
		routeMapC.match.interface.addSC("ATM", "ATM interface");
			routeMapC.match.interface.ATM.addSC("<0-0>", "ATM interface number");
		routeMapC.match.interface.addSC("Async", "Async interface");
			routeMapC.match.interface.Async.addSC("<1-0>", "Async interface number");
		routeMapC.match.interface.addSC("BVI", "Bridge-Group Virtual Interface");
			routeMapC.match.interface.BVI.addSC("<1-255>", "BVI interface number");
		routeMapC.match.interface.addSC("CTunnel", "CTunnel interface");
			routeMapC.match.interface.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
		routeMapC.match.interface.addSC("Dialer", "Dialer interface");
			routeMapC.match.interface.Dialer.addSC("<0-255>", "Dialer interface number");
				routeMapC.match.interface.Dialer["<0-255>"].addSC("ATM", "ATM interface");
					routeMapC.match.interface.Dialer["<0-255>"].ATM.addSC("<0-0>", "ATM interface number");
				routeMapC.match.interface.Dialer["<0-255>"].addSC("Async", "Async interface");
					routeMapC.match.interface.Dialer["<0-255>"].Async.addSC("<1-0>", "Async interface number");
				routeMapC.match.interface.Dialer["<0-255>"].addSC("BVI", "Bridge-Group Virtual Interface");
					routeMapC.match.interface.Dialer["<0-255>"].BVI.addSC("<1-255>", "BVI interface number");
				routeMapC.match.interface.Dialer["<0-255>"].addSC("CTunnel", "CTunnel interface");
					routeMapC.match.interface.Dialer["<0-255>"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
		routeMapC.match.interface.addSC("Ethernet", "IEEE 802.3");
			routeMapC.match.interface.Ethernet.addSC("<0-0>", "Ethernet interface number");
				routeMapC.match.interface.Ethernet["<0-0>"].addSC("ATM", "ATM interface");
					routeMapC.match.interface.Ethernet["<0-0>"].ATM.addSC("<0-0>", "ATM interface number");
				routeMapC.match.interface.Ethernet["<0-0>"].addSC("Async", "Async interface");
					routeMapC.match.interface.Ethernet["<0-0>"].Async.addSC("<1-0>", "Async interface number");
				routeMapC.match.interface.Ethernet["<0-0>"].addSC("BVI", "Bridge-Group Virtual Interface");
					routeMapC.match.interface.Ethernet["<0-0>"].BVI.addSC("<1-255>", "BVI interface number");
				routeMapC.match.interface.Ethernet["<0-0>"].addSC("CTunnel", "CTunnel interface");
					routeMapC.match.interface.Ethernet["<0-0>"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				routeMapC.match.interface.Ethernet["<0-0>"].addSC("Dialer", "Dialer interface");
					routeMapC.match.interface.Ethernet["<0-0>"].Dialer.addSC("<0-255>", "Dialer interface number");
						routeMapC.match.interface.Ethernet["<0-0>"].Dialer["<0-255>"].addSC("ATM", "ATM interface");
						routeMapC.match.interface.Ethernet["<0-0>"].Dialer["<0-255>"].addSC("Async", "Async interface");
						routeMapC.match.interface.Ethernet["<0-0>"].Dialer["<0-255>"].addSC("BVI", "Bridge-Group Virtual Interface");
						routeMapC.match.interface.Ethernet["<0-0>"].Dialer["<0-255>"].addSC("CTunnel", "CTunnel interface");
		routeMapC.match.interface.addSC("Lex", "Lex interface");
			routeMapC.match.interface.Lex.addSC("<0-2147483647>", "Lex interface number");
		routeMapC.match.interface.addSC("Loopback", "Loopback interface");
			routeMapC.match.interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routeMapC.match.interface.Loopback["<0-2147483647>"].addSC("ATM", "ATM interface");
					routeMapC.match.interface.Loopback["<0-2147483647>"].ATM.addSC("<0-0>", "ATM interface number");
				routeMapC.match.interface.Loopback["<0-2147483647>"].addSC("Async", "Async interface");
					routeMapC.match.interface.Loopback["<0-2147483647>"].Async.addSC("<1-0>", "Async interface number");
				routeMapC.match.interface.Loopback["<0-2147483647>"].addSC("BVI", "Bridge-Group Virtual Interface");
					routeMapC.match.interface.Loopback["<0-2147483647>"].BVI.addSC("<1-255>", "BVI interface number");
				routeMapC.match.interface.Loopback["<0-2147483647>"].addSC("CTunnel", "CTunnel interface");
					routeMapC.match.interface.Loopback["<0-2147483647>"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				routeMapC.match.interface.Loopback["<0-2147483647>"].addSC("Dialer", "Dialer interface");
					routeMapC.match.interface.Loopback["<0-2147483647>"].Dialer.addSC("<0-255>", "Dialer interface number");
						routeMapC.match.interface.Loopback["<0-2147483647>"].Dialer["<0-255>"].addSC("ATM", "ATM interface");
						routeMapC.match.interface.Loopback["<0-2147483647>"].Dialer["<0-255>"].addSC("Async", "Async interface");
						routeMapC.match.interface.Loopback["<0-2147483647>"].Dialer["<0-255>"].addSC("BVI", "Bridge-Group Virtual Interface");
						routeMapC.match.interface.Loopback["<0-2147483647>"].Dialer["<0-255>"].addSC("CTunnel", "CTunnel interface");
				routeMapC.match.interface.Loopback["<0-2147483647>"].addSC("Ethernet", "IEEE 802.3");
					routeMapC.match.interface.Loopback["<0-2147483647>"].Ethernet.addSC("<0-0>", "Ethernet interface number");
						routeMapC.match.interface.Loopback["<0-2147483647>"].Ethernet["<0-0>"].addSC("ATM", "ATM interface");
						routeMapC.match.interface.Loopback["<0-2147483647>"].Ethernet["<0-0>"].addSC("Async", "Async interface");
						routeMapC.match.interface.Loopback["<0-2147483647>"].Ethernet["<0-0>"].addSC("BVI", "Bridge-Group Virtual Interface");
						routeMapC.match.interface.Loopback["<0-2147483647>"].Ethernet["<0-0>"].addSC("CTunnel", "CTunnel interface");
						routeMapC.match.interface.Loopback["<0-2147483647>"].Ethernet["<0-0>"].addSC("Dialer", "Dialer interface");
				routeMapC.match.interface.Loopback["<0-2147483647>"].addSC("Lex", "Lex interface");
					routeMapC.match.interface.Loopback["<0-2147483647>"].Lex.addSC("<0-2147483647>", "Lex interface number");
		routeMapC.match.interface.addSC("Multilink", "Multilink-group interface");
			routeMapC.match.interface.Multilink.addSC("<0-2147483647>", "Multilink interface number");
		routeMapC.match.interface.addSC("Null", "Null interface");
			routeMapC.match.interface.Null.addSC("<0-0>", "Null interface number");
				routeMapC.match.interface.Null["<0-0>"].addSC("ATM", "ATM interface");
					routeMapC.match.interface.Null["<0-0>"].ATM.addSC("<0-0>", "ATM interface number");
				routeMapC.match.interface.Null["<0-0>"].addSC("Async", "Async interface");
					routeMapC.match.interface.Null["<0-0>"].Async.addSC("<1-0>", "Async interface number");
				routeMapC.match.interface.Null["<0-0>"].addSC("BVI", "Bridge-Group Virtual Interface");
					routeMapC.match.interface.Null["<0-0>"].BVI.addSC("<1-255>", "BVI interface number");
				routeMapC.match.interface.Null["<0-0>"].addSC("CTunnel", "CTunnel interface");
					routeMapC.match.interface.Null["<0-0>"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				routeMapC.match.interface.Null["<0-0>"].addSC("Dialer", "Dialer interface");
					routeMapC.match.interface.Null["<0-0>"].Dialer.addSC("<0-255>", "Dialer interface number");
						routeMapC.match.interface.Null["<0-0>"].Dialer["<0-255>"].addSC("ATM", "ATM interface");
						routeMapC.match.interface.Null["<0-0>"].Dialer["<0-255>"].addSC("Async", "Async interface");
						routeMapC.match.interface.Null["<0-0>"].Dialer["<0-255>"].addSC("BVI", "Bridge-Group Virtual Interface");
						routeMapC.match.interface.Null["<0-0>"].Dialer["<0-255>"].addSC("CTunnel", "CTunnel interface");
				routeMapC.match.interface.Null["<0-0>"].addSC("Ethernet", "IEEE 802.3");
					routeMapC.match.interface.Null["<0-0>"].Ethernet.addSC("<0-0>", "Ethernet interface number");
						routeMapC.match.interface.Null["<0-0>"].Ethernet["<0-0>"].addSC("ATM", "ATM interface");
						routeMapC.match.interface.Null["<0-0>"].Ethernet["<0-0>"].addSC("Async", "Async interface");
						routeMapC.match.interface.Null["<0-0>"].Ethernet["<0-0>"].addSC("BVI", "Bridge-Group Virtual Interface");
						routeMapC.match.interface.Null["<0-0>"].Ethernet["<0-0>"].addSC("CTunnel", "CTunnel interface");
						routeMapC.match.interface.Null["<0-0>"].Ethernet["<0-0>"].addSC("Dialer", "Dialer interface");
				routeMapC.match.interface.Null["<0-0>"].addSC("Lex", "Lex interface");
					routeMapC.match.interface.Null["<0-0>"].Lex.addSC("<0-2147483647>", "Lex interface number");
				routeMapC.match.interface.Null["<0-0>"].addSC("Loopback", "Loopback interface");
					routeMapC.match.interface.Null["<0-0>"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
						routeMapC.match.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("ATM", "ATM interface");
						routeMapC.match.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("Async", "Async interface");
						routeMapC.match.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("BVI", "Bridge-Group Virtual Interface");
						routeMapC.match.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("CTunnel", "CTunnel interface");
						routeMapC.match.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("Dialer", "Dialer interface");
						routeMapC.match.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("Ethernet", "IEEE 802.3");
						routeMapC.match.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("Lex", "Lex interface");
				routeMapC.match.interface.Null["<0-0>"].addSC("Multilink", "Multilink-group interface");
					routeMapC.match.interface.Null["<0-0>"].Multilink.addSC("<0-2147483647>", "Multilink interface number");
		routeMapC.match.interface.addSC("Tunnel", "Tunnel interface");
			routeMapC.match.interface.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
		routeMapC.match.interface.addSC("Vif", "PGM Multicast Host interface");
			routeMapC.match.interface.Vif.addSC("<1-1>", "Vif interface number");
		routeMapC.match.interface.addSC("Virtual-Template", "Virtual Template interface");
			routeMapC.match.interface["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
		routeMapC.match.interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
			routeMapC.match.interface["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
	routeMapC.match.addSC("ip", "IP specific information");
		routeMapC.match.ip.addSC("address", "Match address of route or match packet");
			routeMapC.match.ip.address.addSC("<1-199>", "IP access-list number");
			routeMapC.match.ip.address.addSC("<1300-2699>", "IP access-list number (expanded range)");
				routeMapC.match.ip.address["<1300-2699>"].addSC("<1-199>", "IP access-list number");
			routeMapC.match.ip.address.addSC("WORD", "IP access-list name");
				routeMapC.match.ip.address.WORD.addSC("<1-199>", "IP access-list number");
				routeMapC.match.ip.address.WORD.addSC("<1300-2699>", "IP access-list number (expanded range)");
					routeMapC.match.ip.address.WORD["<1300-2699>"].addSC("<1-199>", "IP access-list number");
			routeMapC.match.ip.address.addSC("prefix-list", "Match entries of prefix-lists");
				routeMapC.match.ip.address["prefix-list"].addSC("WORD", "IP prefix-list name");
		routeMapC.match.ip.addSC("next-hop", "Match next-hop address of route");
			routeMapC.match.ip["next-hop"].addSC("<1-99>", "IP access-list number");
			routeMapC.match.ip["next-hop"].addSC("<1300-1999>", "IP access-list number (expanded range)");
				routeMapC.match.ip["next-hop"]["<1300-1999>"].addSC("<1-99>", "IP access-list number");
			routeMapC.match.ip["next-hop"].addSC("WORD", "IP standard access-list name");
				routeMapC.match.ip["next-hop"].WORD.addSC("<1-99>", "IP access-list number");
				routeMapC.match.ip["next-hop"].WORD.addSC("<1300-1999>", "IP access-list number (expanded range)");
					routeMapC.match.ip["next-hop"].WORD["<1300-1999>"].addSC("<1-99>", "IP access-list number");
			routeMapC.match.ip["next-hop"].addSC("prefix-list", "Match entries of prefix-lists");
				routeMapC.match.ip["next-hop"]["prefix-list"].addSC("WORD", "IP prefix-list name");
		routeMapC.match.ip.addSC("route-source", "Match advertising source address of route");
			routeMapC.match.ip["route-source"].addSC("<1-99>", "IP access-list number");
			routeMapC.match.ip["route-source"].addSC("<1300-1999>", "IP access-list number (expanded range)");
				routeMapC.match.ip["route-source"]["<1300-1999>"].addSC("<1-99>", "IP access-list number");
			routeMapC.match.ip["route-source"].addSC("WORD", "IP standard access-list name");
				routeMapC.match.ip["route-source"].WORD.addSC("<1-99>", "IP access-list number");
				routeMapC.match.ip["route-source"].WORD.addSC("<1300-1999>", "IP access-list number (expanded range)");
					routeMapC.match.ip["route-source"].WORD["<1300-1999>"].addSC("<1-99>", "IP access-list number");
			routeMapC.match.ip["route-source"].addSC("prefix-list", "Match entries of prefix-lists");
				routeMapC.match.ip["route-source"]["prefix-list"].addSC("WORD", "IP prefix-list name");
	routeMapC.match.addSC("metric", "Match metric of route");
		routeMapC.match.metric.addSC("<0-4294967295>", "Metric value");
	routeMapC.match.addSC("route-type", "Match route-type of route");
	routeMapC.match.addSC("tag", "Match tag of route");
		routeMapC.match.tag.addSC("<0-4294967295>", "Tag value");
routeMapC.addSC("no", "Negate a command or set its defaults");
routeMapC.addSC("set", "Set values in destination routing protocol");
	routeMapC.set.addSC("automatic-tag", "Automatically compute TAG value");
	routeMapC.set.addSC("default", "Set default information");
		routeMapC.set["default"].addSC("interface", "Default output interface");
	routeMapC.set.addSC("interface", "Output interface");
		routeMapC.set.interface.addSC("ATM", "ATM interface");
			routeMapC.set.interface.ATM.addSC("<0-0>", "ATM interface number");
		routeMapC.set.interface.addSC("Async", "Async interface");
			routeMapC.set.interface.Async.addSC("<1-0>", "Async interface number");
		routeMapC.set.interface.addSC("BVI", "Bridge-Group Virtual Interface");
			routeMapC.set.interface.BVI.addSC("<1-255>", "BVI interface number");
		routeMapC.set.interface.addSC("CTunnel", "CTunnel interface");
			routeMapC.set.interface.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
		routeMapC.set.interface.addSC("Dialer", "Dialer interface");
			routeMapC.set.interface.Dialer.addSC("<0-255>", "Dialer interface number");
				routeMapC.set.interface.Dialer["<0-255>"].addSC("ATM", "ATM interface");
					routeMapC.set.interface.Dialer["<0-255>"].ATM.addSC("<0-0>", "ATM interface number");
				routeMapC.set.interface.Dialer["<0-255>"].addSC("Async", "Async interface");
					routeMapC.set.interface.Dialer["<0-255>"].Async.addSC("<1-0>", "Async interface number");
				routeMapC.set.interface.Dialer["<0-255>"].addSC("BVI", "Bridge-Group Virtual Interface");
					routeMapC.set.interface.Dialer["<0-255>"].BVI.addSC("<1-255>", "BVI interface number");
				routeMapC.set.interface.Dialer["<0-255>"].addSC("CTunnel", "CTunnel interface");
					routeMapC.set.interface.Dialer["<0-255>"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
		routeMapC.set.interface.addSC("Ethernet", "IEEE 802.3");
			routeMapC.set.interface.Ethernet.addSC("<0-0>", "Ethernet interface number");
				routeMapC.set.interface.Ethernet["<0-0>"].addSC("ATM", "ATM interface");
					routeMapC.set.interface.Ethernet["<0-0>"].ATM.addSC("<0-0>", "ATM interface number");
				routeMapC.set.interface.Ethernet["<0-0>"].addSC("Async", "Async interface");
					routeMapC.set.interface.Ethernet["<0-0>"].Async.addSC("<1-0>", "Async interface number");
				routeMapC.set.interface.Ethernet["<0-0>"].addSC("BVI", "Bridge-Group Virtual Interface");
					routeMapC.set.interface.Ethernet["<0-0>"].BVI.addSC("<1-255>", "BVI interface number");
				routeMapC.set.interface.Ethernet["<0-0>"].addSC("CTunnel", "CTunnel interface");
					routeMapC.set.interface.Ethernet["<0-0>"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				routeMapC.set.interface.Ethernet["<0-0>"].addSC("Dialer", "Dialer interface");
					routeMapC.set.interface.Ethernet["<0-0>"].Dialer.addSC("<0-255>", "Dialer interface number");
						routeMapC.set.interface.Ethernet["<0-0>"].Dialer["<0-255>"].addSC("ATM", "ATM interface");
						routeMapC.set.interface.Ethernet["<0-0>"].Dialer["<0-255>"].addSC("Async", "Async interface");
						routeMapC.set.interface.Ethernet["<0-0>"].Dialer["<0-255>"].addSC("BVI", "Bridge-Group Virtual Interface");
						routeMapC.set.interface.Ethernet["<0-0>"].Dialer["<0-255>"].addSC("CTunnel", "CTunnel interface");
		routeMapC.set.interface.addSC("Lex", "Lex interface");
			routeMapC.set.interface.Lex.addSC("<0-2147483647>", "Lex interface number");
		routeMapC.set.interface.addSC("Loopback", "Loopback interface");
			routeMapC.set.interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routeMapC.set.interface.Loopback["<0-2147483647>"].addSC("ATM", "ATM interface");
					routeMapC.set.interface.Loopback["<0-2147483647>"].ATM.addSC("<0-0>", "ATM interface number");
				routeMapC.set.interface.Loopback["<0-2147483647>"].addSC("Async", "Async interface");
					routeMapC.set.interface.Loopback["<0-2147483647>"].Async.addSC("<1-0>", "Async interface number");
				routeMapC.set.interface.Loopback["<0-2147483647>"].addSC("BVI", "Bridge-Group Virtual Interface");
					routeMapC.set.interface.Loopback["<0-2147483647>"].BVI.addSC("<1-255>", "BVI interface number");
				routeMapC.set.interface.Loopback["<0-2147483647>"].addSC("CTunnel", "CTunnel interface");
					routeMapC.set.interface.Loopback["<0-2147483647>"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				routeMapC.set.interface.Loopback["<0-2147483647>"].addSC("Dialer", "Dialer interface");
					routeMapC.set.interface.Loopback["<0-2147483647>"].Dialer.addSC("<0-255>", "Dialer interface number");
						routeMapC.set.interface.Loopback["<0-2147483647>"].Dialer["<0-255>"].addSC("ATM", "ATM interface");
						routeMapC.set.interface.Loopback["<0-2147483647>"].Dialer["<0-255>"].addSC("Async", "Async interface");
						routeMapC.set.interface.Loopback["<0-2147483647>"].Dialer["<0-255>"].addSC("BVI", "Bridge-Group Virtual Interface");
						routeMapC.set.interface.Loopback["<0-2147483647>"].Dialer["<0-255>"].addSC("CTunnel", "CTunnel interface");
				routeMapC.set.interface.Loopback["<0-2147483647>"].addSC("Ethernet", "IEEE 802.3");
					routeMapC.set.interface.Loopback["<0-2147483647>"].Ethernet.addSC("<0-0>", "Ethernet interface number");
						routeMapC.set.interface.Loopback["<0-2147483647>"].Ethernet["<0-0>"].addSC("ATM", "ATM interface");
						routeMapC.set.interface.Loopback["<0-2147483647>"].Ethernet["<0-0>"].addSC("Async", "Async interface");
						routeMapC.set.interface.Loopback["<0-2147483647>"].Ethernet["<0-0>"].addSC("BVI", "Bridge-Group Virtual Interface");
						routeMapC.set.interface.Loopback["<0-2147483647>"].Ethernet["<0-0>"].addSC("CTunnel", "CTunnel interface");
						routeMapC.set.interface.Loopback["<0-2147483647>"].Ethernet["<0-0>"].addSC("Dialer", "Dialer interface");
				routeMapC.set.interface.Loopback["<0-2147483647>"].addSC("Lex", "Lex interface");
					routeMapC.set.interface.Loopback["<0-2147483647>"].Lex.addSC("<0-2147483647>", "Lex interface number");
		routeMapC.set.interface.addSC("Multilink", "Multilink-group interface");
			routeMapC.set.interface.Multilink.addSC("<0-2147483647>", "Multilink interface number");
		routeMapC.set.interface.addSC("Null", "Null interface");
			routeMapC.set.interface.Null.addSC("<0-0>", "Null interface number");
				routeMapC.set.interface.Null["<0-0>"].addSC("ATM", "ATM interface");
					routeMapC.set.interface.Null["<0-0>"].ATM.addSC("<0-0>", "ATM interface number");
				routeMapC.set.interface.Null["<0-0>"].addSC("Async", "Async interface");
					routeMapC.set.interface.Null["<0-0>"].Async.addSC("<1-0>", "Async interface number");
				routeMapC.set.interface.Null["<0-0>"].addSC("BVI", "Bridge-Group Virtual Interface");
					routeMapC.set.interface.Null["<0-0>"].BVI.addSC("<1-255>", "BVI interface number");
				routeMapC.set.interface.Null["<0-0>"].addSC("CTunnel", "CTunnel interface");
					routeMapC.set.interface.Null["<0-0>"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				routeMapC.set.interface.Null["<0-0>"].addSC("Dialer", "Dialer interface");
					routeMapC.set.interface.Null["<0-0>"].Dialer.addSC("<0-255>", "Dialer interface number");
						routeMapC.set.interface.Null["<0-0>"].Dialer["<0-255>"].addSC("ATM", "ATM interface");
						routeMapC.set.interface.Null["<0-0>"].Dialer["<0-255>"].addSC("Async", "Async interface");
						routeMapC.set.interface.Null["<0-0>"].Dialer["<0-255>"].addSC("BVI", "Bridge-Group Virtual Interface");
						routeMapC.set.interface.Null["<0-0>"].Dialer["<0-255>"].addSC("CTunnel", "CTunnel interface");
				routeMapC.set.interface.Null["<0-0>"].addSC("Ethernet", "IEEE 802.3");
					routeMapC.set.interface.Null["<0-0>"].Ethernet.addSC("<0-0>", "Ethernet interface number");
						routeMapC.set.interface.Null["<0-0>"].Ethernet["<0-0>"].addSC("ATM", "ATM interface");
						routeMapC.set.interface.Null["<0-0>"].Ethernet["<0-0>"].addSC("Async", "Async interface");
						routeMapC.set.interface.Null["<0-0>"].Ethernet["<0-0>"].addSC("BVI", "Bridge-Group Virtual Interface");
						routeMapC.set.interface.Null["<0-0>"].Ethernet["<0-0>"].addSC("CTunnel", "CTunnel interface");
						routeMapC.set.interface.Null["<0-0>"].Ethernet["<0-0>"].addSC("Dialer", "Dialer interface");
				routeMapC.set.interface.Null["<0-0>"].addSC("Lex", "Lex interface");
					routeMapC.set.interface.Null["<0-0>"].Lex.addSC("<0-2147483647>", "Lex interface number");
				routeMapC.set.interface.Null["<0-0>"].addSC("Loopback", "Loopback interface");
					routeMapC.set.interface.Null["<0-0>"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
						routeMapC.set.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("ATM", "ATM interface");
						routeMapC.set.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("Async", "Async interface");
						routeMapC.set.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("BVI", "Bridge-Group Virtual Interface");
						routeMapC.set.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("CTunnel", "CTunnel interface");
						routeMapC.set.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("Dialer", "Dialer interface");
						routeMapC.set.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("Ethernet", "IEEE 802.3");
						routeMapC.set.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("Lex", "Lex interface");
				routeMapC.set.interface.Null["<0-0>"].addSC("Multilink", "Multilink-group interface");
					routeMapC.set.interface.Null["<0-0>"].Multilink.addSC("<0-2147483647>", "Multilink interface number");
		routeMapC.set.interface.addSC("Tunnel", "Tunnel interface");
			routeMapC.set.interface.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
		routeMapC.set.interface.addSC("Vif", "PGM Multicast Host interface");
			routeMapC.set.interface.Vif.addSC("<1-1>", "Vif interface number");
		routeMapC.set.interface.addSC("Virtual-Template", "Virtual Template interface");
			routeMapC.set.interface["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
		routeMapC.set.interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
			routeMapC.set.interface["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
	routeMapC.set.addSC("ip", "IP specific information");
		routeMapC.set.ip.addSC("default", "Set default information");
			routeMapC.set.ip["default"].addSC("next-hop", "Next hop along path");
				routeMapC.set.ip["default"]["next-hop"].addSC("A.B.C.D", "Default next hop IP address");
				routeMapC.set.ip["default"]["next-hop"].addSC("verify-availability", "Verify if default nexthop is a CDP neighbor");
		routeMapC.set.ip.addSC("df", "Set DF bit");
			routeMapC.set.ip.df.addSC("<0-1>", "DF bit");
		routeMapC.set.ip.addSC("next-hop", "Next hop address");
			routeMapC.set.ip["next-hop"].addSC("A.B.C.D", "IP address of next hop");
			routeMapC.set.ip["next-hop"].addSC("peer-address", "Use peer address (for BGP only)");
			routeMapC.set.ip["next-hop"].addSC("verify-availability", "Verify if nexthop is a CDP neighbor");
		routeMapC.set.ip.addSC("precedence", "Set precedence field");
		routeMapC.set.ip.addSC("qos-group", "Set QOS Group ID");
			routeMapC.set.ip["qos-group"].addSC("<0-99>", "QOS Group ID");
		routeMapC.set.ip.addSC("tos", "Set type of service field");
			routeMapC.set.ip.tos.addSC("<0-15>", "Type of service value");
			routeMapC.set.ip.tos.addSC("max-reliability", "Set max reliable TOS (2)");
			routeMapC.set.ip.tos.addSC("max-throughput", "Set max throughput TOS (4)");
			routeMapC.set.ip.tos.addSC("min-delay", "Set min delay TOS (8)");
			routeMapC.set.ip.tos.addSC("min-monetary-cost", "Set min monetary cost TOS (1)");
			routeMapC.set.ip.tos.addSC("normal", "Set normal TOS (0)");
	routeMapC.set.addSC("level", "Where to import route");
		routeMapC.set.level.addSC("backbone", "Import into OSPF backbone area");
		routeMapC.set.level.addSC("level-1", "Import into a level-1 area");
		routeMapC.set.level.addSC("level-1-2", "Import into level-1 and level-2");
		routeMapC.set.level.addSC("level-2", "Import into level-2 sub-domain");
		routeMapC.set.level.addSC("stub-area", "Import into OSPF NSSA area");
	routeMapC.set.addSC("metric", "Metric value for destination routing protocol");
		routeMapC.set.metric.addSC("+/-<metric>", "Add or subtract metric");
		routeMapC.set.metric.addSC("<0-4294967295>", "Metric value or Bandwidth in Kbits per second");
			routeMapC.set.metric["<0-4294967295>"].addSC("+/-<delay>", "Add or subtract delay");
			routeMapC.set.metric["<0-4294967295>"].addSC("<1-4294967295>", "IGRP delay metric, in 10 microsecond units");
				routeMapC.set.metric["<0-4294967295>"]["<1-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
					routeMapC.set.metric["<0-4294967295>"]["<1-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
						routeMapC.set.metric["<0-4294967295>"]["<1-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
	routeMapC.set.addSC("metric-type", "Type of metric for destination routing protocol");
		routeMapC.set["metric-type"].addSC("external", "IS-IS external metric");
		routeMapC.set["metric-type"].addSC("internal", "Use IGP metric as the MED for BGP");
		routeMapC.set["metric-type"].addSC("type-1", "OSPF external type 1 metric");
		routeMapC.set["metric-type"].addSC("type-2", "OSPF external type 2 metric");
	routeMapC.set.addSC("tag", "Tag value for destination routing protocol");
		routeMapC.set.tag.addSC("<0-4294967295>", "Tag value");
