      enableC.show.ip.addSC("nhrp", "NHRP information");
      enableC.show.ip.addSC("ospf", "OSPF information");
				enableC.show.ip.ospf.interface.addSC("Async", "Async interface");
					enableC.show.ip.ospf.interface.Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf.interface.addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf.interface.BRI.addSC("<0-6>", "BRI interface number");
				enableC.show.ip.ospf.interface.addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf.interface.BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.ospf.interface.addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf.interface.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.ospf.interface.addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf.interface.Dialer.addSC("<0-799>", "Dialer interface number");
				enableC.show.ip.ospf.interface.addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf.interface.Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf.interface.addSC("Lex", "Lex interface");
					enableC.show.ip.ospf.interface.Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.ospf.interface.addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf.interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				enableC.show.ip.ospf.interface.addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf.interface.Multilink.addSC("<1-2147483647>", "Multilink interface number");
				enableC.show.ip.ospf.interface.addSC("Null", "Null interface");
					enableC.show.ip.ospf.interface.Null.addSC("<0-0>", "Null interface number");
				enableC.show.ip.ospf.interface.addSC("Serial", "Serial");
					enableC.show.ip.ospf.interface.Serial.addSC("<0-6>", "Serial interface number");
				enableC.show.ip.ospf.interface.addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf.interface.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.ospf.interface.addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf.interface.Vif.addSC("<1-1>", "Vif interface number");
				enableC.show.ip.ospf.interface.addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.ospf.interface["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
				enableC.show.ip.ospf.interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
					enableC.show.ip.ospf.interface["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			enableC.show.ip.ospf.addSC("mpls", "MPLS related information");
				enableC.show.ip.ospf.mpls.addSC("traffic-eng", "Traffic Engineering information");
					enableC.show.ip.ospf.mpls["traffic-eng"].addSC("fragment", "MPLS fragment information");
					enableC.show.ip.ospf.mpls["traffic-eng"].addSC("link", "MPLS link information");
			enableC.show.ip.ospf.addSC("neighbor", "Neighbor list");
				enableC.show.ip.ospf.neighbor.addSC("Async", "Async interface");
					enableC.show.ip.ospf.neighbor.Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf.neighbor.addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf.neighbor.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.BRI.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.BRI.Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf.neighbor.addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf.neighbor.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.BVI.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.BVI.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.BVI.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.BVI.BRI.addSC("<0-6>", "BRI interface number");
				enableC.show.ip.ospf.neighbor.addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf.neighbor.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.CTunnel.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.CTunnel.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.CTunnel.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.CTunnel.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.CTunnel.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.CTunnel.BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.ospf.neighbor.addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Dialer.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Dialer.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Dialer.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Dialer.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.ospf.neighbor.addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Ethernet.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Ethernet.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Ethernet.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Ethernet.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Ethernet.Dialer.addSC("<0-799>", "Dialer interface number");
				enableC.show.ip.ospf.neighbor.addSC("Hostname or A.B.C.D", "Neighbor ID");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf.neighbor.addSC("Lex", "Lex interface");
					enableC.show.ip.ospf.neighbor.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Lex.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Lex.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Lex.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Lex.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Lex.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Lex.Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf.neighbor.addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("<0-2147483647>", "Loopback interface number");
						enableC.show.ip.ospf.neighbor.Loopback["<0-2147483647>"].addSC("Hostname or A.B.C.D", "Neighbor ID");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Loopback.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Loopback.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Loopback.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Loopback.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Loopback.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Loopback.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Loopback.Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.ospf.neighbor.addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Multilink.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Multilink.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Multilink.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Multilink.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Multilink.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Multilink.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Multilink.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Multilink.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				enableC.show.ip.ospf.neighbor.addSC("Null", "Null interface");
					enableC.show.ip.ospf.neighbor.Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.ospf.neighbor.Null["<0-0>"].addSC("Hostname or A.B.C.D", "Neighbor ID");
					enableC.show.ip.ospf.neighbor.Null.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Null.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Null.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Null.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Null.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Null.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Null.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Null.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Null.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.Null.Multilink.addSC("<1-2147483647>", "Multilink interface number");
				enableC.show.ip.ospf.neighbor.addSC("Serial", "Serial");
					enableC.show.ip.ospf.neighbor.Serial.addSC("<0-6>", "Serial interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Serial.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Serial.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Serial.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Serial.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Serial.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Serial.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Serial.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Serial.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.Serial.Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.Serial.Null.addSC("<0-0>", "Null interface number");
				enableC.show.ip.ospf.neighbor.addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Tunnel.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Tunnel.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Tunnel.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Tunnel.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.Tunnel.Serial.addSC("<0-6>", "Serial interface number");
				enableC.show.ip.ospf.neighbor.addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf.neighbor.Vif.addSC("<1-1>", "Vif interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Vif.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Vif.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Vif.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Vif.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Vif.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Vif.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Vif.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Vif.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.Vif.Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.Vif.Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.Vif.Serial.addSC("<0-6>", "Serial interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor.Vif.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.ospf.neighbor.addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Serial.addSC("<0-6>", "Serial interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Vif", "PGM Multicast Host interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Vif.addSC("<1-1>", "Vif interface number");
				enableC.show.ip.ospf.neighbor.addSC("Virtual-TokenRing", "Virtual TokenRing");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Serial.addSC("<0-6>", "Serial interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Vif", "PGM Multicast Host interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Vif.addSC("<1-1>", "Vif interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Virtual-Template", "Virtual Template interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"]["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
				enableC.show.ip.ospf.neighbor.addSC("detail", "detail of all neighbors");
					enableC.show.ip.ospf.neighbor.detail.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.detail.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.BRI.addSC("<0-6>", "BRI interface number");
						enableC.show.ip.ospf.neighbor.detail.BRI.addSC("Async", "Async interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.BVI.addSC("<1-255>", "BVI interface number");
						enableC.show.ip.ospf.neighbor.detail.BVI.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.BVI.addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
						enableC.show.ip.ospf.neighbor.detail.CTunnel.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.CTunnel.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.CTunnel.addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("<0-799>", "Dialer interface number");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("<0-6>", "Ethernet interface number");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Hostname or A.B.C.D", "Neighbor ID");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf.neighbor.detail.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("<0-2147483647>", "Lex interface number");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf.neighbor.detail.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("<0-2147483647>", "Loopback interface number");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("Lex", "Lex interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("<1-2147483647>", "Multilink interface number");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("<0-6>", "Serial interface number");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Null", "Null interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Serial", "Serial");
					enableC.show.ip.ospf.neighbor.detail.addSC("Vif", "PGM Multicast Host interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("<1-1>", "Vif interface number");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Virtual-Template", "Virtual Template interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Virtual-TokenRing", "Virtual TokenRing");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Vif", "PGM Multicast Host interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Virtual-Template", "Virtual Template interface");
			enableC.show.ip.ospf.addSC("request-list", "Link state request list");
				enableC.show.ip.ospf["request-list"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["request-list"].addSC("Async", "Async interface");
					enableC.show.ip.ospf["request-list"].Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf["request-list"].addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf["request-list"].BRI.addSC("<0-6>", "BRI interface number");
				enableC.show.ip.ospf["request-list"].addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf["request-list"].BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.ospf["request-list"].addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf["request-list"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.ospf["request-list"].addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf["request-list"].Dialer.addSC("<0-799>", "Dialer interface number");
						enableC.show.ip.ospf["request-list"].Dialer["<0-799>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["request-list"].addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf["request-list"].Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf["request-list"].addSC("Lex", "Lex interface");
					enableC.show.ip.ospf["request-list"].Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.ospf["request-list"].addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf["request-list"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
						enableC.show.ip.ospf["request-list"].Loopback["<0-2147483647>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["request-list"].addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf["request-list"].Multilink.addSC("<1-2147483647>", "Multilink interface number");
				enableC.show.ip.ospf["request-list"].addSC("Null", "Null interface");
					enableC.show.ip.ospf["request-list"].Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.ospf["request-list"].Null["<0-0>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["request-list"].addSC("Serial", "Serial");
					enableC.show.ip.ospf["request-list"].Serial.addSC("<0-6>", "Serial interface number");
				enableC.show.ip.ospf["request-list"].addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf["request-list"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.ospf["request-list"].addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf["request-list"].Vif.addSC("<1-1>", "Vif interface number");
				enableC.show.ip.ospf["request-list"].addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.ospf["request-list"]["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
				enableC.show.ip.ospf["request-list"].addSC("Virtual-TokenRing", "Virtual TokenRing");
					enableC.show.ip.ospf["request-list"]["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			enableC.show.ip.ospf.addSC("retransmission-list", "Link state retransmission list");
				enableC.show.ip.ospf["retransmission-list"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["retransmission-list"].addSC("Async", "Async interface");
					enableC.show.ip.ospf["retransmission-list"].Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf["retransmission-list"].BRI.addSC("<0-6>", "BRI interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf["retransmission-list"].BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf["retransmission-list"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf["retransmission-list"].Dialer.addSC("<0-799>", "Dialer interface number");
						enableC.show.ip.ospf["retransmission-list"].Dialer["<0-799>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["retransmission-list"].addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf["retransmission-list"].Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Lex", "Lex interface");
					enableC.show.ip.ospf["retransmission-list"].Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf["retransmission-list"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
						enableC.show.ip.ospf["retransmission-list"].Loopback["<0-2147483647>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["retransmission-list"].addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf["retransmission-list"].Multilink.addSC("<1-2147483647>", "Multilink interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Null", "Null interface");
					enableC.show.ip.ospf["retransmission-list"].Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.ospf["retransmission-list"].Null["<0-0>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["retransmission-list"].addSC("Serial", "Serial");
					enableC.show.ip.ospf["retransmission-list"].Serial.addSC("<0-6>", "Serial interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf["retransmission-list"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf["retransmission-list"].Vif.addSC("<1-1>", "Vif interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.ospf["retransmission-list"]["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Virtual-TokenRing", "Virtual TokenRing");
					enableC.show.ip.ospf["retransmission-list"]["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			enableC.show.ip.ospf.addSC("summary-address", "Summary-address redistribution Information");
			enableC.show.ip.ospf.addSC("virtual-links", "Virtual link information");
      enableC.show.ip.addSC("pgm", "PGM Reliable Transport Protocol");
      enableC.show.ip.addSC("pim", "PIM information");
      enableC.show.ip.addSC("policy", "Policy routing");
      enableC.show.ip.addSC("port-map", "Port to Application Mapping (PAM) information");
      enableC.show.ip.addSC("prefix-list", "List IP prefix lists");
      enableC.show.ip.addSC("protocols", "IP routing protocol process parameters and statistics");
         enableC.show.ip.protocols.addSC("summary", "Short form answer");
         enableC.show.ip.protocols.addSC("vrf", "Display protocols for a VPN Routing/Forwarding instance");
      enableC.show.ip.addSC("redirects", "IP redirects");
      enableC.show.ip.addSC("rip", "IP RIP show commands");
      enableC.show.ip.addSC("route", "IP routing table");
         enableC.show.ip.route.addSC("bgp", "Border Gateway Protocol (BGP)");
            enableC.show.ip.route.bgp.addSC("<1-65535>", "Autonomous system number");
         enableC.show.ip.route.addSC("connected", "Connected");
         enableC.show.ip.route.addSC("egp", "Exterior Gateway Protocol (EGP)");
            enableC.show.ip.route.egp.addSC("<0-65535>", "Remote autonomous system number");
         enableC.show.ip.route.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
            enableC.show.ip.route.eigrp.addSC("<1-65535>", "Autonomous system number");
         enableC.show.ip.route.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
            enableC.show.ip.route.igrp.addSC("<1-65535>", "Autonomous system number");
         enableC.show.ip.route.addSC("isis", "ISO IS-IS");
            enableC.show.ip.route.isis.addSC("WORD", "ISO routing area tag");
         enableC.show.ip.route.addSC("list", "IP Access list");
            enableC.show.ip.route.list.addSC("<1-199>", "IP access list number");
         enableC.show.ip.route.addSC("mobile", "Mobile routes");
         enableC.show.ip.route.addSC("odr", "On Demand stub Routes");
         enableC.show.ip.route.addSC("ospf", "Open Shortest Path First (OSPF)");
            enableC.show.ip.route.ospf.addSC("<1-65535>", "Process ID");
         enableC.show.ip.route.addSC("profile", "IP routing table profile");
         enableC.show.ip.route.addSC("rip", "Routing Information Protocol (RIP)");
         enableC.show.ip.route.addSC("static", "Static routes");
         enableC.show.ip.route.addSC("summary", "Summary of all routes");
         enableC.show.ip.route.addSC("supernets-only", "Show supernet entries only");
         enableC.show.ip.route.addSC("traffic-engineering", "Traffic engineered routes");
         enableC.show.ip.route.addSC("vrf", "Display routes from a VPN Routing/Forwarding instance");
      enableC.show.ip.addSC("rpf", "Display RPF information for multicast source");
      enableC.show.ip.addSC("rsvp", "RSVP information");
      enableC.show.ip.addSC("rtp", "RTP/UDP/IP header-compression statistics");
      enableC.show.ip.addSC("sdr", "Session Directory (SDPv2) cache");
      enableC.show.ip.addSC("sockets", "Open IP sockets");
      enableC.show.ip.addSC("tcp", "TCP/IP header-compression statistics");
      enableC.show.ip.addSC("traffic", "IP protocol statistics");
      enableC.show.ip.addSC("trigger-authentication", "Trigger-authentication host table");
      enableC.show.ip.addSC("vrf", "VPN Routing/Forwarding instance information");
      enableC.show.ip.addSC("wccp", "WCCP information");
   enableC.show.addSC("ipx", "Novell IPX information");
   enableC.show.addSC("isis", "IS-IS routing information");
      enableC.show.isis.addSC("database", "IS-IS link state database");
         enableC.show.isis.database.addSC("detail", "Detailed link state database information");
         enableC.show.isis.database.addSC("l1", "IS-IS Level-1 routing link state database");
         enableC.show.isis.database.addSC("l2", "IS-IS Level-2 routing link state database");
         enableC.show.isis.database.addSC("level-1", "IS-IS Level-1 routing link state database");
         enableC.show.isis.database.addSC("level-2", "IS-IS Level-2 routing link state database");
      enableC.show.isis.addSC("hostname", "IS-IS Dynamic hostname mapping");
      enableC.show.isis.addSC("lsp-log", "IS-IS LSP log");
      enableC.show.isis.addSC("mesh-groups", "IS-IS mesh groups");
      enableC.show.isis.addSC("route", "IS-IS level-1 routing table");
      enableC.show.isis.addSC("spf-log", "IS-IS SPF log");
      enableC.show.isis.addSC("topology", "IS-IS paths to Intermediate Systems");
   enableC.show.addSC("kerberos", "Show Kerberos Values");
   enableC.show.addSC("key", "Key information");
   enableC.show.addSC("keymap", "Terminal keyboard mappings");
   enableC.show.addSC("lat", "DEC LAT information");
   enableC.show.addSC("line", "TTY line information");
      enableC.show.line.addSC("<0-70>", "First Line range");
         enableC.show.line["<0-70>"].addSC("<1-70>", "Last Line range");
      enableC.show.line.addSC("aux", "Auxiliary line");
         enableC.show.line.aux.addSC("<0-0>", "First Line range");
      enableC.show.line.addSC("console", "Primary terminal line");
         enableC.show.line.console.addSC("<0-0>", "First Line range");
      enableC.show.line.addSC("summary", "Quick line status summary");
      enableC.show.line.addSC("tty", "Terminal controller");
         enableC.show.line.tty.addSC("<1-64>", "First Line range");
            enableC.show.line.tty["<1-64>"].addSC("<2-64>", "Last Line range");
            enableC.show.line.tty["<1-64>"].addSC("summary", "Quick line status summary");
      enableC.show.line.addSC("vty", "Virtual terminal");
         enableC.show.line.vty.addSC("<0-133>", "First Line range");
            enableC.show.line.vty["<0-133>"].addSC("<1-133>", "Last Line range");
            enableC.show.line.vty["<0-133>"].addSC("summary", "Quick line status summary");
   enableC.show.addSC("llc2", "IBM LLC2 circuit information");
   enableC.show.addSC("lnm", "IBM LAN manager");
   enableC.show.addSC("local-ack", "Local Acknowledgement virtual circuits");
   enableC.show.addSC("location", "Display the system location");
   enableC.show.addSC("logging", "Show the contents of logging buffers");
      enableC.show.logging.addSC("history", "Show the contents of syslog history table");
   enableC.show.addSC("memory", "Memory statistics");
   enableC.show.addSC("modemcap", "Show Modem Capabilities database");
   enableC.show.addSC("mpoa", "MPOA show commands");
   enableC.show.addSC("nbf", "NBF (NetBEUI) information");
   enableC.show.addSC("ncia", "Native Client Interface Architecture");
   enableC.show.addSC("netbios-cache", "NetBIOS name cache contents");
   enableC.show.addSC("node", "Show known LAT nodes");
   enableC.show.addSC("policy-map", "Show QoS Policy Map");
      enableC.show["policy-map"].addSC("WORD", "policy-map name");
         enableC.show["policy-map"].WORD.addSC("class", "Show Qos Policy actions for a indvidual class");
            enableC.show["policy-map"].WORD.class.addSC("WORD", "class-map name");
      enableC.show["policy-map"].addSC("interface", "Show Qos Policy Interface");
         enableC.show["policy-map"].interface.addSC("Async", "Async interface");
            enableC.show["policy-map"].interface.Async.addSC("<1-65>", "Async interface number");
         enableC.show["policy-map"].interface.addSC("Dialer", "Dialer interface");
            enableC.show["policy-map"].interface.Dialer.addSC("<0-255>", "Dialer interface number");
         enableC.show["policy-map"].interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
            enableC.show["policy-map"].interface.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
         enableC.show["policy-map"].interface.addSC("Loopback", "Loopback interface");
            enableC.show["policy-map"].interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
         enableC.show["policy-map"].interface.addSC("Null", "Null interface");
            enableC.show["policy-map"].interface.Null.addSC("<0-0>", "Null interface number");
         enableC.show["policy-map"].interface.addSC("Serial", "Serial");
            enableC.show["policy-map"].interface.Serial.addSC("<0-1>", "Serial interface number");
   enableC.show.addSC("ppp", "PPP parameters and statistics");
   enableC.show.addSC("printers", "Show LPD printer information");
   enableC.show.addSC("privilege", "Show current privilege level");
   enableC.show.addSC("processes", "Active process statistics");
   enableC.show.addSC("protocols", "Active network routing protocols");
   enableC.show.addSC("qllc", "Display qllc-llc2 and qllc-sdlc conversion information");
   enableC.show.addSC("queue", "Show queue contents");
   enableC.show.addSC("queueing", "Show queueing configuration");
   enableC.show.addSC("registry", "Function registry information");
   enableC.show.addSC("reload", "Scheduled reload information");
   enableC.show.addSC("rhosts", "Remote-host+user equivalences");
   enableC.show.addSC("route-map", "route-map information");
   enableC.show.addSC("rtr", "Response Time Reporter (RTR)");
   enableC.show.addSC("running-config", "Current operating configuration");
      enableC.show["running-config"].addSC("interface", "Show interface configuration");
         enableC.show["running-config"].interface.addSC("Async", "Async interface");
            enableC.show["running-config"].interface.Async.addSC("<1-65>", "Async interface number");
         enableC.show["running-config"].interface.addSC("Dialer", "Dialer interface");
            enableC.show["running-config"].interface.Dialer.addSC("<0-255>", "Dialer interface number");
         enableC.show["running-config"].interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
            enableC.show["running-config"].interface.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
         enableC.show["running-config"].interface.addSC("Loopback", "Loopback interface");
            enableC.show["running-config"].interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
         enableC.show["running-config"].interface.addSC("Null", "Null interface");
            enableC.show["running-config"].interface.Null.addSC("<0-0>", "Null interface number");
         enableC.show["running-config"].interface.addSC("Serial", "Serial");
            enableC.show["running-config"].interface.Serial.addSC("<0-1>", "Serial interface number");
   enableC.show.addSC("sdllc", "Display sdlc - llc2 conversion information");
   enableC.show.addSC("sessions", "Information about Telnet connections");
   enableC.show.addSC("standby", "Hot standby protocol information");
   enableC.show.addSC("startup-config", "Contents of startup configuration");
   enableC.show.addSC("stun", "STUN status and configuration");
   enableC.show.addSC("subscriber-policy", "Subscriber policy");
   enableC.show.addSC("tcp", "Status of TCP connections");
   enableC.show.addSC("terminal", "Display terminal configuration parameters");
   enableC.show.addSC("time-range", "Time range");
   enableC.show.addSC("tn3270", "TN3270 settings");
   enableC.show.addSC("traffic-shape", "traffic rate shaping configuration");
      enableC.show["traffic-shape"].addSC("Async", "Async interface");
      enableC.show["traffic-shape"].addSC("Dialer", "Dialer interface");
      enableC.show["traffic-shape"].addSC("FastEthernet", "FastEthernet IEEE 802.3");
      enableC.show["traffic-shape"].addSC("Loopback", "Loopback interface");
      enableC.show["traffic-shape"].addSC("Null", "Null interface");
      enableC.show["traffic-shape"].addSC("Serial", "Serial");
         enableC.show["traffic-shape"].statistics.addSC("Async", "Async interface");
            enableC.show["traffic-shape"].statistics.Async.addSC("<1-65>", "Async interface number");
         enableC.show["traffic-shape"].statistics.addSC("Loopback", "Loopback interface");
            enableC.show["traffic-shape"].statistics.Loopback.addSC("<0-2147483647>", "Loopback interface number");
         enableC.show["traffic-shape"].statistics.addSC("Serial", "Serial");
            enableC.show["traffic-shape"].statistics.Serial.addSC("<0-1>", "Serial interface number");
   enableC.show.addSC("users", "Display information about terminal lines");
   enableC.show.addSC("version", "System hardware and software status");
enableC.addSC("slip", "Start Serial-line IP (SLIP)");
enableC.addSC("start-chat", "Start a chat-script on a line");
enableC.addSC("systat", "Display information about terminal lines");
enableC.addSC("telnet", "Open a telnet connection");
enableC.addSC("terminal", "Set terminal line parameters");
enableC.addSC("test", "Test subsystems, memory, and interfaces");
enableC.addSC("tn3270", "Open a tn3270 connection");
enableC.addSC("traceroute", "Trace route to destination");
   enableC.traceroute.addSC("WORD", "Trace route to destination address or hostname");
   enableC.traceroute.addSC("clns", "ISO CLNS Trace");
      enableC.traceroute.clns.addSC("WORD", "Trace route to destination address or hostname");
   enableC.traceroute.addSC("ip", "IP Trace");
      enableC.traceroute.ip.addSC("WORD", "Trace route to destination address or hostname");
   enableC.traceroute.addSC("ipx", "IPX Trace");
      enableC.traceroute.ipx.addSC("WORD", "Trace route to destination address or hostname");
enableC.addSC("tunnel", "Open a tunnel connection");
enableC.addSC("verify", "Verify a file");
enableC.addSC("where", "List active connections");
enableC.addSC("which-route", "Do OSI route table lookup and display results");
enableC.addSC("write", "Write running configuration to memory, network, or terminal");
	enableC.write.addSC("erase", "Erase NV memory");
	enableC.write.addSC("memory", "Write to NV memory");
	enableC.write.addSC("network", "Write to network TFTP server");
	enableC.write.addSC("terminal", "Write to terminal");
