
globalC.addSC("aaa", "Authentication, Authorization and Accounting.");
globalC.addSC("access-list", "Add an access list entry");
globalC.addSC("alias", "Create command alias");
globalC.addSC("alps", "Configure Airline Protocol Support");
globalC.addSC("apollo", "Apollo global configuration commands");
globalC.addSC("appletalk", "Appletalk global configuration commands");
globalC.addSC("arap", "Appletalk Remote Access Protocol");
globalC.addSC("arp", "Set a static ARP entry");
globalC.addSC("async-bootp", "Modify system bootp parameters");
globalC.addSC("autonomous-system", "Specify local AS number to which we belong");
globalC.addSC("banner", "Define a login banner");
globalC.addSC("boot", "Modify system boot parameters");
globalC.addSC("bridge", "Bridge Group.");
globalC.addSC("bstun", "BSTUN global configuration commands");
globalC.addSC("buffers", "Adjust system buffer pool parameters");
globalC.addSC("busy-message", "Display message when connection to host fails");
globalC.addSC("call-history-mib", "Define call history mib parameters");
globalC.addSC("cdp", "Global CDP configuration subcommands");
globalC.addSC("chat-script", "Define a modem chat script");
globalC.addSC("class-map", "Configure QoS Class Map");
   globalC["class-map"].addSC("WORD", "class-map name");
globalC.addSC("clns", "Global CLNS configuration subcommands");
globalC.addSC("clock", "Configure time-of-day clock");
globalC.addSC("cns", "CNS Subsystems");
globalC.addSC("config-register", "Define the configuration register");
globalC.addSC("controller", "Configure a specific controller");
globalC.addSC("crypto", "Encryption module");
   globalC.crypto.addSC("ca", "Certification authority");
   globalC.crypto.addSC("cisco", "Configure cisco encryption policy");
   globalC.crypto.addSC("dynamic-map", "Specify a dynamic crypto map template");
   globalC.crypto.addSC("ipsec", "Configure IPSEC policy");
      globalC.crypto.ipsec.addSC("security-association", "Security association parameters");
      globalC.crypto.ipsec.addSC("transform-set", "Define transform and settings");
         globalC.crypto.ipsec["transform-set"].addSC("WORD", "Transform set tag");
            globalC.crypto.ipsec["transform-set"].WORD.addSC("ah-md5-hmac", "AH-HMAC-MD5 transform");
            globalC.crypto.ipsec["transform-set"].WORD.addSC("ah-rfc1828", "AH-MD5 transform (RFC1828)");
            globalC.crypto.ipsec["transform-set"].WORD.addSC("ah-sha-hmac", "AH-HMAC-SHA transform");
            globalC.crypto.ipsec["transform-set"].WORD.addSC("esp-des", "ESP transform using DES cipher (56 bits)");
               globalC.crypto.ipsec["transform-set"].WORD["esp-des"].addSC("ah-md5-hmac", "AH-HMAC-MD5 transform");
               globalC.crypto.ipsec["transform-set"].WORD["esp-des"].addSC("ah-rfc1828", "AH-MD5 transform (RFC1828)");
               globalC.crypto.ipsec["transform-set"].WORD["esp-des"].addSC("ah-sha-hmac", "AH-HMAC-SHA transform");
            globalC.crypto.ipsec["transform-set"].WORD.addSC("esp-md5-hmac", "ESP transform using HMAC-MD5 auth");
               globalC.crypto.ipsec["transform-set"].WORD["esp-md5-hmac"].addSC("ah-md5-hmac", "AH-HMAC-MD5 transform");
               globalC.crypto.ipsec["transform-set"].WORD["esp-md5-hmac"].addSC("ah-rfc1828", "AH-MD5 transform (RFC1828)");
               globalC.crypto.ipsec["transform-set"].WORD["esp-md5-hmac"].addSC("ah-sha-hmac", "AH-HMAC-SHA transform");
               globalC.crypto.ipsec["transform-set"].WORD["esp-md5-hmac"].addSC("esp-des", "ESP transform using DES cipher (56 bits)");
                  globalC.crypto.ipsec["transform-set"].WORD["esp-md5-hmac"]["esp-des"].addSC("ah-md5-hmac", "AH-HMAC-MD5 transform");
                  globalC.crypto.ipsec["transform-set"].WORD["esp-md5-hmac"]["esp-des"].addSC("ah-rfc1828", "AH-MD5 transform (RFC1828)");
                  globalC.crypto.ipsec["transform-set"].WORD["esp-md5-hmac"]["esp-des"].addSC("ah-sha-hmac", "AH-HMAC-SHA transform");
            globalC.crypto.ipsec["transform-set"].WORD.addSC("esp-null", "ESP transform w/o cipher");
               globalC.crypto.ipsec["transform-set"].WORD["esp-null"].addSC("ah-md5-hmac", "AH-HMAC-MD5 transform");
               globalC.crypto.ipsec["transform-set"].WORD["esp-null"].addSC("ah-rfc1828", "AH-MD5 transform (RFC1828)");
               globalC.crypto.ipsec["transform-set"].WORD["esp-null"].addSC("ah-sha-hmac", "AH-HMAC-SHA transform");
               globalC.crypto.ipsec["transform-set"].WORD["esp-null"].addSC("esp-md5-hmac", "ESP transform using HMAC-MD5 auth");
                  globalC.crypto.ipsec["transform-set"].WORD["esp-null"]["esp-md5-hmac"].addSC("ah-md5-hmac", "AH-HMAC-MD5 transform");
                  globalC.crypto.ipsec["transform-set"].WORD["esp-null"]["esp-md5-hmac"].addSC("ah-rfc1828", "AH-MD5 transform (RFC1828)");
                  globalC.crypto.ipsec["transform-set"].WORD["esp-null"]["esp-md5-hmac"].addSC("ah-sha-hmac", "AH-HMAC-SHA transform");
            globalC.crypto.ipsec["transform-set"].WORD.addSC("esp-rfc1829", "ESP-DES-CBC transform (RFC1829)");
               globalC.crypto.ipsec["transform-set"].WORD["esp-rfc1829"].addSC("ah-md5-hmac", "AH-HMAC-MD5 transform");
               globalC.crypto.ipsec["transform-set"].WORD["esp-rfc1829"].addSC("ah-rfc1828", "AH-MD5 transform (RFC1828)");
               globalC.crypto.ipsec["transform-set"].WORD["esp-rfc1829"].addSC("ah-sha-hmac", "AH-HMAC-SHA transform");
            globalC.crypto.ipsec["transform-set"].WORD.addSC("esp-sha-hmac", "ESP transform using HMAC-SHA auth");
   globalC.crypto.addSC("isakmp", "Configure ISAKMP policy");
      globalC.crypto.isakmp.addSC("enable", "Enable ISAKMP");
      globalC.crypto.isakmp.addSC("identity", "Set the identity which ISAKMP will use");
      globalC.crypto.isakmp.addSC("keepalive", "Set a keepalive interval for use with IOS peers");
      globalC.crypto.isakmp.addSC("key", "Set pre-shared key for remote peer");
         globalC.crypto.isakmp.key.addSC("WORD", "pre-shared key");
            globalC.crypto.isakmp.key.WORD.addSC("address", "define shared key with IP address");
               globalC.crypto.isakmp.key.WORD.address.addSC("A.B.C.D", "Peer IP address");
            globalC.crypto.isakmp.key.WORD.addSC("hostname", "define shared key with hostname");
               globalC.crypto.isakmp.key.WORD.hostname.addSC("WORD", "hostname of peer with whom the key is shared");
      globalC.crypto.isakmp.addSC("policy", "Set policy for an ISAKMP protection suite");
         globalC.crypto.isakmp.policy.addSC("<1-10000>", "Priority of protection suite");
   globalC.crypto.addSC("key", "Long term key operations");
   globalC.crypto.addSC("map", "Enter a crypto map");
      globalC.crypto.map.addSC("WORD", "Crypto map tag");
         globalC.crypto.map.WORD.addSC("<0-65535>", "Sequence to insert into crypto map entry");
            globalC.crypto.map.WORD["<0-65535>"].addSC("cisco", "Cisco proprietary encryption");
            globalC.crypto.map.WORD["<0-65535>"].addSC("ipsec-isakmp", "IPSEC w/ISAKMP");
               globalC.crypto.map.WORD["<0-65535>"]["ipsec-isakmp"].addSC("dynamic", "Enable dynamic crypto map support");
                  globalC.crypto.map.WORD["<0-65535>"]["ipsec-isakmp"].dynamic.addSC("WORD", "Name of dynamic-map template");
            globalC.crypto.map.WORD["<0-65535>"].addSC("ipsec-manual", "IPSEC w/manual keying");
         globalC.crypto.map.WORD.addSC("local-address", "Interface to use for local address for this crypto map");
globalC.addSC("decnet", "Global DECnet configuration subcommands");
globalC.addSC("default", "Set a command to its defaults");
globalC.addSC("default-value", "Default character-bits values");
globalC.addSC("dial-control-mib", "Define Dial Control Mib parameters");
globalC.addSC("dial-peer", "Dial Map (Peer) configuration commands");
globalC.addSC("dialer", "Dialer commands");
globalC.addSC("dialer-list", "Create a dialer list entry");
   globalC["dialer-list"].addSC("<1-10>", "Dialer group number");
      globalC["dialer-list"]["<1-10>"].addSC("protocol", "Permit or Deny based on protocols");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("appletalk", "AppleTalk");
            globalC["dialer-list"]["<1-10>"].protocol.appletalk.addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol.appletalk.addSC("list", "Add access list to dialer list");
               globalC["dialer-list"]["<1-10>"].protocol.appletalk.list.addSC("<600-699>", "AppleTalk access list");
            globalC["dialer-list"]["<1-10>"].protocol.appletalk.addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("bridge", "Bridging");
            globalC["dialer-list"]["<1-10>"].protocol.bridge.addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol.bridge.addSC("list", "Add access list to dialer list");
               globalC["dialer-list"]["<1-10>"].protocol.bridge.list.addSC("<200-299>", "Ethernet-typecode access list");
            globalC["dialer-list"]["<1-10>"].protocol.bridge.addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("clns", "OSI Connectionless Network Service");
            globalC["dialer-list"]["<1-10>"].protocol.clns.addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol.clns.addSC("list", "Add access list to dialer list");
               globalC["dialer-list"]["<1-10>"].protocol.clns.list.addSC("WORD", "Name of CLNS filter expression or set");
            globalC["dialer-list"]["<1-10>"].protocol.clns.addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("clns_es", "CLNS End System");
            globalC["dialer-list"]["<1-10>"].protocol["clns_es"].addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol["clns_es"].addSC("list", "Add access list to dialer list");
               globalC["dialer-list"]["<1-10>"].protocol["clns_es"].list.addSC("WORD", "Name of CLNS filter expression or set");
            globalC["dialer-list"]["<1-10>"].protocol["clns_es"].addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("clns_is", "CLNS Intermediate System");
            globalC["dialer-list"]["<1-10>"].protocol["clns_is"].addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol["clns_is"].addSC("list", "Add access list to dialer list");
               globalC["dialer-list"]["<1-10>"].protocol["clns_is"].list.addSC("WORD", "Name of CLNS filter expression or set");
            globalC["dialer-list"]["<1-10>"].protocol["clns_is"].addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("decnet", "DECnet");
            globalC["dialer-list"]["<1-10>"].protocol.decnet.addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol.decnet.addSC("list", "Add access list to dialer list");
               globalC["dialer-list"]["<1-10>"].protocol.decnet.list.addSC("<300-399>", "DECNET access list");
            globalC["dialer-list"]["<1-10>"].protocol.decnet.addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("decnet_node", "DECnet node");
            globalC["dialer-list"]["<1-10>"].protocol["decnet_node"].addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol["decnet_node"].addSC("list", "Add access list to dialer list");
               globalC["dialer-list"]["<1-10>"].protocol["decnet_node"].list.addSC("<300-399>", "DECNET access list");
            globalC["dialer-list"]["<1-10>"].protocol["decnet_node"].addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("decnet_router-L1", "DECnet router L1");
            globalC["dialer-list"]["<1-10>"].protocol["decnet_router-L1"].addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol["decnet_router-L1"].addSC("list", "Add access list to dialer list");
               globalC["dialer-list"]["<1-10>"].protocol["decnet_router-L1"].list.addSC("<300-399>", "DECNET access list");
            globalC["dialer-list"]["<1-10>"].protocol["decnet_router-L1"].addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("decnet_router-L2", "DECnet router L2");
            globalC["dialer-list"]["<1-10>"].protocol["decnet_router-L2"].addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol["decnet_router-L2"].addSC("list", "Add access list to dialer list");
               globalC["dialer-list"]["<1-10>"].protocol["decnet_router-L2"].list.addSC("<300-399>", "DECNET access list");
            globalC["dialer-list"]["<1-10>"].protocol["decnet_router-L2"].addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("hpr", "HPR");
            globalC["dialer-list"]["<1-10>"].protocol.hpr.addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol.hpr.addSC("list", "Add access list to dialer list");
            globalC["dialer-list"]["<1-10>"].protocol.hpr.addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("ip", "IP");
            globalC["dialer-list"]["<1-10>"].protocol.ip.addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol.ip.addSC("list", "Add access list to dialer list");
               globalC["dialer-list"]["<1-10>"].protocol.ip.list.addSC("<1-199>", "IP access list");
               globalC["dialer-list"]["<1-10>"].protocol.ip.list.addSC("<1300-2699>", "IP expanded access list");
            globalC["dialer-list"]["<1-10>"].protocol.ip.addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("ipx", "Novell IPX");
            globalC["dialer-list"]["<1-10>"].protocol.ipx.addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol.ipx.addSC("list", "Add access list to dialer list");
               globalC["dialer-list"]["<1-10>"].protocol.ipx.list.addSC("<800-1099>", "Novell access list");
            globalC["dialer-list"]["<1-10>"].protocol.ipx.addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("llc2", "LLC2");
            globalC["dialer-list"]["<1-10>"].protocol.llc2.addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol.llc2.addSC("list", "Add access list to dialer list");
            globalC["dialer-list"]["<1-10>"].protocol.llc2.addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("netbios", "NETBIOS");
            globalC["dialer-list"]["<1-10>"].protocol.netbios.addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol.netbios.addSC("list", "Add access list to dialer list");
            globalC["dialer-list"]["<1-10>"].protocol.netbios.addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("vines", "Banyan Vines");
            globalC["dialer-list"]["<1-10>"].protocol.vines.addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol.vines.addSC("list", "Add access list to dialer list");
               globalC["dialer-list"]["<1-10>"].protocol.vines.list.addSC("<1-300>", "Vines access list");
            globalC["dialer-list"]["<1-10>"].protocol.vines.addSC("permit", "Permit specified protocol");
         globalC["dialer-list"]["<1-10>"].protocol.addSC("xns", "XNS");
            globalC["dialer-list"]["<1-10>"].protocol.xns.addSC("deny", "Deny specified protocol");
            globalC["dialer-list"]["<1-10>"].protocol.xns.addSC("list", "Add access list to dialer list");
               globalC["dialer-list"]["<1-10>"].protocol.xns.list.addSC("<400-599>", "XNS access list");
            globalC["dialer-list"]["<1-10>"].protocol.xns.addSC("permit", "Permit specified protocol");
globalC.addSC("dlsw", "Data Link Switching global configuration commands");
globalC.addSC("dnsix-dmdp", "Provide DMDP service for DNSIX");
globalC.addSC("dnsix-nat", "Provide DNSIX service for audit trails");
globalC.addSC("downward-compatible-config", "Generate a configuration compatible with older software");
globalC.addSC("dspu", "DownStream Physical Unit Command");
globalC.addSC("enable", "Modify enable password parameters");
   globalC.enable.addSC("last-resort", "Define enable action if no TACACS servers respond");
      globalC.enable["last-resort"].addSC("password", "Enable by giving the local enable password");
      globalC.enable["last-resort"].addSC("succeed", "Enable without further question");
   globalC.enable.addSC("password", "Assign the privileged level password");
      globalC.enable.password.addSC("<0-0>", "Specifies an UNENCRYPTED password will follow");
      globalC.enable.password.addSC("<7-7>", "Specifies a HIDDEN password will follow");
      globalC.enable.password.addSC("LINE", "The UNENCRYPTED (cleartext) 'enable' password");
      globalC.enable.password.addSC("level", "Set exec level password");
         globalC.enable.password.level.addSC("<1-15>", "Level number");
            globalC.enable.password.level["<1-15>"].addSC("<0-0>", "Specifies an UNENCRYPTED password will follow");
            globalC.enable.password.level["<1-15>"].addSC("<7-7>", "Specifies a HIDDEN password will follow");
            globalC.enable.password.level["<1-15>"].addSC("LINE", "The UNENCRYPTED (cleartext) 'enable' password");
   globalC.enable.addSC("secret", "Assign the privileged level secret");
      globalC.enable.secret.addSC("<0-0>", "Specifies an UNENCRYPTED password will follow");
      globalC.enable.secret.addSC("5", "Specifies an ENCRYPTED secret will follow");
      globalC.enable.secret.addSC("LINE", "The UNENCRYPTED (cleartext) 'enable' secret");
      globalC.enable.secret.addSC("level", "Set exec level password");
         globalC.enable.secret.level.addSC("<1-15>", "Level number");
            globalC.enable.secret.level["<1-15>"].addSC("<0-0>", "Specifies an UNENCRYPTED password will follow");
            globalC.enable.secret.level["<1-15>"].addSC("5", "Specifies an ENCRYPTED secret will follow");
            globalC.enable.secret.level["<1-15>"].addSC("LINE", "The UNENCRYPTED (cleartext) 'enable' secret");
   globalC.enable.addSC("use-tacacs", "Use TACACS to check enable passwords");
globalC.addSC("end", "Exit from configure mode");
globalC.addSC("endnode", "SNA APPN endnode command");
globalC.addSC("exception", "Exception handling");
globalC.addSC("exit", "Exit from configure mode");
globalC.addSC("file", "Adjust file system parameters");
globalC.addSC("frame-relay", "global frame relay configuration commands");
globalC.addSC("gateway", "Gateway");
globalC.addSC("gw-accounting", "Enable voip gateway accounting.");
globalC.addSC("help", "Description of the interactive help system");
globalC.addSC("hostname", "Set system's network name");
   globalC.hostname.addSC("WORD", "This system's network name");
globalC.addSC("interface", "Select an interface to configure");
   globalC.interface.addSC("Async", "Async interface");
   globalC.interface.addSC("BVI", "Bridge-Group Virtual Interface");
   globalC.interface.addSC("Dialer", "Dialer interface");
   globalC.interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
      globalC.interface.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
   globalC.interface.addSC("Group-Async", "Async Group interface");
   globalC.interface.addSC("Lex", "Lex interface");
   globalC.interface.addSC("Loopback", "Loopback interface");
      globalC.interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
   globalC.interface.addSC("Multilink", "Multilink-group interface");
   globalC.interface.addSC("Null", "Null interface");
   globalC.interface.addSC("Port-channel", "Ethernet Channel of interfaces");
   globalC.interface.addSC("Serial", "Serial");
      globalC.interface.Serial.addSC("<0-1>", "Serial interface number");
   globalC.interface.addSC("Tunnel", "Tunnel interface");
   globalC.interface.addSC("Virtual-Template", "Virtual Template interface");
   globalC.interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
   globalC.interface.addSC("Vlan", "Catalyst Vlans");
globalC.addSC("ip", "Global IP configuration subcommands");
   globalC.ip.addSC("access-list", "Named access-list");
   //globalC.ip.addSC("accounting-list", "Select hosts for which IP accounting information is kept");
   //globalC.ip.addSC("accounting-threshold", "Sets the maximum number of accounting entries");
   //globalC.ip.addSC("accounting-transits", "Sets the maximum number of transit entries");
   globalC.ip.addSC("address-pool", "Specify default IP address pooling mechanism");
   globalC.ip.addSC("alias", "Alias an IP address to a TCP port");
   globalC.ip.addSC("as-path", "BGP autonomous system path filter");
   globalC.ip.addSC("audit", "Intrusion Detection System");
   globalC.ip.addSC("auth-proxy", "Authentication Proxy");
   globalC.ip.addSC("bgp-community", "format for BGP community");
   globalC.ip.addSC("bootp", "Config BOOTP services");
   globalC.ip.addSC("cef", "Cisco Express Forwarding");
   globalC.ip.addSC("classless", "Follow classless routing forwarding rules");
   globalC.ip.addSC("community-list", "Add a community list entry");
   //globalC.ip.addSC("default-gateway", "Specify default gateway (if not routing IP)");
   globalC.ip.addSC("default-network", "Flags networks as candidates for default routes");
      globalC.ip["default-network"].addSC("A.B.C.D", "IP address of default network");
   globalC.ip.addSC("dhcp", "Configure DHCP server and relay parameters");
		globalC.ip.dhcp.addSC("conflict",          "DHCP address conflict parameters");
		globalC.ip.dhcp.addSC("database",          "Configure DHCP database agents");
		globalC.ip.dhcp.addSC("excluded-address",  "Prevent DHCP from assigning certain addresses");
			globalC.ip.dhcp["excluded-address"].addSC("A.B.C.D",  "Low IP address");
				globalC.ip.dhcp["excluded-address"]["A.B.C.D"].addSC("A.B.C.D",  "Low IP address");
		globalC.ip.dhcp.addSC("ping",              "Specify ping parameters used by DHCP");
		globalC.ip.dhcp.addSC("pool",              "Configure DHCP address pools");
			globalC.ip.dhcp.pool.addSC("WORD",  "Pool name");
		globalC.ip.dhcp.addSC("relay",             "DHCP relay agent parameters");
		globalC.ip.dhcp.addSC("smart-relay",       "Enable Smart Relay feature");
   //globalC.ip.addSC("dhcp-server", "Specify address of DHCP server to use");
   //globalC.ip.addSC("domain-list", "Domain name to complete unqualified host names.");
   globalC.ip.addSC("domain-lookup", "Enable IP Domain Name System hostname translation");
   //globalC.ip.addSC("domain-name", "Define the default domain name");
   globalC.ip.addSC("drp", "Director response protocol configuration commands");
   globalC.ip.addSC("dvmrp", "DVMRP global commands");
   globalC.ip.addSC("finger", "finger server");
  // globalC.ip.addSC("flow-aggregation", "Configure flow aggregation");
  // globalC.ip.addSC("flow-cache", "Configure netflow cache parameters");
  // globalC.ip.addSC("flow-export", "Specify host/port to send flow statistics");
   globalC.ip.addSC("forward-protocol", "Controls forwarding of physical and directed IP broadcasts");
   		  globalC.ip["forward-protocol"].addSC("nd",             "Sun's Network Disk protocol");
		  globalC.ip["forward-protocol"].addSC("sdns",           "Network Security Protocol");
		  globalC.ip["forward-protocol"].addSC("spanning-tree",  "Use transparent bridging to flood UDP broadcasts");
		  globalC.ip["forward-protocol"].addSC("turbo-flood",    "Fast flooding of UDP broadcasts");
  		  globalC.ip["forward-protocol"].addSC("udp",            "Packets to a specific UDP port");
   globalC.ip.addSC("ftp", "FTP configuration commands");
   globalC.ip.addSC("gdp", "Router discovery mechanism");
   globalC.ip.addSC("gratuitous-arps", "Generate gratuitous ARPs for PPP/SLIP peer addresses");
   globalC.ip.addSC("host", "Add an entry to the ip hostname table");
      globalC.ip.host.addSC("WORD", "Name of host");
   globalC.ip.addSC("host-routing", "Enable host-based routing (proxy ARP and redirect)");
   globalC.ip.addSC("hp-host", "Enable the HP proxy probe service");
   globalC.ip.addSC("http", "HTTP server configuration");
   globalC.ip.addSC("icmp", "ICMP options");
   globalC.ip.addSC("identd", "Ident server");
   globalC.ip.addSC("inspect", "Context-based Access Control Engine");
   globalC.ip.addSC("local", "Specify local options");
   globalC.ip.addSC("mobile", "Enable Mobile IP services");
   globalC.ip.addSC("mrm", "Configure IP Multicast Routing Monitor test parameters");
   globalC.ip.addSC("mroute", "Configure static multicast routes");
   //globalC.ip.addSC("multicast", "Global IP Multicast Commands");
   globalC.ip.addSC("multicast-routing", "Enable IP multicast forwarding");
   globalC.ip.addSC("name-server", "Specify address of name server to use");
   globalC.ip.addSC("nat", "NAT configuration commands");
      globalC.ip.nat.addSC("inside", "Inside address translation");
         globalC.ip.nat.inside.addSC("destination", "Destination address translation");
         globalC.ip.nat.inside.addSC("source", "Source address translation");
            globalC.ip.nat.inside.source.addSC("list", "Specify access list describing local addresses");
               globalC.ip.nat.inside.source.list.addSC("<1-199>", "Access list number for local addresses");
                  globalC.ip.nat.inside.source.list["<1-199>"].addSC("interface", "Specify interface for global address");
                  globalC.ip.nat.inside.source.list["<1-199>"].addSC("pool", "Name pool of global addresses");
               globalC.ip.nat.inside.source.list.addSC("WORD", "Access list name for local addresses");
                  globalC.ip.nat.inside.source.list.WORD.addSC("interface", "Specify interface for global address");
                  globalC.ip.nat.inside.source.list.WORD.addSC("pool", "Name pool of global addresses");
            globalC.ip.nat.inside.source.addSC("route-map", "Specify route-map");
            globalC.ip.nat.inside.source.addSC("static", "Specify static local->global mapping");
               globalC.ip.nat.inside.source.static.addSC("A.B.C.D", "Inside local IP address");
                  globalC.ip.nat.inside.source.static["A.B.C.D"].addSC("A.B.C.D", "Inside global IP address");
               globalC.ip.nat.inside.source.static.addSC("network", "Subnet translation");
                  globalC.ip.nat.inside.source.static.network.addSC("A.B.C.D", "Inside local network");
               globalC.ip.nat.inside.source.static.addSC("tcp", "Transmission Control Protocol");
                  globalC.ip.nat.inside.source.static.tcp.addSC("A.B.C.D", "Inside local IP address");
               globalC.ip.nat.inside.source.static.addSC("udp", "User Datagram Protocol");
                  globalC.ip.nat.inside.source.static.udp.addSC("A.B.C.D", "Inside local IP address");
      globalC.ip.nat.addSC("outside", "Outside address translation");
      globalC.ip.nat.addSC("pool", "Define pool of addresses");
         globalC.ip.nat.pool.addSC("WORD", "Pool name");
            globalC.ip.nat.pool.WORD.addSC("A.B.C.D", "Start IP address");
               globalC.ip.nat.pool.WORD["A.B.C.D"].addSC("A.B.C.D", "End IP address");
            globalC.ip.nat.pool.WORD.addSC("netmask", "Specify the network mask");
               globalC.ip.nat.pool.WORD.netmask.addSC("A.B.C.D", "Network mask");
                  globalC.ip.nat.pool.WORD.netmask["A.B.C.D"].addSC("type", "Specify the pool type");
            globalC.ip.nat.pool.WORD.addSC("prefix-length", "Specify the prefix length");
               globalC.ip.nat.pool.WORD["prefix-length"].addSC("<1-32>", "Prefix length");
                  globalC.ip.nat.pool.WORD["prefix-length"]["<1-32>"].addSC("type", "Specify the pool type");
      globalC.ip.nat.addSC("service", "Special translation for application using non-standard port");
      globalC.ip.nat.addSC("translation", "NAT translation entry configuration");
         globalC.ip.nat.translation.addSC("dns-timeout", "Specify timeout for NAT DNS flows");
         globalC.ip.nat.translation.addSC("finrst-timeout", "Specify timeout for NAT TCP flows after a FIN or RST");
         globalC.ip.nat.translation.addSC("icmp-timeout", "Specify timeout for NAT ICMP flows");
         globalC.ip.nat.translation.addSC("max-entries", "Specify maximum number of NAT entries");
         globalC.ip.nat.translation.addSC("port-timeout", "Specify timeout for NAT TCP/UDP port specific flows");
         globalC.ip.nat.translation.addSC("syn-timeout", "Specify timeout for NAT TCP flows after a SYN and no further data");
         globalC.ip.nat.translation.addSC("tcp-timeout", "Specify timeout for NAT TCP flows");
         globalC.ip.nat.translation.addSC("timeout", "Specify timeout for dynamic NAT translations");
            globalC.ip.nat.translation.timeout.addSC("<0-2147483647>", "Timeout in seconds");
            globalC.ip.nat.translation.timeout.addSC("never", "Never timeout");
         globalC.ip.nat.translation.addSC("udp-timeout", "Specify timeout for NAT UDP flows");
   globalC.ip.addSC("ospf", "OSPF");
   globalC.ip.addSC("pgm", "PGM Reliable Transport Protocol");
   globalC.ip.addSC("pim", "PIM global commands");
   globalC.ip.addSC("port-map", "Port to application mapping (PAM) configuration commands");
   globalC.ip.addSC("prefix-list", "Build a prefix list");
   globalC.ip.addSC("radius", "RADIUS configuration commands");
   globalC.ip.addSC("rcmd", "Rcmd commands");
   globalC.ip.addSC("reflexive-list", "Reflexive access list");
   globalC.ip.addSC("route", "Establish static routes");
      globalC.ip.route.addSC("A.B.C.D", "Destination prefix");
         globalC.ip.route["A.B.C.D"].addSC("A.B.C.D", "Destination prefix mask");
            globalC.ip.route["A.B.C.D"]["A.B.C.D"].addSC("A.B.C.D", "Forwarding router's address");
               globalC.ip.route["A.B.C.D"]["A.B.C.D"]["A.B.C.D"].addSC("<1-255>", "Distance metric for this route");
               globalC.ip.route["A.B.C.D"]["A.B.C.D"]["A.B.C.D"].addSC("name", "Specify name of the next hop");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"]["A.B.C.D"].name.addSC("WORD", "Name of the next hop");
               globalC.ip.route["A.B.C.D"]["A.B.C.D"]["A.B.C.D"].addSC("permanent", "permanent route");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"]["A.B.C.D"].permanent.addSC("<1-255>", "Distance metric for this route");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"]["A.B.C.D"].permanent.addSC("name", "Specify name of the next hop");
               globalC.ip.route["A.B.C.D"]["A.B.C.D"]["A.B.C.D"].addSC("tag", "Set tag for this route");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"]["A.B.C.D"].tag.addSC("<1-4294967295>", "Tag value");
            globalC.ip.route["A.B.C.D"]["A.B.C.D"].addSC("Async", "Async interface");
            globalC.ip.route["A.B.C.D"]["A.B.C.D"].addSC("Dialer", "Dialer interface");
            globalC.ip.route["A.B.C.D"]["A.B.C.D"].addSC("FastEthernet", "FastEthernet IEEE 802.3");
               globalC.ip.route["A.B.C.D"]["A.B.C.D"].FastEthernet.addSC("<0-1>", "FastEthernet interface number");
            globalC.ip.route["A.B.C.D"]["A.B.C.D"].addSC("Loopback", "Loopback interface");
               globalC.ip.route["A.B.C.D"]["A.B.C.D"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"].Loopback["<0-2147483647>"].addSC("<1-255>", "Distance metric for this route");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"].Loopback["<0-2147483647>"].addSC("A.B.C.D", "Forwarding router's address");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"].Loopback["<0-2147483647>"].addSC("name", "Specify name of the next hop");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"].Loopback["<0-2147483647>"].addSC("permanent", "permanent route");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"].Loopback["<0-2147483647>"].addSC("tag", "Set tag for this route");
            globalC.ip.route["A.B.C.D"]["A.B.C.D"].addSC("Null", "Null interface");
               globalC.ip.route["A.B.C.D"]["A.B.C.D"].Null.addSC("<0-0>", "Null interface number");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"].Null["<0-0>"].addSC("<1-255>", "Distance metric for this route");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"].Null["<0-0>"].addSC("A.B.C.D", "Forwarding router's address");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"].Null["<0-0>"].addSC("name", "Specify name of the next hop");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"].Null["<0-0>"].addSC("permanent", "permanent route");
                  globalC.ip.route["A.B.C.D"]["A.B.C.D"].Null["<0-0>"].addSC("tag", "Set tag for this route");
            globalC.ip.route["A.B.C.D"]["A.B.C.D"].addSC("Serial", "Serial");
               globalC.ip.route["A.B.C.D"]["A.B.C.D"].Serial.addSC("<0-1>", "Serial interface number");
      globalC.ip.route.addSC("profile", "Enable IP routing table profile");
      globalC.ip.route.addSC("vrf", "Configure static route for a VPN Routing/Forwarding instance");
   globalC.ip.addSC("routing", "Enable IP routing");
   globalC.ip.addSC("rsvp", "Configure static RSVP information");
   globalC.ip.addSC("sap", "Global IP Multicast SAP Commands");
   globalC.ip.addSC("sdr", "Global IP Multicast SDR Commands");
   globalC.ip.addSC("security", "Specify system wide security information");
   globalC.ip.addSC("source-route", "Process packets with source routing header options");
   globalC.ip.addSC("subnet-zero", "Allow 'subnet zero' subnets");
   globalC.ip.addSC("tacacs", "TACACS configuration commands");
   globalC.ip.addSC("tcp", "Global TCP parameters");
   globalC.ip.addSC("telnet", "Specify telnet options");
   globalC.ip.addSC("tftp", "tftp configuration commands");
   globalC.ip.addSC("trigger-authentication", "Trigger-authentication configurations parameters");
   globalC.ip.addSC("vrf", "Configure an IP VPN Routing/Forwarding instance");
   globalC.ip.addSC("wccp", "Web-Cache Coordination Protocol Commands");
globalC.addSC("ipx", "Novell/IPX global configuration commands");
globalC.addSC("isdn", "ISDN configuration commands");
globalC.addSC("isis", "Global ISIS configuration subcommands");
globalC.addSC("kerberos", "Configure Kerberos");
globalC.addSC("key", "Key management");
globalC.addSC("keymap", "Define a new keymap");
globalC.addSC("lane", "Configure LAN Emulation");
globalC.addSC("lat", "DEC Local Area Transport (LAT) transmission protocol");
globalC.addSC("line", "Configure a terminal line");
   globalC.line.addSC("<0-70>", "First Line number");
      globalC.line["<0-70>"].addSC("<1-70>", "Last Line number");
   globalC.line.addSC("aux", "Auxiliary line");
      globalC.line.aux.addSC("<0-0>", "First Line number");
   globalC.line.addSC("console", "Primary terminal line");
      globalC.line.console.addSC("<0-0>", "First Line number");
   globalC.line.addSC("tty", "Terminal controller");
      globalC.line.tty.addSC("<1-64>", "First Line number");
         globalC.line.tty["<1-64>"].addSC("<2-64>", "Last Line number");
   globalC.line.addSC("vty", "Virtual terminal");
      globalC.line.vty.addSC("<0-133>", "First Line number");
         globalC.line.vty["<0-133>"].addSC("<1-133>", "Last Line number");
globalC.addSC("lnm", "IBM Lan Manager");
globalC.addSC("locaddr-priority-list", "Establish queueing priorities based on LU address");
globalC.addSC("location", "Network Management Router location Command");
globalC.addSC("logging", "Modify message logging facilities");
globalC.addSC("login-string", "Define a host-specific login string");
globalC.addSC("map-class", "Configure static map class");
   globalC["map-class"].addSC("atm", "Asynchronous transfer mode");
   globalC["map-class"].addSC("dialer", "Dial on Demand");
   globalC["map-class"].addSC("frame-relay", "Frame Relay");
      globalC["map-class"]["frame-relay"].addSC("WORD", "Static map class name");
globalC.addSC("map-list", "Configure static map list");
globalC.addSC("memory-size", "Adjust memory size by percentage");
globalC.addSC("menu", "Define a user-interface menu");
globalC.addSC("modemcap", "Modem Capabilities database");
globalC.addSC("mop", "Configure the DEC MOP Server");
globalC.addSC("mpoa", "MPOA global configuration commands");
globalC.addSC("multilink", "PPP multilink global configuration");
globalC.addSC("ncia", "Native Client Interface Architecture");
globalC.addSC("netbios", "NETBIOS access control filtering");
globalC.addSC("no", "Negate a command or set its defaults");
   globalC.no.addSC("aaa", "Authentication, Authorization and Accounting.");
   globalC.no.addSC("access-list", "Add an access list entry");
   globalC.no.addSC("alias", "Create command alias");
   globalC.no.addSC("alps", "Configure Airline Protocol Support");
   globalC.no.addSC("apollo", "Apollo global configuration commands");
   globalC.no.addSC("appletalk", "Appletalk global configuration commands");
   globalC.no.addSC("arap", "Appletalk Remote Access Protocol");
   globalC.no.addSC("arp", "Set a static ARP entry");
   globalC.no.addSC("async-bootp", "Modify system bootp parameters");
   globalC.no.addSC("autonomous-system", "Specify local AS number to which we belong");
   globalC.no.addSC("banner", "Define a login banner");
   globalC.no.addSC("boot", "Modify system boot parameters");
   globalC.no.addSC("bridge", "Bridge Group.");
   globalC.no.addSC("bstun", "BSTUN global configuration commands");
   globalC.no.addSC("buffers", "Adjust system buffer pool parameters");
   globalC.no.addSC("busy-message", "Display message when connection to host fails");
   globalC.no.addSC("call-history-mib", "Define call history mib parameters");
   globalC.no.addSC("cdp", "Global CDP configuration subcommands");
   globalC.no.addSC("chat-script", "Define a modem chat script");
   globalC.no.addSC("class-map", "Configure QoS Class Map");
   globalC.no.addSC("clns", "Global CLNS configuration subcommands");
   globalC.no.addSC("clock", "Configure time-of-day clock");
   globalC.no.addSC("cns", "CNS Subsystems");
   globalC.no.addSC("config-register", "Define the configuration register");
   globalC.no.addSC("controller", "Configure a specific controller");
   globalC.no.addSC("crypto", "Encryption module");
   globalC.no.addSC("decnet", "Global DECnet configuration subcommands");
   globalC.no.addSC("default-value", "Default character-bits values");
   globalC.no.addSC("dial-control-mib", "Define Dial Control Mib parameters");
   globalC.no.addSC("dial-peer", "Dial Map (Peer) configuration commands");
   globalC.no.addSC("dialer", "Dialer commands");
   globalC.no.addSC("dialer-list", "Create a dialer list entry");
   globalC.no.addSC("dlsw", "Data Link Switching global configuration commands");
   globalC.no.addSC("dnsix-dmdp", "Provide DMDP service for DNSIX");
   globalC.no.addSC("dnsix-nat", "Provide DNSIX service for audit trails");
   globalC.no.addSC("downward-compatible-config", "Generate a configuration compatible with older software");
   globalC.no.addSC("dspu", "DownStream Physical Unit Command");
   globalC.no.addSC("enable", "Modify enable password parameters");
   globalC.no.addSC("end", "Exit from configure mode");
   globalC.no.addSC("endnode", "SNA APPN endnode command");
   globalC.no.addSC("exception", "Exception handling");
   globalC.no.addSC("exit", "Exit from configure mode");
   globalC.no.addSC("file", "Adjust file system parameters");
   globalC.no.addSC("frame-relay", "global frame relay configuration commands");
   globalC.no.addSC("gateway", "Gateway");
   globalC.no.addSC("gw-accounting", "Enable voip gateway accounting.");
   globalC.no.addSC("hostname", "Set system's network name");
   globalC.no.addSC("interface", "Select an interface to configure");
   globalC.no.addSC("ip", "Global IP configuration subcommands");
      globalC.no.ip.addSC("access-list", "Named access-list");
      globalC.no.ip.addSC("accounting-list", "Select hosts for which IP accounting information is kept");
      globalC.no.ip.addSC("accounting-threshold", "Sets the maximum number of accounting entries");
      globalC.no.ip.addSC("accounting-transits", "Sets the maximum number of transit entries");
      globalC.no.ip.addSC("address-pool", "Specify default IP address pooling mechanism");
      globalC.no.ip.addSC("alias", "Alias an IP address to a TCP port");
      globalC.no.ip.addSC("as-path", "BGP autonomous system path filter");
      globalC.no.ip.addSC("audit", "Intrusion Detection System");
      globalC.no.ip.addSC("auth-proxy", "Authentication Proxy");
      globalC.no.ip.addSC("bgp-community", "format for BGP community");
      globalC.no.ip.addSC("bootp", "Config BOOTP services");
      globalC.no.ip.addSC("cef", "Cisco Express Forwarding");
      globalC.no.ip.addSC("classless", "Follow classless routing forwarding rules");
      globalC.no.ip.addSC("community-list", "Add a community list entry");
      globalC.no.ip.addSC("default-gateway", "Specify default gateway (if not routing IP)");
      globalC.no.ip.addSC("default-network", "Flags networks as candidates for default routes");
      globalC.no.ip.addSC("dhcp", "Configure DHCP server and relay parameters");
      globalC.no.ip.addSC("dhcp-server", "Specify address of DHCP server to use");
      globalC.no.ip.addSC("domain-list", "Domain name to complete unqualified host names.");
      globalC.no.ip.addSC("domain-lookup", "Enable IP Domain Name System hostname translation");
         globalC.no.ip["domain-lookup"].addSC("nsap", "Enable IP DNS queries for CLNS NSAP addresses");
      globalC.no.ip.addSC("domain-name", "Define the default domain name");
      globalC.no.ip.addSC("drp", "Director response protocol configuration commands");
      globalC.no.ip.addSC("dvmrp", "DVMRP global commands");
      globalC.no.ip.addSC("finger", "finger server");
      globalC.no.ip.addSC("flow-aggregation", "Configure flow aggregation");
      globalC.no.ip.addSC("flow-cache", "Configure netflow cache parameters");
      globalC.no.ip.addSC("flow-export", "Specify host/port to send flow statistics");
      globalC.no.ip.addSC("forward-protocol", "Controls forwarding of physical and directed IP broadcasts");
      globalC.no.ip.addSC("ftp", "FTP configuration commands");
      globalC.no.ip.addSC("gdp", "Router discovery mechanism");
      globalC.no.ip.addSC("gratuitous-arps", "Generate gratuitous ARPs for PPP/SLIP peer addresses");
      globalC.no.ip.addSC("host", "Add an entry to the ip hostname table");
      globalC.no.ip.addSC("host-routing", "Enable host-based routing (proxy ARP and redirect)");
      globalC.no.ip.addSC("hp-host", "Enable the HP proxy probe service");
      globalC.no.ip.addSC("http", "HTTP server configuration");
      globalC.no.ip.addSC("icmp", "ICMP options");
      globalC.no.ip.addSC("identd", "Ident server");
      globalC.no.ip.addSC("inspect", "Context-based Access Control Engine");
      globalC.no.ip.addSC("local", "Specify local options");
      globalC.no.ip.addSC("mobile", "Enable Mobile IP services");
      globalC.no.ip.addSC("mrm", "Configure IP Multicast Routing Monitor test parameters");
      globalC.no.ip.addSC("mroute", "Configure static multicast routes");
      globalC.no.ip.addSC("multicast", "Global IP Multicast Commands");
      globalC.no.ip.addSC("multicast-routing", "Enable IP multicast forwarding");
      globalC.no.ip.addSC("name-server", "Specify address of name server to use");
      globalC.no.ip.addSC("nat", "NAT configuration commands");
      globalC.no.ip.addSC("ospf", "OSPF");
      globalC.no.ip.addSC("pgm", "PGM Reliable Transport Protocol");
      globalC.no.ip.addSC("pim", "PIM global commands");
      globalC.no.ip.addSC("port-map", "Port to application mapping (PAM) configuration commands");
      globalC.no.ip.addSC("prefix-list", "Build a prefix list");
      globalC.no.ip.addSC("radius", "RADIUS configuration commands");
      globalC.no.ip.addSC("rcmd", "Rcmd commands");
      globalC.no.ip.addSC("reflexive-list", "Reflexive access list");
      globalC.no.ip.addSC("route", "Establish static routes");
      globalC.no.ip.addSC("routing", "Enable IP routing");
      globalC.no.ip.addSC("rsvp", "Configure static RSVP information");
      globalC.no.ip.addSC("sap", "Global IP Multicast SAP Commands");
      globalC.no.ip.addSC("sdr", "Global IP Multicast SDR Commands");
      globalC.no.ip.addSC("security", "Specify system wide security information");
      globalC.no.ip.addSC("source-route", "Process packets with source routing header options");
      globalC.no.ip.addSC("subnet-zero", "Allow 'subnet zero' subnets");
      globalC.no.ip.addSC("tacacs", "TACACS configuration commands");
      globalC.no.ip.addSC("tcp", "Global TCP parameters");
      globalC.no.ip.addSC("telnet", "Specify telnet options");
      globalC.no.ip.addSC("tftp", "tftp configuration commands");
      globalC.no.ip.addSC("trigger-authentication", "Trigger-authentication configurations parameters");
      globalC.no.ip.addSC("vrf", "Configure an IP VPN Routing/Forwarding instance");
      globalC.no.ip.addSC("wccp", "Web-Cache Coordination Protocol Commands");
   globalC.no.addSC("ipx", "Novell/IPX global configuration commands");
   globalC.no.addSC("isdn", "ISDN configuration commands");
   globalC.no.addSC("isis", "Global ISIS configuration subcommands");
   globalC.no.addSC("kerberos", "Configure Kerberos");
   globalC.no.addSC("key", "Key management");
   globalC.no.addSC("keymap", "Define a new keymap");
   globalC.no.addSC("lane", "Configure LAN Emulation");
   globalC.no.addSC("lat", "DEC Local Area Transport (LAT) transmission protocol");
   globalC.no.addSC("line", "Configure a terminal line");
   globalC.no.addSC("lnm", "IBM Lan Manager");
   globalC.no.addSC("locaddr-priority-list", "Establish queueing priorities based on LU address");
   globalC.no.addSC("location", "Network Management Router location Command");
   globalC.no.addSC("logging", "Modify message logging facilities");
   globalC.no.addSC("login-string", "Define a host-specific login string");
   globalC.no.addSC("map-class", "Configure static map class");
   globalC.no.addSC("map-list", "Configure static map list");
   globalC.no.addSC("memory-size", "Adjust memory size by percentage");
   globalC.no.addSC("menu", "Define a user-interface menu");
   globalC.no.addSC("modemcap", "Modem Capabilities database");
   globalC.no.addSC("mop", "Configure the DEC MOP Server");
   globalC.no.addSC("mpoa", "MPOA global configuration commands");
   globalC.no.addSC("multilink", "PPP multilink global configuration");
   globalC.no.addSC("ncia", "Native Client Interface Architecture");
   globalC.no.addSC("netbios", "NETBIOS access control filtering");
globalC.addSC("ntp", "Configure NTP");
globalC.addSC("num-exp", "Dial Map Number Expansion configuration commands");
globalC.addSC("partition", "Partition device");
globalC.addSC("policy-map", "Configure QoS Policy Map");
   globalC["policy-map"].addSC("WORD", "policy-map name");
globalC.addSC("printer", "Define an LPD printer");
globalC.addSC("priority-list", "Build a priority list");
globalC.addSC("privilege", "Command privilege parameters");
globalC.addSC("prompt", "Set system's prompt");
globalC.addSC("queue-list", "Build a custom queue list");
globalC.addSC("resume-string", "Define a host-specific resume string");
globalC.addSC("rif", "Source-route RIF cache");
globalC.addSC("rlogin", "Rlogin configuration commands");
globalC.addSC("rmon", "Remote Monitoring");
globalC.addSC("route-map", "Create route-map or enter route-map command mode");
globalC.addSC("router", "Enable a routing process");
   globalC.router.addSC("bgp", "Border Gateway Protocol (BGP)");
   globalC.router.addSC("egp", "Exterior Gateway Protocol (EGP)");
   globalC.router.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
      globalC.router.eigrp.addSC("<1-65535>", "Autonomous system number");
   globalC.router.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
   globalC.router.addSC("isis", "ISO IS-IS");
      globalC.router.isis.addSC("WORD", "ISO routing area tag");
   globalC.router.addSC("iso-igrp", "IGRP for OSI networks");
   globalC.router.addSC("mobile", "Mobile routes");
   globalC.router.addSC("odr", "On Demand stub Routes");
   globalC.router.addSC("ospf", "Open Shortest Path First (OSPF)");
      globalC.router.ospf.addSC("<1-65535>", "Process ID");
   globalC.router.addSC("rip", "Routing Information Protocol (RIP)");
   globalC.router.addSC("static", "Static routes");
   globalC.router.addSC("traffic-engineering", "Traffic engineered routes");
globalC.addSC("rsrb", "RSRB LSAP/DSAP filtering");
globalC.addSC("rtr", "RTR Base Configuration");
globalC.addSC("sap-priority-list", "Establish queueing priorities based on SAP and/or MAC address(es)");
globalC.addSC("scheduler", "Scheduler parameters");
globalC.addSC("service", "Modify use of network based services");
globalC.addSC("sgbp", "SGBP Stack Group Bidding Protocol configuration");
globalC.addSC("smrp", "Simple Multicast Routing Protocol configuration commands");
globalC.addSC("sna", "Network Management Physical Unit Command");
globalC.addSC("snmp-server", "Modify SNMP parameters");
globalC.addSC("source-bridge", "Source-route bridging ring groups");
globalC.addSC("stackmaker", "Specify stack name and add its member");
globalC.addSC("state-machine", "Define a TCP dispatch state machine");
globalC.addSC("stun", "STUN global configuration commands");
globalC.addSC("subscriber-policy", "Subscriber policy");
globalC.addSC("tacacs-server", "Modify TACACS query parameters");
globalC.addSC("tarp", "Global TARP configuration subcommands");
globalC.addSC("terminal-queue", "Terminal queue commands");
globalC.addSC("tftp-server", "Provide TFTP service for netload requests");
globalC.addSC("time-range", "Define time range entries");
globalC.addSC("tn3270", "tn3270 configuration command");
globalC.addSC("translate", "Translate global configuration commands");
globalC.addSC("ttycap", "Define a new termcap");
globalC.addSC("username", "Establish User Name Authentication");
globalC.addSC("vines", "VINES global configuration commands");
globalC.addSC("virtual-profile", "Virtual Profile configuration");
globalC.addSC("voice", "Global voice configuration");
globalC.addSC("vpdn", "Virtual Private Dialup Network");
globalC.addSC("vpdn-group", "VPDN group configuration");
globalC.addSC("vty-async", "Enable virtual async line configuration");
globalC.addSC("x25", "X.25 Level 3");
globalC.addSC("x29", "X29 commands");
globalC.addSC("xns", "XNS global configuration commands");
globalC.addSC("xremote", "Configure XRemote");
