Modules: | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | CS | All |
Module 6: Routing and Routing Protocols
| Command | Command Description | Command Syntax
6.1.2 | ip route | To establish static routes, use the ip route global configuration command. To remove static routes, use the no form of this command. | ip route prefix mask {address | interface} [distance] [tag tag] [permanent]
6.1.4 | ip route 0.0.0.0 0.0.0.0 [next-hop-address | outgoing interface] | To establish static routes, use the ip route global configuration command. To remove static routes, use the no form of this command. | ip route prefix mask {address | interface} [distance] [tag tag] [permanent]
6.1.5 | ip default-network | To select a network as a candidate route for computing the gateway of last resort, use the ip default-network global configuration command. | ip default-network network-number
6.1.6 | show ip route | Use the show ip route EXEC command to display the current state of the routing table. | show ip route [address [mask] [longer-prefixes]] | [protocol [process-id]] | [list access-list-number | access-list-name]
6.3.2 | router rip | To configure the Routing Information Protocol (RIP) routing process, use the router rip global configuration command. | router rip
| network x.x.x.x | To specify a list of networks for a Routing Information Protocol (RIP), RIP version 2, or Interior Gateway Routing Protocol (IGRP) routing process, use this form of the network router configuration command. | network network-address

| Close Window |

| All contents copyright © 2003 Cisco Systems, Inc. All rights reserved.