
intLoopBackC.addSC("access-expression", "Build a bridge boolean access expression");
intLoopBackC.addSC("apollo", "Apollo interface subcommands");
intLoopBackC.addSC("appletalk", "Appletalk interface subcommands");
intLoopBackC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
intLoopBackC.addSC("backup", "Modify backup parameters");
intLoopBackC.addSC("bandwidth", "Set bandwidth informational parameter");
	intLoopBackC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
intLoopBackC.addSC("bridge-group", "Transparent bridging interface parameters");
intLoopBackC.addSC("carrier-delay", "Specify delay for interface transitions");
intLoopBackC.addSC("clns", "CLNS interface subcommands");
intLoopBackC.addSC("crypto", "Encryption/Decryption commands");
	intLoopBackC.crypto.addSC("map", "Assign a Crypto Map");
		intLoopBackC.crypto.map.addSC("WORD", "Crypto Map tag");
intLoopBackC.addSC("decnet", "Interface DECnet config commands");
intLoopBackC.addSC("default", "Set a command to its defaults");
intLoopBackC.addSC("delay", "Specify interface throughput delay");
intLoopBackC.addSC("description", "Interface specific description");
intLoopBackC.addSC("dspu", "Down Stream PU");
intLoopBackC.addSC("exit", "Exit from interface configuration mode");
intLoopBackC.addSC("fras", "DLC Switch Interface Command");
intLoopBackC.addSC("h323-gateway", "Configure H323 Gateway");
intLoopBackC.addSC("help", "Description of the interactive help system");
intLoopBackC.addSC("hold-queue", "Set hold queue depth");
intLoopBackC.addSC("ip", "Interface Internet Protocol config commands");
	intLoopBackC.ip.addSC("access-group", "Specify access control for packets");
	intLoopBackC.ip.addSC("accounting", "Enable IP accounting on this interface");
	intLoopBackC.ip.addSC("address", "Set the IP address of an interface");
		intLoopBackC.ip.address.addSC("A.B.C.D", "IP address");
			intLoopBackC.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
				intLoopBackC.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
	intLoopBackC.ip.addSC("audit", "Apply IDS audit name");
	intLoopBackC.ip.addSC("auth-proxy", "Apply authenticaton proxy");
	intLoopBackC.ip.addSC("authentication", "authentication subcommands");
	intLoopBackC.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
			intLoopBackC.ip["bandwidth-percent"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intLoopBackC.ip["bandwidth-percent"].eigrp.addSC("<1-65535>",  "Autonomous system number");
					intLoopBackC.ip["bandwidth-percent"].eigrp["<1-65535>"].addSC("<1-999999>",  "Maximum bandwidth percentage that EIGRP may use");

	intLoopBackC.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
	intLoopBackC.ip.addSC("cgmp", "Enable/disable CGMP");
	intLoopBackC.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
	intLoopBackC.ip.addSC("dvmrp", "DVMRP interface commands");
	intLoopBackC.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
	intLoopBackC.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
			intLoopBackC.ip["helper-address"].addSC("A.B.C.D",  "IP destination address");
	intLoopBackC.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
	intLoopBackC.ip.addSC("igmp", "IGMP interface commands");
	intLoopBackC.ip.addSC("inspect", "Apply inspect name");
	intLoopBackC.ip.addSC("irdp", "ICMP Router Discovery Protocol");
	intLoopBackC.ip.addSC("load-sharing", "Style of load sharing");
	intLoopBackC.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
	intLoopBackC.ip.addSC("mobile", "Mobile IP support");
	intLoopBackC.ip.addSC("mrm", "Configure IP Multicast Routing Monitor tester");
	intLoopBackC.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
	intLoopBackC.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
	intLoopBackC.ip.addSC("multicast", "IP multicast interface commands");
	intLoopBackC.ip.addSC("nat", "NAT interface commands");
		intLoopBackC.ip.nat.addSC("inside", "Inside interface for address translation");
		intLoopBackC.ip.nat.addSC("outside", "Outside interface for address translation");
	intLoopBackC.ip.addSC("ospf", "OSPF interface commands");
		intLoopBackC.ip.ospf.addSC("authentication-key", "Authentication password (key)");
		intLoopBackC.ip.ospf.addSC("cost", "Interface cost");
		intLoopBackC.ip.ospf.addSC("database-filter", "Filter OSPF LSA during synchronization and flooding");
		intLoopBackC.ip.ospf.addSC("dead-interval", "Interval after which a neighbor is declared dead");
			intLoopBackC.ip.ospf["dead-interval"].addSC("<1-65535>", "Seconds");
		intLoopBackC.ip.ospf.addSC("demand-circuit", "OSPF demand circuit");
		intLoopBackC.ip.ospf.addSC("hello-interval", "Time between HELLO packets");
			intLoopBackC.ip.ospf["hello-interval"].addSC("<1-65535>", "Seconds");
		intLoopBackC.ip.ospf.addSC("message-digest-key", "Message digest authentication password (key)");
		intLoopBackC.ip.ospf.addSC("network", "Network type");
		intLoopBackC.ip.ospf.addSC("priority", "Router priority");
		intLoopBackC.ip.ospf.addSC("retransmit-interval", "Time between retransmitting lost link state advertisements");
		intLoopBackC.ip.ospf.addSC("transmit-delay", "Link state transmit delay");
	intLoopBackC.ip.addSC("pgm", "PGM Reliable Transport Protocol");
	intLoopBackC.ip.addSC("pim", "PIM interface commands");
	intLoopBackC.ip.addSC("policy", "Enable policy routing");
	intLoopBackC.ip.addSC("probe", "Enable HP Probe support");
	intLoopBackC.ip.addSC("proxy-arp", "Enable proxy ARP");
	intLoopBackC.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
	intLoopBackC.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
	intLoopBackC.ip.addSC("rip", "Router Information Protocol");
	intLoopBackC.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
	intLoopBackC.ip.addSC("router", "IP router interface commands");
		intLoopBackC.ip.router.addSC("isis", "IS-IS Routing for IP");
			intLoopBackC.ip.router.isis.addSC("WORD", "Routing process tag");
	intLoopBackC.ip.addSC("rsvp", "RSVP interface commands");
	intLoopBackC.ip.addSC("rtp", "RTP parameters");
	intLoopBackC.ip.addSC("sap", "Session Advertisement Protocol interface commands");
	intLoopBackC.ip.addSC("sdr", "Session Directory Protocol interface commands");
	intLoopBackC.ip.addSC("security", "DDN IP Security Option");
	intLoopBackC.ip.addSC("split-horizon", "Perform split horizon");
	intLoopBackC.ip.addSC("summary-address", "Perform address summarization");
      intLoopBackC.ip["summary-address"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
         intLoopBackC.ip["summary-address"].eigrp.addSC("<1-65535>", "Autonomous system number");
            intLoopBackC.ip["summary-address"].eigrp["<1-65535>"].addSC("A.B.C.D", "IP address");
               intLoopBackC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"].addSC("A.B.C.D", "IP network mask");
                  intLoopBackC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"]["A.B.C.D"].addSC("<1-255>", "Administrative distance");
      intLoopBackC.ip["summary-address"].addSC("rip", "Routing Information Protocol (RIP)");
         intLoopBackC.ip["summary-address"].rip.addSC("A.B.C.D", "IP address");
            intLoopBackC.ip["summary-address"].rip["A.B.C.D"].addSC("A.B.C.D", "IP network mask");

	intLoopBackC.ip.addSC("tcp", "TCP header compression parameters");
	intLoopBackC.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
	intLoopBackC.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
	intLoopBackC.ip.addSC("verify", "Enable per packet validation");
	intLoopBackC.ip.addSC("vrf", "VPN Routing/Forwarding parameters on the interface");
	intLoopBackC.ip.addSC("wccp", "WCCP interface commands");
intLoopBackC.addSC("ipx", "Novell/IPX interface subcommands");
intLoopBackC.addSC("isis", "IS-IS commands");
	intLoopBackC.isis.addSC("adjacency-filter", "Filter IS-IS adjacencies");
	intLoopBackC.isis.addSC("circuit-type", "Configure circuit type for interface");
	intLoopBackC.isis.addSC("csnp-interval", "Set CSNP interval in seconds");
	intLoopBackC.isis.addSC("hello", "Add padding to IS-IS hello packets");
	intLoopBackC.isis.addSC("hello-interval", "Set Hello interval in seconds");
		intLoopBackC.isis["hello-interval"].addSC("<1-65535>", "Hello interval value");
			intLoopBackC.isis["hello-interval"]["<1-65535>"].addSC("level-1", "Specify hello-interval for level-1 IIHs");
			intLoopBackC.isis["hello-interval"]["<1-65535>"].addSC("level-2", "Specify hello-interval for level-2 IIHs");
		intLoopBackC.isis["hello-interval"].addSC("minimal", "Holdtime 1 second, interval depends on multiplier");
			intLoopBackC.isis["hello-interval"].minimal.addSC("level-1", "Specify hello-interval for level-1 IIHs");
			intLoopBackC.isis["hello-interval"].minimal.addSC("level-2", "Specify hello-interval for level-2 IIHs");
	intLoopBackC.isis.addSC("hello-multiplier", "Set multiplier for Hello holding time");
	intLoopBackC.isis.addSC("lsp-interval", "Set LSP transmission interval");
	intLoopBackC.isis.addSC("mesh-group", "Set ISIS mesh group");
	intLoopBackC.isis.addSC("metric", "Configure the metric for interface");
	intLoopBackC.isis.addSC("password", "Configure the authentication password for interface");
		intLoopBackC.isis.password.addSC("WORD", "Password");
			intLoopBackC.isis.password.WORD.addSC("level-1", "Specify password for level-1 PDUs");
			intLoopBackC.isis.password.WORD.addSC("level-2", "Specify password for level-2 PDUs");
	intLoopBackC.isis.addSC("priority", "Set priority for Designated Router election");
	intLoopBackC.isis.addSC("retransmit-interval", "Set per-LSP retransmission interval");
	intLoopBackC.isis.addSC("retransmit-throttle-interval", "Set interface LSP retransmission interval");
intLoopBackC.addSC("iso-igrp", "ISO-IGRP interface subcommands");
intLoopBackC.addSC("keepalive", "Enable keepalive");
intLoopBackC.addSC("lan-name", "LAN Name command");
intLoopBackC.addSC("lat", "LAT commands");
intLoopBackC.addSC("llc2", "LLC2 Interface Subcommands");
intLoopBackC.addSC("load-interval", "Specify interval for load calculation for an interface");
	intLoopBackC["load-interval"].addSC("<30-600>", "Load interval delay in seconds");
intLoopBackC.addSC("locaddr-priority", "Assign a priority group");
intLoopBackC.addSC("logging", "Configure logging for interface");
intLoopBackC.addSC("mpoa", "MPOA interface configuration commands");
intLoopBackC.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
intLoopBackC.addSC("multilink-group", "Put interface in a multilink bundle");
intLoopBackC.addSC("netbios", "Use a defined NETBIOS access list or enable name-caching");
intLoopBackC.addSC("no", "Negate a command or set its defaults");
	intLoopBackC.no.addSC("access-expression", "Build a bridge boolean access expression");
	intLoopBackC.no.addSC("apollo", "Apollo interface subcommands");
	intLoopBackC.no.addSC("appletalk", "Appletalk interface subcommands");
	intLoopBackC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	intLoopBackC.no.addSC("backup", "Modify backup parameters");
	intLoopBackC.no.addSC("bandwidth", "Set bandwidth informational parameter");
	intLoopBackC.no.addSC("bridge-group", "Transparent bridging interface parameters");
	intLoopBackC.no.addSC("carrier-delay", "Specify delay for interface transitions");
	intLoopBackC.no.addSC("cdp", "CDP interface subcommands");
	intLoopBackC.no.addSC("clns", "CLNS interface subcommands");
	intLoopBackC.no.addSC("crypto", "Encryption/Decryption commands");
	intLoopBackC.no.addSC("decnet", "Interface DECnet config commands");
	intLoopBackC.no.addSC("delay", "Specify interface throughput delay");
	intLoopBackC.no.addSC("description", "Interface specific description");
	intLoopBackC.no.addSC("dspu", "Down Stream PU");
	intLoopBackC.no.addSC("fras", "DLC Switch Interface Command");
	intLoopBackC.no.addSC("h323-gateway", "Configure H323 Gateway");
	intLoopBackC.no.addSC("hold-queue", "Set hold queue depth");
	intLoopBackC.no.addSC("ip", "Interface Internet Protocol config commands");
		intLoopBackC.no.ip.addSC("access-group", "Specify access control for packets");
		intLoopBackC.no.ip.addSC("accounting", "Enable IP accounting on this interface");
		intLoopBackC.no.ip.addSC("address", "Set the IP address of an interface");
			intLoopBackC.no.ip.address.addSC("A.B.C.D", "IP address");
				intLoopBackC.no.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
					intLoopBackC.no.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
		intLoopBackC.no.ip.addSC("audit", "Apply IDS audit name");
		intLoopBackC.no.ip.addSC("auth-proxy", "Apply authenticaton proxy");
		intLoopBackC.no.ip.addSC("authentication", "authentication subcommands");
		intLoopBackC.no.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
		intLoopBackC.no.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		intLoopBackC.no.ip.addSC("cgmp", "Enable/disable CGMP");
		intLoopBackC.no.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
		intLoopBackC.no.ip.addSC("dvmrp", "DVMRP interface commands");
		intLoopBackC.no.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
		intLoopBackC.no.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
		intLoopBackC.no.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
		intLoopBackC.no.ip.addSC("igmp", "IGMP interface commands");
		intLoopBackC.no.ip.addSC("inspect", "Apply inspect name");
		intLoopBackC.no.ip.addSC("irdp", "ICMP Router Discovery Protocol");
		intLoopBackC.no.ip.addSC("load-sharing", "Style of load sharing");
		intLoopBackC.no.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
		intLoopBackC.no.ip.addSC("mobile", "Mobile IP support");
		intLoopBackC.no.ip.addSC("mrm", "Configure IP Multicast Routing Monitor tester");
		intLoopBackC.no.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
		intLoopBackC.no.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		intLoopBackC.no.ip.addSC("multicast", "IP multicast interface commands");
		intLoopBackC.no.ip.addSC("nat", "NAT interface commands");
		intLoopBackC.no.ip.addSC("ospf", "OSPF interface commands");
		intLoopBackC.no.ip.addSC("pgm", "PGM Reliable Transport Protocol");
		intLoopBackC.no.ip.addSC("pim", "PIM interface commands");
		intLoopBackC.no.ip.addSC("policy", "Enable policy routing");
		intLoopBackC.no.ip.addSC("probe", "Enable HP Probe support");
		intLoopBackC.no.ip.addSC("proxy-arp", "Enable proxy ARP");
		intLoopBackC.no.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
		intLoopBackC.no.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
		intLoopBackC.no.ip.addSC("rip", "Router Information Protocol");
		intLoopBackC.no.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
		intLoopBackC.no.ip.addSC("router", "IP router interface commands");
		intLoopBackC.no.ip.addSC("rsvp", "RSVP interface commands");
		intLoopBackC.no.ip.addSC("rtp", "RTP parameters");
		intLoopBackC.no.ip.addSC("sap", "Session Advertisement Protocol interface commands");
		intLoopBackC.no.ip.addSC("sdr", "Session Directory Protocol interface commands");
		intLoopBackC.no.ip.addSC("security", "DDN IP Security Option");
		intLoopBackC.no.ip.addSC("split-horizon", "Perform split horizon");
		intLoopBackC.no.ip.addSC("summary-address", "Perform address summarization");
		intLoopBackC.no.ip.addSC("tcp", "TCP header compression parameters");
		intLoopBackC.no.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
		intLoopBackC.no.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
		intLoopBackC.no.ip.addSC("verify", "Enable per packet validation");
		intLoopBackC.no.ip.addSC("vrf", "VPN Routing/Forwarding parameters on the interface");
		intLoopBackC.no.ip.addSC("wccp", "WCCP interface commands");
	intLoopBackC.no.addSC("ipx", "Novell/IPX interface subcommands");
	intLoopBackC.no.addSC("isis", "IS-IS commands");
	intLoopBackC.no.addSC("iso-igrp", "ISO-IGRP interface subcommands");
	intLoopBackC.no.addSC("keepalive", "Enable keepalive");
	intLoopBackC.no.addSC("lan-name", "LAN Name command");
	intLoopBackC.no.addSC("lat", "LAT commands");
	intLoopBackC.no.addSC("llc2", "LLC2 Interface Subcommands");
	intLoopBackC.no.addSC("load-interval", "Specify interval for load calculation for an interface");
	intLoopBackC.no.addSC("locaddr-priority", "Assign a priority group");
	intLoopBackC.no.addSC("logging", "Configure logging for interface");
	intLoopBackC.no.addSC("mpoa", "MPOA interface configuration commands");
	intLoopBackC.no.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
	intLoopBackC.no.addSC("netbios", "Use a defined NETBIOS access list or enable name-caching");
intLoopBackC.addSC("ntp", "Configure NTP");
intLoopBackC.addSC("rate-limit", "Rate Limit");
intLoopBackC.addSC("sap-priority", "Assign a priority group");
intLoopBackC.addSC("service-policy", "Configure QoS Service Policy");
intLoopBackC.addSC("shutdown", "Shutdown the selected interface");
intLoopBackC.addSC("smrp", "Simple Multicast Routing Protocol interface subcommands");
intLoopBackC.addSC("sna", "SNA pu configuration");
intLoopBackC.addSC("snapshot", "Configure snapshot support on the interface");
intLoopBackC.addSC("snmp", "Modify SNMP interface parameters");
intLoopBackC.addSC("tarp", "TARP interface subcommands");
intLoopBackC.addSC("timeout", "Define timeout values for this interface");
intLoopBackC.addSC("transmit-interface", "Assign a transmit interface to a receive-only interface");
intLoopBackC.addSC("tx-queue-limit", "Configure card level transmit queue limit");
intLoopBackC.addSC("vines", "VINES interface subcommands");
intLoopBackC.addSC("xns", "XNS interface subcommands");
