
intEC.addSC("access-expression", "Build a bridge boolean access expression");
intEC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
intEC.addSC("bandwidth", "Set bandwidth informational parameter");
	intEC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
intEC.addSC("bridge-group", "Transparent bridging interface parameters");
intEC.addSC("carrier-delay", "Specify delay for interface transitions");
intEC.addSC("cdp", "CDP interface subcommands");
intEC.addSC("custom-queue-list", "Assign a custom queue list to an interface");
intEC.addSC("default", "Set a command to its defaults");
intEC.addSC("delay", "Specify interface throughput delay");
intEC.addSC("description", "Interface specific description");
intEC.addSC("dsl", "ADSL subcommands");
intEC.addSC("exit", "Exit from interface configuration mode");
intEC.addSC("fair-queue", "Enable Fair Queuing on an Interface");
intEC.addSC("h323-gateway", "Configure H323 Gateway");
intEC.addSC("help", "Description of the interactive help system");
intEC.addSC("hold-queue", "Set hold queue depth");
intEC.addSC("ip", "");
	intEC.ip.addSC("access-group", "Specify access control for packets");
	intEC.ip.addSC("accounting", "Enable IP accounting on this interface");
	intEC.ip.addSC("address", "Set the IP address of an interface");
		intEC.ip.address.addSC("A.B.C.D", "IP address");
			intEC.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
				intEC.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
		intEC.ip.address.addSC("dhcp", "IP Address negotiated via DHCP");
			intEC.ip.address.dhcp.addSC("client-id", "Specify client-id to use");
				intEC.ip.address.dhcp["client-id"].addSC("Ethernet", "IEEE 802.3");
					intEC.ip.address.dhcp["client-id"].Ethernet.addSC("<0-0>", "Ethernet interface number");
	intEC.ip.addSC("authentication", "authentication subcommands");
	intEC.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
			intEC.ip["bandwidth-percent"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intEC.ip["bandwidth-percent"].eigrp.addSC("<1-65535>",  "Autonomous system number");
					intEC.ip["bandwidth-percent"].eigrp["<1-65535>"].addSC("<1-999999>",  "Maximum bandwidth percentage that EIGRP may use");

	intEC.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
	intEC.ip.addSC("cef", "Cisco Express Fowarding interface commands");
	intEC.ip.addSC("cgmp", "Enable/disable CGMP");
	intEC.ip.addSC("directed-broadcole", "");
	intEC.ip.addSC("dvmrp", "DVMRP interface commands");
	intEC.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
	intEC.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
	intEC.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
	intEC.ip.addSC("igmp", "IGMP interface commands");
	intEC.ip.addSC("irdp", "ICMP Router Discovery Protocol");
	intEC.ip.addSC("load-sharing", "Style of load sharing");
	intEC.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
	intEC.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
	intEC.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
	intEC.ip.addSC("multicast", "IP multicast interface commands");
	intEC.ip.addSC("nat", "NAT interface commands");
		intEC.ip.nat.addSC("inside", "Inside interface for address translation");
		intEC.ip.nat.addSC("outside", "Outside interface for address translation");
	intEC.ip.addSC("pim", "PIM interface commands");
	intEC.ip.addSC("policy", "Enable policy routing");
	intEC.ip.addSC("probe", "Enable HP Probe support");
	intEC.ip.addSC("proxy-arp", "Enable proxy ARP");
	intEC.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
	intEC.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
	intEC.ip.addSC("rgmp", "Enable/disable RGMP");
	intEC.ip.addSC("rip", "Router Information Protocol");
	intEC.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
	intEC.ip.addSC("rsvp", "RSVP interface commands");
	intEC.ip.addSC("rtp", "RTP parameters");
	intEC.ip.addSC("sap", "Session Advertisement Protocol interface commands");
	intEC.ip.addSC("sdr", "Session Directory Protocol interface commands");
	intEC.ip.addSC("security", "DDN IP Security Option");
	intEC.ip.addSC("split-horizon", "Perform split horizon");
	intEC.ip.addSC("summary-address", "Perform address summarization");
         intEC.ip["summary-address"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
             intEC.ip["summary-address"].eigrp.addSC("<1-65535>", "Autonomous system number");
                 intEC.ip["summary-address"].eigrp["<1-65535>"].addSC("A.B.C.D", "IP address");
                     intEC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"].addSC("A.B.C.D", "IP network mask");
                         intEC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"]["A.B.C.D"].addSC("<1-255>", "Administrative distance");

	intEC.ip.addSC("tcp", "TCP header compression parameters");
	intEC.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
	intEC.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
	intEC.ip.addSC("urd", "Configure URL Rendezvousing");
	intEC.ip.addSC("verify", "Enable per packet validation");
	intEC.ip.addSC("vrf", "VPN Routing/Forwarding parameters on the interface");
intEC.addSC("ipx", "Novell/IPX interface subcommands");
intEC.addSC("keepalive", "Enable keepalive");
intEC.addSC("llc2", "LLC2 Interface Subcommands");
intEC.addSC("load-interval", "Specify interval for load calculation for an interface");
	intEC["load-interval"].addSC("<30-600>", "Load interval delay in seconds");
intEC.addSC("logging", "Configure logging for interface");
intEC.addSC("loopback", "Configure internal loopback on an interface");
intEC.addSC("mac-address", "Manually set interface MAC address");
intEC.addSC("max-reserved-bandwidth", "Maximum Reservable Bandwidth on an Interface");
intEC.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
intEC.addSC("multilink-group", "Put interface in a multilink bundle");
intEC.addSC("netbios", "Use a defined NETBIOS access list or enable name-caching");
intEC.addSC("no", "Negate a command or set its defaults");
	intEC.no.addSC("access-expression", "Build a bridge boolean access expression");
	intEC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	intEC.no.addSC("bandwidth", "Set bandwidth informational parameter");
	intEC.no.addSC("bridge-group", "Transparent bridging interface parameters");
	intEC.no.addSC("carrier-delay", "Specify delay for interface transitions");
	intEC.no.addSC("cdp", "CDP interface subcommands");
	intEC.no.addSC("custom-queue-list", "Assign a custom queue list to an interface");
	intEC.no.addSC("delay", "Specify interface throughput delay");
	intEC.no.addSC("description", "Interface specific description");
	intEC.no.addSC("dsl", "ADSL subcommands");
	intEC.no.addSC("fair-queue", "Enable Fair Queuing on an Interface");
	intEC.no.addSC("h323-gateway", "Configure H323 Gateway");
	intEC.no.addSC("hold-queue", "Set hold queue depth");
	intEC.no.addSC("ip", "Interface Internet Protocol config commands");
		intEC.no.ip.addSC("access-group", "Specify access control for packets");
		intEC.no.ip.addSC("accounting", "Enable IP accounting on this interface");
		intEC.no.ip.addSC("address", "Set the IP address of an interface");
			intEC.no.ip.address.addSC("A.B.C.D", "IP address");
				intEC.no.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
					intEC.no.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
			intEC.no.ip.address.addSC("dhcp", "IP Address negotiated via DHCP");
				intEC.no.ip.address.dhcp.addSC("client-id", "Specify client-id to use");
					intEC.no.ip.address.dhcp["client-id"].addSC("Ethernet", "IEEE 802.3");
						intEC.no.ip.address.dhcp["client-id"].Ethernet.addSC("<0-0>", "Ethernet interface number");
		intEC.no.ip.addSC("authentication", "authentication subcommands");
		intEC.no.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
		intEC.no.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		intEC.no.ip.addSC("cef", "Cisco Express Fowarding interface commands");
		intEC.no.ip.addSC("cgmp", "Enable/disable CGMP");
		intEC.no.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
		intEC.no.ip.addSC("dvmrp", "DVMRP interface commands");
		intEC.no.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
		intEC.no.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
		intEC.no.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
		intEC.no.ip.addSC("igmp", "IGMP interface commands");
		intEC.no.ip.addSC("irdp", "ICMP Router Discovery Protocol");
		intEC.no.ip.addSC("load-sharing", "Style of load sharing");
		intEC.no.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
		intEC.no.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
		intEC.no.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		intEC.no.ip.addSC("multicast", "IP multicast interface commands");
		intEC.no.ip.addSC("nat", "NAT interface commands");
		intEC.no.ip.addSC("pim", "PIM interface commands");
		intEC.no.ip.addSC("policy", "Enable policy routing");
		intEC.no.ip.addSC("probe", "Enable HP Probe support");
		intEC.no.ip.addSC("proxy-arp", "Enable proxy ARP");
		intEC.no.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
		intEC.no.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
		intEC.no.ip.addSC("rgmp", "Enable/disable RGMP");
		intEC.no.ip.addSC("rip", "Router Information Protocol");
		intEC.no.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
		intEC.no.ip.addSC("rsvp", "RSVP interface commands");
		intEC.no.ip.addSC("rtp", "RTP parameters");
		intEC.no.ip.addSC("sap", "Session Advertisement Protocol interface commands");
		intEC.no.ip.addSC("sdr", "Session Directory Protocol interface commands");
		intEC.no.ip.addSC("security", "DDN IP Security Option");
		intEC.no.ip.addSC("split-horizon", "Perform split horizon");
		intEC.no.ip.addSC("summary-address", "Perform address summarization");
		intEC.no.ip.addSC("tcp", "TCP header compression parameters");
		intEC.no.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
		intEC.no.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
		intEC.no.ip.addSC("urd", "Configure URL Rendezvousing");
		intEC.no.ip.addSC("verify", "Enable per packet validation");
		intEC.no.ip.addSC("vrf", "VPN Routing/Forwarding parameters on the interface");
	intEC.no.addSC("ipx", "Novell/IPX interface subcommands");
	intEC.no.addSC("keepalive", "Enable keepalive");
	intEC.no.addSC("llc2", "LLC2 Interface Subcommands");
	intEC.no.addSC("load-interval", "Specify interval for load calculation for an interface");
	intEC.no.addSC("logging", "Configure logging for interface");
	intEC.no.addSC("loopback", "Configure internal loopback on an interface");
	intEC.no.addSC("mac-address", "Manually set interface MAC address");
	intEC.no.addSC("max-reserved-bandwidth", "Maximum Reservable Bandwidth on an Interface");
	intEC.no.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
	intEC.no.addSC("multilink-group", "Put interface in a multilink bundle");
	intEC.no.addSC("netbios", "Use a defined NETBIOS access list or enable name-caching");
	intEC.no.addSC("random-detect", "Enable Weighted Random Early Detection (WRED) on an Interface");
	intEC.no.addSC("shutdown","Shutdown the selected interface");
	intEC.no.addSC("transmit-interface", "Assign a transmit interface to a receive-only interface");
intEC.addSC("pppoe", "pppoe interface subcommands");
intEC.addSC("pppoe-client", "pppoe client");
intEC.addSC("priority-group", "Assign a priority group to an interface");
intEC.addSC("service-policy", "Configure QoS Service Policy");
intEC.addSC("shutdown", "Shutdown the selected interface");
intEC.addSC("snapshot", "Configure snapshot support on the interface");
intEC.addSC("snmp", "Modify SNMP interface parameters");
intEC.addSC("standby", "Interface HSRP configuration commands");
intEC.addSC("timeout", "Define timeout values for this interface");
intEC.addSC("transmit-interface", "Assign a transmit sinterface to a receive-only interface");
intEC.addSC("tx-ring-limit", "Configure PA level transmit ring limit");
