
routerBGPC.addSC("address-family", "Enter Address Family command mode");
	routerBGPC["address-family"].addSC("ipv4", "Address family");
		routerBGPC["address-family"].ipv4.addSC("multicast", "Address Family modifier");
		routerBGPC["address-family"].ipv4.addSC("unicast", "Address Family modifier");
		routerBGPC["address-family"].ipv4.addSC("vrf", "Specify parameters for a VPN Routing/Forwarding instance");
			routerBGPC["address-family"].ipv4.vrf.addSC("WORD", "VPN Routing/Forwarding instance name");
	routerBGPC["address-family"].addSC("vpnv4", "Address family");
routerBGPC.addSC("aggregate-address", "Configure BGP aggregate entries");
	routerBGPC["aggregate-address"].addSC("A.B.C.D", "Aggregate address");
		routerBGPC["aggregate-address"]["A.B.C.D"].addSC("A.B.C.D", "Aggregate mask");
			routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"].addSC("advertise-map", "Set condition to advertise attribute");
				routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["advertise-map"].addSC("WORD", "Route map to control attribute advertisement");
			routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"].addSC("as-set", "Generate AS set path information");
				routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["as-set"].addSC("advertise-map", "Set condition to advertise attribute");
					routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["as-set"]["advertise-map"].addSC("WORD", "Route map to control attribute advertisement");
			routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"].addSC("attribute-map", "Set attributes of aggregate");
				routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["attribute-map"].addSC("WORD", "Route map for parameter control");
					routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["attribute-map"].WORD.addSC("advertise-map", "Set condition to advertise attribute");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["attribute-map"].WORD["advertise-map"].addSC("WORD", "Route map to control attribute advertisement");
					routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["attribute-map"].WORD.addSC("as-set", "Generate AS set path information");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["attribute-map"].WORD["as-set"].addSC("advertise-map", "Set condition to advertise attribute");
			routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"].addSC("route-map", "Set parameters of aggregate");
				routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["route-map"].addSC("WORD", "Route map for parameter control");
					routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["route-map"].WORD.addSC("as-set", "Generate AS set path information");
			routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"].addSC("summary-only", "Filter more specific routes from updates");
				routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["summary-only"].addSC("advertise-map", "Set condition to advertise attribute");
					routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["summary-only"]["advertise-map"].addSC("WORD", "Route map to control attribute advertisement");
				routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["summary-only"].addSC("as-set", "Generate AS set path information");
					routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["summary-only"]["as-set"].addSC("advertise-map", "Set condition to advertise attribute");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["summary-only"]["as-set"]["advertise-map"].addSC("WORD", "Route map to control attribute advertisement");
				routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["summary-only"].addSC("attribute-map", "Set attributes of aggregate");
					routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["summary-only"]["attribute-map"].addSC("WORD", "Route map for parameter control");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["summary-only"]["attribute-map"].WORD.addSC("advertise-map", "Set condition to advertise attribute");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["summary-only"]["attribute-map"].WORD.addSC("as-set", "Generate AS set path information");
				routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["summary-only"].addSC("route-map", "Set parameters of aggregate");
					routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["summary-only"]["route-map"].addSC("WORD", "Route map for parameter control");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["summary-only"]["route-map"].WORD.addSC("as-set", "Generate AS set path information");
			routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"].addSC("suppress-map", "Conditionally filter more specific routes from updates");
				routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].addSC("WORD", "Route map for suppression");
					routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].WORD.addSC("advertise-map", "Set condition to advertise attribute");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].WORD["advertise-map"].addSC("WORD", "Route map to control attribute advertisement");
					routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].WORD.addSC("as-set", "Generate AS set path information");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].WORD["as-set"].addSC("advertise-map", "Set condition to advertise attribute");
					routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].WORD.addSC("attribute-map", "Set attributes of aggregate");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].WORD["attribute-map"].addSC("WORD", "Route map for parameter control");
					routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].WORD.addSC("route-map", "Set parameters of aggregate");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].WORD["route-map"].addSC("WORD", "Route map for parameter control");
					routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].WORD.addSC("summary-only", "Filter more specific routes from updates");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].WORD["summary-only"].addSC("advertise-map", "Set condition to advertise attribute");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].WORD["summary-only"].addSC("as-set", "Generate AS set path information");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].WORD["summary-only"].addSC("attribute-map", "Set attributes of aggregate");
						routerBGPC["aggregate-address"]["A.B.C.D"]["A.B.C.D"]["suppress-map"].WORD["summary-only"].addSC("route-map", "Set parameters of aggregate");
routerBGPC.addSC("auto-summary", "Enable automatic network number summarization");
routerBGPC.addSC("bgp", "BGP specific commands");
	routerBGPC.bgp.addSC("always-compare-med", "Allow comparing MED from different neighbors");
	routerBGPC.bgp.addSC("bestpath", "Change the default bestpath selection");
		routerBGPC.bgp.bestpath.addSC("compare-routerid", "Compare router-id for identical EBGP paths");
		routerBGPC.bgp.bestpath.addSC("med", "MED attribute");
			routerBGPC.bgp.bestpath.med.addSC("confed", "Compare MED among confederation paths");
			routerBGPC.bgp.bestpath.med.addSC("missing-as-worst", "Treat missing MED as the least preferred one");
	routerBGPC.bgp.addSC("client-to-client", "Configure client to client route reflection");
		routerBGPC.bgp["client-to-client"].addSC("reflection", "reflection of routes allowed");
	routerBGPC.bgp.addSC("cluster-id", "Configure Route-Reflector Cluster-id");
		routerBGPC.bgp["cluster-id"].addSC("<1-4294967295>", "Route-Reflector Cluster-id as 32 bit quantity");
		routerBGPC.bgp["cluster-id"].addSC("A.B.C.D", "Route-Reflector Cluster-id in IP address format");
	routerBGPC.bgp.addSC("confederation", "AS confederation parameters");
		routerBGPC.bgp.confederation.addSC("identifier", "as number");
			routerBGPC.bgp.confederation.identifier.addSC("<1-65535>", "Set routing domain confederation AS");
		routerBGPC.bgp.confederation.addSC("peers", "Peer ASs in BGP confederation");
			routerBGPC.bgp.confederation.peers.addSC("<1-65535>", "AS number");
	routerBGPC.bgp.addSC("dampening", "Enable route-flap dampening");
		routerBGPC.bgp.dampening.addSC("<1-45>", "Half-life time for the penalty");
			routerBGPC.bgp.dampening["<1-45>"].addSC("<1-20000>", "Value to start reusing a route");
				routerBGPC.bgp.dampening["<1-45>"]["<1-20000>"].addSC("<1-20000>", "Value to start suppressing a route");
					routerBGPC.bgp.dampening["<1-45>"]["<1-20000>"]["<1-20000>"].addSC("<1-255>", "Maximum duration to suppress a stable route");
		routerBGPC.bgp.dampening.addSC("route-map", "Route-map to specify criteria for dampening");
			routerBGPC.bgp.dampening["route-map"].addSC("WORD", "route-map name");
	routerBGPC.bgp.addSC("default", "Configure BGP defaults");
		routerBGPC.bgp["default"].addSC("ipv4-unicast", "Activate ipv4-unicast for a peer by default");
		routerBGPC.bgp["default"].addSC("local-preference", "local preference (higher=more preferred)");
			routerBGPC.bgp["default"]["local-preference"].addSC("<0-4294967295>", "Configure default local preference value");
		routerBGPC.bgp["default"].addSC("route-target", "Control behavior based on Route-Target attributes");
			routerBGPC.bgp["default"]["route-target"].addSC("filter", "Control automatic VPN Route-Target filtering");
	routerBGPC.bgp.addSC("deterministic-med", "Pick the best-MED path among paths advertised from the neighboring AS");
	routerBGPC.bgp.addSC("fast-external-fallover", "Immediately reset session if a link to a directly connected external peer goes down");
	routerBGPC.bgp.addSC("log-neighbor-changes", "Log neighbor up/down and reset reason");
	routerBGPC.bgp.addSC("redistribute-internal", "Allow redistribution of iBGP into IGPs (dangerous)");
	routerBGPC.bgp.addSC("router-id", "Override configured router identifier");
		routerBGPC.bgp["router-id"].addSC("A.B.C.D", "Manually configured router identifier");
	routerBGPC.bgp.addSC("scan-time", "Configure background scanner interval");
		routerBGPC.bgp["scan-time"].addSC("<5-60>", "Scanner interval (seconds)");
routerBGPC.addSC("default", "Set a command to its defaults");
	routerBGPC["default"].addSC("address-family", "Enter Address Family command mode");
	routerBGPC["default"].addSC("aggregate-address", "Configure BGP aggregate entries");
	routerBGPC["default"].addSC("auto-summary", "Enable automatic network number summarization");
	routerBGPC["default"].addSC("bgp", "BGP specific commands");
routerBGPC.addSC("default-information", "Control distribution of default information");
	routerBGPC["default-information"].addSC("originate", "Distribute a default route");
routerBGPC.addSC("default-metric", "Set metric of redistributed routes");
	routerBGPC["default-metric"].addSC("<1-4294967295>", "Default metric");
routerBGPC.addSC("distance", "Define an administrative distance");
	routerBGPC.distance.addSC("<1-255>", "Administrative distance");
	routerBGPC.distance.addSC("bgp", "BGP distance");
routerBGPC.addSC("distribute-list", "Filter networks in routing updates");
	routerBGPC["distribute-list"].addSC("<1-199>", "IP access list number");
	routerBGPC["distribute-list"].addSC("<1300-2699>", "IP expanded access list number");
	routerBGPC["distribute-list"].addSC("WORD", "Access-list name");
	routerBGPC["distribute-list"].addSC("gateway", "Filtering incoming updates based on gateway");
	routerBGPC["distribute-list"].addSC("prefix", "Filter prefixes in routing updates");
routerBGPC.addSC("exit", "Exit from routing protocol configuration mode");
routerBGPC.addSC("help", "Description of the interactive help system");
routerBGPC.addSC("maximum-paths", "Forward packets over multiple paths");
	routerBGPC["maximum-paths"].addSC("<1-6>", "Number of paths");
routerBGPC.addSC("mpls", "Configure MPLS routing protocol parameters");
routerBGPC.addSC("neighbor", "Specify a neighbor router");
	routerBGPC.neighbor.addSC("A.B.C.D", "Neighbor address");
	routerBGPC.neighbor.addSC("WORD", "Neighbor tag");
routerBGPC.addSC("network", "Specify a network to announce via BGP");
	routerBGPC.network.addSC("A.B.C.D", "Network number");
		routerBGPC.network["A.B.C.D"].addSC("backdoor", "Specify a BGP backdoor route");
		routerBGPC.network["A.B.C.D"].addSC("mask", "Network mask");
			routerBGPC.network["A.B.C.D"].mask.addSC("A.B.C.D", "Network mask");
				routerBGPC.network["A.B.C.D"].mask["A.B.C.D"].addSC("backdoor", "Specify a BGP backdoor route");
		routerBGPC.network["A.B.C.D"].addSC("route-map", "Route-map to modify the attributes");
			routerBGPC.network["A.B.C.D"]["route-map"].addSC("WORD", "Name of the route map");
				routerBGPC.network["A.B.C.D"]["route-map"].WORD.addSC("backdoor", "Specify a BGP backdoor route");
routerBGPC.addSC("no", "Negate a command or set its defaults");
	routerBGPC.no.addSC("address-family", "Enter Address Family command mode");
	routerBGPC.no.addSC("aggregate-address", "Configure BGP aggregate entries");
	routerBGPC.no.addSC("auto-summary", "Enable automatic network number summarization");
	routerBGPC.no.addSC("bgp", "BGP specific commands");
	routerBGPC.no.addSC("default-information", "Control distribution of default information");
	routerBGPC.no.addSC("default-metric", "Set metric of redistributed routes");
	routerBGPC.no.addSC("distance", "Define an administrative distance");
	routerBGPC.no.addSC("distribute-list", "Filter networks in routing updates");
	routerBGPC.no.addSC("maximum-paths", "Forward packets over multiple paths");
	routerBGPC.no.addSC("mpls", "Configure MPLS routing protocol parameters");
	routerBGPC.no.addSC("neighbor", "Specify a neighbor router");
	routerBGPC.no.addSC("network", "Specify a network to announce via BGP");
routerBGPC.addSC("redistribute", "Redistribute information from another routing protocol");
	routerBGPC.redistribute.addSC("bgp", "Border Gateway Protocol (BGP)");
	routerBGPC.redistribute.addSC("connected", "Connected");
	routerBGPC.redistribute.addSC("dvmrp", "Redistribution of DVMRP into BGP IPv4 Multicast");
	routerBGPC.redistribute.addSC("egp", "Exterior Gateway Protocol (EGP)");
	routerBGPC.redistribute.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
	routerBGPC.redistribute.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
	routerBGPC.redistribute.addSC("isis", "ISO IS-IS");
	routerBGPC.redistribute.addSC("iso-igrp", "IGRP for OSI networks");
	routerBGPC.redistribute.addSC("mobile", "Mobile routes");
	routerBGPC.redistribute.addSC("odr", "On Demand stub Routes");
	routerBGPC.redistribute.addSC("ospf", "Open Shortest Path First (OSPF)");
	routerBGPC.redistribute.addSC("rip", "Routing Information Protocol (RIP)");
	routerBGPC.redistribute.addSC("static", "Static routes");
routerBGPC.addSC("synchronization", "Perform IGP synchronization");
routerBGPC.addSC("table-map", "Map external entry attributes into routing table");
	routerBGPC["table-map"].addSC("WORD", "route-map name");
routerBGPC.addSC("timers", "Adjust routing timers");
	routerBGPC.timers.addSC("bgp", "BGP timers");
