
userC.addSC("access-enable", "Create a temporary Access-List entry");
userC.addSC("access-profile", "Apply user-profile to interface");
userC.addSC("clear", "Reset functions");
	userC.clear.addSC("drip", "Clear drip");
	userC.clear.addSC("kerberos", "Clear Kerberos Values");
	userC.clear.addSC("ncia", "Native Client Interface Architecture (NCIA)");
userC.addSC("connect", "Open a terminal connection");
userC.addSC("disable", "Turn off privileged commands");
userC.addSC("disconnect", "Disconnect an existing network connection");
userC.addSC("enable", "Turn on privileged commands");
	userC.enable.addSC("<0-15>", "Enable level");
userC.addSC("exit", "Exit from the EXEC");
userC.addSC("help", "Description of the interactive help system");
userC.addSC("lat", "Open a lat connection");
userC.addSC("lock", "Lock the terminal");
userC.addSC("login", "Log in as a particular user");
userC.addSC("logout", "Exit from the EXEC");
userC.addSC("mrinfo", "Request neighbor and version information from a multicast router");
userC.addSC("mstat", "Show statistics after multiple multicast traceroutes");
userC.addSC("mtrace", "Trace reverse multicast path from destination to source");
userC.addSC("name-connection", "Name an existing network connection");
userC.addSC("pad", "Open a X.29 PAD connection");
userC.addSC("ping", "Send echo messages");
	userC.ping.addSC("WORD", "Ping destination address or hostname");
	userC.ping.addSC("apollo", "Apollo echo");
	userC.ping.addSC("appletalk", "Appletalk echo");
	userC.ping.addSC("clns", "CLNS echo");
	userC.ping.addSC("decnet", "DECnet echo");
	userC.ping.addSC("ip", "IP echo");
		userC.ping.ip.addSC("WORD", "Ping destination address or hostname");
	userC.ping.addSC("ipx", "Novell/IPX echo");
		userC.ping.ipx.addSC("WORD", "Ping destination address or hostname");
	userC.ping.addSC("srb", "srb echo");
		userC.ping.srb.addSC("WORD", "Ping destination address or hostname");
	userC.ping.addSC("tag", "Tag encapsulated IP echo");
		userC.ping.tag.addSC("WORD", "Ping destination address or hostname");
	userC.ping.addSC("vines", "Vines echo");
		userC.ping.vines.addSC("WORD", "Ping destination address or hostname");
	userC.ping.addSC("xns", "XNS echo");
userC.addSC("ppp", "Start IETF Point-to-Point Protocol (PPP)");
userC.addSC("resume", "Resume an active network connection");
userC.addSC("rlogin", "Open an rlogin connection");
userC.addSC("set", "Set system parameter (not config)");
userC.addSC("show", "Show running system information");
	userC.show.addSC("alps", "Alps information");
	userC.show.addSC("backup", "Backup status");
	userC.show.addSC("c2600", "Show c2600 information");
	userC.show.addSC("call", "Show Calls");
	userC.show.addSC("cef", "Cisco Express Forwarding");
	userC.show.addSC("class-map", "Show QoS Class Map");
	userC.show.addSC("clock", "Display the system clock");
	userC.show.addSC("cns", "CNS");
	userC.show.addSC("crypto", "Encryption module");
		userC.show.crypto.addSC("ca", "Show certification authority policy");
		userC.show.crypto.addSC("cisco", "Show cisco encryption policy");
		userC.show.crypto.addSC("key", "Show long term public keys");
	userC.show.addSC("dial-peer", "Dial Plan Mapping Table for, e.g. VoIP Peers");
	userC.show.addSC("dialer", "Dialer parameters and statistics");
	userC.show.addSC("drip", "DRiP DB");
	userC.show.addSC("exception", "exception informations");
	userC.show.addSC("fax", "Show calls stored in the history table for fax");
	userC.show.addSC("flash:", "display information about flash: file system");
	userC.show.addSC("fras-host", "FRAS Host Information");
	userC.show.addSC("gateway", "Show status of gateway");
	userC.show.addSC("history", "Display the session command history");
	userC.show.addSC("hosts", "IP domain-name, lookup style, nameservers, and host table");
	userC.show.addSC("kerberos", "Show Kerberos Values");
	userC.show.addSC("location", "Display the system location");
	userC.show.addSC("modemcap", "Show Modem Capabilities database");
	userC.show.addSC("mpoa", "MPOA show commands");
	userC.show.addSC("ncia", "Native Client Interface Architecture");
	userC.show.addSC("num-exp", "Number Expansion (Speed Dial) information");
	userC.show.addSC("policy-map", "Show QoS Policy Map");
		userC.show["policy-map"].addSC("WORD", "policy-map name");
			userC.show["policy-map"].WORD.addSC("class", "Show Qos Policy actions for a indvidual class");
				userC.show["policy-map"].WORD.class.addSC("WORD", "class-map name");
		userC.show["policy-map"].addSC("interface", "Show Qos Policy Interface");
			userC.show["policy-map"].interface.addSC("Async", "Async interface");
				userC.show["policy-map"].interface.Async.addSC("<1-65>", "Async interface number");
			userC.show["policy-map"].interface.addSC("Dialer", "Dialer interface");
				userC.show["policy-map"].interface.Dialer.addSC("<0-255>", "Dialer interface number");
			userC.show["policy-map"].interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
				userC.show["policy-map"].interface.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
			userC.show["policy-map"].interface.addSC("Loopback", "Loopback interface");
				userC.show["policy-map"].interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			userC.show["policy-map"].interface.addSC("Null", "Null interface");
				userC.show["policy-map"].interface.Null.addSC("<0-0>", "Null interface number");
			userC.show["policy-map"].interface.addSC("Serial", "Serial");
				userC.show["policy-map"].interface.Serial.addSC("<0-1>", "Serial interface number");
	userC.show.addSC("ppp", "PPP parameters and statistics");
	userC.show.addSC("queue", "Show queue contents");
	userC.show.addSC("queueing", "Show queueing configuration");
	userC.show.addSC("rmon", "rmon statistics");
	userC.show.addSC("rtr", "Response Time Reporter (RTR)");
	userC.show.addSC("sessions", "Information about Telnet connections");
	userC.show.addSC("sgbp", "SGBP group information");
	userC.show.addSC("snmp", "snmp statistics");
	userC.show.addSC("tacacs", "Shows tacacs+ server statistics");
	userC.show.addSC("terminal", "Display terminal configuration parameters");
	userC.show.addSC("traffic-shape", "traffic rate shaping configuration");
		userC.show["traffic-shape"].addSC("Async", "Async interface");
		userC.show["traffic-shape"].addSC("Dialer", "Dialer interface");
		userC.show["traffic-shape"].addSC("FastEthernet", "FastEthernet IEEE 802.3");
		userC.show["traffic-shape"].addSC("Loopback", "Loopback interface");
		userC.show["traffic-shape"].addSC("Null", "Null interface");
		userC.show["traffic-shape"].addSC("Serial", "Serial");
		userC.show["traffic-shape"].addSC("queue", "Show shaping queue contents");
		userC.show["traffic-shape"].addSC("statistics", "traffic rate shaping statistics");
			userC.show["traffic-shape"].statistics.addSC("Async", "Async interface");
				userC.show["traffic-shape"].statistics.Async.addSC("<1-65>", "Async interface number");
			userC.show["traffic-shape"].statistics.addSC("Dialer", "Dialer interface");
				userC.show["traffic-shape"].statistics.Dialer.addSC("<0-255>", "Dialer interface number");
			userC.show["traffic-shape"].statistics.addSC("FastEthernet", "FastEthernet IEEE 802.3");
				userC.show["traffic-shape"].statistics.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
			userC.show["traffic-shape"].statistics.addSC("Loopback", "Loopback interface");
				userC.show["traffic-shape"].statistics.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			userC.show["traffic-shape"].statistics.addSC("Null", "Null interface");
				userC.show["traffic-shape"].statistics.Null.addSC("<0-0>", "Null interface number");
			userC.show["traffic-shape"].statistics.addSC("Serial", "Serial");
				userC.show["traffic-shape"].statistics.Serial.addSC("<0-1>", "Serial interface number");
	userC.show.addSC("users", "Display information about terminal lines");
	userC.show.addSC("version", "System hardware and software status");
	userC.show.addSC("voice", "Voice port configuration & stats");
	userC.show.addSC("vpdn", "VPDN information");
userC.addSC("slip", "Start Serial-line IP (SLIP)");
userC.addSC("systat", "Display information about terminal lines");
userC.addSC("telnet", "Open a telnet connection");
userC.addSC("terminal", "Set terminal line parameters");
userC.addSC("tn3270", "Open a tn3270 connection");
userC.addSC("traceroute", "Trace route to destination");
	userC.traceroute.addSC("WORD", "Trace route to destination address or hostname");
	userC.traceroute.addSC("appletalk", "AppleTalk Trace");
		userC.traceroute.appletalk.addSC("WORD", "Trace route to destination address or hostname");
	userC.traceroute.addSC("clns", "ISO CLNS Trace");
		userC.traceroute.clns.addSC("WORD", "Trace route to destination address or hostname");
	userC.traceroute.addSC("ip", "IP Trace");
		userC.traceroute.ip.addSC("WORD", "Trace route to destination address or hostname");
	userC.traceroute.addSC("ipx", "IPX Trace");
		userC.traceroute.ipx.addSC("WORD", "Trace route to destination address or hostname");
	userC.traceroute.addSC("oldvines", "Vines Trace (Cisco)");
		userC.traceroute.oldvines.addSC("WORD", "Trace route to destination address or hostname");
	userC.traceroute.addSC("vines", "Vines Trace (Banyan)");
		userC.traceroute.vines.addSC("WORD", "Trace route to destination address or hostname");
userC.addSC("tunnel", "Open a tunnel connection");
userC.addSC("udptn", "Open an udptn connection");
userC.addSC("where", "List active connections");
userC.addSC("x28", "Become an X.28 PAD");
userC.addSC("x3", "Set X.3 parameters on PAD");
userC.addSC("xremote", "Enter XRemote mode");
