
enableC.addSC("cd", "Set default flash device");
enableC.addSC("clear", "Clear, use 'clear help' for more info");
	enableC.clear.addSC("alias", "Clear aliases of commands");
	enableC.clear.addSC("arp", "Clear ARP table entries");
	enableC.clear.addSC("banner", "Clear Message Of The Day banner");
	enableC.clear.addSC("boot", "Clear booting environment variable");
	enableC.clear.addSC("cam", "Clear CAM table entries");
	enableC.clear.addSC("cgmp", "Clear CGMP statistics");
	enableC.clear.addSC("channel", "Clear PagP statistical information");
	enableC.clear.addSC("config", "Clear configuration and reset system");
		enableC.clear.config.addSC("all", "Clear all configurations");
		enableC.clear.config.addSC("pvlan", "Clear Private Vlan Configuration");
		enableC.clear.config.addSC("snmp", "Clear SNMP");
		enableC.clear.config.addSC("rmon", "Clear RMON");
		enableC.clear.config.addSC("<mod>", "Clear configuration of a module");
	enableC.clear.addSC("counters", "Clear MAC and Port counters");
	enableC.clear.addSC("dot1x", "Clear Dot1x feature");
	enableC.clear.addSC("gmrp", "Clear GMRP statistics");
	enableC.clear.addSC("gvrp", "Clear GVRP statistics");
	enableC.clear.addSC("ip", "Clear IP, use 'clear ip help' for more info");
		enableC.clear.ip.addSC("alias", "Clear IP address aliases");
		enableC.clear.ip.addSC("dns", "Clear IP DNS information");
		enableC.clear.ip.addSC("permit", "Clear IP permit list");
		enableC.clear.ip.addSC("route", "Clear IP routing table entries");
			enableC.clear.ip.route.addSC("all", "Clear all IP routes");
			enableC.clear.ip.route.addSC("<destination>", "Clear IP route destination");
	enableC.clear.addSC("kerberos", "Clear Kerberos configuration information");
	enableC.clear.addSC("key", "Clear config-key string");
	enableC.clear.addSC("log", "Clear log information");
	enableC.clear.addSC("logging", "Clear system logging information");
	enableC.clear.addSC("multicast", "Clear multicast router port");
	enableC.clear.addSC("netstat", "Clear network statistics");
	enableC.clear.addSC("ntp", "Clear NTP servers and timezone");
	enableC.clear.addSC("port", "Clear port features");
		enableC.clear.port.addSC("host", "Clear port host");
			enableC.clear.port.host.addSC("all", "Clear port host for all ports");
			enableC.clear.port.host.addSC("<mod/port>", "Module number and Port number(s)");
		enableC.clear.port.addSC("security", "Clear secure MAC addresses");
	enableC.clear.addSC("pvlan", "Clear Private Vlan Mappings");
		enableC.clear.pvlan.addSC("mapping", "Clear private vlan mappings");
			enableC.clear.pvlan.mapping.addSC("<primary_vlan>", "Primary Vlan");
				enableC.clear.pvlan.mapping["<primary_vlan>"].addSC("<isolated_vlan>", "Isolated Vlan");
					enableC.clear.pvlan.mapping["<primary_vlan>"]["<isolated_vlan>"].addSC("<mod/port>", "Ports");
				enableC.clear.pvlan.mapping["<primary_vlan>"].addSC("<community_vlan>", "Community Vlan");
					enableC.clear.pvlan.mapping["<primary_vlan>"]["<community_vlan>"].addSC("<mod/port>", "Ports");
				enableC.clear.pvlan.mapping["<primary_vlan>"].addSC("<twoway_community_vlan>", "TwoWay Community Vlan");
					enableC.clear.pvlan.mapping["<primary_vlan>"]["<twoway_community_vlan>"].addSC("<mod/port>", "Ports");
			enableC.clear.pvlan.mapping.addSC("<mod/port>", "Clear all mappings from port");
				enableC.clear.pvlan.mapping["<mod/port>"].addSC("<isolated_vlan>", "Isolated Vlan");
					enableC.clear.pvlan.mapping["<mod/port>"]["<isolated_vlan>"].addSC("<mod/port>", "Ports");
				enableC.clear.pvlan.mapping["<mod/port>"].addSC("<community_vlan>", "Community Vlan");
					enableC.clear.pvlan.mapping["<mod/port>"]["<community_vlan>"].addSC("<mod/port>", "Ports");
				enableC.clear.pvlan.mapping["<mod/port>"].addSC("<twoway_community_vlan>", "TwoWay Community Vlan");
					enableC.clear.pvlan.mapping["<mod/port>"]["<twoway_community_vlan>"].addSC("<mod/port>", "Ports");
	enableC.clear.addSC("qos", "Clear QoS features");
	enableC.clear.addSC("radius", "Clear radius information");
	enableC.clear.addSC("rcp", "Clear RCP information for other copy");
	enableC.clear.addSC("snmp", "Clear SNMP trap receiver address");
	enableC.clear.addSC("spantree", "Clear spantree parameters");
		enableC.clear.spantree.addSC("portinstancecost", "Clear spantree port instance cost");
		enableC.clear.spantree.addSC("portinstancepri", "Clear spantree port instance priority");
		enableC.clear.spantree.addSC("portvlancost", "Clear spantree port vlan cost");
			enableC.clear.spantree.portvlancost.addSC("<mod/port>", "Module number and Port number(s)");
				enableC.clear.spantree.portvlancost["<mod/port>"].addSC("<vlans>", "VLAN numbers for PVST+");
		enableC.clear.spantree.addSC("portvlanpri", "Clear spantree port vlan priority");
		enableC.clear.spantree.addSC("root", "Restore STP parameters to default values");
			enableC.clear.spantree.root.addSC("mistp-instance", "Clear root for MISTP instance");
			enableC.clear.spantree.root.addSC("<vlans>", "VLAN numbers for PVST+");
		enableC.clear.spantree.addSC("statistics", "Clear spantree statistics information");
		enableC.clear.spantree.addSC("uplinkfast", "Clear uplinkfast groups");
	enableC.clear.addSC("tacacs", "Clear TACACS server host/key");
	enableC.clear.addSC("timezone", "Clear timezone");
	enableC.clear.addSC("top", "Clear TopN report");
	enableC.clear.addSC("trunk", "Clear trunk ports");
		enableC.clear.trunk.addSC("<mod/port>", "Module number and Port number(s)");
			enableC.clear.trunk["<mod/port>"].addSC("<vlan>", "VLAN number");
	enableC.clear.addSC("vlan", "Clear VLAN information");
		enableC.clear.vlan.addSC("mapping", "Clear the 802.1Q to ISL Vlan Mapping");
		enableC.clear.vlan.addSC("<vlans>", "Vlan Number(s)");
	enableC.clear.addSC("vmps", "Clear VMPS information");
	enableC.clear.addSC("vtp", "Clear VTP statistics");
		enableC.clear.vtp.addSC("pruneeligible", "Clear VTP pruning eligibility");
		enableC.clear.vtp.addSC("statistics", "Clear VTP pruning statistics");
enableC.addSC("configure", "Configure system from network");
	enableC.configure.addSC("<host>", "IP address or hostname");
		enableC.configure["<host>"].addSC("<file>", "File name");
			enableC.configure["<host>"]["<file>"].addSC("rcp", "Download configuration by RCP method");
	enableC.configure.addSC("network", "Get host/file name interactively");
enableC.addSC("copy", "Copy files between TFTP/RCP/module/flash devices");
	enableC.copy.addSC("config", "Copy configuration to a device");
		enableC.copy.config.addSC("flash", "Copy from config to flash");
		enableC.copy.config.addSC("rcp", "Copy from config to RCP server");
		enableC.copy.config.addSC("tftp", "Copy from config to TFTP server");
		enableC.copy.config.addSC("<file-id>", "File name");
	enableC.copy.addSC("flash", "Copy from flash");
		enableC.copy.flash.addSC("config", "Copy from flash to configuration");
		enableC.copy.flash.addSC("rcp", "Copy from flash to RCP server");
		enableC.copy.flash.addSC("tftp", "Copy from flash to TFTP server");
		enableC.copy.flash.addSC("<file-id>", "File name");
	enableC.copy.addSC("rcp", "Copy from RCP server");
	enableC.copy.addSC("tftp", "Copy from TFTP server");
		enableC.copy.tftp.addSC("config", "Copy from TFTP server to configuration");
		enableC.copy.tftp.addSC("flash", "Copy from TFTP server to flash");
		enableC.copy.tftp.addSC("<file-id>", "File name");
	enableC.copy.addSC("<file-id>", "File name");
		enableC.copy["<file-id>"].addSC("config", "Copy from file to configuration");
		enableC.copy["<file-id>"].addSC("flash", "Copy from file to flash");
		enableC.copy["<file-id>"].addSC("rcp", "Copy from file to RCP server");
		enableC.copy["<file-id>"].addSC("tftp", "Copy from file to TFTP server");
enableC.addSC("delete", "Delete a file on flash device");
enableC.addSC("dir", "Show list of files on flash device");
enableC.addSC("disable", "Disable privileged mode");
enableC.addSC("disconnect", "Disconnect user session");
enableC.addSC("download", "Download code to a processor");
enableC.addSC("enable", "Enable privileged mode");
enableC.addSC("format", "Format a flash device");
enableC.addSC("help", "Show this help screen");
enableC.addSC("history", "Show contents of history substitution buffer");
enableC.addSC("l2trace", "Layer2 trace between hosts");
enableC.addSC("ping", "Send echo packets to hosts");
	enableC.ping.addSC("-s", "Ping parameter");
		enableC.ping["-s"].addSC("<host>", "IP address or hostname");
			enableC.ping["-s"]["<host>"].addSC("<packet_size>", "Size of the packet (56..1472 bytes)");
				enableC.ping["-s"]["<host>"]["<packet_size>"].addSC("<packet_count>", "Number of packets");
	enableC.ping.addSC("<host>", "IP address or hostname");
enableC.addSC("pwd", "Show default flash device");
enableC.addSC("quit", "Exit from the Admin session");
enableC.addSC("reconfirm", "Reconfirm VMPS");
enableC.addSC("reset", "Reset system or module");
enableC.addSC("session", "Tunnel to ATM or Router module");
enableC.addSC("set", "Set commands, use 'set help' for more info");
	enableC.set.addSC("accounting", "Set accounting");
	enableC.set.addSC("alias", "Set alias for command");
	enableC.set.addSC("arp", "Set ARP table entry");
	enableC.set.addSC("authentication", "Set authentication");
	enableC.set.addSC("authorization", "Set authorization");
	enableC.set.addSC("banner", "Set system banner");
		enableC.set.banner.addSC("motd", "Set message of the day");
			enableC.set.banner.motd.addSC("<c>[text]<c>", "Message text");
				enableC.set.banner.motd["<c>[text]<c>"].addSC("<c>[text]<c>", "Message text");
	enableC.set.addSC("boot", "Set booting environment variable");
	enableC.set.addSC("cam", "Set CAM table entry");
	enableC.set.addSC("cdp", "Set cdp, use 'set cdp help' for more info");
	enableC.set.addSC("cgmp", "Set CGMP (enable/disable)");
	enableC.set.addSC("channel", "Set channel, use 'set channel help' for more info");
		enableC.set.channel.addSC("cost", "Set channel path cost");
			enableC.set.channel.cost.addSC("all", "All channels");
				enableC.set.channel.cost.all.addSC("<cost>", "Channel cost");
			enableC.set.channel.cost.addSC("<channel_id>", "Channel id");
				enableC.set.channel.cost["<channel_id>"].addSC("<cost>", "Channel cost");
		enableC.set.channel.addSC("vlancost", "Set channel vlancost");
			enableC.set.channel.vlancost.addSC("<channel_id>", "Channel id");
				enableC.set.channel.vlancost["<channel_id>"].addSC("<cost>", "Channel vlan cost");
	enableC.set.addSC("config", "Set system configuration parameters");
	enableC.set.addSC("dot1q-all-tagged", "Set the tag to be dot1q only");
	enableC.set.addSC("dot1x", "Set dot1x timers and variables");
	enableC.set.addSC("enablepass", "Set privilege mode password");
	enableC.set.addSC("errdisable-timeout", "Set errdisable timeout");
	enableC.set.addSC("errordetection", "Set various error detections");
	enableC.set.addSC("feature", "Set feature");
	enableC.set.addSC("garp", "Set GARP timer");
	enableC.set.addSC("gmrp", "Set GMRP (enable/disable)");
	enableC.set.addSC("gvrp", "Set GVRP (enable/disable)");
	enableC.set.addSC("inlinepower", "Set default allocation for inline power");
	enableC.set.addSC("interface", "Set network interface configuration");
		enableC.set.interface.addSC("me1", "Set me1 interface");
			enableC.set.interface.me1.addSC("down", "Shut down the interface");
			enableC.set.interface.me1.addSC("up", "Bring up the interface");
			enableC.set.interface.me1.addSC("<ip_addr>", "IP address");
				enableC.set.interface.me1["<ip_addr>"].addSC("<ipmask>", "IP subnet mask (must be in dot format)");
					enableC.set.interface.me1["<ip_addr>"]["<ipmask>"].addSC("<ip_addr>", "Broadcast interface IP address");
		enableC.set.interface.addSC("sc0", "Set sc0 interface");
			enableC.set.interface.sc0.addSC("dhcp", "Set dhcp interface");
				enableC.set.interface.sc0.dhcp.addSC("release", "Release DHCP address");
				enableC.set.interface.sc0.dhcp.addSC("renew", "Renew DHCP address");
			enableC.set.interface.sc0.addSC("down", "Shut down the interface");
			enableC.set.interface.sc0.addSC("up", "Bring up the interface");
			enableC.set.interface.sc0.addSC("<ip/mask>", "ip_addr/netmask or ip_addr/maskbit");
				enableC.set.interface.sc0["<ip/mask>"].addSC("<ip_addr>", "Broadcast interface IP address");
			enableC.set.interface.sc0.addSC("<ip_addr>", "IP address");
				enableC.set.interface.sc0["<ip_addr>"].addSC("<ip_addr>", "Broadcast interface IP address");
			enableC.set.interface.sc0.addSC("<vlan>", "VLAN number");
				enableC.set.interface.sc0["<vlan>"].addSC("<ip_addr>", "Broadcast interface IP address");
		enableC.set.interface.addSC("sl0", "Set sl0 interface");
			enableC.set.interface.sl0.addSC("down", "Shut down the interface");
			enableC.set.interface.sl0.addSC("up", "Bring up the interface");
			enableC.set.interface.sl0.addSC("<slip_addr>", "IP address");
				enableC.set.interface.sl0["<slip_addr>"].addSC("<ip_addr>", "Destination IP address");
		enableC.set.interface.addSC("trap", "Set interface trap");
			enableC.set.interface.trap.addSC("me1", "Set me1 interface");
				enableC.set.interface.trap.me1.addSC("disable", "Disable trap on the interface");
				enableC.set.interface.trap.me1.addSC("enable", "Enable trap on the interface");
			enableC.set.interface.trap.addSC("sc0", "Set sc0 interface");
				enableC.set.interface.trap.sc0.addSC("disable", "Disable trap on the interface");
				enableC.set.interface.trap.sc0.addSC("enable", "Enable trap on the interface");
			enableC.set.interface.trap.addSC("sl0", "Set sl0 interface");
				enableC.set.interface.trap.sl0.addSC("disable", "Disable trap on the interface");
				enableC.set.interface.trap.sl0.addSC("enable", "Enable trap on the interface");
	enableC.set.addSC("ip", "Set IP, use 'set ip help' for more info");
		enableC.set.ip.addSC("alias", "Set alias for IP Address");
		enableC.set.ip.addSC("dns", "Set DNS information");
		enableC.set.ip.addSC("fragmentation", "Set IP fragmentation enable/disable");
		enableC.set.ip.addSC("http", "Set IP HTTP server information");
		enableC.set.ip.addSC("permit", "Set IP Permit List");
			enableC.set.ip.permit.addSC("disable", "Disable IP permit");
				enableC.set.ip.permit.disable.addSC("telnet", "Disable/Enable telnet permit");
				enableC.set.ip.permit.disable.addSC("snmp", "Disable/Enable snmp permit");
				enableC.set.ip.permit.disable.addSC("ssh", "Disable/Enable ssh permit");
			enableC.set.ip.permit.addSC("enable", "Enable IP permit");
				enableC.set.ip.permit.enable.addSC("telnet", "Disable/Enable telnet permit");
				enableC.set.ip.permit.enable.addSC("snmp", "Disable/Enable snmp permit");
				enableC.set.ip.permit.enable.addSC("ssh", "Disable/Enable ssh permit");
			enableC.set.ip.permit.addSC("<host>", "IP address or hostname");
				enableC.set.ip.permit["<host>"].addSC("<mask>", "Set IP permit mask");
					enableC.set.ip.permit["<host>"]["<mask>"].addSC("telnet", "Set telnet permit entry");
					enableC.set.ip.permit["<host>"]["<mask>"].addSC("snmp", "Set snmp permit entry");
					enableC.set.ip.permit["<host>"]["<mask>"].addSC("ssh", "Set ssh permit entry");
				enableC.set.ip.permit["<host>"].addSC("telnet", "Set telnet permit entry");
				enableC.set.ip.permit["<host>"].addSC("snmp", "Set snmp permit entry");
				enableC.set.ip.permit["<host>"].addSC("ssh", "Set ssh permit entry");
		enableC.set.ip.addSC("redirect", "Set ICMP redirect enable/disable");
		enableC.set.ip.addSC("route", "Set IP routing table entry");
			enableC.set.ip.route.addSC("default", "Set default route");
				enableC.set.ip.route["default"].addSC("<gateway>", "IP address");
					enableC.set.ip.route["default"]["<gateway>"].addSC("primary", "Specify as primary");
			enableC.set.ip.route.addSC("<destination>", "IP address or hostname");
				enableC.set.ip.route["<destination>"].addSC("<gateway>", "IP address");
			enableC.set.ip.route.addSC("<destination/netmask>", "ip_addr or ip_addr/netmask or ip_addr/maskbit");
				enableC.set.ip.route["<destination/netmask>"].addSC("<gateway>", "IP address");
		enableC.set.ip.addSC("unreachable", "Set ICMP unreachable messages");
			enableC.set.ip.unreachable.addSC("disable", "Disable IP unreachable message");
			enableC.set.ip.unreachable.addSC("enable", "Enable IP unreachable message");
	enableC.set.addSC("kerberos", "Set Kerberos configuration");
	enableC.set.addSC("key", "Set DES key for storing the password");
//	enableC.set.addSC("length", "Set number of lines (0 to disable 'more')");
	enableC.set.addSC("logging", "Set system logging configuration information");
	enableC.set.addSC("logout", "Set number of minutes before automatic logout");
	enableC.set.addSC("module", "Set module, use 'set module help' for more info");
		enableC.set.module.addSC("disable", "Disable module");
			enableC.set.module.disable.addSC("<mod>", "Module number");
		enableC.set.module.addSC("enable", "Enable module");
			enableC.set.module.enable.addSC("<mod>", "Module number");
		enableC.set.module.addSC("name", "Set module name");
			enableC.set.module.name.addSC("<mod>", "Module number");
	enableC.set.addSC("multicast", "Set multicast router port");
	enableC.set.addSC("ntp", "Set NTP information");
	enableC.set.addSC("nvramenv", "Set environment variable");
	enableC.set.addSC("password", "Set console password");
	enableC.set.addSC("port", "Set port features");
		enableC.set.port.addSC("auxiliaryvlan", "Set auxiliary vlan for applicable ports");
		enableC.set.port.addSC("channel", "Set port channel (on/off)");
			enableC.set.port.channel.addSC("<port_list>", "Port list (ex: 2/1-4 or 2/1-2 or 2/5,2/6)");
				enableC.set.port.channel["<port_list>"].addSC("<admin_group>", "Admin group");
				enableC.set.port.channel["<port_list>"].addSC("mode", "Channel mode");
					enableC.set.port.channel["<port_list>"].mode.addSC("auto", "Channel auto mode");
						enableC.set.port.channel["<port_list>"].mode.auto.addSC("silent", "silent mode");
						enableC.set.port.channel["<port_list>"].mode.auto.addSC("non-silent", "non-silent mode");
					enableC.set.port.channel["<port_list>"].mode.addSC("desirable", "Channel desirable mode");
						enableC.set.port.channel["<port_list>"].mode.desirable.addSC("silent", "silent mode");
						enableC.set.port.channel["<port_list>"].mode.desirable.addSC("non-silent", "non-silent mode");
					enableC.set.port.channel["<port_list>"].mode.addSC("off", "Turn off Channelling");
					enableC.set.port.channel["<port_list>"].mode.addSC("on", "Turn on Channelling");
			enableC.set.port.channel.addSC("all", "Globally configure all ports");
				enableC.set.port.channel.all.addSC("distribution", "Channel distribution");
					enableC.set.port.channel.all.distribution.addSC("mac", "Channel distribution mac");
						enableC.set.port.channel.all.distribution.mac.addSC("both", "Channel distribution both");
				enableC.set.port.channel.all.addSC("mode", "Turn off channeling on all ports");
					enableC.set.port.channel.all.mode.addSC("off", "Turn off channeling on all ports");
		enableC.set.port.addSC("disable", "Disable a port");
			enableC.set.port.disable.addSC("<mod/port>", "Module number and Port number(s)");
		enableC.set.port.addSC("duplex", "Set port transmission type (full/half duplex)");
			enableC.set.port.duplex.addSC("<mod/port>", "Module number and Port number(s)");
				enableC.set.port.duplex["<mod/port>"].addSC("full", "Full duplex");
				enableC.set.port.duplex["<mod/port>"].addSC("half", "Half duplex");
		enableC.set.port.addSC("enable", "Enable a port");
			enableC.set.port.enable.addSC("<mod/port>", "Module number and Port number(s)");
		enableC.set.port.addSC("dot1x", "Set port dot1x attributes");
		enableC.set.port.addSC("flowcontrol", "Set port traffic flowcontrol");
		enableC.set.port.addSC("gmrp", "Set port gmrp (enable/disable)");
		enableC.set.port.addSC("gvrp", "Set port gvrp (enable/disable)");
		enableC.set.port.addSC("host", "Set port host");
			enableC.set.port.host.addSC("all", "Set all ports");
			enableC.set.port.host.addSC("<mod/port>", "Module number and Port number(s)");
		enableC.set.port.addSC("inlinepower", "Set inline power for a port");
		enableC.set.port.addSC("level", "Set port priority level (normal/high)");
		enableC.set.port.addSC("membership", "Set vlan membership assignment to a port");
			enableC.set.port.membership.addSC("<mod/port>", "Module number and Port number(s)");
				enableC.set.port.membership["<mod/port>"].addSC("dynamic", "Dynamic Vlan");
				enableC.set.port.membership["<mod/port>"].addSC("static", "Static Vlan");
		enableC.set.port.addSC("name", "Set port name");
			enableC.set.port.name.addSC("<mod/port>", "Module number and Port number(s)");
				enableC.set.port.name["<mod/port>"].addSC("<name>", "Name string");
		enableC.set.port.addSC("negotiation", "Set port negotiation");
		enableC.set.port.addSC("protocol", "Set port protocol membership");
			enableC.set.port.protocol.addSC("<mod/port>", "Module number and Port number(s)");
				enableC.set.port.protocol["<mod/port>"].addSC("group", "Set protocol group");
					enableC.set.port.protocol["<mod/port>"].group.addSC("auto", "AUTO mode");
					enableC.set.port.protocol["<mod/port>"].group.addSC("off", "Off mode");
					enableC.set.port.protocol["<mod/port>"].group.addSC("on", "On mode");
				enableC.set.port.protocol["<mod/port>"].addSC("ip", "Set protocol IP");
					enableC.set.port.protocol["<mod/port>"].ip.addSC("auto", "AUTO mode");
					enableC.set.port.protocol["<mod/port>"].ip.addSC("off", "Off mode");
					enableC.set.port.protocol["<mod/port>"].ip.addSC("on", "On mode");
				enableC.set.port.protocol["<mod/port>"].addSC("ipx", "Set protocol IPX");
					enableC.set.port.protocol["<mod/port>"].ipx.addSC("auto", "AUTO mode");
					enableC.set.port.protocol["<mod/port>"].ipx.addSC("off", "Off mode");
					enableC.set.port.protocol["<mod/port>"].ipx.addSC("on", "On mode");
		enableC.set.port.addSC("security", "Set port security attributes");
		enableC.set.port.addSC("speed", "Set port transmission speed (4/10/16/100 Mbps)");
			enableC.set.port.speed.addSC("<mod/port>", "Module number and Port number(s)");
				enableC.set.port.speed["<mod/port>"].addSC("auto", "Set speed to auto");
				enableC.set.port.speed["<mod/port>"].addSC("<port_speed>", "Port speed (10, 100, 1000)");
		enableC.set.port.addSC("trap", "Set port up/down trap (enable/disable)");
			enableC.set.port.trap.addSC("<mod/port>", "Module number and Port number(s)");
				enableC.set.port.trap["<mod/port>"].addSC("disable", "Disable port trap");
				enableC.set.port.trap["<mod/port>"].addSC("enable", "Enable port trap");
	enableC.set.addSC("power", "Set power supplies budget");
	enableC.set.addSC("prompt", "Set prompt");
		enableC.set.prompt.addSC("<prompt_string>", "String used as prompt");
	enableC.set.addSC("protocolfilter", "Set protocol filtering");
	enableC.set.addSC("pvlan", "Set Private Vlan Config");
		enableC.set.pvlan.addSC("<primary_vlan>", "Set association/ Add ports to Private Vlan");
			enableC.set.pvlan["<primary_vlan>"].addSC("<isolated_vlan>", "Isolated Vlan");
				enableC.set.pvlan["<primary_vlan>"]["<isolated_vlan>"].addSC("<mod/port>", "Ports");
				enableC.set.pvlan["<primary_vlan>"]["<isolated_vlan>"].addSC("sc0", "SC0 port");
			enableC.set.pvlan["<primary_vlan>"].addSC("<community_vlan>", "Community Vlan");
				enableC.set.pvlan["<primary_vlan>"]["<community_vlan>"].addSC("<mod/port>", "Ports");
				enableC.set.pvlan["<primary_vlan>"]["<community_vlan>"].addSC("sc0", "SC0 port");
			enableC.set.pvlan["<primary_vlan>"].addSC("<twoway_community_vlan>", "TwoWay Community Vlan");
				enableC.set.pvlan["<primary_vlan>"]["<twoway_community_vlan>"].addSC("<mod/port>", "Ports");
				enableC.set.pvlan["<primary_vlan>"]["<twoway_community_vlan>"].addSC("sc0", "SC0 port");
		enableC.set.pvlan.addSC("mapping", "Set Private Vlan Mapping");
			enableC.set.pvlan.mapping.addSC("<primary_vlan>", "Primary Vlan");
				enableC.set.pvlan.mapping["<primary_vlan>"].addSC("<isolated_vlan>", "Isolated Vlan");
					enableC.set.pvlan.mapping["<primary_vlan>"]["<isolated_vlan>"].addSC("<mod/port>", "Ports");
				enableC.set.pvlan.mapping["<primary_vlan>"].addSC("<community_vlan>", "Community Vlan");
					enableC.set.pvlan.mapping["<primary_vlan>"]["<community_vlan>"].addSC("<mod/port>", "Ports");
				enableC.set.pvlan.mapping["<primary_vlan>"].addSC("<twoway_community_vlan>", "TwoWay Community Vlan");
					enableC.set.pvlan.mapping["<primary_vlan>"]["<twoway_community_vlan>"].addSC("<mod/port>", "Ports");
	enableC.set.addSC("qos", "Set QOS information");
	enableC.set.addSC("radius", "Set RADIUS parameters");
	enableC.set.addSC("rcp", "Set rcp username");
	enableC.set.addSC("rspan", "Set remote switch port analyzer");
	enableC.set.addSC("snmp", "Set SNMP, use 'set snmp help' for more info");
	enableC.set.addSC("span", "Set switch port analyzer");
		enableC.set.span.addSC("disable", "Disable port monitoring");
			enableC.set.span.disable.addSC("all", "Disable SPAN on all ports");
			enableC.set.span.disable.addSC("<mod/port>", "Module number and Port number(s)");
		enableC.set.span.addSC("<mod/port>", "Source module and port numbers");
			enableC.set.span["<mod/port>"].addSC("<mod/port>", "Destination module and port numbers");
				enableC.set.span["<mod/port>"]["<mod/port>"].addSC("both", "Both receiving and transmitting traffic");
				enableC.set.span["<mod/port>"]["<mod/port>"].addSC("create", "Creating new SPAN session");
				enableC.set.span["<mod/port>"]["<mod/port>"].addSC("filter", "Monitor traffic on selected vlans");
				enableC.set.span["<mod/port>"]["<mod/port>"].addSC("inpkts", "Enable/disable destination port incoming packets");
				enableC.set.span["<mod/port>"]["<mod/port>"].addSC("learning", "Enable/disable MAC address learning");
				enableC.set.span["<mod/port>"]["<mod/port>"].addSC("rx", "Receiving traffic");
				enableC.set.span["<mod/port>"]["<mod/port>"].addSC("tx", "Transmitting traffic");
		enableC.set.span.addSC("<vlan>", "Source VLAN numbers");
			enableC.set.span["<vlan>"].addSC("<mod/port>", "Destination module and port numbers");
				enableC.set.span["<vlan>"]["<mod/port>"].addSC("both", "Both receiving and transmitting traffic");
				enableC.set.span["<vlan>"]["<mod/port>"].addSC("create", "Creating new SPAN session");
				enableC.set.span["<vlan>"]["<mod/port>"].addSC("filter", "Monitor traffic on selected vlans");
				enableC.set.span["<vlan>"]["<mod/port>"].addSC("inpkts", "Enable/disable destination port incoming packets");
				enableC.set.span["<vlan>"]["<mod/port>"].addSC("learning", "Enable/disable MAC address learning");
				enableC.set.span["<vlan>"]["<mod/port>"].addSC("rx", "Receiving traffic");
				enableC.set.span["<vlan>"]["<mod/port>"].addSC("tx", "Transmitting traffic");
	enableC.set.addSC("spantree", "Set spanning tree information");
		enableC.set.spantree.addSC("backbonefast", "Enable or disable fast convergence");
		enableC.set.spantree.addSC("bpdu-skewing", "Set spantree BPDU skewing");
		enableC.set.spantree.addSC("defaultcostmode", "Set spantree port cost mode");
		enableC.set.spantree.addSC("disable", "Disable spanning tree");
			enableC.set.spantree.disable.addSC("all", "Disable spanning tree all");
			enableC.set.spantree.disable.addSC("mistp-instance", "Disable MISTP instances");
			enableC.set.spantree.disable.addSC("<vlans>", "VLAN numbers for PVST+");
		enableC.set.spantree.addSC("enable", "Enable spanning tree");
			enableC.set.spantree.enable.addSC("all", "Enable spanning tree all");
			enableC.set.spantree.enable.addSC("mistp-instance", "Enable MISTP instances");
			enableC.set.spantree.enable.addSC("<vlans>", "VLAN numbers for PVST+");
		enableC.set.spantree.addSC("fwddelay", "Set spantree forward delay");
		enableC.set.spantree.addSC("guard", "Set spantree guard");
		enableC.set.spantree.addSC("hello", "Set spantree hello interval");
		enableC.set.spantree.addSC("macreduction", "Set spantree mac address reduction");
		enableC.set.spantree.addSC("maxage", "Set spantree max aging time");
		enableC.set.spantree.addSC("mode", "Set spantree mode");
			enableC.set.spantree.mode.addSC("pvst+", "Run Per VLAN Spanning Tree");
			enableC.set.spantree.mode.addSC("mistp", "Run Per Instance Spanning Tree");
			enableC.set.spantree.mode.addSC("mistp-pvst+", "Run MISTP but allow remote PVST+");
		enableC.set.spantree.addSC("portcost", "Set spantree port cost");
			enableC.set.spantree.portcost.addSC("<mod/port>", "Module number and Port number(s)");
				enableC.set.spantree.portcost["<mod/port>"].addSC("<cost>", "Port cost");
		enableC.set.spantree.addSC("portfast", "Set spantree port fast start");
			enableC.set.spantree.portfast.addSC("<mod/port>", "Module number and Port number(s)");
				enableC.set.spantree.portfast["<mod/port>"].addSC("disable", "Disable port fast start");
				enableC.set.spantree.portfast["<mod/port>"].addSC("enable", "Enable port fast start");
			enableC.set.spantree.portfast.addSC("bpdu-guard", "Portfast BPDU guard");
			enableC.set.spantree.portfast.addSC("bpdu-filter", "Portfast BPDU filter");
		enableC.set.spantree.addSC("portpri", "Set spantree port priority");
		enableC.set.spantree.addSC("portvlancost", "Set spantree port cost per vlan");
		enableC.set.spantree.addSC("portvlanpri", "Set spantree port vlan priority");
		enableC.set.spantree.addSC("portinstancecost", "Set spantree port cost per instance");
		enableC.set.spantree.addSC("portinstancepri", "Set spantree port instance priority");
		enableC.set.spantree.addSC("priority", "Set spantree priority");
			enableC.set.spantree.priority.addSC("<priority>", "Bridge priority number");
				enableC.set.spantree.priority["<priority>"].addSC("mistp-instance", "Set bridge priority for MISTP instance");
				enableC.set.spantree.priority["<priority>"].addSC("<vlans>", "VLAN numbers for PVST+");
		enableC.set.spantree.addSC("root", "Set switch as primary or secondary root");
			enableC.set.spantree.root.addSC("secondary", "Specify as secondary root");
			enableC.set.spantree.root.addSC("mistp-instance", "Set spantree root for MISTP instance");
			enableC.set.spantree.root.addSC("<vlans>", "VLAN numbers for PVST+");
				enableC.set.spantree.root["<vlans>"].addSC("dia", "Specify network diameter");
				enableC.set.spantree.root["<vlans>"].addSC("hello", "Specify hello time");
		enableC.set.spantree.addSC("uplinkfast", "Enable or disable uplinkfast groups");
			enableC.set.spantree.uplinkfast.addSC("disable", "Disable spanning tree uplink fast");
			enableC.set.spantree.uplinkfast.addSC("enable", "Enable spanning tree uplink fast");
	enableC.set.addSC("summertime", "Set summertime");
	enableC.set.addSC("switchacceleration", "Enable/Disable switch acceleration");
	enableC.set.addSC("system", "Set system, use 'set system help' for more info");
		enableC.set.system.addSC("baud", "Set system console port baud rate");
			enableC.set.system.baud.addSC("<rate>", "Baud rate (600,1200,2400,4800,9600,19200,38400)");
		enableC.set.system.addSC("contact", "Set system contact");
		enableC.set.system.addSC("countrycode", "Set system country code");
		enableC.set.system.addSC("location", "Set system location");
		enableC.set.system.addSC("modem", "Set system modem control (enable/disable)");
		enableC.set.system.addSC("name", "Set system name");
			enableC.set.system.name.addSC("<name_string>", "Name for the system");
	enableC.set.addSC("tacacs", "Set TACACS information");
	enableC.set.addSC("test", "Set test, use 'set test help' for more info");
	enableC.set.addSC("time", "Set time");
	enableC.set.addSC("timezone", "Set timezone");
	enableC.set.addSC("traffic", "Set traffic, use 'set traffic help' for more info");
	enableC.set.addSC("trunk", "Set trunk ports");
		enableC.set.trunk.addSC("all", "Turn off trunking on all ports");
			enableC.set.trunk.all.addSC("off", "Turn off trunking on all ports");
		enableC.set.trunk.addSC("<mod/port>", "Module number and Port number(s)");
			enableC.set.trunk["<mod/port>"].addSC("<mode>", "Trunk mode (on,off,desirable,auto,nonegotiate)");
				enableC.set.trunk["<mod/port>"]["<mode>"].addSC("<type>", "Trunk type (dot1q)");
				enableC.set.trunk["<mod/port>"]["<mode>"].addSC("<vlan>", "VLAN number");
			enableC.set.trunk["<mod/port>"].addSC("<type>", "Trunk type (dot1q)");
				enableC.set.trunk["<mod/port>"]["<type>"].addSC("<type>", "Trunk type (dot1q)");
				enableC.set.trunk["<mod/port>"]["<type>"].addSC("<vlan>", "VLAN number");
			enableC.set.trunk["<mod/port>"].addSC("<vlan>", "VLAN number");
				enableC.set.trunk["<mod/port>"]["<vlan>"].addSC("<type>", "Trunk type (dot1q)");
				enableC.set.trunk["<mod/port>"]["<vlan>"].addSC("<vlan>", "VLAN number");
	enableC.set.addSC("udld", "Set uni-directional link detection");
	enableC.set.addSC("vlan", "Set virtual LAN information");
		enableC.set.vlan.addSC("mapping", "Map an 802.1Q vlan to an Ethernet vlan");
		enableC.set.vlan.addSC("<vlans>", "Vlan number(s)");
			enableC.set.vlan["<vlans>"].addSC("aremaxhop", "Set Tokenring vlan ARE max hop");
				enableC.set.vlan["<vlans>"].aremaxhop.addSC("<hopcount>", "ARE max hop count (1..13)");
			enableC.set.vlan["<vlans>"].addSC("backupcrf", "Set Tokenring backupcrf vlan");
				enableC.set.vlan["<vlans>"].backupcrf.addSC("off", "Turn off backup Token Ring TRCRF");
				enableC.set.vlan["<vlans>"].backupcrf.addSC("on", "Turn on backup Token Ring TRCRF");
			enableC.set.vlan["<vlans>"].addSC("bridge", "Set vlan bridge");
				enableC.set.vlan["<vlans>"].bridge.addSC("<bridge>", "Bridge number (0x1..0xf)");
			enableC.set.vlan["<vlans>"].addSC("decring", "Set vlan ring (decimal number)");
				enableC.set.vlan["<vlans>"].decring.addSC("<decimal_ring>", "RING number in decimal (1..4095)");
			enableC.set.vlan["<vlans>"].addSC("mistp-instance", "Set a vlan for an MISTP instance");
				enableC.set.vlan["<vlans>"]["mistp-instance"].addSC("<instance>", "MISTP instance number(1..16)");
				enableC.set.vlan["<vlans>"]["mistp-instance"].addSC("none", "Unmap vlans to any instance");
			enableC.set.vlan["<vlans>"].addSC("mode", "Set vlan mode");
				enableC.set.vlan["<vlans>"].mode.addSC("<bridge_mode>", "Bridge mode (srt, srb)");
			enableC.set.vlan["<vlans>"].addSC("mtu", "Set vlan MTU");
				enableC.set.vlan["<vlans>"].mtu.addSC("<mtu>", "MTU number");
			enableC.set.vlan["<vlans>"].addSC("name", "Set vlan name");
				enableC.set.vlan["<vlans>"].name.addSC("<name>", "VLAN name");
			enableC.set.vlan["<vlans>"].addSC("parent", "Set vlan parent");
				enableC.set.vlan["<vlans>"].parent.addSC("<parent_vlan>", "VLAN number");
			enableC.set.vlan["<vlans>"].addSC("pvlan-type", "Set private vlan type");
				enableC.set.vlan["<vlans>"]["pvlan-type"].addSC("community", "Set private vlan as community vlan");
				enableC.set.vlan["<vlans>"]["pvlan-type"].addSC("isolated", "Set private vlan as isolated vlan");
				enableC.set.vlan["<vlans>"]["pvlan-type"].addSC("none", "Set vlan to be a normal vlan");
				enableC.set.vlan["<vlans>"]["pvlan-type"].addSC("primary", "Set private vlan as primary vlan");
				enableC.set.vlan["<vlans>"]["pvlan-type"].addSC("twoway-community", "Set private vlan as twoway community vlan");
			enableC.set.vlan["<vlans>"].addSC("ring", "Set vlan ring (hex number)");
				enableC.set.vlan["<vlans>"].ring.addSC("<ring>", "RING number (0x1..0xfff)");
			enableC.set.vlan["<vlans>"].addSC("rspan", "Set remote span for vlan");
				enableC.set.vlan["<vlans>"].rspan.addSC("name", "Set vlan name");
					enableC.set.vlan["<vlans>"].rspan.name.addSC("<name>", "VLAN name");
						enableC.set.vlan["<vlans>"].rspan.name["<name>"].addSC("state", "Set vlan state");
				enableC.set.vlan["<vlans>"].rspan.addSC("state", "Set vlan state");
					enableC.set.vlan["<vlans>"].rspan.state.addSC("active", "set VLAN state to active");
						enableC.set.vlan["<vlans>"].rspan.state.active.addSC("name", "Set vlan name");
					enableC.set.vlan["<vlans>"].rspan.state.addSC("suspend", "set VLAN state to suspend");
						enableC.set.vlan["<vlans>"].rspan.state.suspend.addSC("name", "Set vlan name");
			enableC.set.vlan["<vlans>"].addSC("said", "Set vlan said");
				enableC.set.vlan["<vlans>"].said.addSC("<said>", "SAID number");
			enableC.set.vlan["<vlans>"].addSC("state", "Set vlan state");
				enableC.set.vlan["<vlans>"].state.addSC("<state>", "VLAN state (active, suspend)");
			enableC.set.vlan["<vlans>"].addSC("stemaxhop", "Set Tokenring vlan STE max hop");
				enableC.set.vlan["<vlans>"].stemaxhop.addSC("<hopcount>", "STE max hop count (1..13)");
			enableC.set.vlan["<vlans>"].addSC("stp", "Set vlan STP");
				enableC.set.vlan["<vlans>"].stp.addSC("<stp_type>", "STP type (ieee, ibm, auto)");
			enableC.set.vlan["<vlans>"].addSC("translation", "Set vlan translation");
				enableC.set.vlan["<vlans>"].translation.addSC("<translation>", "Translation number (1..1005)");
			enableC.set.vlan["<vlans>"].addSC("type", "Set vlan type");
				enableC.set.vlan["<vlans>"].type.addSC("<type>", "VLAN type (ethernet, fddi, fddinet, trcrf, trbrf)");
			enableC.set.vlan["<vlans>"].addSC("<mod/port>", "Module number and Port number(s)");
	enableC.set.addSC("vmps", "Set VMPS information");
	enableC.set.addSC("vtp", "Set VLAN Trunk Information");
		enableC.set.vtp.addSC("domain", "Set VTP domain");
			enableC.set.vtp.domain.addSC("<name>", "Domain name");
		enableC.set.vtp.addSC("mode", "Set VTP mode");
			enableC.set.vtp.mode.addSC("client", "VTP client mode");
			enableC.set.vtp.mode.addSC("server", "VTP server mode");
			enableC.set.vtp.mode.addSC("transparent", "VTP transparent mode");
		enableC.set.vtp.addSC("passwd", "Set VTP password");
			enableC.set.vtp.passwd.addSC("<passwd>", "Password (0 to clear)");
		enableC.set.vtp.addSC("pruneeligible", "Set VTP pruning");
			enableC.set.vtp.pruneeligible.addSC("<vlan>", "VLAN number");
		enableC.set.vtp.addSC("pruning", "Set VTP pruning");
			enableC.set.vtp.pruning.addSC("disable", "Disable VTP pruning");
			enableC.set.vtp.pruning.addSC("enable", "Enable VTP pruning");
		enableC.set.vtp.addSC("v2", "Set VTP version 2");
			enableC.set.vtp.v2.addSC("disable", "Disable VTP version 2");
			enableC.set.vtp.v2.addSC("enable", "Enable VTP version 2");
enableC.addSC("show", "Show commands, use 'show help' for more info");
	enableC.show.addSC("accounting", "Show accounting information");
	enableC.show.addSC("alias", "Show aliases for commands");
	enableC.show.addSC("arp", "Show ARP table");
	enableC.show.addSC("authentication", "Show authentication information");
	enableC.show.addSC("authorization", "Show authorization information");
	enableC.show.addSC("banner", "Show system banner");
	enableC.show.addSC("boot", "Show booting environment variables");
	enableC.show.addSC("cam", "Show CAM table");
	enableC.show.addSC("cdp", "Show Cisco Discovery Protocol Information");
	enableC.show.addSC("cgmp", "Show CGMP info");
	enableC.show.addSC("channel", "Show channel information");
	enableC.show.addSC("config", "Show system configuration");
	enableC.show.addSC("counters", "Show port counters");
	enableC.show.addSC("dot1q-all-tagged", "Show dot1q tag status");
	enableC.show.addSC("dot1x", "Show dot1x port capability & version");
	enableC.show.addSC("dvlan", "Show dynamic vlan statistics");
	enableC.show.addSC("environment", "Show environment information");
	enableC.show.addSC("errdisable-timeout", "Show err-disable timeout config");
	enableC.show.addSC("errordetection", "Show errordetection settings");
	enableC.show.addSC("file", "Show contents of file");
	enableC.show.addSC("flash", "Show file information on flash device");
	enableC.show.addSC("garp", "Show GARP information");
	enableC.show.addSC("gmrp", "Show GMRP information");
	enableC.show.addSC("gvrp", "Show GVRP information");
	enableC.show.addSC("imagemib", "Show image mib information");
	enableC.show.addSC("interface", "Show network interfaces");
	enableC.show.addSC("ip", "Show IP Information");
		enableC.show.ip.addSC("alias", "Show IP address aliases");
		enableC.show.ip.addSC("dns", "Show IP DNS information");
		enableC.show.ip.addSC("http", "Show IP HTTP information");
		enableC.show.ip.addSC("permit", "Show IP permit list");
		enableC.show.ip.addSC("route", "Show IP routing table");
	enableC.show.addSC("kerberos", "Show kerberos configuration information");
	enableC.show.addSC("log", "Show log information");
	enableC.show.addSC("logging", "Show system logging information");
	enableC.show.addSC("mac", "Show MAC information");
		enableC.show.mac.addSC("<mod>", "Module number");
		enableC.show.mac.addSC("<mod/port>", "Module number and Port number(s)");
	enableC.show.addSC("mls", "Show multilayer switching information");
		enableC.show.mls.addSC("entry", "Show MLS entries");
		enableC.show.mls.addSC("nde", "Show Netflow Data Export information");
		enableC.show.mls.addSC("include", "Show routers included as MLS-RP");
		enableC.show.mls.addSC("multicast", "Show MLS feature info for multicast");
		enableC.show.mls.addSC("rp", "Show information for MLS-RP");
		enableC.show.mls.addSC("statistics", "Show MLS statistics");
	enableC.show.addSC("module", "Show module info");
		enableC.show.module.addSC("<mod>", "Module number");
	enableC.show.addSC("multicast", "Show multicast information");
	enableC.show.addSC("netstat", "Show network statistics");
	enableC.show.addSC("ntp", "Show ntp statistics");
	enableC.show.addSC("nvramenv", "Show environment variables");
	enableC.show.addSC("port", "Show port information");
		enableC.show.port.addSC("auxiliaryvlan", "Show port auxiliary vlan information");
		enableC.show.port.addSC("cdp", "Show port CDP information");
		enableC.show.port.addSC("capabilities", "Show port capabilities");
		enableC.show.port.addSC("channel", "Show port channel information");
		enableC.show.port.addSC("counters", "Show port counters");
		enableC.show.port.addSC("dot1x", "Show port dot1x information");
		enableC.show.port.addSC("flowcontrol", "Show port traffic flowcontrol");
		enableC.show.port.addSC("ifindex", "Show port IfIndex information");
		enableC.show.port.addSC("inlinepower", "Show inline power for port(s)");
		enableC.show.port.addSC("mac", "Show port MAC counters");
		enableC.show.port.addSC("negotiation", "Show port negotiation");
		enableC.show.port.addSC("protocol", "Show port protocol membership");
		enableC.show.port.addSC("security", "Show port security information");
		enableC.show.port.addSC("spantree", "Show port spantree information");
		enableC.show.port.addSC("status", "Show port status");
		enableC.show.port.addSC("trap", "Show port trap information");
		enableC.show.port.addSC("trunk", "Show port trunk information");
		enableC.show.port.addSC("<mod>", "Module number");
		enableC.show.port.addSC("<mod/port>", "Module number and Port number(s)");
	enableC.show.addSC("proc", "Show cpu and processes utilization");
	enableC.show.addSC("protocolfilter", "Show protocolfilter information");
	enableC.show.addSC("pvlan", "Show Private Vlan Information");
		enableC.show.pvlan.addSC("<vlan>", "Show Private Vlan's Config");
		enableC.show.pvlan.addSC("capability", "Determine if a Port can be made a private port");
		enableC.show.pvlan.addSC("community", "Show Config for Community Private Vlans");
		enableC.show.pvlan.addSC("isolated", "Show Config for Isolated Private Vlans");
		enableC.show.pvlan.addSC("mapping", "Show Private Vlan Mappings");
		enableC.show.pvlan.addSC("primary", "Show Config for Primary Private Vlans");
		enableC.show.pvlan.addSC("twoway-community", "Show Config for Twoway Community Private Vlans");
	enableC.show.addSC("qos", "Show QOS information");
	enableC.show.addSC("radius", "Show RADIUS information");
	enableC.show.addSC("rcp", "Show rcp information");
	enableC.show.addSC("reset", "Show schedule reset information");
	enableC.show.addSC("rspan", "Show remote switch port analyzer information");
	enableC.show.addSC("running-config", "Show system runtime configuration");
	enableC.show.addSC("snmp", "Show SNMP information");
	enableC.show.addSC("span", "Show switch port analyzer information");
	enableC.show.addSC("spantree", "Show spantree information");
		enableC.show.spantree.addSC("active", "Show active ports in spanning tree");
		enableC.show.spantree.addSC("backbonefast", "Show spanning tree backbone fast");
		enableC.show.spantree.addSC("blockedports", "Show ports that are blocked");
		enableC.show.spantree.addSC("bpdu-skewing", "Show spanning tree bpdu skewing statistics");
		enableC.show.spantree.addSC("conflicts", "Show spanning tree conflicting info for vlan");
		enableC.show.spantree.addSC("defaultcostmode", "Show spanning tree port cost mode");
		enableC.show.spantree.addSC("guard", "Show spanning tree guard info");
		enableC.show.spantree.addSC("mapping", "Show spanning tree vlan and instance mapping");
		enableC.show.spantree.addSC("mistp-instance", "Show spantree info for MISTP instance");
		enableC.show.spantree.addSC("portfast", "Show spanning tree port fast info");
		enableC.show.spantree.addSC("portinstancecost", "Show spanning tree port instance cost");
		enableC.show.spantree.addSC("portvlancost", "Show spanning tree port vlan cost");
		enableC.show.spantree.addSC("statistics", "Show spanning tree statistic info");
		enableC.show.spantree.addSC("summary", "Show spanning tree summary");
		enableC.show.spantree.addSC("uplinkfast", "Show spanning tree uplink fast");
		enableC.show.spantree.addSC("<mod/port>", "Module number and Port number(s)");
		enableC.show.spantree.addSC("<vlan>", "VLAN number for PVST+");
	enableC.show.addSC("startup-config", "Show system startup configuration");
	enableC.show.addSC("summertime", "Show state of summertime information");
	enableC.show.addSC("switchacceleration", "Show switch acceleration status");
	enableC.show.addSC("system", "Show system information");
	enableC.show.addSC("tacacs", "Show TACACS information");
	enableC.show.addSC("tech-support", "Show system information for Tech-Support");
	enableC.show.addSC("test", "Show results of diagnostic tests");
	enableC.show.addSC("time", "Show time of day");
	enableC.show.addSC("timezone", "Show the current timezone offset");
	enableC.show.addSC("top", "Show TopN report");
	enableC.show.addSC("traffic", "Show Traffic information");
	enableC.show.addSC("trunk", "Show trunk ports");
		enableC.show.trunk.addSC("detail", "Show detailed information");
		enableC.show.trunk.addSC("<mod>", "Module number");
		enableC.show.trunk.addSC("<mod/port>", "Module number and Port number(s)");
	enableC.show.addSC("udld", "Show Uni-directional Link Detection information");
	enableC.show.addSC("users", "Show active Admin sessions");
	enableC.show.addSC("version", "Show version information");
	enableC.show.addSC("vlan", "Show Virtual LAN information");
		enableC.show.vlan.addSC("mapping", "Show Vlan 802.1Q mapping");
		enableC.show.vlan.addSC("trunk", "Show Vlan including trunk ports");
		enableC.show.vlan.addSC("<type>", "Vlan type (ethernet, fddi, fddinet, trbrf, trcrf)");
		enableC.show.vlan.addSC("<vlans>", "Vlan Number(s)");
	enableC.show.addSC("vmps", "Show VMPS information");
	enableC.show.addSC("vtp", "Show VTP Information");
		enableC.show.vtp.addSC("domain", "Show VTP domain information");
		enableC.show.vtp.addSC("statistics", "Show VTP statistic information");
enableC.addSC("slip", "Attach/detach Serial Line IP interface");
enableC.addSC("squeeze", "Reclaim space used by deleted files");
enableC.addSC("telnet", "Telnet to a remote host");
	enableC.telnet.addSC("encrypt", "Perform encryption");
		enableC.telnet.encrypt.addSC("kerberos", "Perform kerberos authentication");
			enableC.telnet.encrypt.kerberos.addSC("<host>", "Specify the host name");
				enableC.telnet.encrypt.kerberos["<host>"].addSC("<port>", "Specify the port number");
	enableC.telnet.addSC("<host>", "Specify the host name");
		enableC.telnet["<host>"].addSC("<port>", "Specify the port number");
enableC.addSC("test", "Test command, use 'test help' for more info");
enableC.addSC("traceroute", "Trace the route to a host");
	enableC.traceroute.addSC("-i", "Specify the initial TTL");
	enableC.traceroute.addSC("-m", "Specify maximum TTL");
	enableC.traceroute.addSC("-n", "No DNS lookup");
	enableC.traceroute.addSC("-p", "Specify base UDP destination port number");
	enableC.traceroute.addSC("-q", "Specify number of queries");
	enableC.traceroute.addSC("-t", "Specify TOS");
	enableC.traceroute.addSC("-w", "Specify wait time");
	enableC.traceroute.addSC("<host>", "IP address or hostname");
		enableC.traceroute["<host>"].addSC("<data_size>", "Size of the packet (0..1420)");
enableC.addSC("undelete", "Undelete a file on flash device");
enableC.addSC("upload", "Upload code from a processor");
enableC.addSC("verify", "Verify checksum of file on flash device");
enableC.addSC("wait", "Wait for x seconds");
enableC.addSC("whichboot", "Which file booted");
enableC.addSC("write", "Write system configuration to terminal/network");
	enableC.write.addSC("memory", "Write to NV memory");
	enableC.write.addSC("network", "Write to network");
	enableC.write.addSC("terminal", "Write to terminal");
		enableC.write.terminal.addSC("all", "Write default and non-default config");
	enableC.write.addSC("tech-support", "Write tech-support");
	enableC.write.addSC("<host>", "IP address or hostname");
