| 7.3 |  | IGRP |
| 7.3.5 |  | Configuring IGRP |

| To configure the IGRP routing process, use the router igrp configuration command. To shut down an IGRP routing process, use the no form of this command. RouterA(config)#router igrp as-number RouterA(config)#no router igrp as-number The Autonomous System number is one that identifies the IGRP process. It is also used to tag the routing information. To specify a list of networks for IGRP routing processes, use the network router configuration command. To remove an entry, use the no form of the command. Figure is an example of how to configure IGRP using AS 101.
| Lab Activity Lab Exercise: Configuring IGRP This lab is to setup an IP addressing scheme using class C networks.
| Lab Activity e-Lab Activity: Configuring IGRP In this lab, the students will learn to configure IGRP.
| Web Links Configuring IGRP http://www.cisco.com/en/US/products/sw/ iosswrel/ps1831/ products_configuration_guide_ chapter09186a00800d97f6.html