
routeMapC.addSC("default", "Set a command to its defaults");
routeMapC.addSC("exit", "Exit from route-map configuration mode");
routeMapC.addSC("help", "Description of the interactive help system");
routeMapC.addSC("match", "Match values from routing table");
   routeMapC.match.addSC("as-path", "Match BGP AS path list");
      routeMapC.match["as-path"].addSC("<1-199>", "AS path access-list");
   routeMapC.match.addSC("clns", "CLNS information");
   routeMapC.match.addSC("community", "Match BGP community list");
   routeMapC.match.addSC("interface", "Match first hop interface of route");
      routeMapC.match.interface.addSC("Async", "Async interface");
         routeMapC.match.interface.Async.addSC("<1-65>", "Async interface number");
      routeMapC.match.interface.addSC("Dialer", "Dialer interface");
         routeMapC.match.interface.Dialer.addSC("<0-255>", "Dialer interface number");
            routeMapC.match.interface.Dialer["<0-255>"].addSC("Async", "Async interface");
               routeMapC.match.interface.Dialer["<0-255>"].Async.addSC("<1-65>", "Async interface number");
      routeMapC.match.interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
         routeMapC.match.interface.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
      routeMapC.match.interface.addSC("Loopback", "Loopback interface");
         routeMapC.match.interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
            routeMapC.match.interface.Loopback["<0-2147483647>"].addSC("Async", "Async interface");
               routeMapC.match.interface.Loopback["<0-2147483647>"].Async.addSC("<1-65>", "Async interface number");
            routeMapC.match.interface.Loopback["<0-2147483647>"].addSC("Dialer", "Dialer interface");
               routeMapC.match.interface.Loopback["<0-2147483647>"].Dialer.addSC("<0-255>", "Dialer interface number");
                  routeMapC.match.interface.Loopback["<0-2147483647>"].Dialer["<0-255>"].addSC("Async", "Async interface");
            routeMapC.match.interface.Loopback["<0-2147483647>"].addSC("FastEthernet", "FastEthernet IEEE 802.3");
               routeMapC.match.interface.Loopback["<0-2147483647>"].FastEthernet.addSC("<0-1>", "FastEthernet interface number");
      routeMapC.match.interface.addSC("Null", "Null interface");
         routeMapC.match.interface.Null.addSC("<0-0>", "Null interface number");
            routeMapC.match.interface.Null["<0-0>"].addSC("Async", "Async interface");
               routeMapC.match.interface.Null["<0-0>"].Async.addSC("<1-65>", "Async interface number");
            routeMapC.match.interface.Null["<0-0>"].addSC("Dialer", "Dialer interface");
               routeMapC.match.interface.Null["<0-0>"].Dialer.addSC("<0-255>", "Dialer interface number");
                  routeMapC.match.interface.Null["<0-0>"].Dialer["<0-255>"].addSC("Async", "Async interface");
            routeMapC.match.interface.Null["<0-0>"].addSC("FastEthernet", "FastEthernet IEEE 802.3");
               routeMapC.match.interface.Null["<0-0>"].FastEthernet.addSC("<0-1>", "FastEthernet interface number");
            routeMapC.match.interface.Null["<0-0>"].addSC("Loopback", "Loopback interface");
               routeMapC.match.interface.Null["<0-0>"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
                  routeMapC.match.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("Async", "Async interface");
                  routeMapC.match.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("Dialer", "Dialer interface");
                  routeMapC.match.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("FastEthernet", "FastEthernet IEEE 802.3");
      routeMapC.match.interface.addSC("Serial", "Serial");
         routeMapC.match.interface.Serial.addSC("<0-1>", "Serial interface number");
   routeMapC.match.addSC("ip", "IP specific information");
      routeMapC.match.ip.addSC("address", "Match address of route or match packet");
         routeMapC.match.ip.address.addSC("<1-199>", "IP access-list number");
         routeMapC.match.ip.address.addSC("<1300-2699>", "IP access-list number (expanded range)");
            routeMapC.match.ip.address["<1300-2699>"].addSC("<1-199>", "IP access-list number");
         routeMapC.match.ip.address.addSC("WORD", "IP access-list name");
            routeMapC.match.ip.address.WORD.addSC("<1-199>", "IP access-list number");
            routeMapC.match.ip.address.WORD.addSC("<1300-2699>", "IP access-list number (expanded range)");
               routeMapC.match.ip.address.WORD["<1300-2699>"].addSC("<1-199>", "IP access-list number");
         routeMapC.match.ip.address.addSC("prefix-list", "Match entries of prefix-lists");
            routeMapC.match.ip.address["prefix-list"].addSC("WORD", "IP prefix-list name");
      routeMapC.match.ip.addSC("next-hop", "Match next-hop address of route");
         routeMapC.match.ip["next-hop"].addSC("<1-99>", "IP access-list number");
         routeMapC.match.ip["next-hop"].addSC("<1300-1999>", "IP access-list number (expanded range)");
            routeMapC.match.ip["next-hop"]["<1300-1999>"].addSC("<1-99>", "IP access-list number");
         routeMapC.match.ip["next-hop"].addSC("WORD", "IP standard access-list name");
            routeMapC.match.ip["next-hop"].WORD.addSC("<1-99>", "IP access-list number");
            routeMapC.match.ip["next-hop"].WORD.addSC("<1300-1999>", "IP access-list number (expanded range)");
               routeMapC.match.ip["next-hop"].WORD["<1300-1999>"].addSC("<1-99>", "IP access-list number");
         routeMapC.match.ip["next-hop"].addSC("prefix-list", "Match entries of prefix-lists");
            routeMapC.match.ip["next-hop"]["prefix-list"].addSC("WORD", "IP prefix-list name");
      routeMapC.match.ip.addSC("route-source", "Match advertising source address of route");
         routeMapC.match.ip["route-source"].addSC("<1-99>", "IP access-list number");
         routeMapC.match.ip["route-source"].addSC("<1300-1999>", "IP access-list number (expanded range)");
            routeMapC.match.ip["route-source"]["<1300-1999>"].addSC("<1-99>", "IP access-list number");
         routeMapC.match.ip["route-source"].addSC("WORD", "IP standard access-list name");
            routeMapC.match.ip["route-source"].WORD.addSC("<1-99>", "IP access-list number");
            routeMapC.match.ip["route-source"].WORD.addSC("<1300-1999>", "IP access-list number (expanded range)");
               routeMapC.match.ip["route-source"].WORD["<1300-1999>"].addSC("<1-99>", "IP access-list number");
         routeMapC.match.ip["route-source"].addSC("prefix-list", "Match entries of prefix-lists");
            routeMapC.match.ip["route-source"]["prefix-list"].addSC("WORD", "IP prefix-list name");
//   routeMapC.match.addSC("length", "Packet length");
//      routeMapC.match.length.addSC("<0-2147483647>", "Minimum packet length");
//         routeMapC.match.length["<0-2147483647>"].addSC("<0-2147483647>", "Maximum packet length");
   routeMapC.match.addSC("metric", "Match metric of route");
      routeMapC.match.metric.addSC("<0-4294967295>", "Metric value");
   routeMapC.match.addSC("route-type", "Match route-type of route");
   routeMapC.match.addSC("tag", "Match tag of route");
      routeMapC.match.tag.addSC("<0-4294967295>", "Tag value");
routeMapC.addSC("no", "Negate a command or set its defaults");
routeMapC.addSC("set", "Set values in destination routing protocol");
   routeMapC.set.addSC("as-path", "Prepend string for a BGP AS-path attribute");
      routeMapC.set["as-path"].addSC("prepend", "Prepend to the as-path");
         routeMapC.set["as-path"].prepend.addSC("<1-65535>", "AS number");
      routeMapC.set["as-path"].addSC("tag", "Set the tag as an AS-path attribute");
   routeMapC.set.addSC("automatic-tag", "Automatically compute TAG value");
   routeMapC.set.addSC("clns", "OSI summary address");
      routeMapC.set.clns.addSC("next-hop", "Next hop address");
         routeMapC.set.clns["next-hop"].addSC("XX.XXXX. ... .XXX.XX", "CLNS summary prefix");
   routeMapC.set.addSC("comm-list", "set BGP community list (for deletion)");
      routeMapC.set["comm-list"].addSC("<1-99>", "Community-list number (standard)");
         routeMapC.set["comm-list"]["<1-99>"].addSC("delete", "Delete matching communities");
      routeMapC.set["comm-list"].addSC("<100-199>", "Communitly-list number (extended)");
         routeMapC.set["comm-list"]["<100-199>"].addSC("delete", "Delete matching communities");
   routeMapC.set.addSC("community", "BGP community attribute");
      routeMapC.set.community.addSC("<1-4294967295>", "community number");
      routeMapC.set.community.addSC("aa:nn", "community number in aa:nn format");
      routeMapC.set.community.addSC("additive", "Add to the existing community");
      routeMapC.set.community.addSC("local-AS", "Do not send outside local AS (well-known community)");
         routeMapC.set.community["local-AS"].addSC("<1-4294967295>", "community number");
         routeMapC.set.community["local-AS"].addSC("aa:nn", "community number in aa:nn format");
         routeMapC.set.community["local-AS"].addSC("additive", "Add to the existing community");
      routeMapC.set.community.addSC("no-advertise", "Do not advertise to any peer (well-known community)");
         routeMapC.set.community["no-advertise"].addSC("<1-4294967295>", "community number");
         routeMapC.set.community["no-advertise"].addSC("aa:nn", "community number in aa:nn format");
         routeMapC.set.community["no-advertise"].addSC("additive", "Add to the existing community");
         routeMapC.set.community["no-advertise"].addSC("local-AS", "Do not send outside local AS (well-known community)");
            routeMapC.set.community["no-advertise"]["local-AS"].addSC("<1-4294967295>", "community number");
            routeMapC.set.community["no-advertise"]["local-AS"].addSC("aa:nn", "community number in aa:nn format");
            routeMapC.set.community["no-advertise"]["local-AS"].addSC("additive", "Add to the existing community");
      routeMapC.set.community.addSC("no-export", "Do not export to next AS (well-known community)");
         routeMapC.set.community["no-export"].addSC("<1-4294967295>", "community number");
         routeMapC.set.community["no-export"].addSC("aa:nn", "community number in aa:nn format");
         routeMapC.set.community["no-export"].addSC("additive", "Add to the existing community");
         routeMapC.set.community["no-export"].addSC("local-AS", "Do not send outside local AS (well-known community)");
            routeMapC.set.community["no-export"]["local-AS"].addSC("<1-4294967295>", "community number");
            routeMapC.set.community["no-export"]["local-AS"].addSC("aa:nn", "community number in aa:nn format");
            routeMapC.set.community["no-export"]["local-AS"].addSC("additive", "Add to the existing community");
         routeMapC.set.community["no-export"].addSC("no-advertise", "Do not advertise to any peer (well-known community)");
            routeMapC.set.community["no-export"]["no-advertise"].addSC("<1-4294967295>", "community number");
            routeMapC.set.community["no-export"]["no-advertise"].addSC("aa:nn", "community number in aa:nn format");
            routeMapC.set.community["no-export"]["no-advertise"].addSC("additive", "Add to the existing community");
            routeMapC.set.community["no-export"]["no-advertise"].addSC("local-AS", "Do not send outside local AS (well-known community)");
               routeMapC.set.community["no-export"]["no-advertise"]["local-AS"].addSC("<1-4294967295>", "community number");
               routeMapC.set.community["no-export"]["no-advertise"]["local-AS"].addSC("aa:nn", "community number in aa:nn format");
               routeMapC.set.community["no-export"]["no-advertise"]["local-AS"].addSC("additive", "Add to the existing community");
      routeMapC.set.community.addSC("none", "No community attribute");
   routeMapC.set.addSC("dampening", "Set BGP route flap dampening parameters");
      routeMapC.set.dampening.addSC("<1-45>", "half-life time for the penalty");
         routeMapC.set.dampening["<1-45>"].addSC("<1-20000>", "penalty to start reusing a route");
            routeMapC.set.dampening["<1-45>"]["<1-20000>"].addSC("<1-20000>", "penalty to start suppressing a route");
               routeMapC.set.dampening["<1-45>"]["<1-20000>"]["<1-20000>"].addSC("<1-255>", "Maximum duration to suppress a stable route");
   routeMapC.set.addSC("default", "Set default information");
   routeMapC.set.addSC("interface", "Output interface");
      routeMapC.set.interface.addSC("Async", "Async interface");
         routeMapC.set.interface.Async.addSC("<1-65>", "Async interface number");
      routeMapC.set.interface.addSC("Dialer", "Dialer interface");
         routeMapC.set.interface.Dialer.addSC("<0-255>", "Dialer interface number");
            routeMapC.set.interface.Dialer["<0-255>"].addSC("Async", "Async interface");
               routeMapC.set.interface.Dialer["<0-255>"].Async.addSC("<1-65>", "Async interface number");
      routeMapC.set.interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
         routeMapC.set.interface.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
      routeMapC.set.interface.addSC("Loopback", "Loopback interface");
         routeMapC.set.interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
            routeMapC.set.interface.Loopback["<0-2147483647>"].addSC("Async", "Async interface");
               routeMapC.set.interface.Loopback["<0-2147483647>"].Async.addSC("<1-65>", "Async interface number");
            routeMapC.set.interface.Loopback["<0-2147483647>"].addSC("Dialer", "Dialer interface");
               routeMapC.set.interface.Loopback["<0-2147483647>"].Dialer.addSC("<0-255>", "Dialer interface number");
                  routeMapC.set.interface.Loopback["<0-2147483647>"].Dialer["<0-255>"].addSC("Async", "Async interface");
            routeMapC.set.interface.Loopback["<0-2147483647>"].addSC("FastEthernet", "FastEthernet IEEE 802.3");
               routeMapC.set.interface.Loopback["<0-2147483647>"].FastEthernet.addSC("<0-1>", "FastEthernet interface number");
      routeMapC.set.interface.addSC("Null", "Null interface");
         routeMapC.set.interface.Null.addSC("<0-0>", "Null interface number");
            routeMapC.set.interface.Null["<0-0>"].addSC("Async", "Async interface");
               routeMapC.set.interface.Null["<0-0>"].Async.addSC("<1-65>", "Async interface number");
            routeMapC.set.interface.Null["<0-0>"].addSC("Dialer", "Dialer interface");
               routeMapC.set.interface.Null["<0-0>"].Dialer.addSC("<0-255>", "Dialer interface number");
                  routeMapC.set.interface.Null["<0-0>"].Dialer["<0-255>"].addSC("Async", "Async interface");
            routeMapC.set.interface.Null["<0-0>"].addSC("FastEthernet", "FastEthernet IEEE 802.3");
               routeMapC.set.interface.Null["<0-0>"].FastEthernet.addSC("<0-1>", "FastEthernet interface number");
            routeMapC.set.interface.Null["<0-0>"].addSC("Loopback", "Loopback interface");
               routeMapC.set.interface.Null["<0-0>"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
                  routeMapC.set.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("Async", "Async interface");
                  routeMapC.set.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("Dialer", "Dialer interface");
                  routeMapC.set.interface.Null["<0-0>"].Loopback["<0-2147483647>"].addSC("FastEthernet", "FastEthernet IEEE 802.3");
      routeMapC.set.interface.addSC("Serial", "Serial");
         routeMapC.set.interface.Serial.addSC("<0-1>", "Serial interface number");
   routeMapC.set.addSC("ip", "IP specific information");
      routeMapC.set.ip.addSC("default", "Set default information");
      routeMapC.set.ip.addSC("next-hop", "Next hop address");
         routeMapC.set.ip["next-hop"].addSC("A.B.C.D", "IP address of next hop");
         routeMapC.set.ip["next-hop"].addSC("peer-address", "Use peer address (for BGP only)");
         routeMapC.set.ip["next-hop"].addSC("verify-availability", "Verify if nexthop is a CDP neighbor");
      routeMapC.set.ip.addSC("precedence", "Set precedence field");
      routeMapC.set.ip.addSC("qos-group", "Set QOS Group ID");
         routeMapC.set.ip["qos-group"].addSC("<0-99>", "QOS Group ID");
      routeMapC.set.ip.addSC("tos", "Set type of service field");
         routeMapC.set.ip.tos.addSC("<0-15>", "Type of service value");
         routeMapC.set.ip.tos.addSC("max-reliability", "Set max reliable TOS (2)");
         routeMapC.set.ip.tos.addSC("max-throughput", "Set max throughput TOS (4)");
         routeMapC.set.ip.tos.addSC("min-delay", "Set min delay TOS (8)");
         routeMapC.set.ip.tos.addSC("min-monetary-cost", "Set min monetary cost TOS (1)");
         routeMapC.set.ip.tos.addSC("normal", "Set normal TOS (0)");
   routeMapC.set.addSC("level", "Where to import route");
      routeMapC.set.level.addSC("backbone", "Import into OSPF backbone area");
      routeMapC.set.level.addSC("level-1", "Import into a level-1 area");
      routeMapC.set.level.addSC("level-1-2", "Import into level-1 and level-2");
      routeMapC.set.level.addSC("level-2", "Import into level-2 sub-domain");
      routeMapC.set.level.addSC("stub-area", "Import into OSPF NSSA area");
   routeMapC.set.addSC("local-preference", "BGP local preference path attribute");
      routeMapC.set["local-preference"].addSC("<0-4294967295>", "Preference value");
   routeMapC.set.addSC("metric", "Metric value for destination routing protocol");
      routeMapC.set.metric.addSC("+/-<metric>", "Add or subtract metric");
      routeMapC.set.metric.addSC("<0-4294967295>", "Metric value or Bandwidth in Kbits per second");
         routeMapC.set.metric["<0-4294967295>"].addSC("+/-<delay>", "Add or subtract delay");
         routeMapC.set.metric["<0-4294967295>"].addSC("<1-4294967295>", "IGRP delay metric, in 10 microsecond units");
            routeMapC.set.metric["<0-4294967295>"]["<1-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
               routeMapC.set.metric["<0-4294967295>"]["<1-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
                  routeMapC.set.metric["<0-4294967295>"]["<1-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
   routeMapC.set.addSC("metric-type", "Type of metric for destination routing protocol");
      routeMapC.set["metric-type"].addSC("external", "IS-IS external metric");
      routeMapC.set["metric-type"].addSC("internal", "Use IGP metric as the MED for BGP");
      routeMapC.set["metric-type"].addSC("type-1", "OSPF external type 1 metric");
      routeMapC.set["metric-type"].addSC("type-2", "OSPF external type 2 metric");
   routeMapC.set.addSC("origin", "BGP origin code");
      routeMapC.set.origin.addSC("egp", "remote EGP");
         routeMapC.set.origin.egp.addSC("<0-65535>", "remote AS");
      routeMapC.set.origin.addSC("igp", "local IGP");
      routeMapC.set.origin.addSC("incomplete", "unknown heritage");
   routeMapC.set.addSC("tag", "Tag value for destination routing protocol");
      routeMapC.set.tag.addSC("<0-4294967295>", "Tag value");
   routeMapC.set.addSC("weight", "BGP weight for routing table");
      routeMapC.set.weight.addSC("<0-4294967295>", "Weight value");
