		enableC.show.ip.addSC("ospf", "OSPF information");
			enableC.show.ip.ospf.addSC("<1-4294967295>", "Process ID number");
				enableC.show.ip.ospf["<1-4294967295>"].addSC("<0-4294967295>", "OSPF area ID as a decimal number");
				enableC.show.ip.ospf["<1-4294967295>"].addSC("A.B.C.D", "OSPF area ID in IP address format");
			enableC.show.ip.ospf.addSC("border-routers", "Border and Boundary Router Information");
			enableC.show.ip.ospf.addSC("database", "Database summary");
				enableC.show.ip.ospf.database.addSC("adv-router", "Advertising Router link states");
					enableC.show.ip.ospf.database["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
				enableC.show.ip.ospf.database.addSC("asbr-summary", "ASBR summary link states");
					enableC.show.ip.ospf.database["asbr-summary"].addSC("A.B.C.D", "Link state ID (as an IP address)");
					enableC.show.ip.ospf.database["asbr-summary"].addSC("adv-router", "Advertising Router link states");
						enableC.show.ip.ospf.database["asbr-summary"]["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
					enableC.show.ip.ospf.database["asbr-summary"].addSC("internal", "Internal LSA information");
						enableC.show.ip.ospf.database["asbr-summary"].internal.addSC("adv-router", "Advertising Router link states");
				enableC.show.ip.ospf.database.addSC("database-summary", "Summary of database");
				enableC.show.ip.ospf.database.addSC("external", "External link states");
					enableC.show.ip.ospf.database.external.addSC("A.B.C.D", "Link state ID (as an IP address)");
					enableC.show.ip.ospf.database.external.addSC("adv-router", "Advertising Router link states");
						enableC.show.ip.ospf.database.external["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
					enableC.show.ip.ospf.database.external.addSC("internal", "Internal LSA information");
						enableC.show.ip.ospf.database.external.internal.addSC("adv-router", "Advertising Router link states");
				enableC.show.ip.ospf.database.addSC("network", "Network link states");
					enableC.show.ip.ospf.database.network.addSC("A.B.C.D", "Link state ID (as an IP address)");
					enableC.show.ip.ospf.database.network.addSC("adv-router", "Advertising Router link states");
						enableC.show.ip.ospf.database.network["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
					enableC.show.ip.ospf.database.network.addSC("internal", "Internal LSA information");
						enableC.show.ip.ospf.database.network.internal.addSC("adv-router", "Advertising Router link states");
				enableC.show.ip.ospf.database.addSC("nssa-external", "NSSA External link states");
					enableC.show.ip.ospf.database["nssa-external"].addSC("A.B.C.D", "Link state ID (as an IP address)");
					enableC.show.ip.ospf.database["nssa-external"].addSC("adv-router", "Advertising Router link states");
						enableC.show.ip.ospf.database["nssa-external"]["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
					enableC.show.ip.ospf.database["nssa-external"].addSC("internal", "Internal LSA information");
						enableC.show.ip.ospf.database["nssa-external"].internal.addSC("adv-router", "Advertising Router link states");
				enableC.show.ip.ospf.database.addSC("opaque-area", "Opaque Area link states");
					enableC.show.ip.ospf.database["opaque-area"].addSC("A.B.C.D", "Link state ID (as an IP address)");
					enableC.show.ip.ospf.database["opaque-area"].addSC("adv-router", "Advertising Router link states");
						enableC.show.ip.ospf.database["opaque-area"]["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
					enableC.show.ip.ospf.database["opaque-area"].addSC("internal", "Internal LSA information");
						enableC.show.ip.ospf.database["opaque-area"].internal.addSC("adv-router", "Advertising Router link states");
				enableC.show.ip.ospf.database.addSC("opaque-as", "Opaque AS link states");
					enableC.show.ip.ospf.database["opaque-as"].addSC("A.B.C.D", "Link state ID (as an IP address)");
					enableC.show.ip.ospf.database["opaque-as"].addSC("adv-router", "Advertising Router link states");
						enableC.show.ip.ospf.database["opaque-as"]["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
					enableC.show.ip.ospf.database["opaque-as"].addSC("internal", "Internal LSA information");
						enableC.show.ip.ospf.database["opaque-as"].internal.addSC("adv-router", "Advertising Router link states");
				enableC.show.ip.ospf.database.addSC("opaque-link", "Opaque Link-Local link states");
					enableC.show.ip.ospf.database["opaque-link"].addSC("A.B.C.D", "Link state ID (as an IP address)");
					enableC.show.ip.ospf.database["opaque-link"].addSC("adv-router", "Advertising Router link states");
						enableC.show.ip.ospf.database["opaque-link"]["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
					enableC.show.ip.ospf.database["opaque-link"].addSC("internal", "Internal LSA information");
						enableC.show.ip.ospf.database["opaque-link"].internal.addSC("adv-router", "Advertising Router link states");
				enableC.show.ip.ospf.database.addSC("router", "Router link states");
					enableC.show.ip.ospf.database.router.addSC("A.B.C.D", "Link state ID (as an IP address)");
					enableC.show.ip.ospf.database.router.addSC("adv-router", "Advertising Router link states");
						enableC.show.ip.ospf.database.router["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
					enableC.show.ip.ospf.database.router.addSC("internal", "Internal LSA information");
						enableC.show.ip.ospf.database.router.internal.addSC("adv-router", "Advertising Router link states");
				enableC.show.ip.ospf.database.addSC("self-originate", "Self-originated link states");
				enableC.show.ip.ospf.database.addSC("summary", "Network summary link states");
					enableC.show.ip.ospf.database.summary.addSC("A.B.C.D", "Link state ID (as an IP address)");
					enableC.show.ip.ospf.database.summary.addSC("adv-router", "Advertising Router link states");
						enableC.show.ip.ospf.database.summary["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
					enableC.show.ip.ospf.database.summary.addSC("internal", "Internal LSA information");
						enableC.show.ip.ospf.database.summary.internal.addSC("adv-router", "Advertising Router link states");
					enableC.show.ip.ospf.database.summary.addSC("self-originate", "Self-originated link states");
			enableC.show.ip.ospf.addSC("flood-list", "Link state flood list");
				enableC.show.ip.ospf["flood-list"].addSC("Async", "Async interface");
					enableC.show.ip.ospf["flood-list"].Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf["flood-list"].addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf["flood-list"].BRI.addSC("<0-6>", "BRI interface number");
				enableC.show.ip.ospf["flood-list"].addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf["flood-list"].BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.ospf["flood-list"].addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf["flood-list"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.ospf["flood-list"].addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf["flood-list"].Dialer.addSC("<0-799>", "Dialer interface number");
				enableC.show.ip.ospf["flood-list"].addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf["flood-list"].Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf["flood-list"].addSC("Lex", "Lex interface");
					enableC.show.ip.ospf["flood-list"].Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.ospf["flood-list"].addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf["flood-list"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
				enableC.show.ip.ospf["flood-list"].addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf["flood-list"].Multilink.addSC("<1-2147483647>", "Multilink interface number");
				enableC.show.ip.ospf["flood-list"].addSC("Null", "Null interface");
					enableC.show.ip.ospf["flood-list"].Null.addSC("<0-0>", "Null interface number");
				enableC.show.ip.ospf["flood-list"].addSC("Serial", "Serial");
					enableC.show.ip.ospf["flood-list"].Serial.addSC("<0-6>", "Serial interface number");
				enableC.show.ip.ospf["flood-list"].addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf["flood-list"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.ospf["flood-list"].addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf["flood-list"].Vif.addSC("<1-1>", "Vif interface number");
				enableC.show.ip.ospf["flood-list"].addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.ospf["flood-list"]["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
				enableC.show.ip.ospf["flood-list"].addSC("Virtual-TokenRing", "Virtual TokenRing");
					enableC.show.ip.ospf["flood-list"]["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			enableC.show.ip.ospf.addSC("interface", "Interface information");
				enableC.show.ip.ospf.interface.addSC("Async", "Async interface");
					enableC.show.ip.ospf.interface.Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf.interface.addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf.interface.BRI.addSC("<0-6>", "BRI interface number");
				enableC.show.ip.ospf.interface.addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf.interface.BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.ospf.interface.addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf.interface.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.ospf.interface.addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf.interface.Dialer.addSC("<0-799>", "Dialer interface number");
				enableC.show.ip.ospf.interface.addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf.interface.Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf.interface.addSC("Lex", "Lex interface");
					enableC.show.ip.ospf.interface.Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.ospf.interface.addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf.interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				enableC.show.ip.ospf.interface.addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf.interface.Multilink.addSC("<1-2147483647>", "Multilink interface number");
				enableC.show.ip.ospf.interface.addSC("Null", "Null interface");
					enableC.show.ip.ospf.interface.Null.addSC("<0-0>", "Null interface number");
				enableC.show.ip.ospf.interface.addSC("Serial", "Serial");
					enableC.show.ip.ospf.interface.Serial.addSC("<0-6>", "Serial interface number");
				enableC.show.ip.ospf.interface.addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf.interface.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.ospf.interface.addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf.interface.Vif.addSC("<1-1>", "Vif interface number");
				enableC.show.ip.ospf.interface.addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.ospf.interface["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
				enableC.show.ip.ospf.interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
					enableC.show.ip.ospf.interface["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			enableC.show.ip.ospf.addSC("mpls", "MPLS related information");
				enableC.show.ip.ospf.mpls.addSC("traffic-eng", "Traffic Engineering information");
					enableC.show.ip.ospf.mpls["traffic-eng"].addSC("fragment", "MPLS fragment information");
					enableC.show.ip.ospf.mpls["traffic-eng"].addSC("link", "MPLS link information");
			enableC.show.ip.ospf.addSC("neighbor", "Neighbor list");
				enableC.show.ip.ospf.neighbor.addSC("Async", "Async interface");
					enableC.show.ip.ospf.neighbor.Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf.neighbor.addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf.neighbor.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.BRI.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.BRI.Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf.neighbor.addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf.neighbor.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.BVI.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.BVI.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.BVI.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.BVI.BRI.addSC("<0-6>", "BRI interface number");
				enableC.show.ip.ospf.neighbor.addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf.neighbor.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.CTunnel.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.CTunnel.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.CTunnel.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.CTunnel.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.CTunnel.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.CTunnel.BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.ospf.neighbor.addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Dialer.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Dialer.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Dialer.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Dialer.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Dialer.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.ospf.neighbor.addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Ethernet.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Ethernet.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Ethernet.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Ethernet.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Ethernet.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Ethernet.Dialer.addSC("<0-799>", "Dialer interface number");
				enableC.show.ip.ospf.neighbor.addSC("Hostname or A.B.C.D", "Neighbor ID");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor["Hostname or A.B.C.D"].Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf.neighbor.addSC("Lex", "Lex interface");
					enableC.show.ip.ospf.neighbor.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Lex.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Lex.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Lex.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Lex.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Lex.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Lex.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Lex.Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf.neighbor.addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("<0-2147483647>", "Loopback interface number");
						enableC.show.ip.ospf.neighbor.Loopback["<0-2147483647>"].addSC("Hostname or A.B.C.D", "Neighbor ID");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Loopback.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Loopback.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Loopback.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Loopback.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Loopback.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Loopback.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Loopback.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Loopback.Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.ospf.neighbor.addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Multilink.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Multilink.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Multilink.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Multilink.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Multilink.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Multilink.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Multilink.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Multilink.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Multilink.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				enableC.show.ip.ospf.neighbor.addSC("Null", "Null interface");
					enableC.show.ip.ospf.neighbor.Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.ospf.neighbor.Null["<0-0>"].addSC("Hostname or A.B.C.D", "Neighbor ID");
					enableC.show.ip.ospf.neighbor.Null.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Null.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Null.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Null.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Null.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Null.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Null.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Null.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Null.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor.Null.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.Null.Multilink.addSC("<1-2147483647>", "Multilink interface number");
				enableC.show.ip.ospf.neighbor.addSC("Serial", "Serial");
					enableC.show.ip.ospf.neighbor.Serial.addSC("<0-6>", "Serial interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Serial.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Serial.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Serial.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Serial.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Serial.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Serial.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Serial.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Serial.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.Serial.Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor.Serial.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.Serial.Null.addSC("<0-0>", "Null interface number");
				enableC.show.ip.ospf.neighbor.addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Tunnel.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Tunnel.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Tunnel.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Tunnel.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.Tunnel.Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.ospf.neighbor.Tunnel.addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.Tunnel.Serial.addSC("<0-6>", "Serial interface number");
				enableC.show.ip.ospf.neighbor.addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf.neighbor.Vif.addSC("<1-1>", "Vif interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.Vif.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.Vif.BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.Vif.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.Vif.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.Vif.Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.Vif.Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.Vif.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.Vif.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.Vif.Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.Vif.Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.Vif.Serial.addSC("<0-6>", "Serial interface number");
					enableC.show.ip.ospf.neighbor.Vif.addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor.Vif.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.ospf.neighbor.addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Serial.addSC("<0-6>", "Serial interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
					enableC.show.ip.ospf.neighbor["Virtual-Template"].addSC("Vif", "PGM Multicast Host interface");
						enableC.show.ip.ospf.neighbor["Virtual-Template"].Vif.addSC("<1-1>", "Vif interface number");
				enableC.show.ip.ospf.neighbor.addSC("Virtual-TokenRing", "Virtual TokenRing");
/*					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].BRI.addSC("<0-6>", "BRI interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Dialer.addSC("<0-799>", "Dialer interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Ethernet.addSC("<0-6>", "Ethernet interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Multilink.addSC("<1-2147483647>", "Multilink interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Serial.addSC("<0-6>", "Serial interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Vif", "PGM Multicast Host interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].Vif.addSC("<1-1>", "Vif interface number");
					enableC.show.ip.ospf.neighbor["Virtual-TokenRing"].addSC("Virtual-Template", "Virtual Template interface");
						enableC.show.ip.ospf.neighbor["Virtual-TokenRing"]["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");

*/
				enableC.show.ip.ospf.neighbor.addSC("detail", "detail of all neighbors");
					enableC.show.ip.ospf.neighbor.detail.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Async.addSC("<1-129>", "Async interface number");
					enableC.show.ip.ospf.neighbor.detail.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.BRI.addSC("<0-6>", "BRI interface number");
						enableC.show.ip.ospf.neighbor.detail.BRI.addSC("Async", "Async interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.BVI.addSC("<1-255>", "BVI interface number");
						enableC.show.ip.ospf.neighbor.detail.BVI.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.BVI.addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
						enableC.show.ip.ospf.neighbor.detail.CTunnel.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.CTunnel.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.CTunnel.addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("<0-799>", "Dialer interface number");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("<0-6>", "Ethernet interface number");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Ethernet.addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Hostname or A.B.C.D", "Neighbor ID");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail["Hostname or A.B.C.D"].addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf.neighbor.detail.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("<0-2147483647>", "Lex interface number");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Lex.addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf.neighbor.detail.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("<0-2147483647>", "Loopback interface number");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("Lex", "Lex interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("<1-2147483647>", "Multilink interface number");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Multilink.addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Null.addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("<0-6>", "Serial interface number");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail.Serial.addSC("Null", "Null interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail.Tunnel.addSC("Serial", "Serial");
					enableC.show.ip.ospf.neighbor.detail.addSC("Vif", "PGM Multicast Host interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("<1-1>", "Vif interface number");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.detail.Vif.addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf.neighbor.detail.addSC("Virtual-Template", "Virtual Template interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-Template"].addSC("Vif", "PGM Multicast Host interface");
/*					enableC.show.ip.ospf.neighbor.detail.addSC("Virtual-TokenRing", "Virtual TokenRing");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Async", "Async interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("BRI", "ISDN Basic Rate Interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Dialer", "Dialer interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Lex", "Lex interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Loopback", "Loopback interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Null", "Null interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Serial", "Serial");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Vif", "PGM Multicast Host interface");
						enableC.show.ip.ospf.neighbor.detail["Virtual-TokenRing"].addSC("Virtual-Template", "Virtual Template interface");
*/
			enableC.show.ip.ospf.addSC("request-list", "Link state request list");
				enableC.show.ip.ospf["request-list"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["request-list"].addSC("Async", "Async interface");
					enableC.show.ip.ospf["request-list"].Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf["request-list"].addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf["request-list"].BRI.addSC("<0-6>", "BRI interface number");
				enableC.show.ip.ospf["request-list"].addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf["request-list"].BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.ospf["request-list"].addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf["request-list"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.ospf["request-list"].addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf["request-list"].Dialer.addSC("<0-799>", "Dialer interface number");
						enableC.show.ip.ospf["request-list"].Dialer["<0-799>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["request-list"].addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf["request-list"].Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf["request-list"].addSC("Lex", "Lex interface");
					enableC.show.ip.ospf["request-list"].Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.ospf["request-list"].addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf["request-list"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
						enableC.show.ip.ospf["request-list"].Loopback["<0-2147483647>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["request-list"].addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf["request-list"].Multilink.addSC("<1-2147483647>", "Multilink interface number");
				enableC.show.ip.ospf["request-list"].addSC("Null", "Null interface");
					enableC.show.ip.ospf["request-list"].Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.ospf["request-list"].Null["<0-0>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["request-list"].addSC("Serial", "Serial");
					enableC.show.ip.ospf["request-list"].Serial.addSC("<0-6>", "Serial interface number");
				enableC.show.ip.ospf["request-list"].addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf["request-list"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.ospf["request-list"].addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf["request-list"].Vif.addSC("<1-1>", "Vif interface number");
				enableC.show.ip.ospf["request-list"].addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.ospf["request-list"]["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
				enableC.show.ip.ospf["request-list"].addSC("Virtual-TokenRing", "Virtual TokenRing");
					enableC.show.ip.ospf["request-list"]["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			enableC.show.ip.ospf.addSC("retransmission-list", "Link state retransmission list");
				enableC.show.ip.ospf["retransmission-list"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["retransmission-list"].addSC("Async", "Async interface");
					enableC.show.ip.ospf["retransmission-list"].Async.addSC("<1-129>", "Async interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("BRI", "ISDN Basic Rate Interface");
					enableC.show.ip.ospf["retransmission-list"].BRI.addSC("<0-6>", "BRI interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.ospf["retransmission-list"].BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.ospf["retransmission-list"].CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Dialer", "Dialer interface");
					enableC.show.ip.ospf["retransmission-list"].Dialer.addSC("<0-799>", "Dialer interface number");
						enableC.show.ip.ospf["retransmission-list"].Dialer["<0-799>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["retransmission-list"].addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.ospf["retransmission-list"].Ethernet.addSC("<0-6>", "Ethernet interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Lex", "Lex interface");
					enableC.show.ip.ospf["retransmission-list"].Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Loopback", "Loopback interface");
					enableC.show.ip.ospf["retransmission-list"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
						enableC.show.ip.ospf["retransmission-list"].Loopback["<0-2147483647>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["retransmission-list"].addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.ospf["retransmission-list"].Multilink.addSC("<1-2147483647>", "Multilink interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Null", "Null interface");
					enableC.show.ip.ospf["retransmission-list"].Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.ospf["retransmission-list"].Null["<0-0>"].addSC("A.B.C.D", "neighbor router ID");
				enableC.show.ip.ospf["retransmission-list"].addSC("Serial", "Serial");
					enableC.show.ip.ospf["retransmission-list"].Serial.addSC("<0-6>", "Serial interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.ospf["retransmission-list"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.ospf["retransmission-list"].Vif.addSC("<1-1>", "Vif interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.ospf["retransmission-list"]["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
				enableC.show.ip.ospf["retransmission-list"].addSC("Virtual-TokenRing", "Virtual TokenRing");
					enableC.show.ip.ospf["retransmission-list"]["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			enableC.show.ip.ospf.addSC("summary-address", "Summary-address redistribution Information");
			enableC.show.ip.ospf.addSC("virtual-links", "Virtual link information");
		enableC.show.ip.addSC("pgm", "PGM Reliable Transport Protocol");
		enableC.show.ip.addSC("pim", "PIM information");
		enableC.show.ip.addSC("policy", "Policy routing");
		enableC.show.ip.addSC("prefix-list", "List IP prefix lists");
		enableC.show.ip.addSC("protocols", "IP routing protocol process parameters and statistics");
			enableC.show.ip.protocols.addSC("summary", "Short form answer");
			enableC.show.ip.protocols.addSC("vrf", "Display protocols for a VPN Routing/Forwarding instance");
				enableC.show.ip.protocols.vrf.addSC("WORD", "VPN Routing/Forwarding instance name");
					enableC.show.ip.protocols.vrf.WORD.addSC("summary", "Short form answer");
		enableC.show.ip.addSC("redirects", "IP redirects");
		enableC.show.ip.addSC("rip", "IP RIP show commands");
		enableC.show.ip.addSC("route", "IP routing table");
			enableC.show.ip.route.addSC("Hostname or A.B.C.D", "Network to display information about or hostname");
				enableC.show.ip.route["Hostname or A.B.C.D"].addSC("A.B.C.D", "Network mask");
				enableC.show.ip.route["Hostname or A.B.C.D"].addSC("longer-prefixes", "Show route matching the specified Network/Mask pair only");
			enableC.show.ip.route.addSC("bgp", "Border Gateway Protocol (BGP)");
				enableC.show.ip.route.bgp.addSC("<1-65535>", "Autonomous system number");
			enableC.show.ip.route.addSC("connected", "Connected");
			enableC.show.ip.route.addSC("egp", "Exterior Gateway Protocol (EGP)");
				enableC.show.ip.route.egp.addSC("<0-65535>", "Remote autonomous system number");
			enableC.show.ip.route.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				enableC.show.ip.route.eigrp.addSC("<1-65535>", "Autonomous system number");
			enableC.show.ip.route.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				enableC.show.ip.route.igrp.addSC("<1-65535>", "Autonomous system number");
			enableC.show.ip.route.addSC("isis", "ISO IS-IS");
				enableC.show.ip.route.isis.addSC("WORD", "ISO routing area tag");
			enableC.show.ip.route.addSC("list", "IP Access list");
				enableC.show.ip.route.list.addSC("<1-199>", "IP access list number");
				enableC.show.ip.route.list.addSC("WORD", "IP access-list name");
			enableC.show.ip.route.addSC("mobile", "Mobile routes");
			enableC.show.ip.route.addSC("odr", "On Demand stub Routes");
			enableC.show.ip.route.addSC("ospf", "Open Shortest Path First (OSPF)");
				enableC.show.ip.route.ospf.addSC("<1-65535>", "Process ID");
					enableC.show.ip.route.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
						enableC.show.ip.route.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
			enableC.show.ip.route.addSC("profile", "IP routing table profile");
			enableC.show.ip.route.addSC("rip", "Routing Information Protocol (RIP)");
			enableC.show.ip.route.addSC("static", "Static routes");
			enableC.show.ip.route.addSC("summary", "Summary of all routes");
			enableC.show.ip.route.addSC("supernets-only", "Show supernet entries only");
			enableC.show.ip.route.addSC("vrf", "Display routes from a VPN Routing/Forwarding instance");
				enableC.show.ip.route.vrf.addSC("WORD", "VPN Routing/Forwarding instance name");
					enableC.show.ip.route.vrf.WORD.addSC("Hostname or A.B.C.D", "Network to display information about or hostname");
						enableC.show.ip.route.vrf.WORD["Hostname or A.B.C.D"].addSC("A.B.C.D", "Network mask");
						enableC.show.ip.route.vrf.WORD["Hostname or A.B.C.D"].addSC("longer-prefixes", "Show route matching the specified Network/Mask pair only");
					enableC.show.ip.route.vrf.WORD.addSC("bgp", "Border Gateway Protocol (BGP)");
						enableC.show.ip.route.vrf.WORD.bgp.addSC("<1-65535>", "Autonomous system number");
					enableC.show.ip.route.vrf.WORD.addSC("connected", "Connected");
					enableC.show.ip.route.vrf.WORD.addSC("egp", "Exterior Gateway Protocol (EGP)");
						enableC.show.ip.route.vrf.WORD.egp.addSC("<0-65535>", "Remote autonomous system number");
					enableC.show.ip.route.vrf.WORD.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
						enableC.show.ip.route.vrf.WORD.eigrp.addSC("<1-65535>", "Autonomous system number");
					enableC.show.ip.route.vrf.WORD.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
						enableC.show.ip.route.vrf.WORD.igrp.addSC("<1-65535>", "Autonomous system number");
					enableC.show.ip.route.vrf.WORD.addSC("isis", "ISO IS-IS");
						enableC.show.ip.route.vrf.WORD.isis.addSC("WORD", "ISO routing area tag");
					enableC.show.ip.route.vrf.WORD.addSC("list", "IP Access list");
						enableC.show.ip.route.vrf.WORD.list.addSC("<1-199>", "IP access list number");
						enableC.show.ip.route.vrf.WORD.list.addSC("WORD", "IP access-list name");
					enableC.show.ip.route.vrf.WORD.addSC("mobile", "Mobile routes");
					enableC.show.ip.route.vrf.WORD.addSC("odr", "On Demand stub Routes");
					enableC.show.ip.route.vrf.WORD.addSC("ospf", "Open Shortest Path First (OSPF)");
						enableC.show.ip.route.vrf.WORD.ospf.addSC("<1-65535>", "Process ID");
					enableC.show.ip.route.vrf.WORD.addSC("profile", "IP routing table profile");
					enableC.show.ip.route.vrf.WORD.addSC("rip", "Routing Information Protocol (RIP)");
					enableC.show.ip.route.vrf.WORD.addSC("static", "Static routes");
					enableC.show.ip.route.vrf.WORD.addSC("summary", "Summary of all routes");
					enableC.show.ip.route.vrf.WORD.addSC("supernets-only", "Show supernet entries only");
		enableC.show.ip.addSC("rpf", "Display RPF information for multicast source");
		enableC.show.ip.addSC("rsvp", "RSVP information");
		enableC.show.ip.addSC("rtp", "RTP/UDP/IP header-compression statistics");
		enableC.show.ip.addSC("sap", "Session Announcement Protocol cache");
		enableC.show.ip.addSC("slb", "SLB information");
		enableC.show.ip.addSC("sockets", "Open IP sockets");
		enableC.show.ip.addSC("ssh", "Information on SSH");
		enableC.show.ip.addSC("tcp", "TCP/IP header-compression statistics");
		enableC.show.ip.addSC("traffic", "IP protocol statistics");
		enableC.show.ip.addSC("trigger-authentication", "Trigger-authentication host table");
		enableC.show.ip.addSC("vrf", "VPN Routing/Forwarding instance information");
		enableC.show.ip.addSC("wccp", "WCCP information");
	enableC.show.addSC("ipx", "Novell IPX information");
	enableC.show.addSC("isdn", "ISDN information");
	enableC.show.addSC("isis", "IS-IS routing information");
	enableC.show.addSC("kerberos", "Show Kerberos Values");
	enableC.show.addSC("key", "Key information");
	enableC.show.addSC("keymap", "Terminal keyboard mappings");
	enableC.show.addSC("lat", "DEC LAT information");
	enableC.show.addSC("line", "TTY line information");
		enableC.show.line.addSC("<0-134>", "First Line range");
			enableC.show.line["<0-134>"].addSC("<1-134>", "Last Line range");
		enableC.show.line.addSC("async-queue", "Show async-queue");
			enableC.show.line["async-queue"].addSC("<1-99>", "rotary group number");
		enableC.show.line.addSC("aux", "Auxiliary line");
			enableC.show.line.aux.addSC("<0-0>", "First Line range");
		enableC.show.line.addSC("console", "Primary terminal line");
			enableC.show.line.console.addSC("<0-0>", "First Line range");
		enableC.show.line.addSC("summary", "Quick line status summary");
		enableC.show.line.addSC("tty", "Terminal controller");
			enableC.show.line.tty.addSC("<1-128>", "First Line range");
				enableC.show.line.tty["<1-128>"].addSC("<2-128>", "Last Line range");
				enableC.show.line.tty["<1-128>"].addSC("summary", "Quick line status summary");
		enableC.show.line.addSC("vty", "Virtual terminal");
			enableC.show.line.vty.addSC("<0-871>", "First Line range");
				enableC.show.line.vty["<0-871>"].addSC("<1-871>", "Last Line range");
				enableC.show.line.vty["<0-871>"].addSC("summary", "Quick line status summary");
	enableC.show.addSC("llc2", "IBM LLC2 circuit information");
	enableC.show.addSC("lnm", "IBM LAN manager");
	enableC.show.addSC("local-ack", "Local Acknowledgement virtual circuits");
	enableC.show.addSC("location", "Display the system location");
	enableC.show.addSC("logging", "Show the contents of logging buffers");
		enableC.show.logging.addSC("history", "Show the contents of syslog history table");
	enableC.show.addSC("management", "Display the management applications");
	enableC.show.addSC("memory", "Memory statistics");
	enableC.show.addSC("mgcp", "Display Media Gateway Control Protocol information");
	enableC.show.addSC("mls", "multilayer switching information");
	enableC.show.addSC("modemcap", "Show Modem Capabilities database");
	enableC.show.addSC("mpls", "MPLS information");
	enableC.show.addSC("mpoa", "MPOA show commands");
	enableC.show.addSC("nbf", "NBF (NetBEUI) information");
	enableC.show.addSC("ncia", "Native Client Interface Architecture");
	enableC.show.addSC("netbios-cache", "NetBIOS name cache contents");
	enableC.show.addSC("node", "Show known LAT nodes");
	enableC.show.addSC("ntp", "Network time protocol");
	enableC.show.addSC("num-exp", "Number Expansion (Speed Dial) information");
	enableC.show.addSC("parser", "Display parser information");
	enableC.show.addSC("pas", "Port Adaptor Information");
	enableC.show.addSC("pci", "PCI Information");
	enableC.show.addSC("policy-map", "Show QoS Policy Map");
		enableC.show["policy-map"].addSC("WORD", "policy-map name");
			enableC.show["policy-map"].WORD.addSC("class", "Show Qos Policy actions for a indvidual class");
				enableC.show["policy-map"].WORD.class.addSC("WORD", "class-map name");
		enableC.show["policy-map"].addSC("interface", "Show Qos Policy Interface");
			enableC.show["policy-map"].interface.addSC("Async", "Async interface");
				enableC.show["policy-map"].interface.Async.addSC("<1-129>", "Async interface number");
			enableC.show["policy-map"].interface.addSC("BRI", "ISDN Basic Rate Interface");
				enableC.show["policy-map"].interface.BRI.addSC("<0-6>", "BRI interface number");
			enableC.show["policy-map"].interface.addSC("BVI", "Bridge-Group Virtual Interface");
				enableC.show["policy-map"].interface.BVI.addSC("<1-255>", "BVI interface number");
			enableC.show["policy-map"].interface.addSC("CTunnel", "CTunnel interface");
				enableC.show["policy-map"].interface.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
			enableC.show["policy-map"].interface.addSC("Dialer", "Dialer interface");
				enableC.show["policy-map"].interface.Dialer.addSC("<0-799>", "Dialer interface number");
			enableC.show["policy-map"].interface.addSC("Ethernet", "IEEE 802.3");
				enableC.show["policy-map"].interface.Ethernet.addSC("<0-6>", "Ethernet interface number");
			enableC.show["policy-map"].interface.addSC("Group-Async", "Async Group interface");
				enableC.show["policy-map"].interface["Group-Async"].addSC("<0-129>", "Group-Async interface number");
			enableC.show["policy-map"].interface.addSC("Lex", "Lex interface");
				enableC.show["policy-map"].interface.Lex.addSC("<0-2147483647>", "Lex interface number");
			enableC.show["policy-map"].interface.addSC("Loopback", "Loopback interface");
				enableC.show["policy-map"].interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			enableC.show["policy-map"].interface.addSC("Multilink", "Multilink-group interface");
				enableC.show["policy-map"].interface.Multilink.addSC("<1-2147483647>", "Multilink interface number");
			enableC.show["policy-map"].interface.addSC("Null", "Null interface");
				enableC.show["policy-map"].interface.Null.addSC("<0-0>", "Null interface number");
			enableC.show["policy-map"].interface.addSC("Serial", "Serial");
				enableC.show["policy-map"].interface.Serial.addSC("<0-6>", "Serial interface number");
			enableC.show["policy-map"].interface.addSC("Tunnel", "Tunnel interface");
				enableC.show["policy-map"].interface.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
			enableC.show["policy-map"].interface.addSC("Vif", "PGM Multicast Host interface");
				enableC.show["policy-map"].interface.Vif.addSC("<1-1>", "Vif interface number");
			enableC.show["policy-map"].interface.addSC("Virtual-Template", "Virtual Template interface");
				enableC.show["policy-map"].interface["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
			enableC.show["policy-map"].interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
				enableC.show["policy-map"].interface["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			enableC.show["policy-map"].interface.addSC("input", "Input policy");
				enableC.show["policy-map"].interface.input.addSC("class", "Show statistics for a indvidual class");
					enableC.show["policy-map"].interface.input.class.addSC("WORD", "class-map name");
			enableC.show["policy-map"].interface.addSC("output", "Output policy");
				enableC.show["policy-map"].interface.output.addSC("class", "Show statistics for a indvidual class");
					enableC.show["policy-map"].interface.output.class.addSC("WORD", "class-map name");
	enableC.show.addSC("ppp", "PPP parameters and statistics");
	enableC.show.addSC("printers", "Show LPD printer information");
	enableC.show.addSC("privilege", "Show current privilege level");
	enableC.show.addSC("processes", "Active process statistics");
	enableC.show.addSC("protocols", "Active network routing protocols");
	enableC.show.addSC("qdm", "Show information about QoS Device Manager");
	enableC.show.addSC("qllc", "Display qllc-llc2 and qllc-sdlc conversion information");
	enableC.show.addSC("queue", "Show queue contents");
	enableC.show.addSC("queueing", "Show queueing configuration");
	enableC.show.addSC("radius", "Shows radius information");
	enableC.show.addSC("random-detect-group", "display random-detetct group");
	enableC.show.addSC("registry", "Function registry information");
	enableC.show.addSC("reload", "Scheduled reload information");
	enableC.show.addSC("rhosts", "Remote-host+user equivalences");
	enableC.show.addSC("rif", "RIF cache entries");
	enableC.show.addSC("rmon", "rmon statistics");
	enableC.show.addSC("route-map", "route-map information");
	enableC.show.addSC("rtpspi", "RTP Service Provider Interface");
	enableC.show.addSC("rtr", "Response Time Reporter (RTR)");
	enableC.show.addSC("running-config", "Current operating configuration");
		enableC.show["running-config"].addSC("interface", "Show interface configuration");
			enableC.show["running-config"].interface.addSC("Async", "Async interface");
				enableC.show["running-config"].interface.Async.addSC("<1-129>", "Async interface number");
			enableC.show["running-config"].interface.addSC("BRI", "ISDN Basic Rate Interface");
				enableC.show["running-config"].interface.BRI.addSC("<0-6>", "BRI interface number");
			enableC.show["running-config"].interface.addSC("BVI", "Bridge-Group Virtual Interface");
				enableC.show["running-config"].interface.BVI.addSC("<1-255>", "BVI interface number");
			enableC.show["running-config"].interface.addSC("CTunnel", "CTunnel interface");
				enableC.show["running-config"].interface.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
			enableC.show["running-config"].interface.addSC("Dialer", "Dialer interface");
				enableC.show["running-config"].interface.Dialer.addSC("<0-799>", "Dialer interface number");
			enableC.show["running-config"].interface.addSC("Ethernet", "IEEE 802.3");
				enableC.show["running-config"].interface.Ethernet.addSC("<0-6>", "Ethernet interface number");
			enableC.show["running-config"].interface.addSC("Group-Async", "Async Group interface");
				enableC.show["running-config"].interface["Group-Async"].addSC("<0-129>", "Group-Async interface number");
			enableC.show["running-config"].interface.addSC("Lex", "Lex interface");
				enableC.show["running-config"].interface.Lex.addSC("<0-2147483647>", "Lex interface number");
			enableC.show["running-config"].interface.addSC("Loopback", "Loopback interface");
				enableC.show["running-config"].interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			enableC.show["running-config"].interface.addSC("Multilink", "Multilink-group interface");
				enableC.show["running-config"].interface.Multilink.addSC("<1-2147483647>", "Multilink interface number");
			enableC.show["running-config"].interface.addSC("Null", "Null interface");
				enableC.show["running-config"].interface.Null.addSC("<0-0>", "Null interface number");
			enableC.show["running-config"].interface.addSC("Serial", "Serial");
				enableC.show["running-config"].interface.Serial.addSC("<0-6>", "Serial interface number");
			enableC.show["running-config"].interface.addSC("Tunnel", "Tunnel interface");
				enableC.show["running-config"].interface.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
			enableC.show["running-config"].interface.addSC("Vif", "PGM Multicast Host interface");
				enableC.show["running-config"].interface.Vif.addSC("<1-1>", "Vif interface number");
			enableC.show["running-config"].interface.addSC("Virtual-Template", "Virtual Template interface");
				enableC.show["running-config"].interface["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
			enableC.show["running-config"].interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
				enableC.show["running-config"].interface["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
		enableC.show["running-config"].addSC("map-class", "Show map class information");
			enableC.show["running-config"]["map-class"].addSC("atm", "ATM map class information");
				enableC.show["running-config"]["map-class"].atm.addSC("WORD", "map class name");
			enableC.show["running-config"]["map-class"].addSC("dialer", "Dialer map class information");
				enableC.show["running-config"]["map-class"].dialer.addSC("WORD", "map class name");
			enableC.show["running-config"]["map-class"].addSC("frame-relay", "Frame Relay map class information");
				enableC.show["running-config"]["map-class"]["frame-relay"].addSC("WORD", "map class name");

	enableC.show.addSC("sdllc", "Display sdlc - llc2 conversion information");
	enableC.show.addSC("services", "LAT learned services");
	enableC.show.addSC("sessions", "Information about Telnet connections");
	enableC.show.addSC("settlement", "Show status of settlement");
	enableC.show.addSC("sgbp", "SGBP group information");
	enableC.show.addSC("sgcp", "Display Simple Gateway Control Protocol information");
	enableC.show.addSC("sip-ua", "Show SIP User Agent");
	enableC.show.addSC("slot0:", "display information about slot0: file system");
	enableC.show.addSC("slot1:", "display information about slot1: file system");
	enableC.show.addSC("smds", "SMDS information");
	enableC.show.addSC("smf", "Software MAC filter");
	enableC.show.addSC("smrp", "Simple Multicast Routing Protocol (SMRP) information");
	enableC.show.addSC("sna", "Display SNA host information");
	enableC.show.addSC("snapshot", "Snapshot parameters and statistics");
	enableC.show.addSC("snmp", "snmp statistics");
	enableC.show.addSC("source-bridge", "Source-bridge parameters and statistics");
	enableC.show.addSC("spanning-tree", "Spanning tree topology");
	enableC.show.addSC("srcp", "Display SRCP Protocol information");
	enableC.show.addSC("ssh", "Status of SSH server connections");
	enableC.show.addSC("ssl", "Show SSL command");
	enableC.show.addSC("stacks", "Process stack utilization");
	enableC.show.addSC("standby", "Hot Standby Router Protocol (HSRP) information");
	enableC.show.addSC("startup-config", "Contents of startup configuration");
	enableC.show.addSC("stun", "STUN status and configuration");
	enableC.show.addSC("subscriber-policy", "Subscriber policy");
	enableC.show.addSC("subsys", "Show subsystem information");
	enableC.show.addSC("tacacs", "Shows tacacs+ server statistics");
	enableC.show.addSC("tag-switching", "Tag Switching information (obsolete use \"show mpls ...\")");
	enableC.show.addSC("tarp", "TARP information");
	enableC.show.addSC("tcp", "Status of TCP connections");
	enableC.show.addSC("tech-support", "Show system information for Tech-Support");
	enableC.show.addSC("template", "Template information");
	enableC.show.addSC("terminal", "Display terminal configuration parameters");
	enableC.show.addSC("tgrm", "Trunk Group Resource Mananger info");
	enableC.show.addSC("time-range", "Time range");
	enableC.show.addSC("tn3270", "TN3270 settings");
	enableC.show.addSC("traffic-shape", "traffic rate shaping configuration");
		enableC.show["traffic-shape"].addSC("Async", "Async interface");
		enableC.show["traffic-shape"].addSC("BRI", "ISDN Basic Rate Interface");
		enableC.show["traffic-shape"].addSC("BVI", "Bridge-Group Virtual Interface");
		enableC.show["traffic-shape"].addSC("CTunnel", "CTunnel interface");
		enableC.show["traffic-shape"].addSC("Dialer", "Dialer interface");
		enableC.show["traffic-shape"].addSC("Ethernet", "IEEE 802.3");
		enableC.show["traffic-shape"].addSC("Lex", "Lex interface");
		enableC.show["traffic-shape"].addSC("Loopback", "Loopback interface");
		enableC.show["traffic-shape"].addSC("Multilink", "Multilink-group interface");
		enableC.show["traffic-shape"].addSC("Null", "Null interface");
		enableC.show["traffic-shape"].addSC("Serial", "Serial");
		enableC.show["traffic-shape"].addSC("Tunnel", "Tunnel interface");
		enableC.show["traffic-shape"].addSC("Vif", "PGM Multicast Host interface");
		enableC.show["traffic-shape"].addSC("Virtual-Template", "Virtual Template interface");
		enableC.show["traffic-shape"].addSC("Virtual-TokenRing", "Virtual TokenRing");
		enableC.show["traffic-shape"].addSC("queue", "Show shaping queue contents");
		enableC.show["traffic-shape"].addSC("statistics", "traffic rate shaping statistics");
			enableC.show["traffic-shape"].statistics.addSC("Async", "Async interface");
				enableC.show["traffic-shape"].statistics.Async.addSC("<1-129>", "Async interface number");
			enableC.show["traffic-shape"].statistics.addSC("BRI", "ISDN Basic Rate Interface");
				enableC.show["traffic-shape"].statistics.BRI.addSC("<0-6>", "BRI interface number");
			enableC.show["traffic-shape"].statistics.addSC("BVI", "Bridge-Group Virtual Interface");
				enableC.show["traffic-shape"].statistics.BVI.addSC("<1-255>", "BVI interface number");
			enableC.show["traffic-shape"].statistics.addSC("CTunnel", "CTunnel interface");
				enableC.show["traffic-shape"].statistics.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
			enableC.show["traffic-shape"].statistics.addSC("Dialer", "Dialer interface");
				enableC.show["traffic-shape"].statistics.Dialer.addSC("<0-799>", "Dialer interface number");
			enableC.show["traffic-shape"].statistics.addSC("Ethernet", "IEEE 802.3");
				enableC.show["traffic-shape"].statistics.Ethernet.addSC("<0-6>", "Ethernet interface number");
			enableC.show["traffic-shape"].statistics.addSC("Lex", "Lex interface");
				enableC.show["traffic-shape"].statistics.Lex.addSC("<0-2147483647>", "Lex interface number");
			enableC.show["traffic-shape"].statistics.addSC("Loopback", "Loopback interface");
				enableC.show["traffic-shape"].statistics.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			enableC.show["traffic-shape"].statistics.addSC("Multilink", "Multilink-group interface");
				enableC.show["traffic-shape"].statistics.Multilink.addSC("<1-2147483647>", "Multilink interface number");
			enableC.show["traffic-shape"].statistics.addSC("Null", "Null interface");
				enableC.show["traffic-shape"].statistics.Null.addSC("<0-0>", "Null interface number");
			enableC.show["traffic-shape"].statistics.addSC("Serial", "Serial");
				enableC.show["traffic-shape"].statistics.Serial.addSC("<0-6>", "Serial interface number");
			enableC.show["traffic-shape"].statistics.addSC("Tunnel", "Tunnel interface");
				enableC.show["traffic-shape"].statistics.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
			enableC.show["traffic-shape"].statistics.addSC("Vif", "PGM Multicast Host interface");
				enableC.show["traffic-shape"].statistics.Vif.addSC("<1-1>", "Vif interface number");
			enableC.show["traffic-shape"].statistics.addSC("Virtual-Template", "Virtual Template interface");
				enableC.show["traffic-shape"].statistics["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
			enableC.show["traffic-shape"].statistics.addSC("Virtual-TokenRing", "Virtual TokenRing");
				enableC.show["traffic-shape"].statistics["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
	enableC.show.addSC("translate", "Protocol translation information");
	enableC.show.addSC("translation-rule", "Show translation rule table");
	enableC.show.addSC("ttycap", "Terminal capability tables");
	enableC.show.addSC("users", "Display information about terminal lines");
	enableC.show.addSC("vc-group", "Show VC Group");
	enableC.show.addSC("version", "System hardware and software status");
	enableC.show.addSC("vines", "VINES information");
	enableC.show.addSC("vlans", "Virtual LANs Information");
	enableC.show.addSC("voice", "Voice port configuration & stats");
	enableC.show.addSC("vpdn", "VPDN information");
	enableC.show.addSC("vtemplate", "Virtual Template interface information");
	enableC.show.addSC("whoami", "Info on current tty line");
	enableC.show.addSC("x25", "X.25 information");
	enableC.show.addSC("x29", "X.29 information");
	enableC.show.addSC("xns", "XNS information");
	enableC.show.addSC("xremote", "XRemote statistics");
enableC.addSC("slip", "Start Serial-line IP (SLIP)");
enableC.addSC("squeeze", "Squeeze a filesystem");
	enableC.squeeze.addSC("/nolog", "Squeeze without squeeze logs");
	enableC.squeeze.addSC("/quiet", "Squeeze without progress update");
	enableC.squeeze.addSC("flash:", "Filesystem to be squeezed");
	enableC.squeeze.addSC("slot0:", "Filesystem to be squeezed");
	enableC.squeeze.addSC("slot1:", "Filesystem to be squeezed");
enableC.addSC("ssh", "Open a secure shell client connection");
	enableC.ssh.addSC("-c", "Select encryption algorithm");
	enableC.ssh.addSC("-l", "Log in using this user name");
	enableC.ssh.addSC("-o", "Specify options");
	enableC.ssh.addSC("-p", "Connect to this port");
	enableC.ssh.addSC("WORD", "IP address or hostname of a remote system");
enableC.addSC("start-chat", "Start a chat-script on a line");
	enableC["start-chat"].addSC("WORD", "Chat Script name or regular expression");
enableC.addSC("systat", "Display information about terminal lines");
	enableC.systat.addSC("all", "Include information about inactive ports");
enableC.addSC("tarp", "TARP (Target ID Resolution Protocol) commands");
	enableC.tarp.addSC("query", "Obtain host's Target ID (TID) using its NSAP");
	enableC.tarp.addSC("resolve", "Resolve a TARP Target ID (TID)");
enableC.addSC("tclquit", "Quit Tool Comand Language  shell");
enableC.addSC("tclsh", "Tool Comand Language a shell");
enableC.addSC("telnet", "Open a telnet connection");
	enableC.telnet.addSC("WORD", "IP address or hostname of a remote system");
enableC.addSC("terminal", "Set terminal line parameters");
/*	enableC.terminal.addSC("autohangup", "Automatically hangup when last connection closes");
	enableC.terminal.addSC("autoselect", "Set line to autoselect");
	enableC.terminal.addSC("data-character-bits", "Size of characters being handled");
	enableC.terminal.addSC("databits", "Set number of data bits per character");
	enableC.terminal.addSC("default", "Set a command to its defaults");
	enableC.terminal.addSC("dispatch-character", "Define the dispatch character");
	enableC.terminal.addSC("dispatch-timeout", "Set the dispatch timer");
	enableC.terminal.addSC("domain-lookup", "Enable domain lookups in show commands");
	enableC.terminal.addSC("download", "Put line into 'download' mode");
	enableC.terminal.addSC("editing", "Enable command line editing");
	enableC.terminal.addSC("escape-character", "Change the current line's escape character");
	enableC.terminal.addSC("exec-character-bits", "Size of characters to the command exec");
	enableC.terminal.addSC("flowcontrol", "Set the flow control");
	enableC.terminal.addSC("full-help", "Provide help to unprivileged user");
	enableC.terminal.addSC("help", "Description of the interactive help system");
	enableC.terminal.addSC("history", "Enable and control the command history function");
	enableC.terminal.addSC("hold-character", "Define the hold character");
	enableC.terminal.addSC("international", "Enable international 8-bit character support");
	enableC.terminal.addSC("ip", "IP options");
	enableC.terminal.addSC("keymap-type", "Specify a keymap entry to use");
	enableC.terminal.addSC("lat", "DEC Local Area Transport (LAT) protocol-specific configuration");
//	enableC.terminal.addSC("length", "Set number of lines on a screen");
	enableC.terminal.addSC("monitor", "Copy debug output to the current terminal line");
	enableC.terminal.addSC("no", "Negate a command or set its defaults");
	enableC.terminal.addSC("notify", "Inform users of output from concurrent sessions");
	enableC.terminal.addSC("padding", "Set padding for a specified output character");
	enableC.terminal.addSC("parity", "Set terminal parity");
	enableC.terminal.addSC("rxspeed", "Set the receive speed");
	enableC.terminal.addSC("special-character-bits", "Size of the escape (and other special) characters");
	enableC.terminal.addSC("speed", "Set the transmit and receive speeds");
	enableC.terminal.addSC("start-character", "Define the start character");
	enableC.terminal.addSC("stop-character", "Define the stop character");
	enableC.terminal.addSC("stopbits", "Set async line stop bits");
	enableC.terminal.addSC("telnet", "Telnet protocol-specific configuration");
	enableC.terminal.addSC("terminal-type", "Set the terminal type");
	enableC.terminal.addSC("transport", "Define transport protocols for line");
	enableC.terminal.addSC("txspeed", "Set the transmit speeds");
	enableC.terminal.addSC("width", "Set width of the display terminal");
*/
/*enableC.addSC("test", "Test subsystems, memory, and interfaces");
	enableC.test.addSC("aaa", "AAA Authentication, Authorization and Accounting");
	enableC.test.addSC("interfaces", "Network interfaces");
	enableC.test.addSC("memory", "Non-volatile and/or multibus memory");
	enableC.test.addSC("pas", "Port Adaptor Tests");
	enableC.test.addSC("sgbp", "");
	enableC.test.addSC("pasvc", "PPP over ATM SVC Test Driver");
	enableC.test.addSC("pppoe", "");
	enableC.test.addSC("appletalk", "APPLETALK diagnostic code");
	enableC.test.addSC("call", "Call test commands");
	enableC.test.addSC("crypto", "Test crypto functions");
	enableC.test.addSC("dsp", "Test DSP functions");
	enableC.test.addSC("eigrp", "IPX EIGRP test commands");
	enableC.test.addSC("gssapi", "GSSAPI test code");
	enableC.test.addSC("ifs", "IFS TEST code");
	enableC.test.addSC("ipmobile", "IP Mobility Test commands");
	enableC.test.addSC("playout", "set playout delay configuration");
	enableC.test.addSC("port", "Diagnose voice ports by forcing conditions");
	enableC.test.addSC("spanning-tree", "Spanning Tree Subsystem");
	enableC.test.addSC("ssl", "SSL Test");
	enableC.test.addSC("tone", "TONE");
	enableC.test.addSC("tpu", "TPU test system");
	enableC.test.addSC("translation-rule", "Test translation rule table");
	enableC.test.addSC("vines", "VINES diagnostic code");
	enableC.test.addSC("voice", "Test voice");
*/
enableC.addSC("tn3270", "Open a tn3270 connection");
	enableC.tn3270.addSC("WORD", "IP address or hostname of a remote system");
enableC.addSC("traceroute", "Trace route to destination");
	enableC.traceroute.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("appletalk", "AppleTalk Trace");
		enableC.traceroute.appletalk.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("clns", "ISO CLNS Trace");
		enableC.traceroute.clns.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("ip", "IP Trace");
		enableC.traceroute.ip.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("ipx", "IPX Trace");
		enableC.traceroute.ipx.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("oldvines", "Vines Trace (Cisco)");
		enableC.traceroute.oldvines.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("vines", "Vines Trace (Banyan)");
		enableC.traceroute.vines.addSC("WORD", "Trace route to destination address or hostname");
enableC.addSC("tunnel", "Open a tunnel connection");
	enableC.tunnel.addSC("WORD", "Address or hostname of a remote system");
enableC.addSC("udptn", "Open an udptn connection");
	enableC.udptn.addSC("WORD", "IP address or hostname of a remote system");
enableC.addSC("undebug", "Disable debugging functions (see also 'debug')");
	enableC.undebug.addSC("aaa", "AAA Authentication, Authorization and Accounting");
	enableC.undebug.addSC("access-expression", "Boolean access expression");
	enableC.undebug.addSC("adjacency", "adjacency");
	enableC.undebug.addSC("all", "Enable all debugging");
//	enableC.undebug.addSC("alps", "ALPS debug information");
//	enableC.undebug.addSC("apollo", "Apollo information");
	enableC.undebug.addSC("apple", "Appletalk information");
	enableC.undebug.addSC("arap", "Appletalk Remote Access");
	enableC.undebug.addSC("arp", "IP ARP and HP Probe transactions");
//	enableC.undebug.addSC("aspp", "ASPP information");
	enableC.undebug.addSC("async", "Async interface information");
	enableC.undebug.addSC("backup", "Backup events");
	enableC.undebug.addSC("bri-interface", "bri network interface events");
//	enableC.undebug.addSC("bsc", "BSC information");
//	enableC.undebug.addSC("bstun", "BSTUN information");
//	enableC.undebug.addSC("call", "Call Information");
	enableC.undebug.addSC("call-mgmt", "Call Management");
	enableC.undebug.addSC("callback", "Callback activity");
//	enableC.undebug.addSC("cca", "CCA activity");
//	enableC.undebug.addSC("ccfrf11", "CCFRF11 information");
//	enableC.undebug.addSC("cch323", "CCH323 information");
//	enableC.undebug.addSC("ccsip", "CCSIP information");
//	enableC.undebug.addSC("ccswvoice", "ccswvoice information");
//	enableC.undebug.addSC("cdapi", "CDAPI information");
	enableC.undebug.addSC("cdp", "CDP information");
//	enableC.undebug.addSC("ces-conn", "Connection Manager CES Client Info");
	enableC.undebug.addSC("chat", "Chat scripts activity");
	enableC.undebug.addSC("clns", "CLNS information");
	enableC.undebug.addSC("cls", "CLS Information");
	enableC.undebug.addSC("cns", "CNS Debugging");
	enableC.undebug.addSC("compress", "COMPRESS traffic");
//	enableC.undebug.addSC("condition", "Condition");
	enableC.undebug.addSC("confmodem", "Modem configuration database");
	enableC.undebug.addSC("conn", "Connection Manager information");
	enableC.undebug.addSC("cops", "COPS");
//	enableC.undebug.addSC("cpp", "Cpp information");
	enableC.undebug.addSC("crypto", "Cryptographic subsystem");
	enableC.undebug.addSC("ctunnel", "Generic CTunnel Interface");
	enableC.undebug.addSC("custom-queue", "Custom output queueing");
//	enableC.undebug.addSC("decnet", "DECnet information");
	enableC.undebug.addSC("dhcp", "DHCP client activity");
	enableC.undebug.addSC("dialer", "Dial on Demand");
	enableC.undebug.addSC("dlsw", "Data Link Switching (DLSw) events");
	enableC.undebug.addSC("dnsix", "Dnsix information");
	enableC.undebug.addSC("domain", "Domain Name System");
//	enableC.undebug.addSC("drip", "DRiP debug information");
//	enableC.undebug.addSC("dspu", "DSPU Information");
//	enableC.undebug.addSC("dss", "Debug DSS");
	enableC.undebug.addSC("dxi", "atm-dxi information");
	enableC.undebug.addSC("eigrp", "EIGRP Protocol information");
	enableC.undebug.addSC("entry", "Incoming queue entries");
	enableC.undebug.addSC("ethernet-interface", "Ethernet network interface events");
	enableC.undebug.addSC("fastethernet", "Fast Ethernet interface information");
	enableC.undebug.addSC("fax", "Fax");
	enableC.undebug.addSC("frame-relay", "Frame Relay");
//	enableC.undebug.addSC("fras", "FRAS Debug");
//	enableC.undebug.addSC("fras-host", "FRAS Host Debug");
//	enableC.undebug.addSC("funi", "FUNI interface packets");
//	enableC.undebug.addSC("gssapi", "GSSAPI debugs");
	enableC.undebug.addSC("h225", "H.225 Library Debugging");
	enableC.undebug.addSC("h245", "H.245 Library Debugging");
	enableC.undebug.addSC("interface", "interface");
	enableC.undebug.addSC("ip", "IP information");
	enableC.undebug.addSC("ipx", "Novell/IPX information");
	enableC.undebug.addSC("isdn", "ISDN information");
	enableC.undebug.addSC("isis", "IS-IS Information");
	enableC.undebug.addSC("kerberos", "KERBEROS authentication and authorization");
	enableC.undebug.addSC("lane", "LAN Emulation");
	enableC.undebug.addSC("lapb", "LAPB protocol transactions");
	enableC.undebug.addSC("lapb-ta", "LAPB Terminal Adapter information");
	enableC.undebug.addSC("lat", "LAT Information");
	enableC.undebug.addSC("ldap", "LDAP debug commands");
	enableC.undebug.addSC("lex", "LAN Extender protocol");
	enableC.undebug.addSC("list", "Set interface or/and access list for the next debug command");
	enableC.undebug.addSC("llc2", "LLC2 type II Information");
	enableC.undebug.addSC("lnm", "Lan Network Manager information");
	enableC.undebug.addSC("lnx", "generic qllc/llc2 conversion activity");
	enableC.undebug.addSC("local-ack", "Local ACKnowledgement information");
	enableC.undebug.addSC("management", "Management applications debugging");
//	enableC.undebug.addSC("mdss", "MDSS information");
	enableC.undebug.addSC("mgcp", "Media Gateway Control Protocol");
	enableC.undebug.addSC("mls", "mls debugger information");
	enableC.undebug.addSC("modem", "Modem control/process activation");
	enableC.undebug.addSC("mop", "DECnet MOP server events");
	enableC.undebug.addSC("mpls", "MPLS debug");
//	enableC.undebug.addSC("mpoa", "MPOA debug options");
	enableC.undebug.addSC("nbf", "NetBIOS information");
	enableC.undebug.addSC("ncia", "Native Client Interface Architecture (NCIA) events");
	enableC.undebug.addSC("netbios-name-cache", "NetBIOS name cache tracing");
	enableC.undebug.addSC("nhrp", "NHRP protocol");
	enableC.undebug.addSC("ntp", "NTP information");
	enableC.undebug.addSC("nvram", "Debug NVRAM behavior");
	enableC.undebug.addSC("packet", "Log unknown packets");
	enableC.undebug.addSC("pad", "X25 PAD protocol");
	enableC.undebug.addSC("ppp", "PPP (Point to Point Protocol) information");
	enableC.undebug.addSC("printer", "LPD printer protocol");
	enableC.undebug.addSC("priority", "Priority output queueing");
	enableC.undebug.addSC("probe", "HP Probe Proxy Requests");
	enableC.undebug.addSC("qdm", "QoS Device Manager");
	enableC.undebug.addSC("qllc", "qllc debug information");
	enableC.undebug.addSC("radius", "RADIUS protocol");
	enableC.undebug.addSC("ras", "H.323 RAS Library");
//	enableC.undebug.addSC("rif", "RIF cache transactions");
	enableC.undebug.addSC("rscmon", "Resource Monitor");
//	enableC.undebug.addSC("rtpspi", "RTP Service Provider Interface.");
	enableC.undebug.addSC("rtr", "RTR Monitor Information");
	enableC.undebug.addSC("sdlc", "SDLC information");
	enableC.undebug.addSC("sdllc", "SDLLC media translation");
	enableC.undebug.addSC("serial", "Serial interface information");
//	enableC.undebug.addSC("sgbp", "SGBP debugging");
	enableC.undebug.addSC("sgcp", "Simple Gateway Control Protocol");
	enableC.undebug.addSC("smf", "Software MAC filter");
//	enableC.undebug.addSC("smrp", "SMRP information");
	enableC.undebug.addSC("sna", "SNA Information");
	enableC.undebug.addSC("snapshot", "Snapshot activity");
	enableC.undebug.addSC("snmp", "SNMP information");
	enableC.undebug.addSC("source", "Source bridging information");
	enableC.undebug.addSC("spanning-tree", "Spanning tree debugging");
//	enableC.undebug.addSC("srcp", "Simple Resource Coordination Protocol");
	enableC.undebug.addSC("ssl", "SSL Debug command");
	enableC.undebug.addSC("standby", "Hot standby protocol");
//	enableC.undebug.addSC("stun", "STUN information");
	enableC.undebug.addSC("tacacs", "TACACS authentication and authorization");
	enableC.undebug.addSC("tag-switching", "Tag Switching (obsolete use \"debug mpls ...\")");
	enableC.undebug.addSC("tarp", "TARP information");
	enableC.undebug.addSC("tbridge", "Transparent Bridging");
	enableC.undebug.addSC("tccs", "Transparent CCS information");
	enableC.undebug.addSC("tdm", "TDM connection information");
	enableC.undebug.addSC("telnet", "Incoming telnet connections");
	enableC.undebug.addSC("template", "Template activity");
	enableC.undebug.addSC("tftp", "TFTP debugging");
	enableC.undebug.addSC("tgrm", "Trunk Group Resource Manager info");
//	enableC.undebug.addSC("token", "Token Ring information");
	enableC.undebug.addSC("translate", "Protocol translation events");
	enableC.undebug.addSC("translation", "translation rule information");
	enableC.undebug.addSC("tsp", "Telephony Service information");
	enableC.undebug.addSC("tunnel", "Generic Tunnel Interface");
//	enableC.undebug.addSC("udptn", "UDPtn async data transport");
	enableC.undebug.addSC("v120", "V120 information");
	enableC.undebug.addSC("vines", "VINES information");
	enableC.undebug.addSC("vlan", "vLAN information");
	enableC.undebug.addSC("voice", "VOICE information");
	enableC.undebug.addSC("voip", "VOIP information");
	enableC.undebug.addSC("vpdn", "VPDN information");
	enableC.undebug.addSC("vpm", "Voice Port Module SPI information");
	enableC.undebug.addSC("vprofile", "Virtual Profile information");
	enableC.undebug.addSC("vtemplate", "Virtual Template information");
	enableC.undebug.addSC("vtsp", "Voice Telephony Call Control information");
	enableC.undebug.addSC("x25", "X.25, CMNS and XOT information");
	enableC.undebug.addSC("x28", "X28 mode");
	enableC.undebug.addSC("xcctsp", "External Call Control TSP information");
	enableC.undebug.addSC("xns", "XNS information");
	enableC.undebug.addSC("xremote", "XREMOTE");
enableC.addSC("verify", "Verify a file");
	enableC.verify.addSC("flash:", "File to be verified");
	enableC.verify.addSC("slot0:", "File to be verified");
	enableC.verify.addSC("slot1:", "File to be verified");
enableC.addSC("where", "List active connections");
enableC.addSC("which-route", "Do OSI route table lookup and display results");
	enableC["which-route"].addSC("XX.XXXX. ... .XXX.XX", "Lookup route to OSI destination address or host name");
enableC.addSC("write", "Write running configuration to memory, network, or terminal");
	enableC.write.addSC("erase", "Erase NV memory");
	enableC.write.addSC("memory", "Write to NV memory");
	enableC.write.addSC("network", "Write to network TFTP server");
	enableC.write.addSC("terminal", "Write to terminal");
enableC.addSC("x28", "Become an X.28 PAD");
	enableC.x28.addSC("debug", "Turn on Debug Messages for X28 Mode");
	enableC.x28.addSC("dns", "Enable DNS based mnemonic address resolution");
	enableC.x28.addSC("escape", "Set the string to escape from X28 PAD mode");
	enableC.x28.addSC("noescape", "Never exit x28 mode (use with caution)");
	enableC.x28.addSC("nuicud", "All calls with NUI, are normal charge with the NUI placed in Call User Data");
	enableC.x28.addSC("profile", "Use a defined X.3 Profile");
	enableC.x28.addSC("reverse", "All calls default to reverse charge");
	enableC.x28.addSC("verbose", "Turn on Verbose Messages for X28 Mode");
enableC.addSC("x3", "Set X.3 parameters on PAD");
	enableC.x3.addSC("<0-22>:<0-255>", "X.3 PAD parameters and values");
enableC.addSC("xremote", "Enter XRemote mode");
	enableC.xremote.addSC("lat", "Start up a LAT session");
	enableC.xremote.addSC("xdm", "Start up a XDM session");
