| 3.1 |  | Configuring a Router |
| 3.1.2 |  | Configuring a router name |

| A router should be given a unique name as one of the first configuration tasks. This task is accomplished in global configuration mode using the following commands: Router(config)#hostname Tokyo Tokyo(config)# As soon as the Enter key is pressed, the prompt changes from the default host name (Router) to the newly configured host name, which is Tokyo in the example.
| Lab Activity Lab Exercise: Command Modes and Router Identification This lab is to identify basic router modes of user EXEC and privileged EXEC and to use commands to enter specific modes.
| Web Links Basic System Management Commands http://www.cisco.com/en/US/products/sw/ iosswrel/ps1835/products_command_reference_ chapter09186a00800ca748.html#1018259