
routerAFC.addSC("aggregate-address", "Configure BGP aggregate entries");
routerAFC.addSC("auto-summary", "Enable automatic network number summarization");
routerAFC.addSC("bgp", "BGP specific commands");
routerAFC.addSC("default", "Set a command to its defaults");
routerAFC.addSC("default-information", "Control distribution of default information");
routerAFC.addSC("default-metric", "Set metric of redistributed routes");
routerAFC.addSC("distance", "Define an administrative distance");
routerAFC.addSC("distribute-list", "Filter networks in routing u");
routerAFC.addSC("exit-address-family", "Exit from Address Family configuration mode");
routerAFC.addSC("help", "Description of the interactive help system");
routerAFC.addSC("maximum-paths", "Forward packets over multiple paths");
routerAFC.addSC("neighbor", "Specify a neighbor router");
routerAFC.addSC("network", "Specify a network to announce via BGP");
	routerAFC.network.addSC("A.B.C.D", "Network number");
		routerAFC.network["A.B.C.D"].addSC("backdoor", "Specify a BGP backdoor route");
		routerAFC.network["A.B.C.D"].addSC("mask", "Network mask");
			routerAFC.network["A.B.C.D"].mask.addSC("A.B.C.D", "Network mask");
				routerAFC.network["A.B.C.D"].mask["A.B.C.D"].addSC("backdoor", "Specify a BGP backdoor route");
		routerAFC.network["A.B.C.D"].addSC("route-map", "Route-map to modify the attributes");
			routerAFC.network["A.B.C.D"]["route-map"].addSC("WORD", "Name of the route map");
				routerAFC.network["A.B.C.D"]["route-map"].WORD.addSC("backdoor", "Specify a BGP backdoor route");
		routerAFC.network["A.B.C.D"].addSC("weight", "Set BGP weight for network");
			routerAFC.network["A.B.C.D"].weight.addSC("<0-65535>", "absolute weight");
				routerAFC.network["A.B.C.D"].weight["<0-65535>"].addSC("backdoor", "Specify a BGP backdoor route");
routerAFC.addSC("no", "Negate a command or set its defaults");
	routerAFC.no.addSC("aggregate-address", "Configure BGP aggregate entries");
	routerAFC.no.addSC("auto-summary", "Enable automatic network number summarization");
	routerAFC.no.addSC("bgp", "BGP specific commands");
	routerAFC.no.addSC("default-information", "Control distribution of default information");
	routerAFC.no.addSC("default-metric", "Set metric of redistributed routes");
	routerAFC.no.addSC("distance", "Define an administrative distance");
	routerAFC.no.addSC("distribute-list", "Filter networks in routing updates");
	routerAFC.no.addSC("help", "Description of the interactive help system");
	routerAFC.no.addSC("maximum-paths", "Forward packets over multiple paths");
	routerAFC.no.addSC("neighbor", "Specify a neighbor router");
	routerAFC.no.addSC("network", "Specify a network to announce via BGP");
routerAFC.addSC("redistribute", "Redistribute information from another routing protocol");
routerAFC.addSC("summary-address", "Configure IP address summaries");
routerAFC.addSC("synchronization", "Perform IGP synchronization");
routerAFC.addSC("table-map", "Map external entry attributes into routing table");
