   Windows 98, Windows 98 SE

   Introduction:
   -------------
   This document describes the procedure to install Windows 98/98 SE
   driver for Planet ENW-9503/-9504 PCI Fast Ethernet adapter.

   Location of Driver :   \Win98\ENW9503.SYS

   Installing driver procedure on Microsoft Win98/Win98 SE :
   -------------------------------------------------------------------
      Before you start with the installation process, make sure that your
      adapter should be properly installed in your PCI bus slot.
      Executing Win98/Win98 SE, it will auto-detect your system 
      configuration and find the adapter hardware.  

      1. When Windows 98/98 SE prompts with "PCI Ethernet Controller" in
         "New Hardware Found" dialog box, click the "Next" button.

      2. Select "Search for the best driver for your device (Recommended)"
         form the "Add New Hardware Wizard" dialog box, then click the
         "Next" button.

      3. Insert the Planet ENW9503 driver disk into drive A and specify
         the setup file pathname A:\Win98, then click the "Next" button. 

      4. Windows 98/98SE will prompt with "ENW-950x RTL-based PCI Fast
         Ethernet Adapter" in the "Add New Hardware Wizard" dialog box.

      5. Click the "Next" button in the "Add New Hardware Wizard" dialog
         box,then Windows 98 will copy the driver(.sys) from A:\Win98
         to the C:\WINDOWS\SYSTEM directory and the driver(.inf) from
         A:\Win98 to the C:\WINDOWS\INF directory.

      6. When Windows prompts with "ENW-950x RTL-based PCI Fast Ethernet
         Adapter" in the "Add New Hardware Wizard" dialog box, click the
         "Finish" button.

      7. Win98/Win98 SE will finish the other installation procedure
         automatically, then you restart the system.



