Modules: | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | CS | All |
Module 10: Intermediate TCP/IP
| Command | Command Description | Command Syntax
10.1.6 | ip http server | To enable a Cisco router to be configured from a browser using the Cisco IOS ClickStart software, and to enable any router to be monitored or have its configuration modified from a browser using the Cisco Web browser interface, use the ip http server global configuration command. To disable this feature, use the no form of this command. | ip http server

| Close Window |

| All contents copyright © 2003 Cisco Systems, Inc. All rights reserved.